 ORAN.WG3.E2SM-RC-v01.03

\\

Technical Specification

O-RAN Working Group 3

Near-Real-time RAN Intelligent Controller  
E2 Service Model (E2SM), RAN Control

Copyright © 2022 by the O-RAN ALLIANCE e.V.

The copying or incorporation into any other work of part or all of the material available in this specification in any form without the prior written permission of O-RAN ALLIANCE e.V. is prohibited, save that you may print or download extracts of the material of this specification for your personal use, or copy the material of this specification for the purpose of sending to individual third parties for their information provided that you acknowledge O-RAN ALLIANCE as the source of the material and that you inform the third party that these conditions apply to them and that they must comply with them.

O-RAN ALLIANCE e.V., Buschkauler Weg 27, 53347 Alfter, Germany

Contents

[1 Scope 6](#_Toc110274506)

[2 References 7](#_Toc110274507)

[3 Definitions and Abbreviations 8](#_Toc110274508)

[3.1 Definitions 8](#_Toc110274509)

[3.2 Abbreviations 8](#_Toc110274510)

[4 General 9](#_Toc110274511)

[4.1 Procedure Specification Principles 9](#_Toc110274512)

[4.2 Forwards and Backwards Compatibility 9](#_Toc110274513)

[4.3 Specification Notations 9](#_Toc110274514)

[4.4 Identifiers 10](#_Toc110274515)

[5 E2SM Services 11](#_Toc110274516)

[6 RAN Function Service Model Description 12](#_Toc110274517)

[6.1 RAN Function Overview 12](#_Toc110274518)

[6.2 RAN Function exposure services 12](#_Toc110274519)

[6.2.1 REPORT service 12](#_Toc110274520)

[6.2.2 INSERT service 12](#_Toc110274521)

[6.2.3 CONTROL service 13](#_Toc110274522)

[6.2.4 POLICY service 13](#_Toc110274523)

[6.3 REPORT service description 14](#_Toc110274524)

[6.4 INSERT service description 14](#_Toc110274525)

[6.5 CONTROL service description 15](#_Toc110274526)

[6.6 POLICY service description 15](#_Toc110274527)

[6.6.1 Overview 15](#_Toc110274528)

[6.6.2 Policy approach "Control" 15](#_Toc110274529)

[6.6.3 Policy Approach "Offset" 16](#_Toc110274530)

[7 RAN Function Description 16](#_Toc110274531)

[7.1 Description 16](#_Toc110274532)

[7.2 RAN Function name 17](#_Toc110274533)

[7.3 Event trigger definition styles 17](#_Toc110274534)

[7.3.1 RIC Event trigger definition IE style list 17](#_Toc110274535)

[7.3.2 RIC Event trigger definition IE style 1: Message Event 17](#_Toc110274536)

[7.3.3 RIC Event trigger definition IE style 2: Call Process Breakpoint 17](#_Toc110274537)

[7.3.4 RIC Event trigger definition IE style 3: E2 Node Information Change 19](#_Toc110274538)

[7.3.5 RIC Event trigger definition IE style 4: UE Information Change 19](#_Toc110274539)

[7.3.6 RIC Event trigger definition IE style 5: On Demand 20](#_Toc110274540)

[7.4 Supported RIC REPORT Services 20](#_Toc110274541)

[7.4.1 REPORT Service style list 20](#_Toc110274542)

[7.4.2 REPORT Service Style 1: Message Copy 20](#_Toc110274543)

[7.4.3 REPORT Service Style 2: Call Process Outcome 21](#_Toc110274544)

[7.4.4 REPORT Service Style 3: E2 Node Information. 22](#_Toc110274545)

[7.4.5 REPORT Service Style 4: UE Information 22](#_Toc110274546)

[7.4.6 REPORT Service Style 5: On Demand Report 23](#_Toc110274547)

[7.5 Supported RIC INSERT Services 24](#_Toc110274548)

[7.5.1 INSERT Service style list 24](#_Toc110274549)

[7.5.2 INSERT Service Style 1: Radio Bearer Control Request 24](#_Toc110274550)

[7.5.3 INSERT Service Style 2: Radio Resource Allocation Control Request 26](#_Toc110274551)

[7.5.4 INSERT Service Style 3: Connected Mode Mobility Request 27](#_Toc110274552)

[7.5.5 INSERT Service Style 4: Radio Access Control Request 28](#_Toc110274553)

[7.5.6 INSERT Service Style 5: Dual Connectivity Control Request 29](#_Toc110274554)

[7.5.7 INSERT Service Style 6: Carrier Aggregation Control Request 30](#_Toc110274555)

[7.5.8 INSERT Service Style 7: Idle Mode Mobility Control Request 31](#_Toc110274556)

[7.5.9 INSERT Service Style 255: Multiple Actions Control Request 32](#_Toc110274557)

[7.6 Supported RIC CONTROL Services 33](#_Toc110274558)

[7.6.1 CONTROL Service Style Types 33](#_Toc110274559)

[7.6.2 CONTROL Service Style 1: Radio Bearer Control 33](#_Toc110274560)

[7.6.3 CONTROL Service Style 2: Radio Resource Allocation Control 35](#_Toc110274561)

[7.6.4 CONTROL Service Style 3: Connected Mode Mobility 37](#_Toc110274562)

[7.6.5 CONTROL Service Style 4: Radio Access Control 38](#_Toc110274563)

[7.6.6 CONTROL Service Style 5: Dual Connectivity Control 40](#_Toc110274564)

[7.6.7 CONTROL Service Style 6: Carrier Aggregation Control 41](#_Toc110274565)

[7.6.8 CONTROL Service Style 7: Idle Mode Mobility Control 43](#_Toc110274566)

[7.6.9 CONTROL Service Style 8: UE information and assignment 44](#_Toc110274567)

[7.6.10 CONTROL Service Style 255: Multiple Actions Control 45](#_Toc110274568)

[7.6.11 CONTROL Service Style 9: Measurement Reporting Configuration Control 46](#_Toc110274569)

[7.7 Supported RIC POLICY Services 47](#_Toc110274570)

[7.7.1 POLICY Service style list 47](#_Toc110274571)

[7.7.2 POLICY Service Style 1: Radio Bearer Control 48](#_Toc110274572)

[7.7.3 POLICY Service Style 2: Radio Resource Allocation Control 49](#_Toc110274573)

[7.7.4 POLICY Service Style 3: Connected Mode Mobility Control 49](#_Toc110274574)

[7.7.5 POLICY Service Style 4: Radio Access Control 50](#_Toc110274575)

[7.7.6 POLICY Service Style 5: Dual Connectivity (DC) Control 51](#_Toc110274576)

[7.7.7 POLICY Service Style 6: Carrier Aggregation (CA) Control 52](#_Toc110274577)

[7.7.8 POLICY Service Style 7: Idle Mode Mobility Control 53](#_Toc110274578)

[7.7.9 POLICY Service Style 8: Measurement Reporting Configuration Control 53](#_Toc110274579)

[7.8 Supported RIC Service Styles and E2SM IE Formats 54](#_Toc110274580)

[8 RAN Parameter assignments 56](#_Toc110274581)

[8.0 Approach 56](#_Toc110274582)

[8.1 RAN parameters for Event Trigger 56](#_Toc110274583)

[8.1.1 Common RAN Parameters 56](#_Toc110274584)

[8.1.2 RAN Parameters for Call Process Breakpoint 106](#_Toc110274585)

[8.1.3 RAN Parameters for UE Identification 161](#_Toc110274586)

[8.1.4 RAN Parameters for Cell Identification 163](#_Toc110274587)

[8.1.5 UE Events 163](#_Toc110274588)

[8.2 RAN parameters for REPORT services 163](#_Toc110274589)

[8.2.1 RAN Parameters for Report Service Style 1 163](#_Toc110274590)

[8.2.2 RAN Parameters for Report Service Style 2 165](#_Toc110274591)

[8.2.3 RAN Parameters for Report Service Style 3 165](#_Toc110274592)

[8.2.4 RAN Parameters for Report Service Style 4 167](#_Toc110274593)

[8.2.5 RAN Parameters for Report Service Style 5 168](#_Toc110274594)

[8.3 RAN parameters for INSERT services 168](#_Toc110274595)

[8.3.1 Approach 168](#_Toc110274596)

[8.3.2 Radio Bearer Control request 168](#_Toc110274597)

[8.3.3 Radio Resource Allocation request 169](#_Toc110274598)

[8.3.4 Connected Mode Mobility Control Request 169](#_Toc110274599)

[8.3.5 Radio Access Control request 169](#_Toc110274600)

[8.3.6 Dual Connectivity Control request 170](#_Toc110274601)

[8.3.7 Carrier Aggregation Control request 170](#_Toc110274602)

[8.3.8 Idle Mode Mobility Control request 170](#_Toc110274603)

[8.3.9 Common RAN Parameters for INSERT Service styles 170](#_Toc110274604)

[8.3.10 Indication Semantics Description for interpretation by the RIC 171](#_Toc110274605)

[8.4 RAN Parameters for Control Actions 171](#_Toc110274606)

[8.4.1 Approach 171](#_Toc110274607)

[8.4.2 Radio Bearer Control 171](#_Toc110274608)

[8.4.3 Radio Resource Allocation Control 181](#_Toc110274609)

[8.4.4 Connected Mode Mobility Control 185](#_Toc110274610)

[8.4.5 Radio Access Control 192](#_Toc110274611)

[8.4.6 Dual Connectivity Control 200](#_Toc110274612)

[8.4.7 Carrier Aggregation Control 211](#_Toc110274613)

[8.4.8 Idle Mode Mobility Control 213](#_Toc110274614)

[8.4.9 UE identification and assignment 214](#_Toc110274615)

[8.4.10 Measurement Reporting Configuration Control 215](#_Toc110274616)

[8.5 RAN parameters for POLICY services 257](#_Toc110274617)

[8.5.1 Approach 257](#_Toc110274618)

[8.5.1A Common RAN Parameters for POLICY services 257](#_Toc110274619)

[8.5.2 Radio Bearer Control 258](#_Toc110274620)

[8.5.3 Radio Resource Allocation Control 260](#_Toc110274621)

[8.5.4 Connected Mode Mobility Control 262](#_Toc110274622)

[8.5.5 Radio Access Control 267](#_Toc110274623)

[8.5.6 Dual Connectivity Control 269](#_Toc110274624)

[8.5.7 Carrier Aggregation Control 272](#_Toc110274625)

[8.5.8 Idle Mode Mobility Control 274](#_Toc110274626)

[8.5.9 Measurement Reporting Configuration Control 275](#_Toc110274627)

[9 Elements for E2SM Service Model 276](#_Toc110274628)

[9.1 General 276](#_Toc110274629)

[9.2 Message Functional Definition and Content 276](#_Toc110274630)

[9.2.1 Messages for RIC Functional procedures 276](#_Toc110274631)

[9.2.2 Messages for RIC Global Procedures 290](#_Toc110274632)

[9.3 Information Element definitions 300](#_Toc110274633)

[9.3.1 General 300](#_Toc110274634)

[9.3.2 RAN Function Name 300](#_Toc110274635)

[9.3.3 RIC Style Type 300](#_Toc110274636)

[9.3.4 RIC Style Name 300](#_Toc110274637)

[9.3.5 RIC Format Type 300](#_Toc110274638)

[9.3.6 Control Action ID 300](#_Toc110274639)

[9.3.7 Control Action Name 300](#_Toc110274640)

[9.3.8 RAN Parameter ID 301](#_Toc110274641)

[9.3.9 RAN Parameter Name 301](#_Toc110274642)

[9.3.10 UE ID 301](#_Toc110274643)

[9.3.11 RAN Parameter Value Type 302](#_Toc110274644)

[9.3.12 RAN Parameter Structure 302](#_Toc110274645)

[9.3.13 RAN Parameter List 303](#_Toc110274646)

[9.3.14 RAN Parameter Value 303](#_Toc110274647)

[9.3.15 Call Process Type ID 303](#_Toc110274648)

[9.3.16 Insert Indication ID 303](#_Toc110274649)

[9.3.17 Insert Indication Name 303](#_Toc110274650)

[9.3.18 RAN Call Process ID 304](#_Toc110274651)

[9.3.19 Call Process Type Name 304](#_Toc110274652)

[9.3.20 Policy Action 304](#_Toc110274653)

[9.3.21 Event Trigger Condition ID 304](#_Toc110274654)

[9.3.22 Event Trigger ID for UE 304](#_Toc110274655)

[9.3.23 Event Trigger ID for UE Event 305](#_Toc110274656)

[9.3.24 Event Trigger ID for Cell 305](#_Toc110274657)

[9.3.25 Logical OR 305](#_Toc110274658)

[9.3.26 Event Trigger UE Information 305](#_Toc110274659)

[9.3.27 Event Trigger Cell Information 306](#_Toc110274660)

[9.3.28 Event Trigger UE Event Information 306](#_Toc110274661)

[9.3.29 RAN Parameter Conditional Criteria Definition 307](#_Toc110274662)

[9.3.30 RAN Parameter Test 307](#_Toc110274663)

[9.3.31 RAN Parameter Test Condition 307](#_Toc110274664)

[9.3.32 Network Interface Type 308](#_Toc110274665)

[9.3.33 Network Interface Identifier 308](#_Toc110274666)

[9.3.34 Network Interface Message ID 308](#_Toc110274667)

[9.3.35 RRC Message ID 308](#_Toc110274668)

[9.3.36 Cell Global ID 308](#_Toc110274669)

[9.3.37 RRC State 309](#_Toc110274670)

[9.3.38 Neighbour Relation Information 310](#_Toc110274671)

[9.3.39 Serving Cell PCI 311](#_Toc110274672)

[9.3.40 Serving Cell ARFCN 311](#_Toc110274673)

[9.3.41 NR CGI 311](#_Toc110274674)

[9.3.42 NR PCI 311](#_Toc110274675)

[9.3.43 NR TAC 311](#_Toc110274676)

[9.3.44 NR Frequency Info 311](#_Toc110274677)

[9.3.45 E-UTRA CGI 311](#_Toc110274678)

[9.3.46 E-UTRA PCI 311](#_Toc110274679)

[9.3.47 E-UTRA TAC 311](#_Toc110274680)

[9.3.48 E-UTRA ARFCN 311](#_Toc110274681)

[9.3.49 Call Process Breakpoint ID 311](#_Toc110274682)

[9.3.50 Call Process Breakpoint Name 312](#_Toc110274683)

[9.3.51 RAN Parameter Definition 312](#_Toc110274684)

[9.4 Information Element Abstract Syntax (with ASN.1) 313](#_Toc110274685)

[9.4.1 General 313](#_Toc110274686)

[9.4.2 Information Element Definitions 313](#_Toc110274687)

[9.5 Message transfer syntax 329](#_Toc110274688)

[10 Handling of Unknown, Unforeseen and Erroneous Protocol Data 329](#_Toc110274689)

[Annex A: Examples on IE Contents 330](#_Toc110274690)

[A.1 Introduction 330](#_Toc110274691)

[A.2 Connected mode mobility based on UE measurement report 330](#_Toc110274692)

[A.2.1 Assumptions 330](#_Toc110274693)

[A.2.2 Solution using RIC Services Insert and Control 330](#_Toc110274694)

[A.2.3 Solution using RIC Service Policy ("Offset" based approach) 330](#_Toc110274695)

[Revision History 334](#_Toc110274696)

[History 336](#_Toc110274697)

# 1 Scope

This Technical Specification has been produced by the O-RAN Alliance.

The contents of the present document are subject to continuing work within O-RAN and may change following formal O-RAN approval. Should the O-RAN Alliance modify the contents of the present document, it will be re-released by O-RAN with an identifying change of release date and an increase in version number as follows:

Release x.y.z

where:

x the first digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc. (the initial approved document will have x=01).

y the second digit is incremented when editorial only changes have been incorporated in the document.

z the third digit included only in working versions of the document indicating incremental changes during the editing process.

The present document specifies the E2 Service Model (E2SM) for the Near RT RIC RAN Control interaction.

# 2 References

[1] 3GPP TR 21.905: “Vocabulary for 3GPP Specifications”.

[2] O-RAN Working Group 3, Near-Real-time RAN Intelligent Controller, Architecture & E2 General Aspects and Principles (E2GAP)

[3] ORAN Working Group 3, Near-Real-time RAN Intelligent Controller, E2 Application Protocol (E2AP).

[4] O-RAN Working Group 3, Near-Real-time RAN Intelligent Controller, E2 Service Model (E2SM)

[5] 3GPP TR 25.921: "Guidelines and principles for protocol description and error handling".

[6] ITU-T Recommendation X.680 (2002-07): "Information technology – Abstract Syntax Notation One (ASN.1): Specification of basic notation".

[7] ITU-T Recommendation X.681 (2002-07): "Information technology – Abstract Syntax Notation One (ASN.1): Information object specification".

[8] ITU-T Recommendation X.691 (2002-07): "Information technology - ASN.1 encoding rules - Specification of Packed Encoding Rules (PER) "

[9] Reserved

[10] TS 38.410: “NG-RAN; NG general aspects and principles”.

[11] TS 38.413: “NG-RAN; NG Application Protocol (NGAP)”.

[12] Reserved

[13] TS 36.413: “E-UTRAN; S1 Application Protocol (S1AP)”.

[14] TS 38.420: “NG-RAN; Xn general aspects and principles”.

[15] TS 38.423: “NG-RAN; Xn Application Protocol (XnAP)”.

[16] TS 36.420: “E-UTRAN; X2 general aspects and principles”.

[17] TS 36.423: “E-UTRAN; X2 Application Protocol (X2AP)”.

[18] TS 38.470: “NG-RAN; F1 general aspects and principles”.

[19] TS 38.473: “NG-RAN; F1 Application Protocol (F1AP)”.

[20] TS 38.460: “NG-RAN; E1 general aspects and principles”.

[21] TS 38.463: “NG-RAN; E1 Application Protocol (E1AP)”.

[22] TS 38.331: “NR; Radio Resource Control (RRC) Protocol Specification”.

[23] TS 36.331: “E-UTRA; Radio Resource Control (RRC) Protocol Specification”.

[24] TS 38.323: “NR; Packet Data Convergence Protocol (PDCP) specification”.

[25] TS 38.322: “NR; Radio Link Control (RLC) protocol specification”.

[26] TS 38.321: “NR; Medium Access Control (MAC) protocol specification”.

[27] TS 25.321: “Medium Access Control (MAC) protocol specification”.

[28] TS 28.552: “Management and orchestration 5G performance measurements”.

[29] Reserved

[30] IETF RFC 5905 (2010-06): “Network Time Protocol Version 4: Protocol and Algorithms Specification”

[31] TS 37.340: “E-UTRA and NR Multiconnectivity Stage 2”.

# 3 Definitions and Abbreviations

## 3.1 Definitions

**E2 Node**: as defined in E2GAP [2].

**RAN Function**: as defined in E2GAP [2]

**E2 Service Model**: The description of the Services exposed by a specific RAN function within an E2 node over the E2 interface towards the Near-RT RIC.

**SpCell**: as defined in TS 37.340 [31].

## 3.2 Abbreviations

For the purposes of the present document, the following abbreviations apply.

O-CU O-RAN Central Unit

O-CU-CP O-RAN Central Unit – Control Plane

O-CU-UP O-RAN Central Unit – User Plane

O-DU O-RAN Distributed Unit

Near-RT RICNear-real-time RAN Intelligent Controller

RC RAN Control

# 4 General

## 4.1 Procedure Specification Principles

The principle for specifying the procedure logic is to specify the functional behaviour of the terminating node exactly and completely. Any rule that specifies the behaviour of the originating node shall be possible to be verified with information that is visible within the system.

The following specification principles have been applied for the procedure text in clause 8:

- The procedure text discriminates between:

1) Functionality which "shall" be executed.

The procedure text indicates that the receiving node "shall" perform a certain function Y under a certain condition. If the receiving node supports procedure X but cannot perform functionality Y requested in the REQUEST message of a Class 1 EP, the receiving node shall respond with the message used to report unsuccessful outcome for this procedure, containing an appropriate cause value.

2) Functionality which "shall, if supported" be executed.

The procedure text indicates that the receiving node "shall, if supported," perform a certain function Y under a certain condition. If the receiving node supports procedure X, but does not support functionality Y, the receiving node shall proceed with the execution of the EP, possibly informing the requesting node about the not supported functionality.

- Any required inclusion of an optional IE in a response message is explicitly indicated in the procedure text. If the procedure text does not explicitly indicate that an optional IE shall be included in a response message, the optional IE shall not be included. For requirements on including *Criticality Diagnostics* IE, see clause 10.

## 4.2 Forwards and Backwards Compatibility

The forwards and backwards compatibility of the protocol is assured by a mechanism where all current and future messages, and IEs or groups of related IEs, include ID and criticality fields that are coded in a standard format that will not be changed in the future. These parts can always be decoded regardless of the standard version.

## 4.3 Specification Notations

For the purposes of the present document, the following notations apply:

Service when referring to a Service in the specification the **SERVICE NAME** is written with upper case characters and in bold followed by the word "service", e.g. **REPORT** service.

Procedure When referring to an elementary procedure in the specification the Procedure Name is written with the first letters in each word in upper case characters followed by the word "procedure", e.g. Handover Preparation procedure.

Message When referring to a message in the specification the MESSAGE NAME is written with all letters in upper case characters followed by the word "message", e.g. HANDOVER REQUEST message.

IE When referring to an information element (IE) in the specification the *Information Element Name* is written with the first letters in each word in upper case characters and all letters in Italic font followed by the abbreviation "IE", e.g. *E-RAB ID* IE.

Value of an IE When referring to the value of an information element (IE) in the specification the "Value" is written as it is specified in the specification enclosed by quotation marks, e.g. "Value".

## 4.4 Identifiers

For the purposes of the present document, the following identifiers are defined:

Style Type The identifier used to nominate a specific approach or Style used to exposing a given RIC Service (REPORT, INSERT, CONTROL and POLICY). The same E2SM may support more than one Style for each RIC Service.

Format Type The identifier used to nominate a specific formatting approach used to encode one of the E2AP IEs defined in this E2SM. The same E2SM may support more than one encoding Formats for each E2AP IE and each E2AP IE message encoding Format may be used by one or more RIC Service Styles.

# 5 E2SM Services

As defined in E2 General Aspects and Principles [1], a given RAN Function offers a set of services to be exposed over the E2 (**REPORT**, **INSERT**, **CONTROL** and/or **POLICY**) using E2AP [3] defined procedures. Each of the E2AP Procedures listed in table 5-1 contains specific E2 Node RAN Function dependent Information Elements (IEs).

Table 5-1: Relationship RAN Function specific E2AP Information elements and E2AP Procedures

|  |  |  |
| --- | --- | --- |
| RAN Function specific E2AP Information Elements | E2AP Information Element reference | Related E2AP Procedures |
| *RIC Event Trigger Definition* IE | E2AP [3] Section 9.2.9 | RIC Subscription |
| *RIC Action Definition* IE | E2AP [3] Section 9.2.12 | RIC Subscription |
| *RIC Indication Header* IE | E2AP [3] Section 9.2.17 | RIC Indication |
| *RIC Indication Message* IE | E2AP [3] Section 9.2.16 | RIC Indication |
| *RIC Call Process ID* IE | E2AP [3] Section 9.2.18 | RIC Indication  RIC Control |
| *RIC Control Header* IE | E2AP [3] Section 9.2.20 | RIC Control |
| *RIC Control Message* IE | E2AP [3] Section 9.2.19 | RIC Control |
| *RIC Control Outcome IE* | E2AP [3] Section 9.2.25 | RIC Control |
| *RAN Function Definition* IE | E2AP [3] Section 9.2.23 | E2 Setup  RIC Service Update |

All of these RAN Function specific E2AP IEs are defined in E2AP [3] as “OCTET STRING”.

The purpose of this specification is to define the contents of these fields for the specific RAN function “RAN Control (RC)”.

# 6 RAN Function Service Model Description

## 6.1 RAN Function Overview

For the purposes of this E2 Service Model, E2SM-RC, the E2 Node terminating the E2 Interface is assumed to host one or more instances of the RAN Function “RAN Control” which performs the following functionalities:

- E2 REPORT services used to expose RAN control and UE context related information

- E2 INSERT services used to suspend RAN control related call processes

- E2 CONTROL services used to resume or initiate RAN control related call processes, modify RAN configuration and/or E2 service-related UE context information

- E2 POLICY services used to modify the behaviour of RAN control related processes

This E2SM specification provides a set of RAN Function exposure services described in clause 6.2 and has been prepared with the assumption that the same E2SM may be used to describe either a single RAN Function in the E2 Node handling all RAN control related call processes or more than one RAN Function in the E2 Node with each instance handling a subset of the RAN control related call processes on the E2 Node.

## 6.2 RAN Function exposure services

### 6.2.1 REPORT service

The “RAN Control” RAN Function provides selective support of the following **REPORT** services:

- Copy of Complete message (from Network Interface or RRC), used for monitoring POLICY services, data gathering (to populate the Near-RT RIC UE-NIB and/or ML services data pipeline), etc.

- Call process outcome with associated information on UE context and/or RAN status information, used for monitoring [CONTROL and] POLICY services, data gathering (to populate the Near-RT RIC UE-NIB and/or ML services data pipeline), etc.

- E2 Node Information and Cell related Information, used for monitoring of E2 Node and Cell configuration changes, triggering POLICY deletion, changing notifications (to reset Near-RT RIC optimization services), etc.

- UE Information, used for monitoring of UE information changes, triggering E2 Control, location tracking, etc.

- On Demand Report, used for reporting Cell related, E2 Node related and UE related information to Near-RT RIC when requested by Near-RT RIC.

NOTE: Only the UE with user consent can be configured to report location information.

### 6.2.2 INSERT service

The “RAN Control” RAN Function provides selective support of the following **INSERT** services:

Fundamental level:

- Radio Bearer Control request, used for requesting the RIC to control DRB QoS modification, QoS flow to DRB (re)mapping, Logical channel (re)configuration, Radio bearer admission control, Split bearer and PDCP duplication control, etc.

- Radio Resource Allocation Control request, used for requesting the RIC to control Discontinuous Reception (DRX), Scheduling request (SR), Semi-Persistent Scheduling (SPS), Configured Grant, Channel Quality Indicator (CQI) table, Slice level PRB quota, etc.

- Connected Mode Mobility Control request, used for requesting the RIC to control operations of Handover (HO), Conditional handover (CHO), Dual Active Protocol Stack (DAPS) HO, etc.

- Radio Access Control request, used for requesting the RIC to control parameters related to RACH back-off, RRC connection reject, RRC connection release, Access barring, UE admission, etc.

- Dual Connectivity (DC) Control request, used for requesting the RIC to control operations of Dual Connectivity (DC) including Change of bearer termination point (MN or SN) and/or bearer types, etc.

- Carrier Aggregation (CA) Control request, used for requesting the RIC to control operations of Carrier Aggregation (CA) involving secondary cell re-selection.

- Idle Mode Mobility Control request, used for requesting the RIC to control intra-frequency, inter-frequency, inter-RAT cell reselection priority, idle timers, etc.

Integrated level:

- Multiple Actions Control request, used for requesting the RIC to command multiple actions of the selected fundamental level INSERT services.

### 6.2.3 CONTROL service

The “RAN Control” RAN Function provides selective support of the following **CONTROL** services:

Fundamental level:

- Radio Bearer Control, used for DRB QoS modification, QoS flow to DRB (re)mapping, Logical channel (re)configuration, Radio bearer admission control, Split bearer and PDCP duplication control, etc.

- Radio Resource Allocation Control, used to control Discontinuous Reception (DRX), Scheduling request (SR), Semi-Persistent Scheduling (SPS), Configured Grant, Channel Quality Indicator (CQI) table, Slice level PRB quota, etc.

- Connected Mode Mobility Control, used to control operations of Handover (HO), Conditional handover (CHO), Dual Active Protocol Stack (DAPS) HO, etc.

- Radio Access Control, used for modification of RACH back-off, RRC connection reject, RRC connection release, Access barring, UE admission, etc.

- Dual Connectivity (DC) Control, used to control operations of Dual Connectivity (DC) including Change of bearer termination point (MN or SN) and/or bearer types, etc.

- Carrier Aggregation (CA) Control, used to control operations of Carrier Aggregation (CA).

- Idle Mode Mobility Control, used for modification of intra-frequency, inter-frequency, inter-RAT cell reselection priority, idle timers, etc.

- UE to RAN UE group assignment, used to support POLICY services.

- Measurement Report (MR) Configuration Control, used to control configuration of RRC measurement objects, reporting objects, etc.

Integrated level:

- Multiple Actions Control, used to command multiple actions of the selected fundamental level CONTROL services in one message.

### 6.2.4 POLICY service

The “RAN Control” RAN Function provides selective support of the following **POLICY** services:

- Radio Bearer Policy, used to modify the behaviour of call processes related to DRB QoS control, QoS flow to DRB mapping, Logical channel configuration, Radio bearer admission control, Split bearer and PDCP duplication control, etc.

- Radio Resource Allocation Policy, used to modify the behaviour of call processes related to DRX, SR, SPS, Configured Grant, CQI table, Slice level PRB quota, etc.

- Connected Mode Mobility Policy, used to modify the behaviour of call processes related to HO, CHO, DAPS HO, etc. for both serving and target RAN nodes.

- Radio Access Policy, used to modify the behaviour of call processes related to RACH back-off, RRC connection reject, RRC connection release, Access barring, UE admission, etc.

- Dual Connectivity (DC) Policy, used to modify the behaviour of call processes related to DC related operations for both master and secondary RAN nodes, Change of bearer termination point (MN or SN) and/or bearer types, etc.

- Carrier Aggregation (CA) Policy, used to modify the behaviour of call processes related to CA related operations for both primary and secondary cells.

- Idle Mode Mobility Policy, used to modify the behaviour of call processes related to intra-frequency, inter-frequency, inter-RAT cell reselection priority, inactivity timers, etc.

- Measurement Report (MR) Configuration Policy, used to configure policy for RRC measurement objects, reporting objects, etc.

## 6.3 REPORT service description

The E2SM-RC REPORT service requirements defined in Section 6.2.1 are offered using a set of REPORT Styles. All REPORT styles are implemented using a set of IEs for Action Definition, RIC Indication Header and RIC Indication Message and have specific Event Trigger approach. For each Report style, a single RAN Parameter table is used to specify the required information to be reported.

The following REPORT styles are supported:

- Message copy: This REPORT style is initiated by “Message Event” Event Trigger and is used to report complete NI or RRC message along with UE associated information when the event trigger conditions are satisfied.

- Call Process Outcome: This REPORT style is initiated by the corresponding "Call Process Breakpoint" Event Trigger and is used to report on the outcome of a call process providing information on current, and in certain cases previous, UE or E2 Node information depending upon the nature of the target call process.

- E2 Node Information: This REPORT style is initiated by “E2 Node Information Change” Event Trigger and is used to report cell related and E2 Node related information upon event trigger conditions are satisfied.

- UE information: This REPORT style is initiated by “UE Information Change” Event Trigger and is used to report UE related information and UE state variables upon the event trigger conditions are satisfied.

- On demand report: This REPORT style is initiated by “On Demand” Event Trigger and is used to report cell-related and UE-related information on an adhoc basis upon request from Near-RT RIC.

## 6.4 INSERT service description

The E2SM-RC INSERT service requirements defined in Section 6.2.2 are offered using a set of INSERT Styles. Each style corresponds to a set of “INSERT Indications”, where each “INSERT Indication” deals with a specific functionality and has a set of associated RAN parameters, provided in a mapping table. All INSERT Service styles are implemented using a set of IEs that constitute “Action Definition”, “RIC Indication Header” and “RIC Indication Message” to deliver RAN Control-related INSERT services. Each INSERT service style is associated with a specific “Event Trigger” approach. An “INSERT Indication” is used to request the RIC to control a functionality associated with the respective INSERT service style, and to set or modify the values of one or more associated RAN parameters.

As an example, upon the arrival of an RRC Measurement Report in the E2 node due to the occurrence of an A3 event pertaining to a UE (which constitutes the event trigger), the E2 node can send amessage to the RIC using the “Connected Mode Mobility” INSERT service style and the “Handover Control Request” INSERT Indication along with the “target cell ID” parameter. This RIC should then accept/deny the “Handover Control Request”, and if it accepts, it should set the value of the “target cell ID” parameter and send a CONTROL action back to the RIC. Up until then, the E2 node suspends the ongoing call processing for the UE.

## 6.5 CONTROL service description

The E2SM-RC CONTROL service requirements defined in Section 6.2.3 are offered using a set of CONTROL Styles. Each style corresponds to a set of “CONTROL Action”, where each “CONTROL Action” deals with a specific functionality and has a set of associated RAN parameters, provided in a mapping table. All CONTROL Service styles are implemented using a set of IEs constituting a “RIC Control Request Header” and a “RIC Control Request Message” to deliver RAN Control-related CONTROL services. A “CONTROL Action” containing one or more RAN parameters and their associated values can either be sent from the RIC, either asynchronously to the E2 node or as a response to a previous “INSERT Indication” from the E2 node.

Referring to the previous example in Section 6.4, the RIC sends a “CONTROL action” that accepts/denies the incoming “INSERT Indication” requesting for “Handover Control”, along with the value of the “Target Primary Cell”. As another example, the RIC can also asynchronously send a “CONTROL action” asking the E2 node to configure the UE in Carrier Aggregation mode and setup one or more secondary cells to the UE, whose values are assigned by the RIC via the “CONTROL action”.

## 6.6 POLICY service description

### 6.6.1 Overview

The E2SM-RC POLICY service requirements defined in Section 6.2.4 are offered using a set of POLICY Styles. Each style is implemented using multiple "Policy Approach" strategies, each with a specific methodology defined to use the E2AP IE "Action Definition" to deliver RAN Control related POLICY services.

The following Policy Approaches are defined:

- Control: POLICY for a given Style and Action ID is defined as a single case of a specific Policy condition with the corresponding Policy Action defined using the same data structure as CONTROL which would be used to replace default RAN behaviour.

- Offset: POLICY for a given Style and Action ID is defined as a set of different cases applicable for a range of different Policy conditions with the corresponding Policy Action defined using the dedicated data structure defined for POLICY which would be used to modify default RAN behaviour.

### 6.6.2 Policy approach "Control"

The “control” Policy Approach is similar to the CONTROL service, with static conditions and actions in the RIC Subscription used to select an appropriate CONTROL Action. When a set of Policy conditions are satisfied, then E2 Node is instructed to execute a Policy Action with a set of supplementary or default set of RAN parameters.

A single Policy Action shall be a result of execution of multiple policy conditions.

- Each Policy Condition is defined using a combination of RAN Parameters and conditional tests associated with UE and Call process related information.

- Each Policy Action is defined with a single Policy Action ID (command) which instructs E2 Node to perform a certain action when the conditions are satisfied. The Policy Action ID shall be supplemented with a set of RAN Parameters which may be used to provide information on default values to E2 Node. The Policy Decision indicates to the E2 Node, whether to accept or reject a RRM function, when the Policy conditions are met.

Examples include:

- Connected mode mobility policy, Handover Execution: Message Arrival breakpoint event trigger is defined to initiate the Policy service. On the arrival of A3 Measurement Report, the Policy service kicks in. Policy service installs a set of Policy Conditions like RSRP > ‘x’ db + Target Node Load < ‘x’ value + Number of successful HO to target Node > ‘x’ value. When these Policy conditions are satisfied, then perform Policy Action - “Execute HO” defined in the CONTROL service in Section 6.5. The Policy Action may be provided as a standalone Policy Action ID “Execute HO” without any RAN parameters. As an alternative, Policy Action “Execute HO” may be supplemented with default RAN parameters like Handover only QCI 5 and 9 bearers.

- Carrier Aggregation Policy, CA Release decision: A call process breakpoint event trigger is defined to initiate the POLICY service. The call process breakpoint shall define conditions for Buffer occupancy. A call process breakpoint event shall be triggered when the Buffer Occupancy (BO) < ‘x’ KB. In this scenario, the event trigger satisfies the Policy condition. Hence there is no need to define a Policy condition in the Policy service, When the BO < ‘x’ KB kicks in, then Policy Action shall instruct E2 Node to “Release Scell”.

### 6.6.3 Policy Approach "Offset"

The "offset" Policy Approach is based on the design assumption that the Policy Action IE is used to carry one or more RAN Parameters that are used to modify default E2 Node behaviour via the addition of an "offset" to be applied to given target threshold or other parameter used in the target call process.

The applicable Policy Action is dependent upon a set of Policy Conditions and a given POLICY service may support one or more Policy conditions and so provide a targeted Policy Action for a range of different specific cases, each defined using a unique Policy condition where:

- Each Policy Condition is defined using a combination of RAN Parameters and conditional tests associated with UE and Call process related information. The first positive match in a list of Policy conditions is used to select the corresponding Policy Action.

- Each Policy Action is defined using a list of RAN Parameters of data type INTEGER or REAL which may to used directly for default values of type INTEGER or REAL (i.e. Default+Offset) and indirectly to for default values of type ENUMERATED (i.e. select value in list that is Offset before or after default value).

Examples include:

- Connected mode mobility policy, Handover decision: A call process breakpoint event trigger is defined to initiate the POLICY service from within the call process handling UE measurement reports related to handover decisions for a specific target Slice and primary cell currently subject to Traffic Steering guidance. The Policy conditions list of RAN Parameters supports the definition of different A3 measurement threshold criteria offset values to be applied to UEs with a specific combination of slice ID, active QoS bearers, velocity and throughput and subject to overall E2 Node load and cell level load balancing requirements. Handover is accepted if the reported A3 measurement is greater than the default A3 measurement threshold+offset.

- Carrier Aggregation Policy, CA release decision: A call process breakpoint event trigger is defined to initiate the POLICY service from within the call process related to Carrier Aggregation (CA) release decisions for a specific target Slice currently subject to QoE guidance. The Policy conditions list of RAN Parameters supports the definition of different CA release threshold criteria offset values to be applied to UEs with a specific combination of slice ID, active QoS bearers, velocity and throughput and subject to overall E2 Node load and cell level load balancing requirements. CA release is initiated if the UE throughput is less than the default UE throughput threshold+offset.

# 7 RAN Function Description

## 7.1 Description

The E2AP [3] procedures E2 Setup and RIC Service Update are used to transport the RAN Function Description.

For the specific RAN Function, the *RAN Function Description* IE shall report the following information:

- RAN Function name along with associated information on E2SM definition

- Event trigger styles list along with the corresponding encoding type for each associated E2AP IE.

- RIC **REPORT** Service styles list along with the corresponding encoding type for each associated E2AP IE.

- RIC **INSERT** Service styles list along with the corresponding encoding type for each associated E2AP IE.

- RIC **CONTROL** Service styles list along with the corresponding encoding type for each associated E2AP IE.

- RIC **POLICY** Service styles list along with the corresponding encoding type for each associated E2AP IE.

## 7.2 RAN Function name

RAN Function Short Name “ORAN-E2SM-RC”

RAN Function name description “RAN Control”

RAN Function Instance, required when and if E2 Node exposes more than one instance of a RAN Function based on this E2SM.

## 7.3 Event trigger definition styles

### 7.3.1 RIC Event trigger definition IE style list

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RIC Style Type** | **Style Name** | **Supported RIC Service Style** | | | **Style Description** |
| **Report** | **Insert** | **Policy** |
| 1 | Message Event | 1 | - | 1-7 | Triggering conditions are based on arrival or departure of network interface message or RRC message. |
| 2 | Call Process Breakpoint | 2 | 1-7 | 1-8 | Triggering conditions are based on call process breakpoint. |
| 3 | E2 Node Information Change | 3 | - | - | Triggering conditions are based on change of E2 Node or cell related configuration information. |
| 4 | UE Information Change | 4 | - | - | Triggering conditions are based on change of UE Information. |
| 5 | On Demand | 5 | - | - | Event is immediately triggered when RIC subscription with this event trigger is accepted. |

### 7.3.2 RIC Event trigger definition IE style 1: Message Event

This *RIC Event Trigger Definition* IE style is used to detect a specific Network Interface or RRC message event in E2 Node. The dection can be based on only for incoming or outgoing message. The E2 Node can also be configured to detect multiple messages simultaneously and to trigger only when all the configured message events happen or for any logical combination of message events.

Each message event configured can be further conditioned to be associated only for a certain UE or group of UEs as indicated by the *Associated UE Info* IE if included, or only for some specific UE events defined in Section 8.1.5 as indicated by the *Associated UE Event* IE if included. In case that the *Global Associated UE Info* IE is included, the information is applied uniformly to all the message events configured and the IE shall override any *Associated UE Info* IE included for some message events.

For each message event configured, Event Trigger Condition ID is assigned so that E2 Node can reply to Near-RT RIC in the RIC INDICATION message to inform which event(s) are the cause for triggering.

This *RIC Event Trigger Definition* IE style uses *RIC Event Trigger Definition* IE Format 1 (9.2.1.1.1).

### 7.3.3 RIC Event trigger definition IE style 2: Call Process Breakpoint

This *RIC Event Trigger Definition* IE style is used to detect a call process in E2 Node based on a specified call process identifier and breakpoint identifier. The call process and breakpoint configured for event triggering can also be conditioned to be associated with a certain E2 Node related information.

The following table specifies the supported call process types, call breakpoints, the associated RAN Parameters for possible E2 Node related conditioning for event triggering, as well as the supported INSERT or POLICY services.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Call Process Type ID | Call Process Type | Call Break-point ID | Call Breakpoint Name | Associated RAN Parameters | Supported INSERT Service Styles | Supported POLICY Service Styles | Supported REPORT Service Styles | Description |
| 1 | UE Context Management | 1 | UE Context Setup | 8.1.2.1.1 | 1,2,3,4,6,7 | 1,2,3,4,6,7,8 | 2 | TS 38.470 [18] clause 5.2.3 and TS 38.410 [10] clause 5.3. |
| 2 | UE Context Modification | 8.1.2.1.2 |
| 3 | UE Context Release | 8.1.2.1.3 |
| 2 | Bearer Context Management | 1 | Bearer Context Setup | 8.1.2.2.1 | 1,4,5,6 | 1,4,5,6,8 | 2 | TS 38.460 [20] clause 5.1.2 |
| 2 | Bearer Context Modification | 8.1.2.2.2 |
| 3 | Bearer Context Release | 8.1.2.2.3 |
| 3 | Mobility Management | 1 | Handover Preparation | 8.1.2.3.1 | 3 | 3,8 | 2 | TS 38.420 [14] clause 5.2.2 and TS 38.410 [10] clause 5.4. It also handles the F1AP: Mobility Management aspects of the *UE Context Management* procedure from TS 38.470 and TS 38.473 |
| 2 | Handover Cancel | 8.1.2.3.2 |
| 3 | Handover Resource Allocation | 8.1.2.3.3 |
| 4 | Multi-RAT Dual Connectivity Management | 1 | SN Addition | 8.1.2.4.1 | 5 | 5,8 | 2 | TS 38.420 [14] clause 5.2.3 and TS 36.420 [16] clauses 5.2.1.5 and 5.2.1.6 |
| 2 | SN Modification and Release | 8.1.2.4.2 |
| 5 | Radio Resource Control Management | 1 | RRC CG-Config Information Transfer | 8.1.2.5.1 | 1-7 | 1-7 | 2 | TS 38.470 [18] clause 5.2.4 |
| 2 | RRC Cell Group Config Transfer | 8.1.2.5.2 |
| 6 | PDU Session Management | 1 | PDU Session Resource Setup | 8.1.2.6.1 | 1,3,4,5 | 1,3,4,5,8 | 2 | TS 38.410 [10] clause 5.5 |
| 2 | PDU Session Resource Modification | 8.1.2.6.2 |
| 3 | PDU Session Resource Release | 8.1.2.6.3 |

Table 7.3.3-1: Event Trigger Definition Style 2 – Supported Call Processes and associated RAN Parameters

Each event configured can be further conditioned to be associated only for a certain UE or group of UEs as indicated by the *Associated UE Info* IE if included.

This *RIC Event Trigger Definition* IE style uses *RIC Event Trigger Definition* IE Format 2 (9.2.1.1.2).

### 7.3.4 RIC Event trigger definition IE style 3: E2 Node Information Change

This *RIC Event Trigger Definition* IE style is used to detect E2 Node related information change from the subscribed E2 Node. The E2 Node can also be configured to detect multiple changes simultaneously and to trigger only when all the configured changes happen or for any logical combination of the configured changes.

In this version of E2SM-RC specification, the following E2 Node related information changes are supported for event triggering.

|  |  |  |
| --- | --- | --- |
| **E2 Node Information Change ID** | **E2 Node Information Change Type** | **Description** |
| 1 | Cell Configuration Change | Triggered when any serving cell’s context information defined by the *Served Cell Information* IE in TS 38.473 [19] clause 9.3.1.10 has changed. |
| 2 | Cell Neighbor Relation Change | Triggered when any serving cell’s neighbor relation information defined by Section 9.3.38 has changed. |
| 3 | Slice Configuration Change | Triggered when slice configuration in any serving cell has changed. |

Table 7.3.4-1: Event Trigger Definition Style 3 – Supported E2 Node information changes

Each E2 Node information change configured can also be conditioned to be associated with a specific cell or group of cells for event triggering, as indicated by the *Associated Cell Info* IE if included.

For each information change configured for event triggering, Event Trigger Condition ID is also assigned so that E2 Node can reply to Near-RT RIC in the RIC INDICATION message to inform which event(s) are the cause for triggering.

This *RIC Event Trigger Definition* IE style uses *RIC Event Trigger Definition* IE Format 3 (9.2.1.1.3).

### 7.3.5 RIC Event trigger definition IE style 4: UE Information Change

This *RIC Event Trigger Definition* IE style is used to detect UE Context related information change from the subscribed E2 Node. The E2 Node can also be configured to detect multiple changes simultaneously and to trigger only when all the configured changes happen or for any logical combination of the configured changes.

In this version of E2SM-RC specification, the supported UE Context information changes for event triggering are

- RRC state change

- UE identifier change (based on UE ID defined in Section 9.3.10)

- RLC/PDCP state variable or MAC state variable change (based on RAN Parameters defined in Sections 8.1.1.4 and 8.1.1.8)

For UE identifier change, the following cases are supported for event triggering.

|  |  |  |
| --- | --- | --- |
| **UE Identifier Change ID** | **UE Identifier Change Type** | **Description** |
| 1 | New UE Connected | Triggered when new UE ID is assigned for a new UE connected. |
| 2 | UE Handed Over | Triggered when new UE ID is assigned due to HO from another node. |
| 3 | UE ID Changed | Triggered when any content of the assigned UE ID (based on the definition of UE ID in Section 9.3.10) has changed. |
| 4 | UE ID Removed | Triggered when a UE is released, and its UE ID is removed. |

Table 7.3.5-1: Event Trigger Definition Style 4 – Supported UE Identifier changes

The detection for each UE information change configured can be based on for any UEs, or only for a certain UE or group of UEs as indicated by the *Associated UE Info* IE if included.

For each information change configured, Event Trigger Condition ID is assigned so that E2 Node can reply to Near-RT RIC in the RIC INDICATION message to inform which event(s) are the cause for triggering.

This *RIC Event Trigger Definition* IE style uses *RIC Event Trigger Definition* IE Format 4 (9.2.1.1.4).

### 7.3.6 RIC Event trigger definition IE style 5: On Demand

This *RIC Event Trigger Definition* IE style is used to be immediately triggered by E2 Node when a RIC subscription having this event trigger is accepted. Once accepted, the E2 Node shall consider that this RIC subscription shall expire automatically once all the requested actions for this RIC subscription are performed by the E2 Node.

The event can be further conditioned to be associated only for a certain UE or group of UEs as indicated by the *Associated UE Info* IE if included, or for a specific cell or group of cells as indicated by the *Associated Cell Info* IE if included. In this case, Near-RT RIC shall ensure that additional conditions imposed by the *Associated UE Info* IE or *Associated Cell Info* IE does not prevent event triggering as soon as the RIC subscription is accepted by the E2 Node.

This *RIC Event Trigger Definition* IE style uses the *RIC Event Trigger Definition* IE Format 5 (9.2.1.1.5).

## 7.4 Supported RIC REPORT Services

### 7.4.1 REPORT Service style list

|  |  |  |
| --- | --- | --- |
| RIC Style Type | Style Name | Style Description |
| 1 | Message copy | This style is used to report a copy of complete Network Interface or RRC message. |
| 2 | Call Process Outcome | This style is used to report the outcome of an ongoing call process. |
| 3 | E2 Node Information | This style is used to report E2 Node information, Serving Cell Configuration and Neighbour Relation related information. |
| 4 | UE Information | This style is used to report the UE related information like PDCP, RLC, MAC UE state variables and RRC UE State. |
| 5 | On Demand Report | This style is used to report snapshot of UE related information and Cell related information upon request from Near-RT RIC. |

### 7.4.2 REPORT Service Style 1: Message Copy

#### 7.4.2.1 REPORT Service Style description

This **REPORT** Service style provides the complete copy of a Network Interface or RRC message to be carried as a transparent container in the *RIC Indication Message* IE.

This **REPORT** service style may also be used to report UE specific information associated with the Network Interface/RRC messages as provided in Section 8.2.1 RAN Parameters. Examples include reporting of UEID to Near-RT RIC when UE attaches to the E2 Node or when the UEID changes during Xn Handover, UE events like Secondary Cell addition, Arrival of A3 Measurement Report (see Section 8.1.5 for the list of UE events).

This **REPORT** Service style is initiated by Event Trigger style 1: Message Event.

#### 7.4.2.2 REPORT Service *RIC Action Definition* IE contents

The Action Definition for this service style is used to request E2 Node to report a copy of NI and/or RRC message and may be used to report UE specific information. The action definition indicates which related UE information is to be reported along with the NI or RRC message that triggers this report service.

This **REPORT** Service style uses the *RIC Action Definition* IE Format 1 (9.2.1.2.1). The supported Parameters for this format are provided inSection 8.2.1*.*

#### 7.4.2.3 REPORT Service *RIC Indication Header* IE contents

This **REPORT** Service style uses the *RIC Indication Header* IE Format 1 (9.2.1.3.1)

#### 7.4.2.4 REPORT Service *RIC Indication Message* IE contents

The **REPORT** Service *RIC Indication Message* IE carries the complete Network Interface or RRC message as transparent containers. The *RIC Indication Message* IE may also carry UE specific information related to the Network Interface or RRC message as provided in Section 8.2.1.

This **REPORT** Service style uses the *RIC Indication Message* IE Format 1 (9.2.1.4.1). The supported Parameters for this message format are provided in Section 8.2.1.

### 7.4.3 REPORT Service Style 2: Call Process Outcome

#### 7.4.3.1 REPORT Service Style description

This **REPORT** Service style provides the outcome of a target call process related mechanism to be carried in the *RIC Indication Message* IE along with an associated *RIC Indication Header* IE providing information related event trigger conditions.

This **REPORT** Service style is initiated by Event Trigger style 2: Call Process Breakpoint.

#### 7.4.3.2 REPORT Service *RIC Action Definition* IE contents

The Action Definition for this service style is used to request an E2 Node to report call process outcome information including UE specific information. The Action Definition indicates which related UE information is to be reported related to the outcome of the event that triggers this report service.

This **REPORT** Service style uses the *RIC Action Definition* IE Format 1 (9.2.1.2.1). The supported Parameters for this message format are provided in Section 8.2.2.

#### 7.4.3.3 REPORT Service *RIC Indication Header* IE contents

This **REPORT** Service style uses the *RIC Indication Header* IE Format 1 (9.2.1.3.1).

#### 7.4.3.4 REPORT Service *RIC Indication Message* IE contents

The **REPORT** Service *RIC Indication Message* IE carries the UE specific information as a result of call process outcome. The Parameters supporting UE specific information is provided in Section 8.2.2.

This **REPORT** Service style uses the *RIC Indication Message* IE Format 2 (9.2.1.4.2). The supported Parameters for this message format are provided in Section 8.2.2.

### 7.4.4 REPORT Service Style 3: E2 Node Information.

#### 7.4.4.1 REPORT Service Style description

This **REPORT** Service style provides essential RAN control related E2 Node Configuration Information that is not provided by E2AP [3]. The information is carried in the *RIC Indication Message* IE along with an associated *RIC Indication Header* IE providing information related event trigger conditions. The required information to be provided is controlled using the associated *RIC Action Definition* IE parameters.

This **REPORT** Service style provides information related to:

- Serving Cell configuration

- Neighbour Relation Information

whenever the corresponding event trigger for change in information content is satisfied. With every change in the information content of the Neighbour Relation Information, complete list of Neighbour relation table is sent to Near-RT RIC with indicaton on the modified information.

This **REPORT** Service style is initiated by Event Trigger style 3: E2 Node Information Change.

#### 7.4.4.2 REPORT Service *RIC Action Definition* IE contents

The Action Definition for this service style indicates the E2 Node related information requested by Near-RT RIC.

The **REPORT** Service style uses the *RIC Action Definition* IE Format 1 (9.2.1.2.1). The supported Parameters for this format are provided in Section 8.2.3*.*

#### 7.4.4.3 REPORT Service *RIC Indication Header* IE contents

This **REPORT** Service style uses the *RIC Indication Header* IE Format 1 (9.2.1.3.1).

#### 7.4.4.4 REPORT Service *RIC Indication Message* IE contents

The **REPORT** Service *RIC Indication Message* IE carries the E2 node related information as subscribed by the *RIC Action Definition* IE.

This **REPORT** Service style uses the *RIC Indication Message* Format 3 (9.2.1.4.3). The mapping of RAN paramerters configured in the *RIC Action Definition* IE to the reported IEs in the *RIC Indication Message* IE Format 3 is provided in the semantics description of the IEs.

### 7.4.5 REPORT Service Style 4: UE Information

#### 7.4.5.1 REPORT Service Style description

This **REPORT** Service style provides UE related Information. The information is carried in the *RIC Indication Message* IE along with an associated *RIC Indication Header* IE providing information related event trigger conditions. The required information to be provided is controlled using the associated *RIC Action Definition* IE parameters.

This **REPORT** Service style enables the E2 Node to report on a per UE basis:

- L2 UE State variable values including

- PDCP UE State variables

- RLC UE State variables

- MAC UE variables.

- L3 UE State variable values including

- RRC State

- UE ID Information

- UE ID change information including

- Current UE ID

- Old UE ID

- NI or RRC message which triggered the UE ID change

This **REPORT** Service style is initiated by Event Trigger style 4: UE Information Change.

#### 7.4.5.2 REPORT Service *RIC Action Definition* IE contents

The Action Definition for this service style indicates the set of UE information parameters to be reported when event trigger to report is satisfied.

The **REPORT** Service style uses the *RIC Action Definition* IE Format 1 (9.2.1.2.1). The supported Parameters for this message format are provided in Section 8.2.4*.*

#### 7.4.5.3 REPORT Service *RIC Indication Header* IE contents

This **REPORT** Service style uses the *RIC Indication Header* IE Format 1 (9.2.1.3.1).

#### 7.4.5.4 REPORT Service *RIC Indication Message* IE contents

The **REPORT** Service *RIC Indication Message* IE carries the requested UE related information.

This **REPORT** Service style uses the *RIC Indication Message* IE Format 2 (9.2.1.4.2). The supported Parameters for this message format are provided in Section 8.2.4.

### 7.4.6 REPORT Service Style 5: On Demand Report

#### 7.4.6.1 REPORT Service Style description

This **REPORT** Service style provides the snapshot of the following information at the time of subscription request received from Near-RT RIC:

- Cell Configuration related information

- Neighbour Relation related information

- UE Context related information

The subscription for this **REPORT** Service style expires once the RIC Indication message is sent with the requested information. The E2AP RIC Subscription Delete procedure or RIC Subscription Delete Required procedure [3] is not required to delete this subscription. The reporting shall be per UE based or per cell based depending on the information requested to be reported.

#### 7.4.6.2 REPORT Service *RIC Action Definition* IE contents

The Action Definition for this service style indicates the information type (e.g. UE Context information) requested by Near-RT RIC.

The **REPORT** Service style uses the *RIC Action Definition* IE Format 1 (9.2.1.2.1). The supported Parameters for this format are provided in Section 8.2.5.

#### 7.4.6.3 REPORT Service *RIC Indication Header* IE contents

This **REPORT** Service style uses the *RIC Indication Header* IE Format 1 (9.2.1.3.1).

#### 7.4.6.4 REPORT Service *RIC Indication Message* IE contents

This **REPORT** Service style uses the *RIC Indication Message* IE Format 4 (9.2.1.4.4). The mapping of RAN paramerters configured in the *RIC Action Definition* IE to the reported IEs in the *RIC Indication Message* IE Format 4 is provided in the semantics description of the IEs.

## 7.5 Supported RIC INSERT Services

### 7.5.1 INSERT Service style list

|  |  |  |
| --- | --- | --- |
| **RIC Style Type** | **Style Name** | **Style Description** |
| 1 | Radio Bearer Control Request | Used to request modification of the configuration of Radio Bearer Control (RBC) related parameters.  Belongs to Fundamental level INSERT Services. |
| 2 | Radio Resource Allocation Control Request | Used to request modification of the configuration of Radio Resource Allocation control related parameters.  Belongs to Fundamental level INSERT Services. |
| 3 | Connected Mode Mobility Control Request | Used to request initiation of a connected mode mobility procedure (Handover or Conditional Handover), optionally with Dual Active Protocol Stack (DAPS), for a specific UE towards either a target cell (for HO) or a list of candidate cells (for CHO).  Belongs to Fundamental level INSERT Services. |
| 4 | Radio Access Control Request | Used to request modification of radio access related functions for controlling UE access to cells.  Belongs to Fundamental level INSERT Services. |
| 5 | Dual Connectivity Control Request | Used to request initiation of dual connectivity (DC) mechanisms  Belongs to Fundamental level INSERT Services. |
| 6 | Carrier Aggregation Control Request | Used to request initiation of carrier aggregation (CA) mechanisms  Belongs to Fundamental level INSERT Services. |
| 7 | Idle Mode Mobility Control Request | Used to request modification of idle mode mobility related functions in order to control UE re-selection of cells  Belongs to Fundamental level INSERT Services. |
| 255 | Mutiple Actions Control Request | Used to request multiple parallel actions of the selected fundamental level INSERT Service style(s).  Belongs to Integrated level INSERT Services. |

Apart from the individual set of RAN parameters associated with each INSERT Service style and INSERT Indication name as described in Sections 7.5.2 to 7.5.8, there is also a common set of RAN parameters for all INSERT service styles as elucidated in Section 8.3.9.

### 7.5.2 INSERT Service Style 1: Radio Bearer Control Request

#### 7.5.2.1 INSERT Service Style description

This **INSERT** Service style provides a mechanism to initiate request to the RIC for controlling the functionalities of a radio bearer related process pertaining to a UE using the *RIC Indication Message* IE and associated *RIC Indication Header* IE. The E2 node sends a *RIC Indication* message to the near-RT RIC and the ongoing call process is suspended at the E2 node until the E2 node hears back from the RIC. The optional *RIC Call Process ID* IE is used by the E2 node to match a *RIC Control Request* message to a *RIC Indication* message, following which the E2 node can resume the suspended call processing for the UE.

Applications of this service include:

- Request for DRB QoS Modification, to tune DRB level QoS related parameters to meet the QoS optimization targets.

- Request for QoS Flow (re)mapping, to adjust the mapping relationship between QoS flows and DRBs.

- Request for Logical channel (re)configuration

- Request for Radio Bearer Admission Control, to configure DRB admission control such as reject or release may be applied.

- Request for Split bearer and PDCP duplication control

This Insert style supports the following *Indication* services, each service listed below with a corresponding *Indication* ID. The RAN parameters, associated with each Insert Indication service, are listed in the sections shown below.

|  |  |  |  |
| --- | --- | --- | --- |
| **Indication**  **ID** | **Indication Name** | **Insert Indication description** | **Associated RAN Parameters** |
| 1 | DRB QoS Configuration request | To request the configuration of DRB QoS profile | 8.3.2.1 |
| 2 | QoS flow mapping configuration request | To request the multiplexing of QoS flows to a DRB (addition, modification, deletion | 8.3.2.2 |
| 3 | Logical channel configuration request | To request the LCID configuration of a DRB | 8.3.2.3 |
| 4 | Radio admission control request | To request radio admission control of a UE | 8.3.2.4 |
| 5 | DRB termination control request | To request a change in the bearer termination point | 8.3.2.5 |
| 6 | DRB split ratio control request | To request the split ratio of a DRB to be controlled across its RLC entities | 8.3.2.6 |
| 7 | PDCP Duplication control request | To request controlling the activation or de-activation of PDCP duplication for a DRB and control/configure the number of legs or RLC entities for the DRB | 8.3.2.7 |

#### 7.5.2.2 INSERT Service *RIC Action Definition* IE contents

This **INSERT** Service style uses the *RIC Action Definition* IE Format 3 (9.2.1.2.3). This Insert style deals with the supported *Indication* services, each service with a corresponding *Indication* ID listed in Section 7.5.2.1. The RAN parameters, associated with each Insert *RIC Indication* service, are included by the E2 node in the *RIC Indication* message. Via the *RIC Indication* message, the E2 node seeks the near-RT RIC to accept or deny the request raised by the E2 node and to accordingly set the values for the associated RAN parameters by the RIC via the control action in the ensuing *RIC Control Request* message from the RIC.

#### 7.5.2.3 INSERT Service *RIC Indication Header* IE contents

This **INSERT** Service style uses *RIC Indication header* IE Format 2 (9.2.1.3.2). The *RIC Indication header* IE has the UE ID, the *Insert* Service Style ID and the corresponding *Insert* Indication ID.

#### 7.5.2.4 INSERT Service *RIC Indication Message* IE contents

This **INSERT** Service style uses *RIC Indication Message* IE Format 5 (9.2.1.4.5). The *RIC Indication Message* IE includes a sequence of associated RAN parameters for which the E2 node seeks the near-RT RIC to accept/deny the request raised by the E2 node and accordingly set the values for the associated RAN parameters, via the control action in the ensuing *RIC Control Request* IE.

#### 7.5.2.5 INSERT Service *RIC Call Process ID* IE contents

This **INSERT** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

### 7.5.3 INSERT Service Style 2: Radio Resource Allocation Control Request

#### 7.5.3.1 INSERT Service Style description

This **INSERT** Service style provides a mechanism to initiate request to the RIC for controlling the allocation of radio resources to the UE using the *RIC Indication Message* IE and associated *RIC Indication Header* IE. The E2 node sends a *RIC Indication* message to the near-RT RIC and the ongoing call process is suspended at the E2 node until the E2 node hears back from the RIC. The optional *RIC Call Process ID* IE is used by the E2 node to match a *RIC Control Request* message to a *RIC Indication* message, following which the E2 node can resume the suspended call processing for the UE.

Applications of this service include:

- Request for Discontinuous Reception (DRX) control

- Request for Scheduling request (SR) control

- Request for Semi-Persistent Scheduling (SPS) control

- Request for Configured Grant control

- Request for Channel Quality Indicator (CQI) table

- Request for Slice level PRB quota

This Insert style supports the following *Indication* services, each service listed below with a corresponding *Indication* ID. The RAN parameters, associated with each Insert Indication service, are listed in the sections shown below.

|  |  |  |  |
| --- | --- | --- | --- |
| Indication  ID | Indication  Name | Insert Indication description | Associated RAN Parameters |
| 1 | DRX parameter configuration request | To request the configuration of DRX parameters | 8.3.3.1 |
| 2 | SR periodicity configuration request | To request the configuration of SR periodicity parameters | 8.3.3.2 |
| 3 | SPS parameters configuration request | To request the configuration of SPS parameters | 8.3.3.3 |
| 4 | Configured grant control request | To request the configuration of uplink grants to the UE | 8.3.3.4 |
| 5 | CQI table configuration request | To request the configuration of CQI table. | 8.3.3.5 |
| 6 | Slice-level PRB quota request | To request setting the slice-specific PRB quota | 8.3.3.6 |

#### 7.5.3.2 INSERT Service *RIC Action Definition* IE contents

This **INSERT** Service style uses the *RIC Action Definition* IE Format 3 (9.2.1.2.3). The Insert style deals with the supported *Indication* services, each service with a corresponding *Indication* ID listed in Section 7.5.3.1. The RAN parameters, associated with each Insert *Indication* service, are included by the E2 node in the *RIC Indication* message. Via the *RIC Indication* message, the E2 node seeks the near-RT RIC to accept or deny the request raised by the E2 node and to accordingly set the values for the associated RAN parameters by the RIC via the control action in the ensuing *RIC Control Request* message from the RIC.

#### 7.5.3.3 INSERT Service *RIC Indication Header* IE contents

This **INSERT** Service style uses *RIC Indication Header* IE Format 2 (9.2.1.3.2). The *RIC Indication Header* IE has the UE ID, the *Insert* Service Style ID and the corresponding *Insert* Indication ID.

#### 7.5.3.4 INSERT Service *RIC Indication Message* IE contents

This **INSERT** Service style uses *RIC Indication Message* IE Format 5 (9.2.1.4.5). The *RIC Indication Message* IE includes a sequence of associated RAN parameters for which the E2 node seeks the near-RT RIC to accept/deny the request raised by the E2 node and accordingly set the values for the associated RAN parameters, via the control action in the ensuing *RIC Control Request* IE.

#### 7.5.3.5 INSERT Service *RIC Call Process ID* IE contents

This **INSERT** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

### 7.5.4 INSERT Service Style 3: Connected Mode Mobility Request

#### 7.5.4.1 INSERT Service Style description

This **INSERT** Service style provides a mechanism to initiate request for controlling the handover and mobility management of the UE using the *RIC Indication Message* IE and associated *RIC Indication Header* IE. The E2 node sends a *RIC Indication* message to the near-RT RIC and the ongoing call process is suspended at the E2 node until the E2 node hears back from the RIC. The optional *RIC Call Process ID* IE is used by the E2 node to match a *RIC Control Request* message to a *RIC Indication* message, following which the E2 node can resume the suspended call processing for the UE.

Applications of this service include:

- Request for Handover (HO) initiation for a selected UE towards a target cell

- Request for Conditional handover (CHO) initiation for a selected UE towards a list of candidate cell(s)

- Request for Handover (HO) initiation with Dual Active Protocol Stack (DAPS) for a selected UE towards a target cell

This Insert style supports the following *Indication* services, each service listed below with a corresponding *Indication* ID. The RAN parameters, associated with each Insert Indication service, are listed in the sections shown below.

|  |  |  |  |
| --- | --- | --- | --- |
| **Indication**  **ID** | **Indication Name** | **Insert Indication description** | **Associated RAN parameters** |
| 1 | Handover Control request | To request the handover of the primary cell and subsequent secondary cell reselection | 8.3.4.1 |
| 2 | Conditional Handover Control request | To request the conditional handover involving target primary cells | 8.3.4.2 |
| 3 | DAPS (Dual Active Protocol Stack) Handover Control request | To request the dual active protocol stack handover involving the target primary cell. | 8.3.4.3 |

#### 7.5.4.2 INSERT Service *RIC Action Definition* IE contents

This **INSERT** Service style uses the *RIC Action Definition* IE Format 3 (9.2.1.2.3). The Insert style deals with the supported *Indication* services, each service with a corresponding *Indication* ID listed in Section 7.5.4.1. The RAN parameters, associated with each Insert *RIC Indication* service, are included by the E2 node in the *RIC Indication* message. Via the *RIC Indication* message, the E2 node seeks the near-RT RIC to accept or deny the request raised by the E2 node and to accordingly set the values for the associated RAN parameters by the RIC via the control action in the ensuing *RIC Control Request* message from the RIC.

#### 7.5.4.3 INSERT Service *RIC Indication Header* IE contents

This **INSERT** Service style uses *RIC Indication Header* IE Format 2 (9.2.1.3.2). The *RIC Indication Header* IE has the UE ID, the *Insert* Service Style ID and the corresponding *Insert* Indication ID.

#### 7.5.4.4 INSERT Service *RIC Indication Message* IE contents

This **INSERT** Service style uses *RIC Indication Message* IE Format 5 (9.2.1.4.5). The *RIC Indication Message* IE includes a sequence of associated RAN parameters for which the E2 node seeks the near-RT RIC to accept/deny the request raised by the E2 node and accordingly set the values for the associated RAN parameters, via the control action in the ensuing *RIC Control Request* IE.

#### 7.5.4.5 INSERT Service *RIC Call Process ID* IE contents

This **INSERT** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

### 7.5.5 INSERT Service Style 4: Radio Access Control Request

#### 7.5.5.1 INSERT Service Style description

This **INSERT** Service style provides a mechanism to initiate request for controlling the radio access of the UE using the *RIC Indication Message* IE and associated *RIC Indication Header* IE. The E2 node sends a *RIC Indication* message to the near-RT RIC and the ongoing call process is suspended at the E2 node until the E2 node hears back from the RIC. The optional *RIC Call Process ID* IE is used by the E2 node to match a *RIC Control Request* message to a *RIC Indication* message, following which the E2 node can resume the suspended call processing for the UE.

Applications of this service include:

- Request for configuring RACH back-off

- Request for UE admission

- Request for RRC connection reject

- Request for RRC connection releaseRequest for Access barring

This Insert style supports the following *Indication* services, each service listed below with a corresponding *Indication* ID. The RAN parameters, associated with each Insert Indication service, are listed in the sections shown below.

|  |  |  |  |
| --- | --- | --- | --- |
| **Indication**  **ID** | **Indication Name** | **Insert Indication Description** | **Associated RAN Parameters** |
| 1 | UE Admission Control request | To request UE admission control. | 8.3.5.1 |
| 2 | RACH backoff control request | To request control of RACH backoff parameters | 8.3.5.2 |
| 3 | Access barring control request | To request access barring configuration parameters configuration | 8.3.5.3 |
| 4 | RRC connection release | To request release of an RRC connection for a UE | 8.3.5.4 |
| 5 | RRC connection reject | To request rejection of an RRC connection for a UE | 8.3.5.5 |

#### 7.5.5.2 INSERT Service *RIC Action Definition* IE contents

This **INSERT** Service style uses the *RIC Action Definition* IE Format 3 (9.2.1.2.3). The Insert style deals with the supported *Indication* services, each service with a corresponding *Indication* ID listed in Section 7.5.5.1. The RAN parameters, associated with each Insert *Indication* service, are included by the E2 node in the *RIC Indication* message. Via the *RIC Indication* message, the E2 node seeks the near-RT RIC to accept or deny the request raised by the E2 node and to accordingly set the values for the associated RAN parameters by the RIC via the control action in the ensuing *RIC Control Request* message from the RIC.

#### 7.5.5.3 INSERT Service *RIC Indication Header* IE contents

This **INSERT** Service style uses *RIC Indication Header* IE Format 2 (9.2.1.3.2). The *RIC Indication Header* IE has the UE ID, the *Insert* Service Style ID and the corresponding *Insert* Indication ID.

#### 7.5.5.4 INSERT Service *RIC Indication Message* IE contents

This **INSERT** Service style uses *RIC Indication Message* IE Format 5 (9.2.1.4.5). The *RIC Indication Message* IE includes a sequence of associated RAN parameters for which the E2 node seeks the near-RT RIC to accept/deny the request raised by the E2 node and accordingly set the values for the associated RAN parameters, via the control action in the ensuing *RIC Control Request* IE.

#### 7.5.5.5 INSERT Service *RIC Call Process ID* IE contents

This **INSERT** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

### 7.5.6 INSERT Service Style 5: Dual Connectivity Control Request

#### 7.5.6.1 INSERT Service Style description

This **INSERT** Service style provides a mechanism to initiate request for controlling the dual connectivity of the UE using the *RIC Indication Message* IE and associated *RIC Indication Header* IE. The E2 node sends a *RIC Indication* message to the near-RT RIC and the ongoing call process is suspended at the E2 node until the E2 node hears back from the RIC. The optional *RIC Call Process ID* IE is used by the E2 node to match a *RIC Control Request* message to a *RIC Indication* message, following which the E2 node can resume the suspended call processing for the UE.

Applications of this service include:

- Request for Dual connectivity (EN-DC, MR-DC or NR-NR DC) initiation for a selected UE towards a target secondary cell (PScell)

- Request for Secondary cell change for a selected UE towards a target secondary cell (PScell)

- Request for Dual connectivity (EN-DC, MR-DC or NR-NR DC) modification for a selected UE

- Request for Dual connectivity (EN-DC, MR-DC or NR-NR DC) release initiation for a selected UE

- Request for Change of bearer termination point (MN or SN) and/or bearer types for a selected UE

This Insert style supports the following *Indication* services, each service listed below with a corresponding *Indication* ID. The RAN parameters, associated with each Insert Indication service, are listed in the sections shown below.

|  |  |  |  |
| --- | --- | --- | --- |
| Indication  ID | Indication Name | Insert Indication Description | Associated RAN parameters |
| 1 | DC Secondary Node  Addition Control request | To request secondary node addition for dual connectivity | 8.3.6.1 |
| 2 | DC Secondary Node Modification and Release Control request | To request modification of secondary node for DC | 8.3.6.2 |
| 3 | DC PSCell Change control request | To request PSCell change of a UE within a secondary node or to another secondary node | 8.3.6.3 |
| 4 | DC Secondary Node Change Control request | To request changing the secondary node of a UE for DC | 8.3.6.4 |
| 5 | DC DRB termination control request | To request a change in the bearer termination point | 8.3.2.5 |

#### 7.5.6.2 INSERT Service *RIC Action Definition* IE contents

This **INSERT** Service style uses the *RIC Action Definition* IE Format 3 (9.2.1.2.3). The Insert style deals with the supported *Indication* services, each service with a corresponding *Indication* ID listed in Section 7.5.6.1. The RAN parameters, associated with each Insert *Indication* service, are included by the E2 node in the *RIC Indication* message. Via the *RIC Indication* message, the E2 node seeks the near-RT RIC to accept or deny the request raised by the E2 node and to accordingly set the values for the associated RAN parameters by the RIC via the control action in the ensuing *RIC Control Request* message from the RIC.

#### 7.5.6.3 INSERT Service *RIC Indication Header* IE contents

This **INSERT** Service style uses *RIC Indication Header* IE Format 2 (9.2.1.3.2). The *RIC Indication Header* IE has the UE ID, the *Insert* Service Style ID and the corresponding *Insert* Indication ID.

#### 7.5.6.4 INSERT Service *RIC Indication Message* IE contents

This **INSERT** Service style uses *RIC Indication Message* IE Format 5 (9.2.1.4.5). The *RIC Indication Message* IE includes a sequence of associated RAN parameters for which the E2 node seeks the near-RT RIC to accept/deny the request raised by the E2 node and accordingly set the values for the associated RAN parameters, via the control action in the ensuing *RIC Control Request* IE.

#### 7.5.6.5 INSERT Service *RIC Call Process ID* IE contents

This **INSERT** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

### 7.5.7 INSERT Service Style 6: Carrier Aggregation Control Request

#### 7.5.7.1 INSERT Service Style description

This **INSERT** Service style provides a mechanism to initiate request for controlling the carrier aggregation of the UE using the *RIC Indication Message* IE and associated *RIC Indication Header* IE. The E2 node sends a *RIC Indication* message to the near-RT RIC and the ongoing call process is suspended at the E2 node until the E2 node hears back from the RIC. The optional *RIC Call Process ID* IE is used by the E2 node to match a *RIC Control Request* message to a *RIC Indication* message, following which the E2 node can resume the suspended call processing for the UE.

Applications of this service include:

- Request for Carrier Aggregation (CA) initiation for a selected UE towards a target secondary cell or cells

- Request for Carrier Aggregation (CA) modification for a selected UE, or Secondary cell change for a selected UE towards a target secondary cell or cells

- Request for Carrier Aggregation (CA) release initiation for a selected UE

This Insert style supports the following *Indication* services, each service listed below with a corresponding *Indication* ID. The RAN parameters, associated with each Insert Indication service, are listed in the sections shown below.

|  |  |  |  |
| --- | --- | --- | --- |
| **Indication**  **ID** | **Indication Name** | **Insert Indication Description** | **Associated RAN parameters** |
| 1 | CA Secondary Cell Addition Control request | To request control of the secondary cell addition for a UE | 8.3.7.1 |
| 2 | CA Secondary Cell Modification and Release Control request | To request control of the modification and release of secondary cells for a UE | 8.3.7.2 |

#### 7.5.7.2 INSERT Service *RIC Action Definition* IE contents

This **INSERT** Service style uses the *RIC Action Definition* IE Format 3 (9.2.1.2.3). The Insert style deals with the supported *Indication* services, each service with a corresponding *Indication* ID listed in Section 7.5.7.1. The RAN parameters, associated with each Insert *Indication* service, are included by the E2 node in the *RIC Indication* message. Via the *RIC Indication* message, the E2 node seeks the near-RT RIC to accept or deny the request raised by the E2 node and to accordingly, set the values for the associated RAN parameters by the RIC via the control action in the ensuing *RIC Control Request* message from the RIC.

#### 7.5.7.3 INSERT Service *RIC Indication Header* IE contents

This **INSERT** Service style uses *RIC Indication Header* IE Format 2 (9.2.1.3.2). The *RIC Indication Header* IE has the UE ID, the *Insert* Service Style ID and the corresponding *Insert* Indication ID.

#### 7.5.7.4 INSERT Service *RIC Indication Message* IE contents

This **INSERT** Service style uses *RIC Indication Message* IE Format 5 (9.2.1.4.5). The *RIC Indication Message* IE includes a sequence of associated RAN parameters for which the E2 node seeks the near-RT RIC to accept/deny the request raised by the E2 node and accordingly set the values for the associated RAN parameters, via the control action in the ensuing *RIC Control Request* IE**.**

#### 7.5.7.5 INSERT Service *RIC Call Process ID* IE contents

This **INSERT** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

### 7.5.8 INSERT Service Style 7: Idle Mode Mobility Control Request

#### 7.5.8.1 INSERT Service Style description

This **INSERT** Service style provides a mechanism to initiate request for controlling the idle mode mobility of the UE using the *RIC Indication Message* IE and associated *RIC Indication Header* IE. The E2 node sends a *RIC Indication* message to the near-RT RIC and the ongoing call process is suspended at the E2 node until the E2 node hears back from the RIC. The optional *RIC Call Process ID* IE is used by the E2 node to match a *RIC Control Request* message to a *RIC Indication* message, following which the E2 node can resume the suspended call processing for the UE.

Applications of this service include:

- Intra-frequency, inter-frequency, inter-RAT cell reselection priority

- Idle timers

This Insert style supports the following *Indication* services, each service listed below with a corresponding *Indication* ID. The RAN parameters, associated with each Insert Indication service, are listed in the sections shown below.

|  |  |  |  |
| --- | --- | --- | --- |
| **Indication**  **ID** | **Indication Name** | **Insert Indication Description** | **Associated RAN parameters** |
| 1 | Cell re-selection priority request | To request assignment of cell re-selection priorities for a UE during idle mode (RRC\_IDLE) | 8.3.8.1 |

#### 7.5.8.2 INSERT Service *RIC Action Definition* IE contents

This **INSERT** Service style uses the *RIC Action Definition* IE Format 3 (9.2.1.2.3). The Insert style deals with the supported *Indication* services, each service with a corresponding *Indication* ID listed in Section 7.5.8.1. The RAN parameters, associated with each Insert *Indication* service, are included by the E2 node in the *RIC Indication* message. Via the *RIC Indication* message, the E2 node seeks the near-RT RIC to accept or deny the request raised by the E2 node and to accordingly, set the values for the associated RAN parameters by the RIC via the control action in the ensuing *RIC Control Request* message from the RIC.

#### 7.5.8.3 INSERT Service *RIC Indication Header* IE contents

This **INSERT** Service style uses *RIC Indication Header* IE Format 2 (9.2.1.3.2). The *RIC Indication Header* IE has the UE ID, the *Insert* Service Style ID and the corresponding *Insert* Indication ID.

#### 7.5.8.4 INSERT Service *RIC Indication Message* IE contents

This **INSERT** Service style uses *RIC Indication Message* IE Format 5 (9.2.1.4.5). The *RIC Indication Message* IE includes a sequence of associated RAN parameters for which the E2 node seeks the near-RT RIC to accept/deny the request raised by the E2 node or accordingly set the values for the associated RAN parameters, via the control action in the ensuing *RIC Control Request* IE**.**

#### 7.5.8.5 INSERT Service *RIC Call Process ID* IE contents

This **INSERT** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

### 7.5.9 INSERT Service Style 255: Multiple Actions Control Request

#### 7.5.9.1 INSERT Service Style description

This **INSERT** Service style provides a mechanism which contains multiple Insert Indication actions of the selected fundamental level INSERT Service style(s), in order to initiate request to the Near-RT RIC for controlling multiple actions of the supporting functionalities related to the corresponding fundamental level CONTROL Service style(s). If at least one of the embedded Insert Indications is not admitted by E2 node, then the E2 node shall declare the INSERT Action as failed.

7.5.9.2 INSERT Service *RIC Action Definition* IE contents

This **INSERT** Service style uses the *RIC Action Definition* IE Format 4 (9.2.1.2.4).

For each Insert Indicationaction, the corresponding *Insert Indication ID* IE and the associated RAN parameters follow the definitions of the selected fundamental level INSERT Service style indicated by the *Requested Insert Style* IE.

7.5.9.3 INSERT Service *RIC Indication Header* IE contents

This **INSERT** Service style uses *RIC Indication Header* IE Format 3 (9.2.1.3.3).

The *RIC Indication Header* IE may contain the *UE ID* IE, to indicate to the Near-RT RIC that this INSERT indication is only for that specific UE.

7.5.9.4 INSERT Service *RIC Indication Message* IE contents

This **INSERT** Service style uses *RIC Indication Message* IE Format 6 (9.2.1.4.6).

For each Insert Indicationaction, the corresponding *Insert Indication ID* IE and the associated RAN parameters follow the definitions of the selected fundamental level INSERT Service style indicated by the *Indicated Insert Style* IE.

#### 7.5.9.5 INSERT Service *RIC Call Process ID* IE contents

This **INSERT** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

## 7.6 Supported RIC CONTROL Services

### 7.6.1 CONTROL Service Style Types

|  |  |  |
| --- | --- | --- |
| **RIC Style Type** | **Style Name** | **Style Description** |
| 1 | Radio Bearer control | Used to modify the configuration the Radio Bearer Control (RBC) related parameters and/or behaviours at the E2 Node for a specific UE  Belongs to Fundamental level CONTROL Services. |
| 2 | Radio resource allocation control | Used to modify the configuration the Radio Resource Allocation control related parameters and/or behaviours at the E2 Node for a specific E2 Node, cell, slice, UE and/or QoS  Belongs to Fundamental level CONTROL Services. |
| 3 | Connected mode mobility control | Used to initiate a connected mode mobility procedure (Handover or Conditional Handover), optionally with Dual Active Protocol Stack (DAPS), for a specific UE towards either a target cell (for HO) or a list of candidate cells (for CHO)  Belongs to Fundamental level CONTROL Services. |
| 4 | Radio access control | Used to modify Radio access related functions used to control UE access to cells  Belongs to Fundamental level CONTROL Services. |
| 5 | Dual connectivity (DC) control | Used to initiate Dual connectivity (DC) mechanisms  Belongs to Fundamental level CONTROL Services. |
| 6 | Carrier Aggregation (CA) control | Used to initiate Carrier Aggregation (CA) mechanisms  Belongs to Fundamental level CONTROL Services. |
| 7 | Idle mode mobility control | Used to modify Idle mode mobility related functions used to control UE reselection of cells  Belongs to Fundamental level CONTROL Services. |
| 8 | UE information and assignment | Used for *Explicit UE list* assignment, UE information report generation and to complete UE identification. These services are used to support other RIC services.  Belongs to Fundamental level CONTROL Services. |
| 9 | Measurement Reporting Configuration control | Used to control the measurement report configuration |
| 255 | Multiple Actions Control | Used for multiple actions of the selected fundamental level CONTROL Service style(s).  Belongs to lntegrated level CONTROL Services. |

Each of the Control Service styles 1-9 listed above points to adopt the following common features:

- Control Action ID: The index ID for the individual control action under a given Control Service style.

- Control Action Name: Indicates the functionality of the E2 node which is controlled by Near-RT RIC

- Control Action Description: Describes the control action and functionality of the receiving E2 Node.

- Associated RAN parameters: Identifies the RAN parameters to be controlled by Near-RT RIC pertaining to the given control action.

The Control Service style 255 supports multiple parallel actions configured per *RIC Control Request* message by reusing the control actions and the associated RAN parameters defined in the selected fundamental level Control Service style(s).

The details of the individual Control Service styles are provided in subsequent sections.

### 7.6.2 CONTROL Service Style 1: Radio Bearer Control

#### 7.6.2.1 CONTROL Service Style description

This **CONTROL** Service style provides a mechanism to initiate or resume a radio bearer control related process using the *RIC Control Message* IE and associated *RIC Control Header* IE and the optional *RIC Call Process ID* IE used when resuming a call process following a previous INSERT service. The corresponding INSERT service is service style 1 covered in Section 7.5.2.

Applications of this service include:

- DRB QoS Modification, to tune DRB level QoS related parameters to meet the QoS optimization targets.

- QoS Flow (re)mapping, to adjust the mapping relationship between QoS flows and DRBs.

- Logical channel (re)configuration

- Radio Bearer Admission Control, to configure DRB admission control such as reject or release may be applied

- Split bearer and PDCP duplication control

The supported RAN control actions and the corresponding RAN parameters are as follows.

|  |  |  |  |
| --- | --- | --- | --- |
| **Control**  **Action**  **ID** | **Control Action Name** | **Control Action description** | **Associated RAN Parameters** |
| 1 | DRB QoS Configuration | To control the configuration of DRB QoS profile | 8.4.2.1 |
| 2 | QoS flow mapping configuration | To control the multiplexing of QoS flows to a DRB (addition, modification, deletion | 8.4.2.2 |
| 3 | Logical channel configuration | To control the LCID configuration of a DRB | 8.4.2.3 |
| 4 | Radio admission control | To control radio admission of a UE | 8.4.2.4 |
| 5 | DRB termination control | To control the change in bearer termination point | 8.4.2.5 |
| 6 | DRB split ratio control | To control the split ratio of a DRB across its RLC entities | 8.4.2.6 |
| 7 | PDCP Duplication control | To control activation or de-activation of PDCP duplication for a DRB and control/configure the number of legs or RLC entities for the DRB | 8.4.2.7 |

#### 7.6.2.2 CONTROL Service *RIC Control Header* IE contents

This **CONTROL** Service *RIC Control Header* IE has the *UE ID* IE, the *Control* Service Style ID, the *Control Action ID* IE and the *RIC* *Control Decision* IE that indicates whether the RIC accepts or rejects the INDICATION request from the previous incoming INSERT indication, if any (with matching *RAN Call Process ID* IE), from the E2 node.

This **CONTROL** style uses *RIC* *Control Header* IE Format 1 (9.2.1.6.1).

#### 7.6.2.3 CONTROL Service *RIC Control Message* IE contents

This **CONTROL** Service *RIC Control Message* IE contains the sequence of RAN parameters, associated with a given Control Action within this Control Service style, controlled by the near-RT RIC along with the values for these parameters, as set by the RIC.

This **CONTROL** style uses *RIC Control Message* IE Format 1 (9.2.1.7.1).

If there is a previous INSERT Indication Request to the RIC, then the corresponding Control Action ID used by the RIC for the ensuing CONTROL Request message is the one that matches the Insert Indication ID, among the ones provided in the table shown in Section 7.6.2.1. It is to be noted that the control action “Radio admission control” (corresponding to control action ID 4) is used only as a response to an incoming INSERT indication with the corresponding service style and indication request ID and cannot be used asynchronously without a previous INSERT indication.

#### 7.6.2.4 CONTROL Service *RIC Call Process ID* IE contents

This **CONTROL** Service *RIC Call Process ID* IE contains identifier used by the Near-RT RIC to allow the RAN Function to match the outgoing **INSERT** Service message with a subsequent incoming **CONTROL** Service message.

This **CONTROL** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

#### 7.6.2.5 CONTROL Service *RIC Control Outcome* IE contents

This **CONTROL** Service *RIC Control Outcome* IE contains a transparent container that is used to carry the outcome of processing the incoming *RIC Control Request* message. However, this does not reflect the outcome of the call processing upon receiving the message.

This **CONTROL** style uses *RIC Control Outcome* IE Format 1 (9.2.1.8.1).

|  |  |  |  |
| --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter Name | RAN Parameter Type | Parameter Description |
| 1 | ReceivedTimestamp | OCTET STRING (SIZE(8)) | Time RIC Control Request message received by RAN Function over E2 interface.  Carries UTC time encoded as the 64-bit timestamp format as defined in section Section 6 of IETF RFC 5905 [30] containing both seconds and fraction parts. |

### 7.6.3 CONTROL Service Style 2: Radio Resource Allocation Control

#### 7.6.3.1 CONTROL Service Style description

This **CONTROL** Service style provides a mechanism to initiate or resume a radio resource allocation control related process using the *RIC Control Message* IE and associated *RIC Control Header* IE and the optional *RIC Call Process ID* IE used when resuming a call process following a previous INSERT service. The corresponding INSERT service is service style 2 covered in Section 7.5.3.

Applications of this service include:

- Discontinuous Reception (DRX) control

- Scheduling request (SR) control

- Semi-Persistent Scheduling (SPS) control

- Configured Grant control

- Channel Quality Indicator (CQI) table

- Slice level PRB quota

The supported RAN control actions and the corresponding RAN parameters are as follows.

|  |  |  |  |
| --- | --- | --- | --- |
| **Control**  **Action**  **ID** | **Control Action Name** | **Control Action description** | **Associated RAN Parameters** |
| 1 | DRX parameter configuration | To control the configuration of DRX parameters | 8.4.3.1 |
| 2 | SR periodicity configuration | To control the configuration of SR periodicity parameters | 8.4.3.2 |
| 3 | SPS parameters configuration | To control the configuration of SPS parameters | 8.4.3.3 |
| 4 | Configured grant control | To control the configuration of uplink grants to the UE | 8.4.3.4 |
| 5 | CQI table configuration | To control the configuration of CQI table. | 8.4.3.5 |
| 6 | Slice-level PRB quota | To control the radio resource management policy for slice-specific PRB quota allocation | 8.4.3.6 |

#### 7.6.3.2 CONTROL Service *RIC Control Header* IE contents

This **CONTROL** Service *RIC Control Header* IE has the *UE ID* IE, the *Control* Service Style ID, the *Control Action ID* IE and the *RIC* *Control Decision* IE that indicates whether the RIC accepts or rejects the INDICATION request from the previous incoming INSERT indication, if any (with matching *RAN Call Process ID* IE), from the E2 node.

This **CONTROL** style uses *RIC* *Control Header* IE Format 1 (9.2.1.6.1).

#### 7.6.3.3 CONTROL Service *RIC Control Message* IE contents

This **CONTROL** Service *RIC Control Message* IE contains the sequence of RAN parameters, associated with a given Control Action within this Control Service style, controlled by the near-RT RIC along with the values for these parameters, as set by the RIC.

This **CONTROL** style uses *RIC Control Message* IE Format 1 (9.2.1.7.1).

If there is a previous INSERT Indication Request to the RIC, then the corresponding Control Action ID used by the RIC for the ensuing CONTROL Request message is the one that matches the Insert Indication ID, among the ones provided in the table shown in Section 7.6.3.1.

#### 7.6.3.4 CONTROL Service *RIC Call Process ID* IE contents

This **CONTROL** Service *RIC Call Process ID* IE contains identifier used by the Near-RT RIC to allow the RAN Function to match the outgoing **INSERT** Service message with a subsequent incoming **CONTROL** Service message.

This **CONTROL** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

#### 7.6.3.5 CONTROL Service *RIC Control Outcome* IE contents

This **CONTROL** Service *RIC Control Outcome* IE contains a transparent container that is used to carry the outcome of processing the incoming *RIC Control Request* message. However, this does not reflect the outcome of the call processing upon receiving the message.

This **CONTROL** style uses *RIC Control Outcome* IE Format 1 (9.2.1.8.1).

|  |  |  |  |
| --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter Name | RAN Parameter Type | Parameter Description |
| 1 | ReceivedTimestamp | OCTET STRING (SIZE(8)) | Time RIC Control Request message received by RAN Function over E2 interface.  Carries UTC time encoded as the 64-bit timestamp format as defined in section Section 6 of IETF RFC 5905 [30] containing both seconds and fraction parts. |

### 7.6.4 CONTROL Service Style 3: Connected Mode Mobility

#### 7.6.4.1 CONTROL Service Style description

This **CONTROL** Service style provides a mechanism to initiate or resume a connected mode mobility control related process using the *RIC Control Message* IE and associated *RIC Control Header* IE and the optional *RIC Call Process ID* IE used when resuming a call process following a previous INSERT service. The corresponding INSERT service is service style 3 covered in Section 7.5.4.

Applications of this service include:

- Handover (HO) initiation for a selected UE towards a target cell

- Conditional handover (CHO) initiation for a selected UE towards a list of candidate cell(s)

- Handover (HO) initiation with Dual Active Protocol Stack (DAPS) for a selected UE towards a target cell

The supported RAN control actions and the corresponding RAN parameters are as follows.

|  |  |  |  |
| --- | --- | --- | --- |
| **Control**  **Action**  **ID** | **Control Action Name** | **Control Action description** | **Associated RAN parameters** |
| 1 | Handover Control | To control the handover of the primary cell and subsequent secondary cell reselection | 8.4.4.1 |
| 2 | Conditional Handover Control | To control the conditional handover involving target primary cells | 8.4.4.2 |
| 3 | DAPS (Dual Active Protocol Stack) Handover Control | To control the DAPS handover of the UE between source cell and target cell | 8.4.4.3 |

#### 7.6.4.2 CONTROL Service *RIC Control Header* IE contents

This **CONTROL** Service *RIC Control Header* IE has the *UE ID* IE, the *Control* Service Style ID, the *Control Action ID* IE and the *RIC* *Control Decision* IE that indicates whether the RIC accepts or rejects the INDICATION request from the previous incoming INSERT indication, if any (with matching *RAN Call Process ID* IE), from the E2 node.

This **CONTROL** style uses *RIC* *Control Header* IE Format 1 (9.2.1.6.1).

#### 7.6.4.3 CONTROL Service *RIC Control Message* IE contents

This **CONTROL** Service *RIC Control Message* IE contains the sequence of RAN parameters, associated with a given Control Action within this Control Service style, controlled by the near-RT RIC along with the values for these parameters, as set by the RIC.

This **CONTROL** style uses *RIC Control Message* IE Format 1 (9.2.1.7.1).

If there is a previous INSERT Indication Request to the RIC, then the corresponding Control Action ID used by the RIC for the ensuing CONTROL Request message is the one that matches the Insert Indication ID, among the ones provided in the table shown in Section 7.6.4.1.

#### 7.6.4.4 CONTROL Service *RIC Call Process ID* IE contents

This **CONTROL** Service *RIC Call Process ID* IE contains identifier used by the Near-RT RIC to allow the RAN Function to match the outgoing **INSERT** Service message with a subsequent incoming **CONTROL** Service message.

This **CONTROL** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

#### 7.6.4.5 CONTROL Service *RIC Control Outcome* IE content

This **CONTROL** Service *RIC Control Outcome* IE contains a transparent container that is used to carry the outcome of processing the incoming *RIC Control Request* message. However, this does not reflect the outcome of the call processing upon receiving the message.

This **CONTROL** style uses *RIC Control Outcome* IE Format 1 (9.2.1.8.1).

|  |  |  |  |
| --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter Name | RAN Parameter Type | Parameter Description |
| 1 | ReceivedTimestamp | OCTET STRING (SIZE(8)) | Time RIC Control Request message received by RAN Function over E2 interface.  Carries UTC time encoded as the 64-bit timestamp format as defined in section Section 6 of IETF RFC 5905 [30] containing both seconds and fraction parts. |

### 7.6.5 CONTROL Service Style 4: Radio Access Control

#### 7.6.5.1 CONTROL Service Style description

This **CONTROL** Service style provides a mechanism to initiate or resume a radio access control related process using the *RIC Control Message* IE and associated *RIC Control Header* IE and the optional *RIC Call Process ID* IE used when resuming a call process following a previous INSERT service. The corresponding INSERT service is service style 4 covered in Section 7.5.5.

Applications of this service include:

- RACH back-off

- RRC connection reject

- RRC connection release

- Access barring

- UE admission

The supported RAN control actions and the corresponding RAN parameters are as follows.

|  |  |  |  |
| --- | --- | --- | --- |
| **Control**  **Action**  **ID** | **Control Action Name** | **Control Action Description** | **Associated RAN Parameters** |
| 1 | UE Admission Control | To control UE admission. | 8.4.5.1 |
| 2 | RACH backoff control | To control RACH backoff parameters | 8.4.5.2 |
| 3 | Access barring control | To control access barring configuration parameters | 8.4.5.3 |
| 4 | RRC Connection Release control | To control release of RRC connection of the UE | 8.4.5.4 |
| 5 | RRC Connection Reject control | To reject RRC connection request of the UE | 8.4.5.5 |

#### 7.6.5.2 CONTROL Service *RIC Control Header* IE contents

This **CONTROL** Service *RIC Control Header* IE has the *UE ID* IE, the *Control* Service Style ID, the *Control Action ID* IE and the *RIC* *Control Decision* IE that indicates whether the RIC accepts or rejects the INDICATION request from the previous incoming INSERT indication, if any (with matching *RAN Call Process ID* IE), from the E2 node.

This **CONTROL** style uses *RIC* *Control Header* IE Format 1 (9.2.1.6.1).

#### 7.6.5.3 CONTROL Service *RIC Control Message* IE contents

This **CONTROL** Service *RIC Control Message* IE contains the sequence of RAN parameters, associated with a given Control Action within this Control Service style, controlled by the near-RT RIC along with the values for these parameters, as set by the RIC.

This **CONTROL** style uses *RIC Control Message* IE Format 1 (9.2.1.7.1).

If there is a previous INSERT Indication Request to the RIC, then the corresponding Control Action ID used by the RIC for the ensuing CONTROL Request message is the one that matches the Insert Indication ID, among the ones provided in the table shown in Section 7.6.5.1. However, the control action “RRC Connection Reject control” (corresponding to control action ID 5) can also be used to handle an incoming INSERT Indication Request corresponding to service style 4 that uses Indication request ID 1 (that corresponds to UE Admission Control Request). It is also to be noted that the control action “UE admission control” (corresponding to control action ID 1) is used only as a response to an incoming INSERT indication with the corresponding service style and indication request ID and cannot be used asynchronously without a previous INSERT indication.

#### 7.6.5.4 CONTROL Service *RIC Call Process ID* IE contents

This **CONTROL** Service *RIC Call Process ID* IE contains identifier used by the Near-RT RIC to allow the RAN Function to match the outgoing **INSERT** Service message with a subsequent incoming **CONTROL** Service message.

This **CONTROL** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

#### 7.6.5.5 CONTROL Service *RIC Control Outcome* IE contents

This **CONTROL** Service *RIC Control Outcome* IE contains a transparent container that is used to carry the outcome of processing the incoming *RIC Control Request* message. However, this does not reflect the outcome of the call processing upon receiving the message.

This **CONTROL** style uses *RIC Control Outcome* IE Format 1 (9.2.1.8.1).

|  |  |  |  |
| --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter Name | RAN Parameter Type | Parameter Description |
| 1 | ReceivedTimestamp | OCTET STRING (SIZE(8)) | Time RIC Control Request message received by RAN Function over E2 interface.  Carries UTC time encoded as the 64-bit timestamp format as defined in section Section 6 of IETF RFC 5905 [30] containing both seconds and fraction parts. |

### 7.6.6 CONTROL Service Style 5: Dual Connectivity Control

#### 7.6.6.1 CONTROL Service Style description

This **CONTROL** Service style provides a mechanism to initiate or resume a dual connectivity control related process using the *RIC Control Message* IE and associated *RIC Control Header* IE and the optional *RIC Call Process ID* IE used when resuming a call process following a previous INSERT service. The corresponding INSERT service is service style 5 covered in Section 7.5.6.

Applications of this service include:

- Dual connectivity (EN-DC, MR-DC or NR-NR DC) initiation for a selected UE towards a target secondary cell (PScell)

- Secondary cell change for a selected UE towards a target secondary cell (PScell)

- Dual connectivity (EN-DC, MR-DC or NR-NR DC) modification for a selected UE

- Dual connectivity (EN-DC, MR-DC or NR-NR DC) release initiation for a selected UE

- Change of bearer termination point (MN or SN) and/or bearer types for a selected UE

The supported RAN control actions and the corresponding RAN parameters are as follows.

|  |  |  |  |
| --- | --- | --- | --- |
| **Control**  **Action**  **ID** | **Control Action Name** | **Control Action Description** | **Associated RAN parameters** |
| 1 | DC Secondary Node  Addition Control | To control secondary node addition for dual connectivity | 8.4.6.1 |
| 2 | DC Secondary Node Modification and release Control | To control modification and release of secondary node for DC | 8.4.6.2 |
| 3 | DC PSCell Change control | To control PSCell change of a UE within a secondary node or to another secondary node | 8.4.6.3 |
| 4 | DC Secondary Node Change Control | To control changing the secondary node of a UE for DC | 8.4.6.4 |

#### 7.6.6.2 CONTROL Service *RIC Control Header* IE contents

This **CONTROL** Service *RIC Control Header* IE has the *UE ID* IE, the *Control* Service Style ID, the *Control Action ID* IE and the *RIC* *Control Decision* IE that indicates whether the RIC accepts or rejects the INDICATION request from the previous incoming INSERT indication, if any (with matching *RAN Call Process ID* IE), from the E2 node.

This **CONTROL** style uses *RIC* *Control Header* IE Format 1 (9.2.1.6.1).

#### 7.6.6.3 CONTROL Service *RIC Control Message* IE contents

This **CONTROL** Service *RIC Control Message* IE contains the sequence of RAN parameters, associated with a given Control Action within this Control Service style, controlled by the near-RT RIC along with the values for these parameters, as set by the RIC.

This **CONTROL** style uses *RIC Control Message* IE Format 1 (9.2.1.7.1).

If there is a previous INSERT Indication Request to the RIC, then the corresponding Control Action ID used by the RIC for the ensuing CONTROL Request message is the one that matches the Insert Indication ID, among the ones provided in the table shown in Section 7.6.6.1.

#### 7.6.6.4 CONTROL Service *RIC Call Process ID* IE contents

This **CONTROL** Service *RIC Call Process ID* IE contains identifier used by the Near-RT RIC to allow the RAN Function to match the outgoing **INSERT** Service message with a subsequent incoming **CONTROL** Service message.

This **CONTROL** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

#### 7.6.6.5 CONTROL Service *RIC Control Outcome* IE contents

This **CONTROL** Service *RIC Control Outcome* IE contains a transparent container that is used to carry the outcome of processing the incoming *RIC Control Request* message. However, this does not reflect the outcome of the call processing upon receiving the message.

This **CONTROL** style uses *RIC Control Outcome* IE Format 1 (9.2.1.8.1).

|  |  |  |  |
| --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter Name | RAN Parameter Type | Parameter Description |
| 1 | ReceivedTimestamp | OCTET STRING (SIZE(8)) | Time RIC Control Request message received by RAN Function over E2 interface.  Carries UTC time encoded as the 64-bit timestamp format as defined in section Section 6 of IETF RFC 5905 [30] containing both seconds and fraction parts. |

### 7.6.7 CONTROL Service Style 6: Carrier Aggregation Control

#### 7.6.7.1 CONTROL Service Style description

This **CONTROL** Service style provides a mechanism to initiate or resume a carrier aggregation control related process using the *RIC Control Message* IE and associated *RIC Control Header* IE and the optional *RIC Call Process ID* IE used when resuming a call process following a previous INSERT service. The corresponding INSERT service is service style 6 covered in Section 7.5.7.

Applications of this service include:

- Carrier Aggregation (CA) initiation for a selected UE towards a target secondary cell or cells

- Secondary cell change for a selected UE towards a target secondary cell or cells

- Carrier Aggregation (CA) modification for a selected UE

- Carrier Aggregation (CA) release initiation for a selected UE

The supported RAN control actions and the corresponding RAN parameters are as follows.

|  |  |  |  |
| --- | --- | --- | --- |
| **Control**  **Action**  **ID** | **Control Action Name** | **Control Action Description** | **Associated RAN parameters** |
| 1 | CA Secondary Cell Addition Control | To control secondary cell addition for a UE | 8.4.7.1 |
| 2 | CA Secondary Cell Modification Control | To control modification and release of secondary cells for a UE | 8.4.7.2 |

#### 7.6.7.2 CONTROL Service *RIC Control Header* IE contents

This **CONTROL** Service *RIC Control Header* IE has the *UE ID* IE, the *Control* Service Style ID, the *Control Action ID* IE and the *RIC* *Control Decision* IE that indicates whether the RIC accepts or rejects the INDICATION request from the previous incoming INSERT indication, if any (with matching *RAN Call Process ID* IE), from the E2 node.

This **CONTROL** style uses *RIC* *Control Header* IE Format 1 (9.2.1.6.1).

#### 7.6.7.3 CONTROL Service *RIC Control Message* IE contents

This **CONTROL** Service *RIC Control Message* IE contains the sequence of RAN parameters, associated with a given Control Action within this Control Service style, controlled by the near-RT RIC along with the values for these parameters, as set by the RIC.

This **CONTROL** style uses *RIC Control Message* IE Format 1 (9.2.1.7.1).

If there is a previous INSERT Indication Request to the RIC, then the corresponding Control Action ID used by the RIC for the ensuing CONTROL Request message is the one that matches the Insert Indication ID, among the ones provided in the table shown in Section 7.6.7.1.

#### 7.6.7.4 CONTROL Service *RIC Call Process ID* IE contents

This **CONTROL** Service *RIC Call Process ID* IE contains identifier used by the Near-RT RIC to allow the RAN Function to match the outgoing **INSERT** Service message with a subsequent incoming **CONTROL** Service message.

This **CONTROL** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

#### 7.6.7.5 CONTROL Service *RIC Control Outcome* IE contents

This **CONTROL** Service *RIC Control Outcome* IE contains a transparent container that is used to carry the outcome of processing the incoming *RIC Control Request* message. However, this does not reflect the outcome of the call processing upon receiving the message.

This **CONTROL** style uses *RIC Control Outcome* IE Format 1 (9.2.1.8.1).

|  |  |  |  |
| --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter Name | RAN Parameter Type | Parameter Description |
| 1 | ReceivedTimestamp | OCTET STRING (SIZE(8)) | Time RIC Control Request message received by RAN Function over E2 interface.  Carries UTC time encoded as the 64-bit timestamp format as defined in section Section 6 of IETF RFC 5905 [30] containing both seconds and fraction parts. |

### 7.6.8 CONTROL Service Style 7: Idle Mode Mobility Control

#### 7.6.8.1 CONTROL Service Style description

This **CONTROL** Service style provides a mechanism to initiate or resume a idle mode mobility control related process using the *RIC Control Message* IE and associated *RIC Control Header* IE and the optional *RIC Call Process ID* IE used when resuming a call process following a previous INSERT service. The corresponding INSERT service is service style 6 covered in Section 7.5.7.

Applications of this service include:

- Intra-frequency, inter-frequency, inter-RAT cell reselection priority

- Idle timers

The supported RAN control actions and the corresponding RAN parameters are as follows.

|  |  |  |  |
| --- | --- | --- | --- |
| **Control Action**  **ID** | **Control Action Name** | **Control Action Description** | **Associated RAN parameters** |
| 1 | Cell re-selection priority control | To assign cell re-selection priorities for a UE during idle mode (RRC\_IDLE) | 8.4.8.1 |

#### 7.6.8.2 CONTROL Service *RIC Control Header* IE contents

This **CONTROL** Service *RIC Control Header* IE has the *UE ID* IE, the *Control* Service Style ID, the *Control Action ID* IE and the *RIC* *Control Decision* IE that indicates whether the RIC accepts or rejects the INDICATION request from the previous incoming INSERT indication, if any (with matching *RAN Call Process ID* IE), from the E2 node.

This **CONTROL** style uses *RIC* *Control Header* IE Format 1 (9.2.1.6.1).

#### 7.6.8.3 CONTROL Service *RIC Control Message* IE contents

This **CONTROL** Service *RIC Control Message* IE contains the sequence of RAN parameters, associated with a given Control Action within this Control Service style, controlled by the near-RT RIC along with the values for these parameters, as set by the RIC.

This **CONTROL** style uses *RIC Control Message* IE Format 1 (9.2.1.7.1)

If there is a previous INSERT Indication Request to the RIC, then the corresponding Control Action ID used by the RIC for the ensuing CONTROL Request message is the one that matches the Insert Indication ID, among the ones provided in the table shown in Section 7.6.8.1.

#### 7.6.8.4 CONTROL Service *RIC Call Process ID* IE contents

This **CONTROL** Service *RIC Call Process ID* IE contains identifier used by the Near-RT RIC to allow the RAN Function to match the outgoing **INSERT** Service message with a subsequent incoming **CONTROL** Service message.

This **CONTROL** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

#### 7.6.8.5 CONTROL Service *RIC Control Outcome* IE contents

This **CONTROL** Service *RIC Control Outcome* IE contains a transparent container that is used to carry the outcome of processing the incoming *RIC Control Request* message. However, this does not reflect the outcome of the call processing upon receiving the message.

This **CONTROL** style uses *RIC Control Outcome* IE Format 1 (9.2.1.8.1).

|  |  |  |  |
| --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter Name | RAN Parameter Type | Parameter Description |
| 1 | ReceivedTimestamp | OCTET STRING (SIZE(8)) | Time RIC Control Request message received by RAN Function over E2 interface.  Carries UTC time encoded as the 64-bit timestamp format as defined in section Section 6 of IETF RFC 5905 [30] containing both seconds and fraction parts. |

### 7.6.9 CONTROL Service Style 8: UE information and assignment

#### 7.6.9.1 CONTROL Service Style description

This **CONTROL** Service style provides a mechanism to both directly and indirectly monitor and control UE information and to add or remove explicit UE assignments to Explicit UE lists.

Applications of this service include:

- UE to Explicit UE list assignment command: Used to Add or Remove the nominated UE to the *Explicit UE list* name, also used to request list of supported *Explicit UE list*

- UE information request: Used to obtain UE information including list of *Explicit UE List* assignments

- UE identification request: Used to complete UE identification

The supported RAN control actions and the corresponding RAN parameters are as follows.

|  |  |  |  |
| --- | --- | --- | --- |
| **Control**  **Action**  **ID** | **Control Action Name** | **Required information** | **RAN Parameter assignment** |
| 1 | UE to Explicit UE list assignment command | - Explicit UE list identifier  - Assignment Command (add UE, remove UE, send list of supported *Explicit UE list*) | 8.4.9.1 |

#### 7.6.9.2 CONTROL Service *RIC Control Header* IE contents

This **CONTROL** Service *RIC Control Header* IE contains the *UE ID* IE, *RIC Style Type* IE and *Control Action ID* IE. There is no previous INSERT Indication request from the E2 node for this service style.

Note that for RIC Action ID =3 "UE identification request", the *UE ID* IE in the *RIC Control Header* IE shall contain information elements set to zero (for INTEGER values), all bits = 0 (for OCTET STRING) or NULL (for PRINTABLE STRING values) if information is not known.

This **CONTROL** style uses *RIC* *Control Header* IE Format 1 (9.2.1.6.1).

#### 7.6.9.3 CONTROL Service *RIC Control Message* IE contents

This **CONTROL** Service *RIC Control Message* IE contains a list of RAN Parameters used to support the information list of Control actions shown in Section 7.6.9.1.

This **CONTROL** style uses *RIC Control Message* IE Format 1 (9.2.1.7.1).

#### 7.6.9.4 CONTROL Service *RIC Call Process ID* IE contents

This **CONTROL** Service *RIC Call Process ID* IE is not supported for this CONTROL service style.

#### 7.6.9.5 CONTROL Service *RIC Control Outcome* IE contents

This **CONTROL** Service *RIC Control Outcome* IE contains a list of RAN Parameters and is used to carry information concerning the outcome of executing the RIC Control Request.

|  |  |  |  |
| --- | --- | --- | --- |
| **Control**  **Action**  **ID** | **Control Action Name** | **Expected information** | **RAN Parameter assignment** |
| 1 | UE to Explicit UE list assignment command | Success case:  - not used (for add/remove commands)  - list of supported Explicit UE list (for assignment command =3)  Failure case:  - Failure Cause | 8.4.9.1 |

This **CONTROL** style uses *RIC Control Outcome* IE Format 1 (9.2.1.8.1).

7.6.10 CONTROL Service Style 255: Multiple Actions Control

7.6.10.1 CONTROL Service Style description

This **CONTROL** Service style provides a mechanism to initiate multiple control actions of the selected fundamental level CONTROL Service style(s) that should be processed in an integrated manner by the E2 Node, i.e. the RIC Control procedure is considered failed if at least one of the indicated control actions is unsuccessfully executed, and RIC CONTROL FAILURE message shall be sent containing the RIC Control Outcome for failed Control Action.

7.6.10.2 CONTROL Service *RIC Control Header* IE contents

This **CONTROL** style uses *RIC* *Control Header* IE Format 2 (9.2.1.6.2).

The *RIC Indication Header* IE may contain the *UE ID* IE to indicate to the E2 Node that this control request is only for that specific UE. The *RIC Control Decision* IE may also be included to indicate to the E2 Node whether the Near-RT RIC accepts or rejects the INDICATION request from the previous incoming INSERT indication, if any (with matching *RAN Call Process ID* IE), from the E2 node.

7.6.10.3 CONTROL Service *RIC Control Message* IE contents

This **CONTROL** style uses *RIC Control Message* IE Format 2 (9.2.1.7.2).

The RAN control actions and the corresponding RAN parameters under a fundamental level Control Service style contained in the *RIC Control Message* IE follows the definitions of the indicated Control Service style.

If this control request is sent as a response to a previous INSERT indication from the E2 node, then the *Control Action ID* IE in the *RIC Control Message* IE is set in accordance with the triggered Insert Indication ID.

7.6.10.4 CONTROL Service *RIC Call Process ID* IE contents

This **CONTROL** Service style uses *RIC Call Process ID* IE Format 1 (9.2.1.5.1).

The optional *RIC Call Process ID* IE is used when resuming a call process following a previous INSERT indication from the E2 Node.

7.6.10.5 CONTROL Service *RIC Control Outcome* IE contents

This **CONTROL** style uses *RIC Control Outcome* IE Format 2 (9.2.1.8.2).

For each control action indicated by the *Control Action ID* IE, the associated RAN parameters are used to carry the corresponding processing outcome.

|  |  |  |  |
| --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter Name | RAN Parameter Type | Parameter Description |
| 1 | ReceivedTimestamp | OCTET STRING (SIZE(8)) | Time RIC Control Request message received by RAN Function over E2 interface.  Carries UTC time encoded as the 64-bit timestamp format as defined in section Section 6 of IETF RFC 5905 [30] containing both seconds and fraction parts. |
| 2 | Cause | OCTET STRING | FFS |

### 7.6.11 CONTROL Service Style 9: Measurement Reporting Configuration Control

#### 7.6.11.1 CONTROL Service Style description

This CONTROL Service style provides a mechanism to add, modify or delete measurement report configuration for the UE to the network using the *RIC Control Message* IE and the *RIC Control Header* IE.

Applications of this service include:

- Add configuration of measurement objects, reporting objects, measurement gaps, etc. for UE reporting

- Modify configuration of measurement objects, reporting objects, measurement gaps, etc. for UE reporting

- Delete configuration of measurement objects, reporting objects, measurement gaps, etc. for UE reporting

The supported RAN control actions and the corresponding RAN parameters are as follows:

|  |  |  |  |
| --- | --- | --- | --- |
| **Control**  **Action**  **ID** | **Control Action Name** | **Control Action description** | **Associated RAN Parameters** |
| 1 | Add MR Configuration | To add configuration of measurement objects, reporting objects, measurement gaps | 8.4.10.1 |
| 2 | Modify MR Configuration | To modify configuration of measurement objects, reporting objects, measurement gaps | 8.4.10.2 |
| 3 | Delete MR Configuration | To delete configuration of measurement objects, reporting objects, measurement gaps | 8.4.10.3 |

#### 7.6.11.2 CONTROL Service *RIC Control Header* IE contents

The CONTROL Service *RIC Control Header* IE has the *UE ID* IE, the *Control Service Style ID* IE, the *Control Action ID* IE. The *RIC Control Decision* IE for this service style is currently not supported for this control service style.

This **CONTROL** style uses *RIC* *Control Header* IE Format 1 (9.2.1.6.1).

#### 7.6.11.3 CONTROL Service *RIC Control Message* IE contents

This **CONTROL** Service *RIC Control Message* IE contains the sequence of RAN parameters, associated with a given Control Action within this Control Service style.

This **CONTROL** style uses *RIC Control Message* IE Format 1 (9.2.1.7.1).

#### 7.6.11.4 CONTROL Service *RIC Call Process ID* IE contents

This **CONTROL** Service *RIC Call Process ID* IE is currently not supported for this CONTROL service style.

#### 7.6.11.5 CONTROL Service *RIC Control Outcome* IE contents

This **CONTROL** Service *RIC Control Outcome* IE is used to carry the outcome of processing the incoming *RIC Control Request* message.  The corresponding RAN parameters supported for *RIC Control Outcome* IE are given in Section 8.4.10.4.

This **CONTROL** style uses *RIC Control Outcome* IE Format 3 (9.2.1.8.3).

## 7.7 Supported RIC POLICY Services

### 7.7.1 POLICY Service style list

|  |  |  |
| --- | --- | --- |
| **RIC Style Type** | **Style Name** | **Style Description** |
| 1 | Policy for Radio Bearer control | Used to define a policy for modifying the behaviour of Radio Bearer Control (RBC) of call processes for a specific RAN UE Group based on cell, slice, UE list and/or QoS |
| 2 | Policy for Radio resource allocation control | Used to define a policy for modifying the behaviour of Radio Resource Allocation control of call processes for a specific RAN UE Group based on cell, slice, UE list and/or QoS |
| 3 | Policy for Connected mode mobility control | Used to define a policy for modifying the behaviour of connected mode mobility procedure (Handover or Conditional Handover), optionally with Dual Active Protocol Stack (DAPS), call processes for a specific RAN UE Group based on cell, slice, UE list and/or QoS |
| 4 | Policy for Radio access control | Used to define a policy for modifying the behaviour of radio access control processes |
| 5 | Policy for Dual connectivity (DC) control | Used to define a policy for modifying the behaviour of dual connectivity (DC) call processes for a specific RAN UE Group based on cell, slice, UE list and/or QoS |
| 6 | Policy for Carrier Aggregation (CA) control | Used to define a policy for modifying the behaviour of carrier aggregation (CA) call processes for a specific RAN UE Group based on cell, slice, UE list and/or QoS |
| 7 | Policy for Idle mode mobility control | Used to define a policy for modifying the behaviour of idle mode configuration call processes for a specific RAN UE Group based on cell, slice and/or UE list. |
| 8 | Policy for Measurement Reporting Configuration Control | Used to define a policy for configuration of measurement objects and reporting objects |

Each of the POLICY Service Styles 1-8 listed above are supported using the following common features:

• Event Trigger: POLICY service is initiated by either Event Trigger style 1: Message Event or Event Trigger style 2: Call process breakpoint.

• Action ID: The index ID for the individual action under a given POLICY Service style.

• Action Name: Indicates the functionality of the E2 node which is controlled by Near-RT RIC

• Action Description: Describes the action and functionality of the receiving E2 Node.

• Associated RAN parameters: Identifies the RAN parameters to be controlled by Near-RT RIC pertaining to the given Policy action, used to define Policy Condition and RAN Imperative Policy.

All **POLICY** Service styles use *RIC Action Definition* IE Format 2 (9.2.1.2.2) which provides the policy conditions and corresponding Policy Action. All of these factors are defined as a sequence of RAN Parameters assigned according to a given Policy Style and Policy Action where:

- *Policy Action ID* is a Policy specific identifier of a specific Action for a specific Policy style.

*- Policy Condition* is a Policy specific condition to select a specific *Policy Action*. *Policy Condition* is described in terms of a list of test conditions concerning UE and E2 Node information selection criteria using RAN Parameters defined with a *Conditional Criteria Definition*. Default RAN behaviour is to be applied to any UE when none of the Policy conditions are met.

- *Policy Action* is encoded in terms of a list of specific RAN Parameters and shall be applied to any UE that meets a specific Policy Condition. Policy Action may contain optional Policy Decision to indicate acceptance or rejection of a RRM function when the Policy Conditions are met.

The details of the individual POLICY Service Styles and specific Policy Actions are provided in subsequent sections.

### 7.7.2 POLICY Service Style 1: Radio Bearer Control

#### 7.7.2.1 POLICY Service Style description

This **POLICY** Service style provides an Imperative Policy to control execution of a radio bearer control related process.

Applications of this service include:

- DRB QoS Modification, to tune DRB level QoS related parameters to meet the QoS optimization targets.

- QoS Flow mapping, to adjust the mapping relationship between QoS flows and DRBs.

- Logical channel configuration

- Radio Bearer Admission, to guide DRB admission control algorithms for admission and/or rejection of DRB requests

- DRB termination

- DRB Split bearer

- PDCP duplication control

#### 7.7.2.2 POLICY Service *RIC Action Definition* IE contents

This **POLICY** Service style uses *RIC Action Definition* IE Format 2 (9.2.1.2.2) using the approach described in Section 7.7.1.

The supported Policy Actions for this Policy style are as follows:

|  |  |  |  |
| --- | --- | --- | --- |
| **Policy Action**  **ID** | **Policy Action Name** | **Policy Action Description** | **Associated RAN Parameters** |
| 1 | Policy for DRB QoS Configuration | To setup a policy for the configuration of DRB QoS profile | 8.5.2.1 |
| 2 | Policy for QoS flow mapping configuration | To setup a policy for the multiplexing of QoS flows to a DRB (addition, modification, deletion | 8.5.2.2 |
| 3 | Policy for Logical channel (re-) configuration | To setup a policy for the LCID configuration of a DRB | 8.5.2.3 |
| 4 | Policy for Radio admission control | To setup a policy for radio admission control of a UE | 8.5.2.4 |
| 5 | Policy for DRB termination control | To setup a policy for change in the bearer termination point | 8.5.2.5 |
| 6 | Policy for DRB split ratio control | To setup a policy for controlling the split ratio of a DRB across its RLC entities | 8.5.2.6 |
| 7 | Policy for PDCP Duplication control | To setup a policy for controlling the activation or de-activation of PDCP duplication for a DRB and control/configure the number of legs or RLC entities for the DRB | 8.5.2.7 |

### 7.7.3 POLICY Service Style 2: Radio Resource Allocation Control

#### 7.7.3.1 POLICY Service Style description

This **POLICY** Service style provides an Imperative Policy to control execution of a radio resource allocation control related process.

Applications of this service include:

- Discontinuous Reception (DRX) control

- Scheduling request (SR) control

- Semi-Persistent Scheduling (SPS) control

- Configured grant

- Channel Quality Indicator (CQI) table

- Slice level PRB quota

#### 7.7.3.2 POLICY Service *RIC Action Definition* IE contents

This **POLICY** Service style uses *RIC Action Definition* IE Format 2 (9.2.1.2.2) using the approach described in Section 7.7.1.

The supported Policy Actions for this Policy style are as follows:

|  |  |  |  |
| --- | --- | --- | --- |
| **Policy**  **Action**  **ID** | **Policy Action Name** | **Policy Action description** | **Associated RAN Parameters** |
| 1 | Policy for DRX parameter configuration | To setup a policy for the configuration of DRX parameters | 8.5.3.1 |
| 2 | Policy for SR periodicity configuration | To setup a policy for the configuration of SR periodicity parameters | 8.5.3.2 |
| 3 | Policy for SPS parameters configuration | To setup a policy for the configuration of SPS parameters | 8.5.3.3 |
| 4 | Policy for Configured grant control | To setup a policy for the configuration of uplink grants to the UE | 8.5.3.4 |
| 5 | Policy for CQI table configuration | To setup a policy for the configuration of CQI table. | 8.5.3.5 |
| 6 | Policy for Slice level PRB quota | To setup a policy for the configuration of slice-level PRB quota | 8.5.3.6 |

### 7.7.4 POLICY Service Style 3: Connected Mode Mobility Control

#### 7.7.4.1 POLICY Service Style description

This **POLICY** Service style provides an Imperative Policy to control execution of a connected mode mobility control related process.

Applications of this service, for both serving and target RAN nodes, include:

- Handover (HO) or Conditional handover (CHO) mode selection

- Measurement configuration for handover candidate cell detection (intra-frequency, inter-frequency, inter-RAT)

- Handover decision and target cell selection

- Dual Active Protocol Stack (DAPS) usage

#### 7.7.4.2 POLICY Service *RIC Action Definition* IE contents

This **POLICY** Service style uses *RIC Action Definition* IE Format 2 (9.2.1.2.2) using the approach described in Section 7.7.1.

The supported Policy Actions for this Policy style are as follows:

|  |  |  |  |
| --- | --- | --- | --- |
| **Policy**  **Action**  **ID** | **Policy Action Name** | **Policy Action description** | **Associated RAN parameters** |
| 1 | Policy for Handover Control | To setup a policy for the handover of the primary cell and subsequent secondary cell reselection | 8.5.4.1 |
| 2 | Policy for Conditional Handover Control | To setup a policy for the conditional handover involving target primary cells | 8.5.4.2 |
| 3 | Policy for DAPS (Dual Active Protocol Stack) Handover Control | To setup a policy for the DAPS handover of a UE involving source and target cells. | 8.5.4.3 |

### 7.7.5 POLICY Service Style 4: Radio Access Control

#### 7.7.5.1 POLICY Service Style description

This **POLICY** Service style provides an Imperative Policy to control execution of a radio access control related process.

Applications of this service include:

- RACH back-off

- RRC connection admission

- RRC connection release

- Access barring

- UE Admission

#### 7.7.5.2 POLICY Service *RIC Action Definition* IE contents

This **POLICY** Service style uses *RIC Action Definition* IE Format 2 (9.2.1.2.2) using the approach described in Section 7.7.1.

The supported Policy Actions for this Policy style are as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Policy**  **Action**  **ID** | **Policy Action Name** | | **Policy Action Description** | | **Associated RAN Parameters** |
| 1 | Policy for UE Admission Control | | To setup a policy for controlling UE admission. | | 8.5.5.1 |
| 2 | Policy for RACH backoff control | | To setup a policy for controlling RACH backoff parameters | | 8.5.5.2 |
| 3 | Policy for Access barring control | | To setup a policy for controlling access barring configuration parameters | | 8.5.5.3 |
| 4 | | Policy for RRC Connection Release control | | To setup a policy for controlling the release of RRC connection of the UE | 8.5.5.4 |
| 5 | | Policy for RRC Connection Reject control | | To setup a policy for controlling the rejection of RRC connection request of the UE | 8.5.5.5 |

### 7.7.6 POLICY Service Style 5: Dual Connectivity (DC) Control

#### 7.7.6.1 POLICY Service Style description

This **POLICY** Service style provides an Imperative Policy to control execution of a dual connectivity control related process.

Applications of this service, for both Master and Secondary nodes, include:

- DC (EN-DC, MR-DC or NR-NR DC) mode selection

- Measurement configuration for candidate secondary cell detection

- DC initiation decision (M-NG-RAN or MeNB role)

- DC change decision (M-NG-RAN or MeNB role)

- DC addition request acceptance (S-NG-RAN or SgNB role)

- Target secondary cell selection

- DC release decision

- Change of bearer termination point (MN or SN) and/or bearer types

#### 7.7.6.2 POLICY Service *RIC Action Definition* IE contents

This **POLICY** Service style uses *RIC Action Definition* IE Format 2 (9.2.1.2.2) using the approach described in Section 7.7.1.

The supported Policy Actions for this Policy style are as follows:

|  |  |  |  |
| --- | --- | --- | --- |
| **Control**  **Action**  **ID** | **Control Action Name** | **Control Action Description** | **Associated RAN parameters** |
| 1 | Policy for DC Secondary Node  Addition Control | To setup a policy for controlling secondary node addition for dual connectivity | 8.5.6.1 |
| 2 | Policy for DC Secondary Node Modification and release Control | To setup a policy for controlling modification and release of secondary node for DC | 8.5.6.2 |
| 3 | Policy for DC PSCell Change control | To setup a policy for controlling PSCell change of a UE within a secondary node or to another secondary node | 8.5.6.3 |
| 4 | Policy for DC Secondary Node Change Control | To setup a policy for controlling the change of the secondary node of a UE for DC | 8.5.6.4 |

### 7.7.7 POLICY Service Style 6: Carrier Aggregation (CA) Control

#### 7.7.7.1 POLICY Service Style description

This **POLICY** Service style provides an Imperative Policy to control execution of a carrier aggregation control related process.

Applications of this service include:

- Measurement configuration for candidate secondary cell detection

- CA initiation decision

- Target secondary cell selection

- CA release decision

#### 7.7.7.2 POLICY Service *RIC Action Definition* IE contents

This **POLICY** Service style uses *RIC Action Definition* IE Format 2 (9.2.1.2.2) using the approach described in Section 7.7.1.

The supported Policy Actions for this Policy style are as follows:

|  |  |  |  |
| --- | --- | --- | --- |
| **Policy**  **Action**  **ID** | **Policy Action Name** | **Control Action Description** | **Associated RAN parameters** |
| 1 | Policy for CA Secondary Cell Addition Control | To setup a policy for controlling secondary cell addition for a UE | 8.5.7.1 |
| 2 | Policy for CA Secondary Cell Modification and Release Control | To setup a policy for controlling the modification and release of secondary cells for a UE | 8.5.7.2 |

### 7.7.8 POLICY Service Style 7: Idle Mode Mobility Control

#### 7.7.8.1 POLICY Service Style description

This **POLICY** Service style provides an Imperative Policy to control execution of a idle mode mobility control related process.

Applications of this service include:

- Cell re-selection criteria (intra-frequency, inter-frequency, inter-RAT)

- Inactivity timer

#### 7.7.8.2 POLICY Service RIC Action Definition IE contents

This **POLICY** Service style uses *RIC Action Definition* IE Format 2 (9.2.1.2.2) using the approach described in Section 7.7.1.

The supported Policy Actions for this Policy style are as follows:

|  |  |  |  |
| --- | --- | --- | --- |
| **Policy Action**  **ID** | **Policy Action Name** | **Policy Action Description** | **Associated RAN parameters** |
| 1 | Policy for Cell re-selection priority control | To setup a policy for assigning cell re-selection priorities for a UE during idle mode (RRC\_IDLE) | 8.5.8.1 |

### 7.7.9 POLICY Service Style 8: Measurement Reporting Configuration Control

#### 7.7.9.1 POLICY Service Style description

This POLICY Service style provides an imperative policy to add, modify or delete measurement report configuration for the UE to the network.

Applications of this service include:

- Policy to add configuration of measurement objects, reporting objects, measurement gaps, etc.

- Policy to modify configuration of measurement objects, reporting objects, measurement gaps, etc.

- Policy to delete configuration of measurement objects, reporting objects, measurement gaps, etc.

#### 7.7.9.2 POLICY Service *RIC Action Definition* IE contents

This POLICY Service style uses *RIC Action Definition* IE Format 2 (9.2.1.2.2) using the approach described in Section 7.7.1.

The supported Policy Actions for this Policy style are as follows:

|  |  |  |  |
| --- | --- | --- | --- |
| **Policy**  **Action**  **ID** | **Policy Action Name** | **Policy Action description** | **Associated RAN Parameters** |
| 1 | Policy for MR Configuration addition | To setup a policy for adding configuration of measurement objects, reporting objects, measurement gaps | 8.5.9.1 |
| 2 | Policy for MR Configuration modification | To setup a policy for modifying configuration of measurement objects, reporting objects, measurement gaps | 8.5.9.2 |
| 3 | Delete MR Configuration | To setup a policy for deleting configuration of measurement objects, reporting objects, measurement gaps | 8.5.9.3 |

## 7.8 Supported RIC Service Styles and E2SM IE Formats

Table 7.8-1and Table 7.8-2provide a summary of the E2SM IE Formats defined to support this E2SM specification.

Table 7.8-1: Summary of the E2SM IE Formats defined to support RIC Event Trigger Styles

|  |  |
| --- | --- |
| RIC Event Trigger Style | Event Trigger Definition Format |
| Style 1 | 1 |
| Style 2 | 2 |
| Style 3 | 3 |
| Style 4 | 4 |
| Style 5 | 5 |

Table 7.8-2: Summary of the E2SM IE Formats defined to support RIC Service Styles

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| RIC Service Style | Action Definition Format | Indication Header Format | Indication Message Format | Call Process ID Format | Control Header Format | Control Message Format | Control Outcome Format |
| REPORT | | | | | | |  |
| Style 1 | 1 | 1 | 1 |  |  |  |  |
| Style 2 | 1 | 1 | 2 |  |  |  |  |
| Style 3 | 1 | 1 | 3 |  |  |  |  |
| Style 4 | 1 | 1 | 2 |  |  |  |  |
| Style 5 | 1 | 1 | 4 |  |  |  |  |
|  |  |  |  |  |  |  |  |
| INSERT | | | | | | |  |
| Style 1 | 3 | 2 | 5 | 1 |  |  |  |
| Style 2 | 3 | 2 | 5 | 1 |  |  |  |
| Style 3 | 3 | 2 | 5 | 1 |  |  |  |
| Style 4 | 3 | 2 | 5 | 1 |  |  |  |
| Style 5 | 3 | 2 | 5 | 1 |  |  |  |
| Style 6 | 3 | 2 | 5 | 1 |  |  |  |
| Style 7 | 3 | 2 | 5 | 1 |  |  |  |
| Style 255 | 4 | 3 | 6 | 1 |  |  |  |
|  |  |  |  |  |  |  |  |
| CONTROL | | | | | | |  |
| Style 1 |  |  |  | 1 | 1 | 1 | 1 |
| Style 2 |  |  |  | 1 | 1 | 1 | 1 |
| Style 3 |  |  |  | 1 | 1 | 1 | 1 |
| Style 4 |  |  |  | 1 | 1 | 1 | 1 |
| Style 5 |  |  |  | 1 | 1 | 1 | 1 |
| Style 6 |  |  |  | 1 | 1 | 1 | 1 |
| Style 7 |  |  |  | 1 | 1 | 1 | 1 |
| Style 8 |  |  |  |  | 1 | 1 | 1 |
| Style 9 |  |  |  |  | 1 | 1 | 3 |
| Style 255 |  |  |  | 1 | 2 | 2 | 2 |
|  |  |  |  |  |  |  |  |
| POLICY | | | | | | |  |
| Style 1 | 2 |  |  |  |  |  |  |
| Style 2 | 2 |  |  |  |  |  |  |
| Style 3 | 2 |  |  |  |  |  |  |
| Style 4 | 2 |  |  |  |  |  |  |
| Style 5 | 2 |  |  |  |  |  |  |
| Style 6 | 2 |  |  |  |  |  |  |
| Style 7 | 2 |  |  |  |  |  |  |
| Style 8 | 2 |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

# 8 RAN Parameter assignments

## 8.0 Approach

The RAN parameters associated with each RIC service described in Section 7 are listed here in Section 8. Each RAN parameter belongs to one of the following value types:

* ELEMENT: a singleton variable, which does not have any other associated RAN parameters.
* STRUCTURE: a sequence of RAN parameters, each of which can be either an ELEMENT or a STRUCTURE or a LIST
* LIST: a list of STRUCTURES, where each STRUCTURE is as defined above. The sequence of RAN parameters is the same across all the STRUCTURES within the list.

The corresponding 3GPP standard definitions of these RAN parameters (if available) are referenced in the tables below under the “RAN Parameter Definition” column. These RAN parameters having 3GPP standard definitions are not freshly defined or redefined here.

Note that only those RAN parameters identified as ELEMENT are subject to test conditions by the RIC in the “Event Trigger Definition”.

Any RAN parameter within a STRUCTURE or LIST shall not be referenced individually. Hierarchy of a LIST or a STRUCTURE shall be traversed to access any RAN parameter within the LIST or STRUCTURE

Note that a RAN parameter may be associated with as a key where its corresponding *Key Flag* is set to “TRUE”. These RAN parameters serve as a reference to other RAN parameters within a structure that may be a part of LIST to enable the E2 Node interpret the scope of RAN parameters that are controlled by Near-RT RIC.

If the “key flag” is specified in the RIC Event Trigger Definition, then the RAN parameters corresponding to “that specific itemized structure” in the list indexed by the “key flag” are subject to test condition, but if the “key flag” is not mentioned in the RIC Event Trigger Definition, then the RAN parameters corresponding to “any itemized structure” within the list are subject to test condition.

For e.g., The ‘QFI’ can be considered a ‘key parameter’ to identify a QoS flow among the list of flows in a UE-specific PDU session. If the QFI parameter is NOT mentioned and the RIC subscribes to an event pertaining to 5QI 8, then “any QoS flow” in the list of flows of a PDU session for the UE that matches the condition of 5QI being equal to 8 would be covered by this event trigger definition. On the other hand, if the QFI parameter is mentioned in the event trigger definition, then only that specific QoS flow pertaining to the indicated QFI within the list is covered

## 8.1 RAN parameters for Event Trigger

The RAN Parameters pertaining to “Event Trigger” that are used across multiple service styles are listed here. All RAN Parameters defined in section 8.1 may also be used to define Policy Condition, see also section 8.5.

8.1.1 Common RAN Parameters

This section contains the common set of RAN parameters that can be accessed via RAN parameters defined in each service style across multiple services.

#### 8.1.1.1 NR Cell

The following RAN Parameters are associated with the NR cell.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | ***Semantics Description*** |
| 10001 | NR CGI | ELEMENT | FALSE | *NR CGI* IE in TS 38.423 [15] Section 9.2.2.7 |  |
| 10002 | NR PCI | ELEMENT | FALSE | *NR PCI* IE in TS 38.473 [19] Section 9.3.1.10 |  |
| 10003 | 5GS TAC | ELEMENT | FALSE | *5GS TAC* IE in TS 38.473 [19] Section 9.3.1.29 |  |
| 10004 | CHOICE *NR-Mode-Info* | STRUCTURE |  |  | *NR-Mode-Info* IE in TS 38.473 [19] Section 9.3.1.10 |
| 10005 | >FDD | STRUCTURE |  |  | *FDD* IE in TS 38.473 [19] Section 9.3.1.10 |
| 10006 | >>FDD Info | STRUCTURE |  |  | *FDD Info* IE in TS 38.473 [19] Section 9.3.1.10 |
| 10007 | >>>UL FreqInfo | STRUCTURE |  |  | *UL FreqInfo* IE in TS 38.473 [19] Section 9.3.1.10 |
| 10008 | >>>>NR ARFCN | ELEMENT | FALSE | *NR ARFCN* IE in TS 38.473 [19] Section 9.3.1.17 |  |
| 10009 | >>>>Frequency Band List | LIST |  |  | *Frequency Band List* IE in TS 38.473 [19] Section 9.3.1.17 |
| 10010 | >>>>>Frequency Band item | STRUCTURE |  |  | *Frequency Band Item* IE in TS 38.473 [19] Section 9.3.1.17 |
| 10011 | >>>>>>NR Frequency band | ELEMENT | FALSE | *NR Frequency Band* IE in TS 38.473 [19] Section 9.3.1.17 |  |
| 10012 | >>>DL FreqInfo | STRUCTURE |  |  | *DL FreqInfo* IE in TS 38.473 [19] Section 9.3.1.10 |
| 10013 | >>>>NR ARFCN | ELEMENT | FALSE | *NR ARFCN* IE in TS 38.473 [19] Section 9.3.1.17 |  |
| 10014 | >>>>Frequency Band List | LIST |  |  | *Frequency Band List* IE in TS 38.473 [19] Section 9.3.1.17 |
| 10015 | >>>>>Frequency Band item | STRUCTURE |  |  | *Frequency Band Item* IE in TS 38.473 [19] Section 9.3.1.17 |
| 10016 | >>>>>>NR Frequency band | ELEMENT | FALSE | *NR Frequency Band* IE in TS 38.473 [19] Section 9.3.1.17 |  |
| 10017 | >>>UL Transmission Bandwidth | STRUCTURE |  |  | *Transmission Bandwidth* IE in TS 38.473 [19] Section 9.3.1.15 |
| 10018 | >>>>NR SCS | ELEMENT | FALSE | *NR SCS* IE in TS 38.473 [19] Section 9.3.1.15 |  |
| 10019 | >>>>NRB | ELEMENT | FALSE | *NRB* IE in TS 38.473 [19] Section 9.3.1.15 |  |
| 10020 | >>>DL Transmission Bandwidth | STRUCTURE |  |  | *Transmission Bandwidth* IE in TS 38.473 [19] Section 9.3.1.15 |
| 10021 | >>>>NR SCS | ELEMENT | FALSE | *NR SCS* IE in TS 38.473 [19] Section 9.3.1.15 |  |
| 10022 | >>>>NRB | ELEMENT | FALSE | *NRB* IE in TS 38.473 [19] Section 9.3.1.15 |  |
| 10023 | >>>UL Carrier List | LIST |  |  | *UL Carrier List* IE in TS 38.473 [19] Section 9.3.1.10 |
| 10024 | >>>>NR Carrier Item | STRUCTURE |  | *NR Carrier Item* IE in TS 38.473 [19] Section 9.3.1.137 |  |
| 10025 | >>>>>NR SCS | ELEMENT | FALSE | *NR SCS* IE in TS 38.473 [19] Section 9.3.1.15 |  |
| 10026 | >>>>>Offset to Carrier | ELEMENT | FALSE | *Offset to Carrier* IE in TS 38.473 [19] Sec 137 |  |
| 10027 | >>>>>Carrier Bandwidth | ELEMENT | FALSE | *Carrier Bandwidth* IE |  |
| 10028 | >>>DL Carrier List | LIST |  |  | *DL Carrier List* IE in TS 38.473 [19] Section 9.3.1.10 |
| 10029 | >>>>NR Carrier Item | STRUCTURE |  | *NR Carrier Item* IE in TS 38.473 [19] Section 9.3.1.137 |  |
| 10030 | >>>>>NR SCS | ELEMENT | FALSE | *NR SCS* IE in TS 38.473 [19] Section 9.3.1.15 |  |
| 10031 | >>>>>Offset to Carrier | ELEMENT | FALSE | *Offset to Carrier* IE in TS 38.473 [19] Section 9.3.1.137 |  |
| 10032 | >>>>>Carrier Bandwidth | ELEMENT | FALSE | *Carrier Bandwidth* IE in TS 38.473 [19] Section 9.3.1.137 |  |
| 10033 | >TDD | STRUCTURE |  |  | *TDD* IE in TS 38.473 [19] Section 9.3.1.10 |
| 10034 | >>TDD Info | STRUCTURE |  |  | *TDD Info* IE in TS 38.473 [19] Section 9.3.1.10 |
| 10035 | >>>NR FreqInfo | STRUCTURE |  |  |  |
| 10036 | >>>>NR ARFCN | ELEMENT | FALSE | *NR ARFCN* IE in TS 38.473 [19] Section 9.3.1.17 |  |
| 10037 | >>>>Frequency Band List | LIST |  |  | *Frequency Band List* IE in TS 38.473 [19] Section 9.3.1.17 |
| 10038 | >>>>>Frequency Band item | STRUCTURE |  |  | *Frequency Band Item* IE in TS 38.473 [19] Section 9.3.1.17 |
| 10039 | >>>>>>NR Frequency band | ELEMENT | FALSE | *NR Frequency Band* IE in TS 38.473 [19] Section 9.3.1.17 |  |
| 10040 | >>>Transmission Bandwidth | STRUCTURE |  |  | *Transmission Bandwidth* IE in TS 38.473 [19] Section 9.3.1.15 |
| 10041 | >>>>NR SCS | ELEMENT | FALSE | *NR SCS* IE in TS 38.473 [19] Section 9.3.1.15 |  |
| 10042 | >>>>NRB | ELEMENT | FALSE | *NRB* IE in TS 38.473 [19] Section 9.3.1.15 |  |
| 10043 | >>>Carrier List | LIST |  |  | *Transmission Bandwidth* IE in TS 38.473 [19] Section 9.3.1.15 |
| 10044 | >>>>NR Carrier Item | STRUCTURE |  | *NR SCS* IE in TS 38.473 [19] Section 9.3.1.15 |  |
| 10045 | >>>>>NR SCS | ELEMENT | FALSE | *NR SCS* IE in TS 38.473 [19] Section 9.3.1.15 |  |
| 10046 | >>>>>Offset to Carrier | ELEMENT | FALSE | *Offset to Carrier* IE in TS 38.473 [19] Section 9.3.1.137 |  |
| 10047 | >>>>>Carrier Bandwidth | ELEMENT | FALSE | *Carrier Bandwidth* IE in TS 38.473 [19] Section 9.3.1.137 |  |
| 10048 | >>>Intended TDD DL-UL Configuration | STRUCTURE |  |  | *Intended TDD DL-UL Configuration* IE in TS 38.473 [19] Section 9.3.1.89 |
| 10049 | >>>>NR SCS | ELEMENT | FALSE | *NR SCS* IE in TS 38.473 [19] Section 9.3.1.89 |  |
| 10050 | >>>>NR Cyclic Prefix | ELEMENT | FALSE | *NR Cyclic Prefix* IE in TS 38.473 [19] Section 9.3.1.89 |  |
| 10051 | >>>>NR DL-UL Transmission Periodicity | ELEMENT | FALSE | *NR DL-UL Transmission Periodicity* IE in TS 38.473 [19] Section 9.3.1.89 |  |
| 10052 | >>>>Slot Configuration List | LIST |  |  | *Slot Configuration List* IE in TS 38.473 [19] Section 9.3.1.89 |
| 10053 | >>>>>Slot Configuration Item | STRUCTURE |  |  | *Slot Configuration Item* IE in TS 38.473 [19] Section 9.3.1.89 |
| 10054 | >>>>>>Slot Index | ELEMENT | TRUE | *Slot Index* IE in TS 38.473 [19] Section 9.3.1.89 |  |
| 10055 | >>>>>>CHOICE Symbol Allocation in Slot | STRUCTURE |  | *Symbol Allocation in Slot* IE in TS 38.473 [19] Section 9.3.1.89 |  |
| 10056 | >>>>>>>All DL | ELEMENT | FALSE | *All DL* IE in TS 38.473 [19] Section 9.3.1.89 |  |
| 10057 | >>>>>>>All UL | ELEMENT | FALSE | *All UL* IE in TS 38.473 [19] Section 9.3.1.89 |  |
| 10058 | >>>>>>>Both DL and UL | STRUCTURE |  |  | *Both DL and UL* IE in TS 38.473 [19] Section 9.3.1.89 |
| 10059 | >>>>>>>>Number of DL symbols | ELEMENT | FALSE | *Number of DL symbols* IE in TS 38.473 [19] Section 9.3.1.89 |  |
| 10060 | >>>>>>>>Number of UL symbols | ELEMENT | FALSE | *Number of UL symbols* IE in TS 38.473 [19] Section 9.3.1.89 |  |
| 10061 | Count of FDD UL Frequency band list | ELEMENT | FALSE | INTEGER (0..63) |  |
| 10062 | Count of FDD DL Frequency band list | ELEMENT | FALSE | INTEGER (0..63) |  |
| 10063 | Count of FDD UL Carrier list | ELEMENT | FALSE | INTEGER (0..63) |  |
| 10064 | Count of FDD DL Carrier list | ELEMENT | FALSE | INTEGER (0..63) |  |
| 10065 | Count of TDD Frequency band list | ELEMENT | FALSE | INTEGER (0..63) |  |
| 10066 | Count of TDD Carrier list | ELEMENT | FALSE | INTEGER (0..63) |  |
| 10067 | Count of TDD DL-UL Slot Configuration list | ELEMENT | FALSE | INTEGER (0..63) |  |
| 10101 | Reported NR RRC Measurements | STRUCTURE |  |  | *measResult* IE in TS 38.331 [22] |
| 10102 | >Cell Results | STRUCTURE |  |  | *cellResults* IE in TS 38.331 [22] |
| 10103 | >>SSB Results | STRUCTURE |  | 8.1.1.3 | *resultsSSB-Cell* IE in TS 38.331 [22] |
| 10106 | >>CSI-RS Results | STRUCTURE |  | 8.1.1.3 | *resultsCSI-RS-Cell* IE in TS 38.331 [22] |
| 10110 | PM Measurements | STRUCTURE |  |  | *Cell Measurement Result* IE in TS 38.423 [15] Section 9.1.3.21 |
| 10111 | >Radio Resource Status | STRUCTURE |  |  | *Radio Resource Status* IE in TS 38.473 [19] |
| 10112 | >>SSB Area Radio Resource Status List | LIST |  |  | *SSB Area Radio Resource Status List* IE in TS 38.473 [19] Section 9.3.1.129 |
| 10113 | >>>SSB Area Radio Resource Status Item | STRUCTURE |  |  | *SSB Area Radio Resource Status Item* IE in TS 38.473 [19] Section 9.3.1.129 |
| 10114 | >>>>SSB Index | ELEMENT | TRUE | *SSB Index* IE in TS 38.473 [19] Section 9.3.1.129 |  |
| 10115 | >>>>SSB Area DL GBR PRB Usage | ELEMENT | FALSE | *SSB Area DL GBR PRB Usage* IE in TS 38.473 [19] Section 9.3.1.129 |  |
| 10116 | >>>>SSB Area UL GBR PRB Usage | ELEMENT | FALSE | *SSB Area UL GBR PRB Usage* IE in TS 38.473 [19] Section 9.3.1.129 |  |
| 10117 | >>>>SSB Area DL non-GBR PRB Usage | ELEMENT | FALSE | *SSB Area DL non-GBR PRB Usage* IE in TS 38.473 [19] Section 9.3.1.129 |  |
| 10118 | >>>>SSB Area UL non-GBR PRB Usage | ELEMENT | FALSE | *SSB Area UL non-GBR PRB Usage* IE in TS 38.473 [19] Section 9.3.1.129 |  |
| 10119 | >>>>SSB Area DL Total PRB Usage | ELEMENT | FALSE | *SSB Area DL Total PRB Usage* IE in TS 38.473 [19] Section 9.3.1.129 |  |
| 10120 | >>>>SSB Area UL Total PRB Usage | ELEMENT | FALSE | *SSB Area UL Total PRB Usage* IE in TS 38.473 [19] Section 9.3.1.129 |  |
| 10121 | >>>>DL scheduling PDCCH CCE Usage | ELEMENT | FALSE | *DL Scheduling PDCCH CCE* IE in TS 38.473 [19] Section 9.3.1.129 |  |
| 10122 | >>>>UL scheduling PDCCH CCE Usage | ELEMENT | FALSE | *UL Scheduling PDCCH CCE* IE in TS 38.473 [19] Section 9.3.1.129 |  |
| 10123 | >Available DL PRBs in the cell | ELEMENT | FALSE | INTEGER | *DL Total available PRB* IE in TS 28.552 [28] Sec 5.1.1.2.6 |
| 10124 | >Available UL PRBs in the cell | ELEMENT | FALSE | INTEGER | *UL Total available PRB* IE in TS 28.552 [28] Sec 5.1.1.2.8 |
| 10125 | >Number of active DL UEs in the cell | ELEMENT | FALSE | *Number of Active UEs* IE in TS 38.473 [19] Section 9.3.1.135 |  |
| 10126 | >Number of active UL UEs in the cell | ELEMENT | FALSE | *Number of Active UEs* IE in TS 38.473 [19] Section 9.3.1.135 |  |
| 10127 | >Composite Available Capacity Group | STRUCTURE |  |  | *Composite Available Capacity Group* IE in TS 38.473 [19] Section 9.3.1.130 |
| 10128 | >>Composite Available Capacity Downlink | STRUCTURE |  |  | *Composite Available Capacity* IE in TS 38.473 [19] Section 9.3.1.131 |
| 10129 | >>>Cell Capacity Class Value | ELEMENT | FALSE | *Cell Capacity Class Value* IE in TS 38.473 [19] Section 9.3.1.132 |  |
| 10130 | >>>Capacity Value | ELEMENT | FALSE | *Capacity Value* IE in TS 38.473 [19] Section 9.3.1.133 |  |
| 10131 | >>>SSB Area Capacity Value List | LIST |  |  | *SSB Area Capacity Value List* IE in TS 38.473 [19] Section 9.3.1.133 |
| 10132 | >>>>SSB Area Capacity Value Item | STRUCTURE |  |  | *SSB Area Capacity Value Item* IE in TS 38.473 [19] Sec 9.3.1.133 |
| 10133 | >>>>>SSB Index | ELEMENT | TRUE | *SSB Index* IE in TS 38.473 [19] Section 9.3.1.133 |  |
| 10134 | >>>>>SSB Area Capacity Value | ELEMENT | FALSE | *SSB Area Capacity Value* IE in TS 38.473 [19] Sec 9.3.1.133 |  |
| 10141 | >>Composite Available Capacity Uplink | STRUCTURE |  |  | *Composite Available Capacity* IE in TS 38.473 [19] Section 9.3.1.131 |
| 10142 | >>>Cell Capacity Class Value | ELEMENT | FALSE | *Cell Capacity Class Value* IE in TS 38.473 [19] Section 9.3.1.132 |  |
| 10143 | >>>Capacity Value | ELEMENT | FALSE | *Capacity Value* IE in TS 38.473 [19] Section 9.3.1.133 |  |
| 10144 | >>>SSB Area Capacity Value List | LIST |  |  | *SSB Area Capacity Value List* IE in TS 38.473 [19] Section 9.3.1.133 |
| 10145 | >>>>SSB Area Capacity Value Item | STRUCTURE |  |  | *SSB Area Capacity Value Item* IE in TS 38.473 [19] Sec 9.3.1.133 |
| 10146 | >>>>>SSB Index | ELEMENT | TRUE | *SSB Index* IE in TS 38.473 [19] Section 9.3.1.133 |  |
| 10147 | >>>>>SSB Area Capacity Value | ELEMENT | FALSE | *SSB Area Capacity Value* IE in TS 38.473 [19] Sec 9.3.1.133 |  |
| 10151 | >Slice Available Capacity List | LIST |  |  | *Slice Available Capacity List* IE in TS 38.473 [19] Section 9.3.1.134 |
| 10152 | >>Slice Available Capacity Item | STRUCTURE |  |  | *Slice Available Capacity Item* IE in TS 38.473 [19] Section 9.3.1.134 |
| 10153 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.473 [19] Section 9.3.1.14 |  |
| 10154 | >>>S-NSSAI Available Capacity List | LIST |  |  | *S-NSSAI Available Capacity List* IE in TS 38.473 [19] Section 9.3.1.134 |
| 10155 | >>>>S-NSSAI Available Capacity Item | STRUCTURE |  |  | *S-NSSAI Available Capacity Item* IE in TS 38.473 [19] Section 9.3.1.134 |
| 10156 | >>>>>S-NSSAI | ELEMENT | FALSE |  | *S-NSSAI* IE in TS 38.473 [19] Section 9.3.1.38 |
| 10160 | >>>>>>SST | ELEMENT | FALSE | *SST* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 10161 | >>>>>>SD | ELEMENT | FALSE | *SD* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 10157 | >>>>>Slice Available Capacity Value Downlink | ELEMENT | FALSE | *Slice Available Capacity Value Downlink* IE in TS 38.473 [19] Section 9.3.1.134 |  |
| 10158 | >>>>>Slice Available Capacity Value Uplink | ELEMENT | FALSE | *Slice Available Capacity Value Uplink* IE in TS 38.473 [19] Section 9.3.1.134 |  |
| 10201 | Cell-specific offset | ELEMENT | FALSE | Ocp (or Ocn) IE as defined in TS 38.331 [22] INTEGER |  |
| 10202 | Cell Measurement object specific offset | ELEMENT | FALSE | Ofp (or Ofn) IE as defined in TS 38.331 [22] INTEGER |  |

#### 8.1.1.2 E-UTRA Cell

The following RAN Parameters are associated with the E-UTRA cell.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | ***Semantics Description*** |
| 12001 | E-UTRA CGI | ELEMENT | FALSE | *E-UTRA CGI* IE in TS 38.423 [15] Section 9.2.2.8 |  |
| 12002 | PCI | ELEMENT | FALSE | *PCI* IE in TS 36.423 [15] within Section 9.2.8, INTEGER(0..503,...) |  |
| 12003 | TAC | ELEMENT | FALSE | *TAC* IE in TS 36.423 [15] within Section 9.2.8, OCTET STRING(2) |  |
| 12004 | CHOICE *EUTRA-Mode-Info* | STRUCTURE |  |  | *EUTRA-Mode-Info* IE in TS 36.423 [17] Section 9.2.8 |
| 12005 | >FDD | STRUCTURE |  |  | *FDD* IE in TS 36.423 [17] Section 9.2.8 |
| 12006 | >>FDD Info | STRUCTURE |  |  | *FDD Info* IE in TS 36.423 [17] Section 9.2.8 |
| 12007 | >>>UL EARFCN | STRUCTURE |  |  | *UL EARFCN* IE in TS 36.423 [17] Section 9.2.8 |
| 12008 | >>>>EARFCN | ELEMENT | FALSE | *EARFCN* IE in TS 36.423 [17] Section 9.2.26 |  |
| 12009 | >>>DL EARFCN | ELEMENT | FALSE |  | *DL EARFCN* IE in TS 36.423 [17] Section 9.2.8 |
| 12010 | >>>>EARFCN | STRUCTURE |  | *EARFCN* IE in TS 36.423 [17] Section 9.2.26 |  |
| 12011 | >>>UL Transmission Bandwidth | STRUCTURE |  |  | *UL Transmission Bandwidth* IE in TS 36.423 [17] Section 9.2.8 |
| 12012 | >>>>Transmission Bandwidth | ELEMENT | FALSE | *Transmission Bandwidth* IE in TS 36.423 [17] Section 9.2.27 |  |
| 12013 | >>>DL Transmission Bandwidth | STRUCTURE |  |  | *DL Transmission Bandwidth* IE in TS 36.423 [17] Section 9.2.8 |
| 12014 | >>>>Transmission Bandwidth | ELEMENT | FALSE | *Transmission Bandwidth* IE in TS 36.423 [17] Section 9.2.27 |  |
| 12015 | >TDD | STRUCTURE |  |  | *TDD* IE in TS 36.423 [17] Section 9.2.8 |
| 12016 | >>TDD Info | STRUCTURE |  |  | *TDD Info* IE in TS 36.423 [17] Section 9.2.8 |
| 12017 | >>>EARFCN | ELEMENT | FALSE | *EARFCN* IE in TS 36.423 [17] Section 9.2.26 |  |
| 12018 | >>>Transmission Bandwidth | ELEMENT | FALSE | *Transmission Bandwidth* IE in TS 36.423 [17] Section 9.2.27 |  |
| 12019 | >>>Subframe assignment | ELEMENT | FALSE | *Subframe Assignment* IE in TS 36.423 [17] Section 9.2.8 |  |
| 12020 | >>>Special Subframe Info | ELEMENT | FALSE | *Special Subframe Info* IE in TS 36.423 [17] Section 9.2.8 |  |
| 12021 | >>>>Special Subframe Patterns | ELEMENT | FALSE | *Special Subframe Patterns* IE in TS 36.423 [17] Section 9.2.8 |  |
| 12022 | >>>>Cyclic Prefix DL | ELEMENT | FALSE | *Cyclic Prefix DL* IE in TS 36.423 [17] Section 9.2.8 |  |
| 12023 | >>>>Cyclic Prefix UL | ELEMENT | FALSE | *Cyclic Prefix UL* IE in TS 36.423 [17] Section 9.2.8 |  |
| 12024 | Reported LTE RRC Measurements | STRUCTURE |  | 8.1.1.3 | *MeasResults* IE in TS 36.331 [23] |
| 12025 | PM Measurements | STRUCTURE |  |  | *CellMeasurementResultItem* IE in TS 36.423 [17] Section 9.1.2.14 |
| 12026 | >Radio Resource Status | STRUCTURE |  |  | *Radio Resource Status* IE in TS 36.423 [17] Section 9.2.37 |
| 12027 | >>DL GBR PRB Usage | ELEMENT | FALSE | *DL GBR PRB Usage* IE in TS 36.423 [17] Section 9.2.37 |  |
| 12028 | >>UL GBR PRB Usage | ELEMENT | FALSE | *UL GBR PRB Usage* IE in TS 36.423 [17] Section 9.2.37 |  |
| 12029 | >>DL non-GBR PRB Usage | ELEMENT | FALSE | *DL non-GBR PRB Usage* IE in TS 36.423 [17] Section 9.2.37 |  |
| 12030 | >>UL non-GBR PRB usage | ELEMENT | FALSE | *UL non-GBR PRB Usage* IE in TS 36.423 [17] Section 9.2.37 |  |
| 12031 | >>DL Total PRB Usage | ELEMENT | FALSE | *DL Total PRB Usage* IE in TS 36.423 [17] Section 9.2.37 |  |
| 12032 | >>UL Total PRB Usage | ELEMENT | FALSE | *UL Total PRB Usage* IE in TS 36.423 [17] Section 9.2.37 |  |
| 12033 | >>DL scheduling PDCCH CCE Usage | ELEMENT | FALSE | *DL scheduling PDCCH CCE Usage* IE in TS 36.423 [17] Section 9.2.37 |  |
| 12034 | >>UL scheduling PDCCH CCE Usage | ELEMENT | FALSE | *UL scheduling PDCCH CCE Usage* IE in TS 36.423 [17] Section 9.2.37 |  |
| 12051 | >Composite Available Capacity Group | STRUCTURE |  |  | *Composite Available Capacity Group* IE in TS 36.423 [17] Section 9.2.44 |
| 12052 | >>Composite Available Capacity Downlink | STRUCTURE |  |  | *Composite Available Capacity Downlink* IE in TS 36.423 [17] Section 9.2.45 |
| 12053 | >>>Cell capacity Class Value | ELEMENT | FALSE | *Cell Capacity Class Value* IE in TS 36.423 [17] Section 9.2.46 |  |
| 12054 | >>>Capacity Value | ELEMENT | FALSE | *Capacity Value* IE in TS 36.423 [17] Section 9.2.47 |  |
| 12055 | >>Composite Available Capacity Uplink | STRUCTURE |  |  | *Composite Available Capacity Uplink* IE in TS 36.423 [17] Section 9.2.45 |
| 12056 | >>>Cell capacity Class Value | ELEMENT | FALSE | *Cell Capacity Class Value* IE in TS 36.423 [17] Section 9.2.46 |  |
| 12057 | >>>Capacity Value | ELEMENT | FALSE | *Capacity Value* IE in TS 36.423 [17] Section 9.2.47 |  |
| 12058 | >Available DL PRBs in the cell | ELEMENT | FALSE | INTEGER |  |
| 12059 | >Available UL PRBs in the cell | ELEMENT | FALSE | INTEGER |  |
| 12060 | >Number of active DL UEs in the cell | ELEMENT | FALSE | INTEGER |  |
| 12061 | >Number of active UL UEs in the cell | ELEMENT | FALSE | INTEGER |  |
| 12062 | >ABS Status | STRUCTURE |  |  | *ABS Status* IE in TS 36.423 [17] Section 9.2.58 |
| 12063 | >>DL ABS Status | ELEMENT | FALSE | *DL ABS status* IE in TS 36.423 [17] Section 9.2.58 |  |
| 12064 | >>CHOICE *Usable ABS Information* | STRUCTURE |  |  | *Usable ABS Information* IE in TS 36.423 [17] Section 9.2.58 |
| 12065 | >>>FDD | STRUCTURE |  |  | *FDD* IE in TS 36.423 [17] Section 9.2.58 |
| 12066 | >>>>Usable ABS Pattern Info | ELEMENT | FALSE | *Usable ABS Pattern Info* IE in TS 36.423 [17] Section 9.2.58 |  |
| 12067 | >>>TDD | STRUCTURE |  |  | *TDD* IE in TS 36.423 [17] Section 9.2.58 |
| 12068 | >>>>Usable ABS Pattern Info | ELEMENT | FALSE | *Usable ABS Pattern Info* IE in TS 36.423 [17] Section 9.2.58 |  |
| 12075 | >CSI Report per CSI Process List | LIST |  |  | *CSI Report per CSI Process* IE in TS 36.423 [17] Section 9.2.79 |
| 12076 | >>CSI Process per CSI Item | STRUCTURE |  |  | *CSI Report per CSI Process Item* IE in TS 36.423 [17] Section 9.2.79 |
| 12077 | >>>CSI Process Configuration Index | ELEMENT | FALSE | *CSI Process Configuration Index* IE in TS 36.423 [17] Section 9.2.79 |  |
| 12078 | >>>RI | ELEMENT | FALSE | *RI* IE in TS 36.423 [17] Section 9.2.79 |  |
| 12079 | >>>Wideband CQI | STRUCTURE |  |  | *Wideband CQI* IE in TS 36.423 [17] Section 9.2.80 |
| 12101 | >>>>Wideband CQI Codeword 0 | ELEMENT | FALSE | *Wideband CQI Codeword 0*IE in TS 36.423 [17] Section 9.2.80 |  |
| 12102 | >>>>CHOICE *Wideband CQI Codeword 1* | STRUCTURE |  |  | *Wideband CQI Codeword 1* IE in TS 36.423 [17] Section 9.2.80 |
| 12103 | >>>>>4-bit CQI | ELEMENT | FALSE | *4-bit CQI* IE in TS 36.423 [17] Section 9.2.80 |  |
| 12104 | >>>>>3-bit spatial differential CQI | ELEMENT | FALSE | *3-bit spatial differential CQI* IE in TS 36.423 [17] Section 9.2.80 |  |
| 12080 | >>>Subband Size | ELEMENT | FALSE | *Subband Size* IE in TS 36.423 [17] Section 9.2.79 |  |
| 12081 | >>>Subband CQI List | LIST |  |  | *Subband CQI List* IE in TS 36.423 [17] Section 9.2.79 |
| 12082 | >>>>Subband CQI Item | STRUCTURE |  |  | *Subband CQI Item* IE in TS 36.423 [17] Section 9.2.79 |
| 12083 | >>>>>Subband CQI Index | ELEMENT | FALSE | *Subband Index* IE in TS 36.423 [17] Section 9.2.79 |  |
| 12084 | >>>>>Subband CQI | STRUCTURE |  |  | *Subband CQI* IE in TS 36.423 [17] Section 9.2.81 |
| 12085 | >>>>>>CHOICE Subband CQI Codeword 0 | STRUCTURE |  |  | *Subband CQI Codeword 0* IE in TS 36.423 [17] Section 9.2.81 |
| 12086 | >>>>>>>4-bit CQI | ELEMENT | FALSE | *4-bit CQI* IE in TS 36.423 [17] Section 9.2.81 |  |
| 12087 | >>>>>>>2-bit subband differential CQI | ELEMENT | FALSE | *2-bit Subband differential CQI* IE in 36.423 Section 9.2.81 |  |
| 12088 | >>>>>>>2-bit differential CQI | ELEMENT | FALSE | *2-bit differential CQI* IE in 36.423 Section 9.2.81 |  |
| 12089 | >>>>>>CHOICE Subband CQI Codeword 1 | STRUCTURE |  |  | *Subband CQI Codeword 1* IE in TS 36.423 [17] Section 9.2.81 |
| 12090 | >>>>>>>4-bit CQI | ELEMENT | FALSE | *4-bit CQI* IE in TS 36.423 [17] Section 9.2.81 |  |
| 12091 | >>>>>>>3-bit spatial differential CQI | ELEMENT | FALSE | *3-bit spatial differential CQI* IE in 36.423 Section 9.2.81 |  |
| 12092 | >>>>>>>2-bit subband differential CQI | ELEMENT | FALSE | *2-bit Subband differential CQI* IE in 36.423 Section 9.2.81 |  |
| 12093 | >>>>>>>2-bit differential CQI | ELEMENT | FALSE | *2-bit differential CQI* IE in 36.423 Section 9.2.81 |  |

#### 8.1.1.3 RRC Signal Measurements

The following RAN Parameters are associated with RRC measurements.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 12501 | RSRP | ELEMENT | FALSE | *RSRP-Range* IE in TS 38.331 [22] |  |
| 12502 | RSRQ | ELEMENT | FALSE | *RSRQ-Range* IE in TS 38.331 [22] |  |
| 12503 | SINR | ELEMENT | FALSE | *SINR-Range* IE in TS 38.331 [22] |  |

#### 8.1.1.4 L2 MAC State Variables

The following RAN Parameters are associated with UE-specific L2 MAC state variables.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 13001 | Buffer Occupancy | STRUCTURE |  |  | Buffer Occupancy (BO) in number of bytes as defined in TS 25.321 [27] clause 8.2.2(c). LCID indicates logical channel ID. |
| 13002 | >LCID | ELEMENT | TRUE | INTEGER (0.. 63) |
| 13003 | >BO in Bytes | ELEMENT | FALSE | INTEGER |
| 13004 | Buffer Status Report | STRUCTURE |  |  | MCE Control Elements as defined in TS 38.321 [26] clause 6.1.3. |
| 13005 | >Short BSR | ELEMENT | FALSE | OCTET STRING (SIZE(1)) |
| 13006 | >Long BSR | ELEMENT | FALSE | OCTET STRING |
| 13007 | >Short Truncated BSR | ELEMENT | FALSE | OCTET STRING (SIZE(1)) |
| 13008 | >Long Truncated BSR | ELEMENT | FALSE | OCTET STRING |
| 13009 | >Pre-emptive BSR | ELEMENT | FALSE | OCTET STRING |
| 13010 | SCell Activation/Deactivation | STRUCTURE |  |  |
| 13011 | >One Octet | ELEMENT | FALSE | OCTET STRING (SIZE(1)) |
| 13012 | >Four Octet | ELEMENT | FALSE | OCTET STRING (SIZE(4)) |
| 13013 | Duplication Activation/Deactivation | ELEMENT | FALSE | OCTET STRING (SIZE(1)) |
| 13014 | Duplication RLC Activation/Deactivation | ELEMENT | FALSE | OCTET STRING (SIZE(1)) |

#### 8.1.1.5 NG-RAN Data Radio Bearer

The following RAN Parameters are associated with the NG-RAN data radio bearer.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 14001 | 5QI | ELEMENT | FALSE | *5QI* IE in TS 38.463 [21] Section 9.3.1.27 or TS 38.463 [21] Section 9.3.1.28 |  |
| 14002 | Packet Delay Budget | ELEMENT | FALSE | *Packet Delay Budget* IE in TS 38.463 [21] Section 9.3.1.47 |  |
| 14003 | Packet Error Rate | ELEMENT | FALSE | *Packet Error Rate* IE in TS 38.463 [21] Section 9.3.1.48 |  |
| 14004 | NG-RAN DRB Allocation and Retention Priority | STRUCTURE |  |  | *NG-RAN Allocation and Retention Priority* IE in TS 38.463 [21] Section 9.3.1.29 |
| 14005 | >Priority Level | ELEMENT | FALSE | *Priority Level* IE in TS 38.463 [21] Section 9.3.1.29 |  |
| 14006 | >Pre-emption Capability | ELEMENT | FALSE | *Pre-emption Capability* IE in TS 38.463 [21] Section 9.3.1.29 |  |
| 14007 | >Pre-emption Vulnerability | ELEMENT | FALSE | *Pre-emption Vulnerability* IE in TS 38.463 [21] Section 9.3.1.29 |  |
| 14008 | Priority Level of the mapped QoS flows | ELEMENT | FALSE | *Priority Level* IE in TS 38.463 [21] Section 9.3.1.51 |  |
| 14009 | QoS parameters for GBR flows in NG-RAN Bearer | STRUCTURE |  |  | *GBR QoS Flow Information* IE in TS 38.463 [21] Section 9.3.1.30 |
| 14010 | >Maximum Flow Bit Rate Downlink | ELEMENT | FALSE | *Bit Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 14011 | >Guaranteed Flow Bit Rate Downlink | ELEMENT | FALSE | *Bit Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 14012 | >Maximum Packet Loss Rate Downlink | ELEMENT | FALSE | *Packet Loss Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 14013 | >Maximum Flow Bit Rate Uplink | ELEMENT | FALSE | *Bit Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 14014 | >Guaranteed Flow Bit Rate Uplink | ELEMENT | FALSE | *Bit Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 14015 | >Maximum Packet Loss Rate Uplink | ELEMENT | FALSE | *Packet Loss Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 14016 | QoS Monitoring Enable Request | ELEMENT | FALSE | *QoS Monitoring Request* IE in TS 38.463 [21] Section 9.3.1.26 |  |
| 14017 | QoS Monitoring Reporting Frequency | ELEMENT | FALSE | *QoS Monitoring Reporting Frequency* IE in TS 38.463 [21] Section 9.3.1.26 |  |
| 14018 | QoS Monitoring Disabled | ELEMENT | FALSE | *QoS Monitoring Disabled* IE in TS 38.463 [21] Section 9.3.1.26 |  |
| 14019 | Reflective QoS Mapping | ELEMENT | FALSE | *RDI* IE in TS 38.463 [21] Section 9.3.1.26 |  |
| 14101 | List of cell groups to be added | LIST |  |  | *Cell Group To Add* IE in TS 38.463 [21] Section 9.3.3.11 |
| 14102 | >Cell group item | STRUCTURE |  |  | *Cell Group Item* IE in TS 38.463 [21] Section 9.3.1.11 |
| 14103 | >>Cell Group ID | ELEMENT | TRUE | *Cell Group ID* IE in TS 38.463 [21] Section 9.3.1.11 |  |
| 14104 | >>Cell Group | STRUCTURE |  | 8.1.1.7 |  |
| 14201 | SDAP Configuration | STRUCTURE |  |  | *SDAP Configuration* IE in TS 38.463 [21] Section 9.3.1.39 |
| 14202 | >PDU Session ID | ELEMENT | TRUE | *PDU-SessionID* IE in TS 38.331 [22] Sec 6 |  |
| 14203 | >Default DRB | ELEMENT | FALSE | *Default DRB* IE in TS 38.463 [21] Section 9.3.1.39 |  |
| 14210 | >PDU Session | STRUCTURE |  | 8.1.1.16 |  |
| 14301 | PDCP Configuration | STRUCTURE |  |  | *PDCP Configuration* IE in TS 38.463 [21] Section 9.3.1.38 |
| 14302 | >RLC mode | ELEMENT | FALSE | *RLC mode* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 14303 | >PDCP Duplication | ELEMENT | FALSE | *PDCP Duplication* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 14304 | >UL Data Split Threshold | ELEMENT | FALSE | *UL Data Split Threshold* IE in TS 38.463 [21] Section 9.3.1.43 |  |
| 14305 | >PDCP Re-establishment | ELEMENT | FALSE | *PDCP Re-establishment* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 14306 | >PDCP Data Recovery | ELEMENT | FALSE | *PDCP Data Recovery* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 14307 | >Out-of-Order Delivery | ELEMENT | FALSE | *Out of Order Delivery* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 14308 | >PDCP Status Report Indication | ELEMENT | FALSE | *PDCP Status Report Indication* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 14309 | >Number of PDCP duplication | ELEMENT | FALSE | *Additional PDCP duplication Information* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 14310 | >UL More than one RLC | STRUCTURE |  |  | *moreThanOneRLC* IE in TS 38.331 [22] Section 6 |
| 14311 | >>Primary Path | STRUCTURE |  |  | *primaryPath* IE in TS 38.331 [22] Section 6 |
| 14312 | >>>Cell Group ID | ELEMENT | TRUE | *cellGroup* IE in TS 38.331 [22] Section 6 |  |
| 14313 | >>>Logical Channel ID | ELEMENT | FALSE | *logicalChannelIdentity* IE in TS 38.331 [22] Sec 6 |  |
| 14314 | >UL More than two RLC | STRUCTURE |  |  | *moreThanTwoRLC-DRB-r16* IE in TS 38.331 [22] Section 6 |
| 14315 | >>Split Secondary Path | ELEMENT | FALSE | *splitSecondaryPath* IE in TS 38.331 [22] Sec 6 |  |
| 14316 | >>Duplication State | ELEMENT | FALSE | *duplicationState* IE in TS 38.331 [22] Sec 6 |  |

#### 8.1.1.6 QoS flow

The following RAN Parameters are associated with the NG-RAN QoS flow.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 15001 | 5QI | ELEMENT | FALSE | *5QI* IE in TS 38.463 [21] Section 9.3.1.27 or TS 38.463 [21] Section 9.3.1.28 |  |
| 15002 | Packet Delay Budget | ELEMENT | FALSE | *Packet Delay Budget* IE in TS 38.463 [21] Section 9.3.1.47 |  |
| 15003 | Packet Error Rate | ELEMENT | FALSE | *Packet Error Rate* IE in TS 38.463 [21] Section 9.3.1.48 |  |
| 15004 | NG-RAN DRB Allocation and Retention Priority | STRUCTURE |  |  | *NG-RAN Allocation and Retention Priority* IE in TS 38.463 [21] Section 9.3.1.29 |
| 15005 | >Priority Level | ELEMENT | FALSE | *Priority Level* IE in TS 38.463 [21] Section 9.3.1.29 |  |
| 15006 | >Pre-emption Capability | ELEMENT | FALSE | *Pre-emption Capability* IE in TS 38.463 [21] Section 9.3.1.29 |  |
| 15007 | >Pre-emption Vulnerability | ELEMENT | FALSE | *Pre-emption Vulnerability* IE in TS 38.463 [21] Section 9.3.1.29 |  |
| 15008 | Priority Level of the mapped QoS flows | ELEMENT | FALSE | *Priority Level* IE in TS 38.463 [21] Section 9.3.1.51 |  |
| 15009 | QoS parameters for GBR flows in NG-RAN Bearer | STRUCTURE |  |  | *GBR QoS Flow Information* IE in TS 38.463 [21] Section 9.3.1.30 |
| 15010 | >Maximum Flow Bit Rate Downlink | ELEMENT | FALSE | *Bit Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 15011 | >Guaranteed Flow Bit Rate Downlink | ELEMENT | FALSE | *Bit Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 15012 | >Maximum Packet Loss Rate Downlink | ELEMENT | FALSE | *Packet Loss Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 15013 | Maximum Flow Bit Rate Uplink | ELEMENT | FALSE | *Bit Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 15014 | >Guaranteed Flow Bit Rate Uplink | ELEMENT | FALSE | *Bit Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 15015 | >Maximum Packet Loss Rate Uplink | ELEMENT | FALSE | *Packet Loss Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 15016 | QoS Monitoring Enable Request | ELEMENT | FALSE | *QoS Monitoring Request* IE in TS 38.463 [21] Section 9.3.1.26 |  |
| 15017 | QoS Monitoring Reporting Frequency | ELEMENT | FALSE | *QoS Monitoring Reporting Frequency* IE in TS 38.463 [21] Section 9.3.1.26 |  |
| 15018 | QoS Monitoring Disabled | ELEMENT | FALSE | *QoS Monitoring Disabled* IE in TS 38.463 [21] Section 9.3.1.26 |  |
| 15019 | Reflective QoS Mapping | ELEMENT | FALSE | *RDI* IE in TS 38.463 [21] Section 9.3.1.26 |  |
| 15020 | Redundant QoS Flow Indicator | ELEMENT | FALSE | *Redundant QoS Flow Indicator* IE in TS 38.463 [21] Section 9.3.1.74 |  |

#### 8.1.1.7 Cell Group

The following RAN Parameters are associated with the NR cell group item.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 15502 | UL Configuration | ELEMENT | FALSE | *UL Configuration* IE in TS 38.463 [21] Section 9.3.1.11 |  |
| 15503 | RAT Type | ELEMENT | FALSE | *RAT Type* IE in TS 38.463 [21] Section 9.3.1.11 |  |
| 15504 | Number of Tunnels | ELEMENT | FALSE | *Number of Tunnels* IE in TS 38.463 [21] Section 9.3.1.11 |  |

#### 8.1.1.8 L2 Bearer State Variables

The following RAN Parameters are associated with UE-specific L2 bearer state variables across PDCP, RLC layers.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 16001 | PDCP State Variables | STRUCTURE |  |  | PDCP State Variables defined in TS 38.323 [24] clause 7.1. LCID indicates logical channel ID, to pinpoint which PDCP entity. |
| 16002 | >LCID | ELEMENT | TRUE | INTEGER (0.. 63) |
| 16003 | >TX\_Next | ELEMENT | FALSE | INTEGER (0.. 232-1) |
| 16004 | >RX\_Next | ELEMENT | FALSE | INTEGER (0.. 232-1) |
| 16005 | >RX\_Deliv | ELEMENT | FALSE | INTEGER (0.. 232-1) |
| 16006 | >RX\_Reord | ELEMENT | FALSE | INTEGER (0.. 232-1) |
| 16010 | RLC UM State Variables | STRUCTURE |  |  | RLC UM State Variables defined in TS 38.322 [25] clause 7.1. LCID indicates logical channel ID, to pinpoint which RLC UM entity. |
| 16011 | >LCID | ELEMENT | TRUE | INTEGER (0.. 63) |
| 16012 | >TX\_Next | ELEMENT | FALSE | INTEGER (0.. 4095) |
| 16013 | >RX\_Next\_Reassembly | ELEMENT | FALSE | INTEGER (0.. 4095) |
| 16014 | >RX\_Timer\_Trigger | ELEMENT | FALSE | INTEGER (0.. 4095) |
| 16015 | >RX\_Next\_Highest | ELEMENT | FALSE | INTEGER (0.. 4095) |
| 16020 | RLC AM State Variables | STRUCTURE |  |  | RLC AM State Variables defined in TS 38.322 [25] clause 7.1. LCID indicates logical channel ID, to pinpoint which RLC AM entity. |
| 16021 | >LCID | ELEMENT | TRUE | INTEGER (0.. 63) |
| 16022 | >TX\_Next\_Ack | ELEMENT | FALSE | INTEGER (0.. 262143) |
| 16023 | >TX\_Next | ELEMENT | FALSE | INTEGER (0.. 262143) |
| 16024 | >POLL\_SN | ELEMENT | FALSE | INTEGER (0.. 262143) |
| 16025 | >RX\_Next | ELEMENT | FALSE | INTEGER (0.. 262143) |
| 16026 | >RX\_Next\_Status\_Trigger | ELEMENT | FALSE | INTEGER (0.. 262143) |
| 16027 | >RX\_Highest\_Status | ELEMENT | FALSE | INTEGER (0.. 262143) |
| 16028 | >RX\_Next\_Highest | ELEMENT | FALSE | INTEGER (0.. 262143) |

#### 8.1.1.9 E-RAB QoS Parameters

The following RAN Parameters are associated with E-RAB QoS.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 16201 | QCI | ELEMENT | FALSE | *QCI* IE in TS 36.423 [17] Section 9.2.9 |  | |
| 16202 | Allocation and Retention Priority | STRUCTURE |  |  | *Allocation and Retention Priority* IE in TS 36.423 [17] Section 9.2.31 | |
| 16203 | >Priority Level | ELEMENT | FALSE | *Priority Level* IE in TS 36.423 [17] Section 9.2.31 |  | |
| 16204 | >Pre-emption Capability | ELEMENT | FALSE | *Pre-emption Capability* IE in TS 36.423 [17] Section 9.2.31 |  | |
| 16205 | >Pre-emption Vulnerability | ELEMENT | FALSE | *Pre-emption Vulnerability* IE in TS 36.423 [17] Section 9.2.31 |  | |
| 16206 | GBR QoS Information | STRUCTURE |  |  | *GBR QoS Information* IE in TS 36.423 [17] Section 9.2.9 | |
| 16207 | >E-RAB Maximum Bit Rate Downlink | ELEMENT | FALSE | *Bit Rate* IE in TS 36.423 [17] Section 9.2.11 | *E-RAB Maximum Bit Rate Downlink* IE in TS 36.423 [17] Section 9.2.10 | |
| 16208 | >E-RAB Maximum Bit Rate Uplink | ELEMENT | FALSE | *Bit Rate* IE in TS 36.423 [17] Section 9.2.11 | *E-RAB Maximum Bit Rate Uplink* IE in TS 36.423 [17] Section 9.2.10 | |
| 16209 | >E-RAB Guaranteed Bit Rate Downlink | ELEMENT | FALSE | *Bit Rate* IE in TS 36.423 [17] Section 9.2.11 | *E-RAB Guaranteed Bit Rate Downlink* IE in TS 36.423 [17] Section 9.2.10 | |
| 16210 | >E-RAB Guaranteed Bit Rate Downlink | ELEMENT | FALSE | *Bit Rate* IE in TS 36.423 [17] Section 9.2.11 | *E-RAB Guarnateed Bit Rate Downlink* IE in TS 36.423 [17] Section 9.2.10 | |
| 16211 | Downlink Maximum Packet Loss Rate | ELEMENT | FALSE | *Packet Loss Rate* IE in TS 36.423 [17] Section 9.2.124 | *Downlink Maximum Packet Loss Rate* IE in TS 36.423 [17] Section 9.2.10 | |
| 16212 | Uplink Maximum Packet Loss Rate | ELEMENT | FALSE | *Packet Loss Rate* IE in TS 36.423 [17] Section 9.2.124 | *Uplink Maximum Packet Loss Rate* IE in TS 36.423 [17] Section 9.2.10 | |

#### 8.1.1.10 Connectivity and Mobility Event thresholds

The following RAN Parameters are associated with connectivity and mobility event thresholds, mainly related to A1, A2, A3, A4, A5, A6 events and inter-RAT B1 and B2 events.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** | |
| 16500 | Event AN Trigger Config | STRUCTURE |  |  | *EventTriggerConfig* IE in TS 38.331 [22] | |
| 16501 | **>CHOICE *AN Event*** | STRUCTURE |  |  | *eventID* IE in TS 38.331 [22] | |
| 16502 | >>A1 Event | STRUCTURE |  |  | | *EventA1* IE in TS 38.331 [22] |
| 16503 | >>>A1-Threshold | STRUCTURE |  | 8.1.1.3 | |  |
| 16504 | >>>Hysteresis | ELEMENT | FALSE | *Hysteresis* IE in TS 38.331 [22] | |  |
| 16505 | >>RS-Type | ELEMENT | FALSE | *rsType* IE in TS 38.331 [22] | |  |
| 16506 | >>A2 Event | STRUCTURE |  |  | | *EventA2* IE in TS 38.331 [22] |
| 16507 | >>>A2-Threshold | STRUCTURE |  | 8.1.1.3 | |  |
| 16508 | >>>Hysteresis | ELEMENT | FALSE | *Hysteresis* IE in TS 38.331 [22] | |  |
| 16509 | >>>RS-Type | ELEMENT | FALSE | *rsType* IE in TS 38.331 [22] | |  |
| 16510 | >>A3 Event | STRUCTURE |  |  | | *EventA3* IE in TS 38.331 [22] |
| 16511 | >>>A3-Offset | STRUCTURE |  | 8.1.1.3 | |  |
| 16512 | >>>Hysteresis | ELEMENT | FALSE | *Hysteresis* IE in TS 38.331 [22] | |  |
| 16513 | >>>RS-Type | ELEMENT | FALSE | *rsType* IE in TS 38.331 [22] | |  |
| 16514 | >>A4 Event | STRUCTURE |  |  | | *EventA4* IE in TS 38.331 [22] |
| 16515 | >>>A4-Threshold | STRUCTURE |  | 8.1.1.3 | |  |
| 16516 | >>>Hysteresis | ELEMENT | FALSE | *Hysteresis* IE in TS 38.331 [22] | |  |
| 16517 | >>>RS-Type | ELEMENT | FALSE | *rsType* IE in TS 38.331 [22] | |  |
| 16518 | >>A5 Event | STRUCTURE |  |  | | *EventA5* IE in TS 38.331 [22] |
| 16519 | >>>A5-Threshold1 | STRUCTURE |  | 8.1.1.3 | |  |
| 16520 | >>>A5-Threshold2 | STRUCTURE |  | 8.1.1.3 | |  |
| 16521 | >>>Hysteresis | ELEMENT | FALSE | *Hysteresis* IE in TS 38.331 [22] | |  |
| 16522 | >>>RS-Type | ELEMENT | FALSE | *rsType* IE in TS 38.331 [22] | |  |
| 16523 | >>A6 Event | STRUCTURE |  |  | | *EventA6* IE in TS 38.331 [22] |
| 16524 | >>>A6-Offset | STRUCTURE |  | 8.1.1.3 | |  |
| 16525 | >>>Hysteresis | ELEMENT | FALSE | *Hysteresis* IE in TS 38.331 [22] | |  |
| 16526 | >>>RS-Type | ELEMENT | FALSE | *rsType* IE in TS 38.331 [22] | |  |
| 16550 | Event Trigger Config Inter RAT | STRUCTURE |  |  | | *EventTriggerConfigInterRAT* IE in TS 38.331 [22] |
| 16551 | **>CHOICE *Inter-RAT Event*** | STRUCTURE |  |  | | *eventId* IE in TS 38.331 [22] |
| 16552 | >>B1 Event | STRUCTURE |  |  | | *eventB1* IE in TS 38.331 [22] |
| 16553 | >>>B1-Threshold | STRUCTURE |  | 8.1.1.3 | |  |
| 16554 | >>>Hysteresis | ELEMENT | FALSE | *Hysteresis* IE in TS 38.331 [22] | |  |
| 16555 | >>>RS-Type | ELEMENT | FALSE | *rsType* IE in TS 38.331 [22] | |  |
| 16556 | >>B2 Event | STRUCTURE |  |  | | *eventB2* IE in TS 38.331 [22] |
| 16557 | >>>B2-Threshold-NR | STRUCTURE |  | 8.1.1.3 | |  |
| 16558 | >>>B2-Threshold-EUTRA | STRUCTURE |  | 8.1.1.3 | |  |
| 16559 | >>>Hysteresis | ELEMENT | FALSE | *Hysteresis* IE in TS 38.331 [22] | |  |
| 16560 | >>>RS-Type | ELEMENT | FALSE | *rsType* IE in TS 38.331 [22] | |  |

#### 8.1.1.11 E2 Node

The following RAN Parameters are associated with the E2 node.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 17001 | CHOICE E2 Node Component Type | STRUCTURE |  |  | O-RAN WG3 E2AP Section 9.2.26 |
| 17010 | >NG-RAN gNB | STRUCTURE |  |  | O-RAN WG3 E2AP Section 9.2.27 |
| 17011 | >>Global gNB ID | STRUCTURE |  |  | TS 38.413 [11] Section 9.3.1.6 |
| 17012 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.413 [11] Section 9.3.3.5 |  |
| 17013 | >>>CHOICE *gNB ID* | STRUCTURE |  |  | *gNB ID* IE in TS 38.413 [11] Section 9.3.1.6 |
| 17014 | >>>>*gNB ID* | STRUCTURE |  |  | *gNB ID* IE in TS 38.413 [11] Section 9.3.1.6 |
| 17015 | >>>>>gNB ID | ELEMENT | FALSE | *gNB ID* IE *in* TS 38.413 [11] Section 9.3.1.6 |  |
| 17016 | >>List of NR served cells | LIST |  |  | *List of Served Cells NR* IE in TS 38.423 [15] Section 9.1.3.1 |
| 17017 | >>>Served NR cell item | STRUCTURE |  |  | Individual cell item in the *List of Served Cells* NR |
| 17028 | >>>>Served NR cell | STRUCTURE |  | *NR Cell* IE in 8.1.1.1 |  |
| 17018 | >>Count of list of NR served cells | ELEMENT | FALSE | INTEGER (1..16384) |  |
| 17019 | >>List of NR neighbor cells | LIST |  |  | *Neighbor Information* IE in TS 38.423 [15] Section 9.2.2.13 |
| 17020 | >>>NR neighbor cell item | STRUCTURE |  |  | Individual cell item in the *Neighor Information* IE NR |
| 17031 | >>>>Neighbor NR cell | STRUCTURE |  | *NR Cell* IE in 8.1.1.1 |  |
| 17021 | >>Number of RRC connections | ELEMENT | FALSE | *Number of RRC connections* IE in TS 38.423 [15] Section 9.2.2.57 |  |
| 17022 | >>gNB Performance Measurements | STRUCTURE |  | 8.1.1.15 |  |
| 17050 | >en-gNB | STRUCTURE |  |  | O-RAN WG3 E2AP Section 9.2.27 |
| 17051 | >>Global en-gNB ID | STRUCTURE |  |  | TS 36.423 [17] Section 9.2.112 |
| 17052 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 36.423 [17] Section 9.2.4 |  |
| 17053 | >>>CHOICE *en-gNB ID* | STRUCTURE |  | *en-gNB ID* IE in TS 36.423 [17] Section 9.2.112 |  |
| 17054 | >>>>*en-gNB ID* | STRUCTURE |  | *en-gNB ID* IE in TS 36.423 [17] Section 9.2.112 |  |
| 17055 | >>>>>en-gNB ID | ELEMENT | FALSE | *en-gNB ID* IE in TS 36.423 [17] Section 9.2.112 |  |
| 17056 | >>List of served NR cells | LIST |  |  | *List of Served Cells NR* IE in TS 38.423 [15] Section 9.1.3.1 |
| 17057 | >>>Served NR cell item | STRUCTURE |  |  | Individual cell item in the *List of Served Cells NR* IE |
| 17068 | >>>>Served NR cell | STRUCTURE |  | *NR Cell* IE in 8.1.1.1 |  |
| 17058 | >>Count of list of NR served cells | ELEMENT | FALSE | INTEGER (1..16384) |  |
| 17059 | >>List of NR neighbour cells | LIST |  |  | *Neighbor Information* IE in TS 38.423 [15] Section 9.2.2.13 |
| 17060 | >>>NR neighbor cell item | STRUCTURE |  |  | Individual cell item in *Neighbor Information* IE |
| 17065 | >>>>NR neighbor cell | STRUCTURE |  | *NR Cell* IE in 8.1.1.1 |  |
| 17061 | >>gNB Performance Measurements | STRUCTURE |  | 8.1.1.15 | *gNB Measurements* IE in Sec 8.1.1.15 |
| 17070 | >ng-eNB | STRUCTURE |  |  | O-RAN WG3 E2AP Section 9.2.27 |
| 17071 | >>ng-eNB ID | STRUCTURE |  |  | *ng-eNB ID* IE TS 38.413 [11] Section 9.2.2.2 |
| 17072 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.413 [11] Section 9.3.1.6 |  |
| 17073 | >>>CHOICE *ng-eNB ID* | STRUCTURE |  |  | *Ng-eNB ID* IE in TS 38.413 [11] Section 9.2.2.2 |
| 17074 | >>>>Macro *ng-eNB ID* | STRUCTURE |  |  | *Macro ng-eNB ID* IE in TS 38.413 [11] Section 9.2.2.2 |
| 17075 | >>>>>Macro *ng-eNB ID* | ELEMENT | FALSE | *Macro ng-eNB ID* IE in TS 38.413 [11] Section 9.2.2.2 |  |
| 17076 | >>>>Short Macro *ng-eNB ID* | STRUCTURE |  |  | *Short Macro ng-eNB ID* IE in TS 38.413 [11] Section 9.2.2.2 |
| 17077 | >>>>>Short Macro *ng-eNB ID* | ELEMENT | FALSE | *Short Macro ng-eNB ID* IE in TS 38.413 [11] Section 9.2.2.2 |  |
| 17078 | >>>>Long Macro *ng-eNB ID* | STRUCTURE |  |  | *Long Macro ng-eNB ID* IE in TS 38.413 [11] Section 9.2.2.2 |
| 17079 | >>>>>Long Macro *ng-eNB ID* | ELEMENT | FALSE | *Long Macro ng-eNB ID* IE in TS 38.413 [11] Section 9.2.2.2 |  |
| 17080 | >>List of E-UTRA served cells | LIST |  |  | *List of Served Cells E-UTRA* IE in TS 38.423 [15] Section 9.1.3.1 |
| 17081 | >>>Served E-UTRA cell item | STRUCTURE |  |  | Individual cell item in *List of Served Cells E-UTRA* IE |
| 17092 | >>>>Served E-UTRA cell | STRUCTURE |  | 8.1.1.2 |  |
| 17082 | >>Count of list of E-UTRA served cells | ELEMENT | FALSE | INTEGER (0..16384) |  |
| 17083 | >>List of E-UTRA neighbor cells | LIST |  |  | *Neighbor Information E-UTRA* IE in TS 38.423 [15] Section 9.2.2.14 |
| 17084 | >>>E-UTRA neighbor cell item | STRUCTURE |  |  | Individual cell item in *Neighbor Information E-UTRA* IE |
| 17095 | >>>>E-UTRA neighbor cell | STRUCTURE |  | 8.1.1.2 |  |
| 17085 | >>Number of RRC connections | ELEMENT | FALSE | *Number of RRC connections* IE in TS 38.423 [15] Section 9.2.2.57 |  |
| 17086 | >>eNB Performance Measurements | STRUCTURE |  | 8.1.1.18 |  |
| 17100 | >NG-RAN gNB CU-CP | STRUCTURE |  |  | O-RAN WG3 E2AP Section 9.2.27 |
| 17101 | >>Global gNB CU-CP ID | STRUCTURE |  |  | TS 38.413 [11] Section 9.3.1.6 |
| 17102 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.413 [11] Section 9.3.3.5 |  |
| 17103 | >>>CHOICE *gNB ID* | STRUCTURE |  |  | *gNB ID* IE in TS 38.413 [11] Section 9.3.1.6 |
| 17104 | >>>>*gNB ID* | STRUCTURE |  |  | *gNB ID* IE in TS 38.413 [11] Section 9.3.1.6 |
| 17105 | >>>>>gNB ID | ELEMENT | FALSE | *gNB ID* IE *in* TS 38.413 [11] Section 9.3.1.6 |  |
| 17107 | >>List of activated NR cells | LIST |  |  | *Cells to be Activated List* IE in TS 38.473 [19] Section 9.2.1.10 |
| 17108 | >>>NR cell item | STRUCTURE |  |  | *Cells to be Activated Item* IE in TS 38.473 [19] Section 9.2.1.10 |
| 17109 | >>>>NR cell | STRUCTURE |  | *NR Cell* IE in 8.1.1.1 |  |
| 17110 | >>>>Available PLMN List | LIST |  |  | *Available PLMN List* IE in TS 38.473 [19] Section 9.2.1.10 |
| 17111 | >>>>>PLMN Item | STRUCTURE |  |  | *Available PLMN Item IEs* IE in TS 38.473 [19] Section 9.3.1.65 |
| 17112 | >>>>>>PLMN ID | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.413 [11] Section 9.3.3.5 |  |
| 17113 | >>List of de-activated NR cells | LIST |  |  | *Cells to be Deactivated List* IE in TS 38.473 [19] Section 9.2.1.10 |
| 17114 | >>>NR cell item | STRUCTURE |  |  | Individual cell item in *Cells to be Deactivated List* IE |
| 17515 | >>>>NR cell | STRUCTURE |  | *NR Cell* IE in 8.1.1.1 |  |
| 17115 | >>List of barred NR cells | LIST |  |  | *Cells to be barred List* IE in TS 38.473 [19] Section 9.2.1.10 |
| 17116 | >>>NR cell item | STRUCTURE |  |  | Individual cell item in *Cells to be barred List* IE |
| 17517 | >>>>NR cell | STRUCTURE |  | *NR Cell* IE in 8.1.1.1 |  |
| 17117 | >>Count of list of NR served cells | ELEMENT | FALSE | INTEGER (0..16384) |  |
| 17118 | >>List of NR neighbor cells | LIST |  |  | *Neighbour Cell Information List* IE in TS 38.473 [19] Section 9.2.1.10 |
| 17119 | >>>NR neighbor cell item | STRUCTURE |  |  | Individual Cell Item in *Neighbour Cell Information List* IE |
| 17520 | >>>>NR neighbor cell | STRUCTURE |  | *NR Cell* IE in 8.1.1.1 |  |
| 17120 | >>Number of RRC connected UEs | ELEMENT | FALSE | *Number of RRC connections* IE in TS 38.423 [15] Section 9.2.2.57 |  |
| 17121 | >>gNB CU-CP Performance Measurements | STRUCTURE |  | 8.1.1.12 |  |
| 17130 | >NG-RAN gNB DU | STRUCTURE |  |  | O-RAN WG3 E2AP Section 9.2.27 |
| 17132 | >>gNB-DU ID | ELEMENT | FALSE | *gNB-DU ID* IE in TS 38.473 [19] Section 9.3.1.9 |  |
| 17133 | >>List of NR served cells | LIST |  |  | *List of Served Cells NR*  IE in TS 38.423 [15] Section 9.1.3.1 |
| 17134 | >>>Served NR cell item | STRUCTURE |  |  | Individual cell item in *List of Served Cells* NR IE |
| 17535 | >>>>Served NR cell | STRUCTURE |  | *NR Cell* IE in 8.1.1.1 |  |
| 17135 | >>gNB DU Measurements | STRUCTURE |  | 8.1.1.14 |  |
| 17140 | >NG-RAN gNB CU-UP | STRUCTURE |  |  | O-RAN WG3 E2AP Section 9.2.27 |
| 17141 | >>gNB CU-UP ID | ELEMENT | TRUE | *gNB-CU-UP ID* IE in TS 38.463 [21] Section 9.3.1.15 |  |
| 17142 | >>gNB CU-UP Capacity | ELEMENT | FALSE | *gNB-CU-UP Capacity* IE in TS 38.463 [21] Section 9.3.1.56 |  |
| 17143 | >>gNB CU-UP Performance Measurements | STRUCTURE |  | 8.1.1.13 |  |
| 17150 | >eNB | STRUCTURE |  |  | O-RAN WG3 E2AP Section 9.2.27 |
| 17151 | >>eNB ID | STRUCTURE |  |  | *eNB ID* IE TS 36.423 [17] Section 9.2.2.2 |
| 17152 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 36.423 [17] Section 9.2.4 |  |
| 17153 | >>>CHOICE *eNB ID* | STRUCTURE |  |  | *Global eNB ID* IE in TS 36.423 [17] Section 9.2.22 |
| 17154 | >>>>Macro eNB ID | STRUCTURE |  |  | *Macro eNB ID* IE in TS 36.423 [17] Section 9.2.22 |
| 17155 | >>>>>Macro eNB ID | ELEMENT | FALSE | *Macro eNB ID* IE in TS 36.423 [17] Section 9.2.22 |  |
| 17156 | >>>>Home eNB ID | STRUCTURE |  |  | *Home eNB ID* IE in TS 36.423 [17] Section 9.2.22 |
| 17157 | >>>>>Home eNB ID | ELEMENT | FALSE | *Home eNB ID* IE in TS 36.423 [17] Section 9.2.22 |  |
| 17158 | >>>>Short Macro eNB ID | STRUCTURE |  |  | *Short Macro eNB ID* IE in TS 36.423 [17] Section 9.2.22 |
| 17159 | >>>>>Short Macro eNB ID | ELEMENT | FALSE | *Short Macro eNB ID* IE in TS 36.423 [17] Section 9.2.22 |  |
| 17160 | >>>>Long Macro eNB ID | STRUCTURE |  |  | *Long Macro eNB ID* IE in TS 36.423 [17] Section 9.2.22 |
| 17161 | >>>>>Long Macro eNB ID | ELEMENT | FALSE | *Long Macro eNB ID* IE in TS 36.423 [17] Section 9.2.22 |  |
| 17162 | >>List of E-UTRA served cells | LIST |  |  | *List of Served Cells E-UTRA* IE in TS 38.423 [15] Section 9.1.3.1 |
| 17163 | >>>Served E-UTRA cell item | STRUCTURE |  |  | Individual cell item in *List of Served Cells E-UTRA* IE |
| 17564 | >>>>Served E-UTRA cell | STRUCTURE |  | 8.1.1.2 |  |
| 17164 | >>Count of list of E-UTRA served cells | ELEMENT | FALSE | INTEGER (0..16384) |  |
| 17165 | >>List of E-UTRA neighbor cells | LIST |  |  | *Neighbor Information E-UTRA* IE in TS 38.423 [15] Section 9.2.2.14 |
| 17166 | >>>E-UTRA neighbor cell item | STRUCTURE |  |  | Individual cell item in *Neighbor Information E-UTRA* IE |
| 17567 | >>>>E-UTRA neighbor cell | STRUCTURE |  | 8.1.1.2 |  |
| 17167 | >>Number of RRC connected UEs | ELEMENT | FALSE | *Number of RRC connections* IE in TS 38.423 [15] Section 9.2.2.57 |  |
| 17168 | >>List of NR neighbor cells | LIST |  |  | *Neighbor Information* IE in TS 38.423 [15] Section 9.2.2.13 |
| 17169 | >>>NR neighbor cell item | STRUCTURE |  |  | Individual cell item in *Neighbor Information* IE |
| 17570 | >>>>NR neighbor cell | STRUCTURE |  | 8.1.1.1 |  |
| 17170 | >>eNB Performance Measurements | STRUCTURE |  | 8.1.1.18 |  |
| 17200 | TAI Support List | LIST |  |  | *TAI Support List* IE in TS 38.423 [15] Section 9.2.3.20 |
| 17201 | >TAI Support Item | STRUCTURE |  |  | *TAI Support Item* IE in TS 38.423 [15] Section 9.2.3.20 |
| 17202 | >>TAC | ELEMENT | FALSE | *TAC* IE in TS 38.423 [15] Section 9.2.2.5 |  |
| 17203 | >>List of Broadcast PLMNs | LIST |  |  | *Broadcast PLMNs* IE in TS 38.423 [15] Section 9.2.3.20 |
| 17204 | >>>Broadcast PLMN Item | STRUCTURE |  |  | *Broadcast PLMNs* IE in TS 38.423 [15] Section 9.2.3.20 |
| 17205 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.413 [11] Section 9.3.3.5 |  |
| 17206 | >>>TAI Slice Support List | LIST |  |  | *TAI Slice Support List* IE in TS 38.423 [15] Section 9.2.3.20 |
| 17207 | >>>>Slice Support Item | STRUCTURE |  |  | *Slice Support Item* IE in TS 38.423 [15] Section 9.2.3.20 |
| 17208 | >>>>>S-NSSAI | STRUCTURE |  |  | *S-NSSAI* IE in TS 38.473 [19] Section 9.3.1.38 |
| 17209 | >>>>>>SST | ELEMENT | TRUE | *SST* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 17210 | >>>>>>SD | ELEMENT | FALSE | *SD* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 17211 | >>>Count of TAI Slice Support List | ELEMENT | FALSE | INTEGER (0..1024) |  |
| 17212 | >>>NR CGI Support List | LIST |  |  | *List of Served Cells NR* IE in TS 38.423 [15] Section 9.1.3.1 |
| 17213 | >>>>NR CGI Cell Support Item | STRUCTURE |  |  | Individual cell item in *List of Served Cells NR* IE |
| 17614 | >>>>>NR CGI Cell | STRUCTURE |  | *NR Cell* IE in 8.1.1.1 |  |
| 17214 | >>>E-UTRA CGI Support List | LIST |  |  | *List of Served Cells E-UTRA* IE in TS 38.423 [15] Section 9.1.3.1 |
| 17215 | >>>>E-UTRA CGI Cell Support Item | STRUCTURE |  |  | Individual cell item in *List of Served Cells E-UTRA* IE |
| 17616 | >>>>>E-UTRA CGI | STRUCTURE |  | *E-UTRA Cell* IE in 8.1.1.2 |  |
| 17216 | >>>QoS Parameters Support List | LIST |  |  | *QoS Flow List* IE in TS 38.463 [21] Section 9.3.1.12 |
| 17217 | >>>>QoS Parameters Support Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.12 |
| 17218 | >>>>>CHOICE QoS Parameters Support Item | STRUCTURE |  |  |  |
| 17219 | >>>>>>NG-RAN QoS Support Item | STRUCTURE |  | 8.1.1.6 |  |
| 17221 | >>>>>>E-UTRA QoS Support Item | STRUCTURE |  | 8.1.1.9 |  |
| 17223 | >>Count of list of broadcast PLMNs | ELEMENT | FALSE | INTEGER (0..12) |  |
| 17224 | Count of TAI Support List | ELEMENT | FALSE | INTEGER (0..256) |  |

#### 8.1.1.12 gNB CU-CP Measurements

The following RAN Parameters are associated with the gNB CU-CP measurements.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 18001 | Inter-gNB Handovers | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.6.1 |
| 18002 | >Number of requested handover operations | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.7.1.1 |
| 18003 | >Number of successful handover preparations | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.7.1.2 |
| 18004 | >List of failure causes in handover preparations | LIST |  | *0..<maxnoofcauses>* | TS 28.552 [28] Sec 5.1.1.6.1.3 |
| 18005 | >>Failure Cause Item | STRUCTURE |  |  |  |
| 18006 | >>>Failure Cause | ELEMENT | TRUE | *Cause* IE in TS 38.423 [15] Section 9.2.3.2 |  |
| 18007 | >>Number of failed handover preparations for the cause | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.1.3 |
| 18008 | >Number of requested handover resource allocations | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.1.4 |
| 18009 | >Number of successful handover resource allocations | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.1.5 |
| 18010 | >List of failure causes | LIST |  | *0..<maxnoofcauses>* | TS 28.552 [28] Sec 5.1.1.6.1.6 |
| 18011 | >>Failure Cause Item | STRUCTURE |  |  |  |
| 18012 | >>>Failure Cause | ELEMENT | TRUE | *Cause* IE in TS 38.413 [11] Section 9.3.1.2 |  |
| 18013 | >>>Number of failed handover resource allocations for the cause | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.1.6 |
| 18014 | >Number of requested handover executions | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.1.7 |
| 18015 | >Number of successful handover executions | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.1.8 |
| 18016 | >List of failure causes in handover execution | LIST |  | *0..<maxnoofcauses>* | TS 28.552 [28] Sec 5.1.1.6.1.9 |
| 18017 | >>Failure cause Item | STRUCTURE |  |  |  |
| 18018 | >>>Failure Cause | ELEMENT | TRUE | *Cause* IE in TS 38.423 [15] Section 9.2.3.2 |  |
| 18019 | >>>Number of failed handover executions for the cause | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.1.9 |
| 18020 | >List of Slices | LIST |  | *0..<maxnoofslices>* | TS 28.552 [28] Sec 5.1.1.6.1.10 |
| 18021 | >>Slice Item | STRUCTURE |  |  |  |
| 18022 | >>>S-NSSAI | STRUCTURE |  |  | *S-NSSAI* IE in TS 38.473 [19] Section 9.3.1.38 |
| 18023 | >>>>SST | ELEMENT | TRUE | *SST* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 18024 | >>>>SD | ELEMENT | FALSE | *SD* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 18025 | >>>Mean Time of requested handover executions | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.1.10 |
| 18026 | >>>Max Time of requested handover executions | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.1.11 |
| 18031 | >MRO Measurements | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.25 |
| 18032 | >>Number of too-early handovers | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.25.1 |
| 18033 | >>Number of too-late handovers | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.25.1 |
| 18034 | >>Number of wrong cell handovers | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.25.1 |
| 18051 | Intra-gNB Handovers | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.3.7.1 |
| 18052 | >Number of requested handover executions | ELEMENT | FALSE |  | TS 28.552 [28] Sec 5.1.1.6.2.1 |
| 18053 | >Number of successful handover executions | ELEMENT | FALSE |  | TS 28.552 [28] Sec 5.1.1.6.2.2 |
| 18054 | List of UE Context release causes | LIST |  | *0..<maxnoofcauses>* | TS 28.552 [28] Sec 5.1.3.5.2 |
| 18055 | >Release Cause Item | STRUCTURE |  |  |  |
| 18056 | >>Release Cause | ELEMENT | TRUE | *Cause* IE in TS 38.473 [19] Section 9.3.1.2 |  |
| 18057 | >>Number of UE Context Release Requests | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.5.2 |
| 18061 | >MRO Measurements | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.25 |
| 18062 | >>Number of too-early handovers | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.25.1 |
| 18063 | >>Number of too-late handovers | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.25.1 |
| 18064 | >>Number of wrong cell handovers | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.25.1 |
| 18400 | Average normally-released call duration for 5QI 1 QoS flow | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.24.1 |
| 18071 | Distribution bins for normally-released call duration for 5QI 1 QoS flow | LIST |  | *0..<maxnoofbins>* | TS 28.552 [28] Sec 5.1.3.8 |
| 18072 | >Distribution bin item | STRUCTURE |  |  |  |
| 18073 | >>Call Duration Bin Value | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.8 |
| 18074 | >>Number of samples | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.8 |
| 18450 | Average abnormally-released call duration for 5QI 1 QoS flow | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.24.2 |
| 18075 | Distribution bins for abnormally-released call duration for 5QI 1 QoS flow | LIST |  | *0..<maxnoofbins>* | TS 28.552 [28] Sec 5.1.3.9 |
| 18076 | >Distribution bin item | STRUCTURE |  |  |  |
| 18077 | >>Call Duration Bin Value | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.9 |
| 18078 | >>Number of samples | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.9 |
| 18100 | RRC connection related measurements | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.15 |
| 18101 | >List of attempted RRC connection establishment causes | LIST |  | *0..<maxnoofcauses>* | TS 28.552 [28] Sec 5.1.1.15.1 |
| 18102 | >>Attempted RRC connection establishment cause item | STRUCTURE |  |  |  |
| 18103 | >>>Cause | ELEMENT | TRUE | *Cause* IE in TS 38.331 [22] Sec 6.2.2 |  |
| 18104 | >>>Number of attempted RRC connection establishments | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.15.1 |
| 18111 | >List of successful RRC connection establishment causes | LIST |  | *0..<maxnoofcauses>* | TS 28.552 [28] Sec 5.1.1.15.2 |
| 18112 | >>Succesful RRC connection establishment cause item | STRUCTURE |  |  |  |
| 18113 | >>>Cause | ELEMENT | TRUE | *Cause* IE in TS 38.331 [22] Sec 6.2.2 |  |
| 18114 | >>>Number of successful RRC connection establishments | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.15.2 |
| 18121 | >Number of RRC connection re-establishment attempts | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.17.1 |
| 18122 | >Successful number of RRC connection re-establishment with UE context | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.17.2 |
| 18123 | >Successful number of RRC connection re-establishment without UE context | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.17.3 |
| 18131 | >List of RRC connection resuming attempt causes | LIST |  | *0..<maxnoofcauses>* | TS 28.552 [28] Sec 5.1.1.18.1 |
| 18132 | >>Cause item | STRUCTURE |  |  |  |
| 18133 | >>>Cause | ELEMENT | TRUE | *Cause* IE in TS 38.331 [22] Sec 6.2.2 |  |
| 18134 | >>>Number of RRC connection resuming attempts | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.18.1 |
| 18141 | >List of successful RRC connection resuming causes | LIST |  | *0..<maxnoofcauses>* | TS 28.552 [28] Sec 5.1.1.18.2 |
| 18142 | >>Cause item | STRUCTURE |  |  |  |
| 18143 | >>>Cause | ELEMENT | TRUE | *Cause* IE in TS 38.331 [22] Sec 6.2.2 |  |
| 18144 | >>>Number of successful RRC connection resuming attempts | ELEMENT | FALSE |  | TS 28.552 [28] Sec 5.1.1.18.2 |
| 18151 | >List of causes for successful RRC connection resuming with fallback | LIST |  | *0..<maxnoofcauses>* | TS 28.552 [28] Sec 5.1.1.18.3 |
| 18152 | >>Cause item | STRUCTURE |  |  |  |
| 18153 | >>>Cause | ELEMENT | TRUE | *Cause* IE in TS 38.331 [22] Sec 6.2.2 |  |
| 18154 | >>>Number of successful RRC connection resuming attempts with fallback | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.18.3 |
| 18161 | >Number of RRC connection resuming processes followed by network release | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.18.4 |
| 18162 | >Number of RRC connection resuming processes followed by network suspension | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.18.5 |
| 18163 | >Mean number of RRC connections | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.4.1 |
| 18164 | >Maximum number of RRC connections | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.4.2 |
| 18165 | >Mean number of stored inactive RRC connections | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.4.3 |
| 18166 | >Maximum number of stored inactive RRC connections | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.4.4 |
| 18200 | QoS flow related measurements | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.13 |
| 18201 | >List of QoS levels | LIST |  | *0..<maxnoofflows>* | TS 28.552 [28] Sec 5.1.1.13 |
| 18202 | >>QoS level item | STRUCTURE |  |  |  |
| 18203 | >>>CHOICE QoS level | STRUCTURE |  |  |  |
| 18204 | >>>>5QI | ELEMENT | TRUE | *5QI* IE in TS 38.413 [11] Section 9.3.1.28 |  |
| 18205 | >>>>S-NSSAI | STRUCTURE |  |  | *S-NSSAI* IE in TS 38.473 [19] Section 9.3.1.38 |
| 18206 | >>>>>SST | ELEMENT | TRUE | *SST* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 18207 | >>>>>SD | ELEMENT | FALSE | *SD* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 18210 | >>>Number of QoS flows attempted to release | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.13.1.2 |
| 18211 | >>>In-session activity time | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.13.2.1 |
| 18212 | >>>Number of QoS flows attempted to setup | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.13.3.1 |
| 18213 | >>>Number of QoS flows successfully established | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.13.2.1 |
| 18214 | >>>Number of QoS flows attempted to modify | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.13.4.1 |
| 18215 | >>>Number of QoS flows successfully modified | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.13.4.2 |
| 18216 | >>>Number of QoS flows failed to modify | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.13.4.3 |
| 18250 | DRB related measurements | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.10 |
| 18251 | >List of QoS levels | LIST |  | *0..<maxnoofflows>* | TS 28.552 [28] Sec 5.1.1.10 |
| 18252 | >>QoS level item | STRUCTURE |  |  |  |
| 18253 | >>>CHOICE QoS level | STRUCTURE |  |  |  |
| 18254 | >>>>5QI | ELEMENT | TRUE | *5QI* IE in TS 38.413 [11] Section 9.3.1.28 |  |
| 18255 | >>>>S-NSSAI | STRUCTURE |  |  | *S-NSSAI* IE in TS 38.473 [19] Section 9.3.1.38 |
| 18256 | >>>>>SST | ELEMENT | TRUE | *SST* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 18257 | >>>>>SD | ELEMENT | FALSE | *SD* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 18258 | >>>Number of DRBs attempted to setup | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.10.1 |
| 18259 | >>>Number of DRBs successfully setup | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.10.2 |
| 18260 | >>>Number of released active DRBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.10.3 |
| 18261 | >>>In-session activity time for DRBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.10.4 |
| 18262 | >Total number of DRBs successfully setup aggregated across QoS levels | ELEMENT | FALSE | INTEGER |  |
| 18270 | PDU Session Management | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.5 |
| 18271 | >List of slices | LIST |  | *0..<maxnoofslices>* | TS 28.552 [28] Sec 5.1.1.18.5 |
| 18272 | >>Slice Item | STRUCTURE |  |  |  |
| 18273 | >>>S-NSSAI | STRUCTURE |  |  | *S-NSSAI* IE in TS 38.473 [19] Section 9.3.1.38 |
| 18274 | >>>>SST | ELEMENT | TRUE | *SST* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 18275 | >>>>SD | ELEMENT | FALSE | *SD* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 18276 | >>>Number of PDU sessions requested for setup | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.5.1 |
| 18277 | >>>Number of PDU sessions successfully setup | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.5.2 |
| 18278 | >>>Number of PDU sessions failed to setup | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.5.3 |
| 18301 | Inter-system mobility measurements between 5GS and EPS | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.6.3 |
| 18302 | >Number of requested HO preparations | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.3.1 |
| 18303 | >Number of successful HO preparations | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.3.2 |
| 18304 | >Number of failed HO preparations | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.3.3 |
| 18305 | >Number of requested resource allocations for HO | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.3.4 |
| 18306 | >Number of successful resource allocations for HO | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.3.5 |
| 18307 | >Number of failed resource allocations for HO | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.3.6 |
| 18308 | >Number of requested HO executions | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.3.7 |
| 18309 | >Number of successful HO executions | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.3.8 |
| 18310 | >Number of failed HO executions | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.6.3.9 |
| 18321 | >MRO measurements | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.25 |
| 18322 | >>Number of too early handovers | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.25.2 |
| 18323 | >>Number of too late handovers | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.25.2 |
| 18324 | >>Number of unnecessary handovers | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.25.3 |
| 18325 | >>Number of ping-pong handovers | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.25.4 |

#### 8.1.1.13 gNB CU-UP Measurements

The following RAN Parameters are associated with gNB CU-UP measurements.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 19001 | Packet delay measurements | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.3.3 and 5.1.1.1 |
| 19002 | >List of QoS levels | LIST |  |  | TS 28.552 [28] Sec 5.1.3.3 and 5.1.1.1 |
| 19003 | >>QoS level item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.3.3 and 5.1.1.1 |
| 19004 | >>>CHOICE QoS level | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.3.3 and 5.1.1.1 |
| 19005 | >>>>5QI | ELEMENT | TRUE | *5QI* IE in TS 38.413 [11] Section 9.3.1.28 |  |
| 19006 | >>>>S-NSSAI | STRUCTURE |  |  | *S-NSSAI* IE in TS 38.473 [19] Section 9.3.1.38 |
| 19007 | >>>>>SST | ELEMENT | TRUE | *SST* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 19008 | >>>>>SD | ELEMENT | FALSE | *SD* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 19009 | >>>PDCP re-ordering delay in the UL | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.1.5 |
| 19010 | >>>Distribution bins for DL packet delay | LIST |  | *0..<maxnoofbins>* | TS 28.552 [28] Sec 5.1.1.1.6 and 5.1.3.3.4 |
| 19011 | >>>>Distribution bin item | STRUCTURE |  |  |  |
| 19012 | >>>>>DL packet delay bin value | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.1.6 and 5.1.3.3.4 |
| 19013 | >>>>>Number of samples | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.1.6 and 5.1.3.3.4 |
| 19021 | >>>Distribution bins for UL packet delay | LIST |  |  | TS 28.552 [28] Sec 5.1.1.1.7 |
| 19022 | >>>>Distribution bin item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.1.7 |
| 19023 | >>>>>DL packet delay bin value | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.1.7 |
| 19024 | >>>>>Number of samples | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.1.7 |
| 19051 | >>>UL PDCP SDU Loss Rate | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.1.1 |
| 19052 | >>>UL F1-U Packet Loss Rate | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.1.2 |
| 19053 | >>>DL PDCP SDU Drop Rate | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.2.1 |
| 19054 | >>>Average delay DL | ELEMENT | FALSE | REAL | TS 28.552 [28] Sec 5.1.3.3.1 |
| 19055 | >>>Average delay DL on F1-U | ELEMENT | FALSE | REAL | TS 28.552 [28] Sec 5.1.3.3.2 |
| 19056 | >>>Distribution bins for DL packet delay on F1-U | LIST |  |  | TS 28.552 [28] Sec 5.1.3.3.5 |
| 19057 | >>>>Distribution bin item | STRUCTURE |  |  |  |
| 19058 | >>>>>DL packet delay bin value | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.3.5 |
| 19059 | >>>>>Number of samples | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.3.5 |
| 19071 | PDCP data volume Measurement | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.3.6 |
| 19072 | >List of QoS levels | LIST |  |  | TS 28.552 [28] Sec 5.1.3.6 |
| 19073 | >>QoS level item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.3.6 |
| 19074 | >>>CHOICE QoS level | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.3.6 |
| 19075 | >>>>5QI | ELEMENT | TRUE | *5QI* IE in TS 38.413 [11] Section 9.3.1.28 |  |
| 19076 | >>>>S-NSSAI | STRUCTURE |  |  | *S-NSSAI* IE in TS 38.473 [19] Section 9.3.1.38 |
| 19077 | >>>>>SST | ELEMENT | TRUE | *SST* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 19078 | >>>>>SD | ELEMENT | FALSE | *SD* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 19079 | >>>DL PDCP PDU Data Volume | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.6.1 |
| 19080 | >>>DL PDCP SDU Data Volume | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.6.2 |

#### 8.1.1.14 gNB DU Measurements

The following RAN Parameters are associated with gNB DU measurements.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 20001 | Packet delay measurements | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.3.3 and 5.1.1.1 |
| 20002 | >List of QoS levels | LIST |  |  | TS 28.552 [28] Sec 5.1.3.3 and 5.1.1.1 |
| 20003 | >>QoS level item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.3.3 and 5.1.1.1 |
| 20004 | >>>CHOICE QoS level | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.3.3 and 5.1.1.1 |
| 20005 | >>>>5QI | ELEMENT | TRUE | *5QI* IE in TS 38.413 [11] Section 9.3.1.28 |  |
| 20006 | >>>>S-NSSAI | STRUCTURE |  |  | *S-NSSAI* IE in TS 38.473 [19] Section 9.3.1.38 |
| 20007 | >>>>>SST | ELEMENT | TRUE | *SST* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 20008 | >>>>>SD | ELEMENT | FALSE | *SD* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 20009 | >>>Average delay DL air-interface | ELEMENT | FALSE | REAL | TS 28.552 [28] Sec 5.1.1.1 |
| 20010 | >>>Average delay UL on over-the-air interface | ELEMENT | FALSE | REAL | TS 28.552 [28] Sec 5.1.1.1 |
| 20011 | >>>Average RLC packet delay in the UL | ELEMENT | FALSE | REAL | TS 28.552 [28] Sec 5.1.1.1.4 |
| 20012 | >>>Distribution bins for DL air-interface delay | LIST |  |  | TS 28.552 [28] Sec 5.1.1.1.2 |
| 20013 | >>>>Distribution bin item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.1.2 |
| 20014 | >>>>>Bin value | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.1.2 |
| 20015 | >>>>>Number of samples | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.1.2 |
| 20018 | List of NR cells | LIST |  |  | Cell-specific measurements as in TS 28.552 [28] Sec 5.1.1.2 |
| 20019 | >NR Cell Item | STRUCTURE |  | 8.1.1.1 |  |
| 20020 | >>NR CGI | ELEMENT | TRUE | *NR CGI* IE in TS 38.423 [15] Section 9.2.2.7 |  |
| 20021 | >>Radio Resource Utilization | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.2 |
| 20022 | >>>DL Total PRB Usage | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.2.1 |
| 20023 | >>>UL Total PRB Usage | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.2.2 |
| 20024 | >>>Distribution bins for DL Total PRB Usage | LIST |  |  | TS 28.552 [28] Sec 5.1.1.2.3 |
| 20025 | >>>>Distribution bin item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.2.3 |
| 20026 | >>>>>Bin value | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.2.3 |
| 20027 | >>>>>Number of samples | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.2.3 |
| 20028 | >>>Distribution bins for UL Total PRB Usage | LIST |  |  | TS 28.552 [28] Sec 5.1.1.2.4 |
| 20029 | >>>>Distribution bin item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.2.4 |
| 20030 | >>>>>Bin value | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.2.4 |
| 20031 | >>>>>Number of samples | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.2.4 |
| 20032 | >>>List of QoS levels | LIST |  |  | TS 28.552 [28] Sec 5.1.1.2.5 |
| 20033 | >>>>QoS level item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.2.5 |
| 20034 | >>>>>CHOICE QoS level | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.2.5 |
| 20035 | >>>>>>5QI | ELEMENT | TRUE | *5QI* IE in TS 38.413 [11] Section 9.3.1.28 |  |
| 20036 | >>>>>>S-NSSAI | STRUCTURE |  |  | *S-NSSAI* IE in TS 38.473 [19] Section 9.3.1.38 |
| 20037 | >>>>>>>SST | ELEMENT | TRUE | *SST* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 20038 | >>>>>>>SD | ELEMENT | FALSE | *SD* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 20039 | >>>>>DL PRB used for data traffic | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.2.5 |
| 20040 | >>>>>UL PRB used for data traffic | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.2.5 |
| 20041 | >>>DL total available PRB | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.2.6 |
| 20042 | >>>UL total available PRB | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.2.8 |
| 20051 | UE Throughput Measurements | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.3 |
| 20052 | >List of QoS levels | LIST |  |  | TS 28.552 [28] Sec 5.1.1.3 |
| 20053 | >>QoS level item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.3 |
| 20054 | >>>CHOICE QoS level | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.3 |
| 20055 | >>>>5QI | ELEMENT | TRUE | *5QI* IE in TS 38.413 [11] Section 9.3.1.28 |  |
| 20056 | >>>>S-NSSAI | STRUCTURE |  |  | *S-NSSAI* IE in TS 38.473 [19] Section 9.3.1.38 |
| 20057 | >>>>>SST | ELEMENT | TRUE | *SST* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 20058 | >>>>>SD | ELEMENT | FALSE | *SD* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 20059 | >>Average DL UE throughput | ELEMENT | FALSE | REAL | TS 28.552 [28] Sec 5.1.1.3.1 |
| 20060 | >>Average UL UE throughput | ELEMENT | FALSE | REAL | TS 28.552 [28] Sec Sec 5.1.1.3.3 |
| 20061 | >>Percentage of unrestricted DL UE throughput | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec Sec 5.1.1.3.5 |
| 20062 | >>Percentage of unrestricted UL UE throughput | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec Sec 5.1.1.3.6 |
| 20063 | >>Distribution bins for DL UE throughput | LIST |  |  | TS 28.552 [28] Sec 5.1.1.3.2 |
| 20064 | >>>Distribution bin item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.3.2 |
| 20065 | >>>>Bin value | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.3.2 |
| 20066 | >>>>Number of samples | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.3.2 |
| 20067 | >>Distribution bins for UL UE throughput | LIST |  |  | TS 28.552 [28] Sec 5.1.1.3.4 |
| 20068 | >>>Distribution bin item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.3.4 |
| 20069 | >>>>Bin value | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.3.4 |
| 20070 | >>>>Number of samples | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.3.4 |
| 20098 | List of NR Cells | LIST |  |  | Cell-specific measurements as in TS 28.552 [28] Sec 5.1.1.7 |
| 20099 | >NR Cell Item | STRUCTURE |  | 8.1.1.1 |  |
| 20100 | >>NR CGI | ELEMENT | TRUE | *NR CGI* IE in TS 38.423 [15] Section 9.2.2.7 |  |
| 20101 | >>TB-related Measurements | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.7 |
| 20102 | >>>DL initial TBs | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.7 |
| 20103 | >>>>Total number of DL initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.1 |
| 20104 | >>>>Total number of DL QPSK initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.1 |
| 20105 | >>>>Total number of DL 16QAM initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.1 |
| 20106 | >>>>Total number of DL 64QAM initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.1 |
| 20107 | >>>UL initial TBs | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.7.6 |
| 20108 | >>>>Total number of UL initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.6 |
| 20109 | >>>>Total number of UL QPSK initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.6 |
| 20110 | >>>>Total number of UL 16QAM initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.6 |
| 20111 | >>>>Total number of UL 64QAM initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.6 |
| 20121 | >>>Initial error number of DL TBs | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.7.2 |
| 20122 | >>>>Error number of DL initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.2 |
| 20123 | >>>>Error number of DL QPSK initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.2 |
| 20124 | >>>>Error number of DL 16QAM initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.2 |
| 20125 | >>>>Error number of DL 64QAM initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.2 |
| 20126 | >>>Initial error number of UL TBs | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.7.7 |
| 20127 | >>>>Error number of UL initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.7 |
| 20128 | >>>>Error number of UL QPSK initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.7 |
| 20129 | >>>>Error number of UL 16QAM initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.7 |
| 20130 | >>>>Error number of UL 64QAM initial TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.7 |
| 20131 | >>>DL total TBs | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.7.3 |
| 20132 | >>>>Total number of DL TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.3 |
| 20133 | >>>>Total number of DL QPSK TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.3 |
| 20134 | >>>>Total number of DL 16QAM TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.3 |
| 20135 | >>>>Total number of DL 64QAM TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.3 |
| 20136 | >>>UL total TBs | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.7.8 |
| 20137 | >>>>Total number of UL TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.8 |
| 20138 | >>>>Total number of UL QPSK TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.8 |
| 20139 | >>>>Total number of UL 16QAM TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.8 |
| 20140 | >>>>Total number of UL 64QAM TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.8 |
| 20141 | >>>Total error number of DL TBs | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.7.3 |
| 20142 | >>>>Total error number of DL TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.3 |
| 20143 | >>>>Total error number of DL QPSK TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.3 |
| 20144 | >>>>Total error number of DL 16QAM TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.3 |
| 20145 | >>>>Total error number of DL 64QAM TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.3 |
| 20146 | >>>Total error number of UL TBs | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.7.9 |
| 20147 | >>>>Total error number of UL TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.9 |
| 20148 | >>>>Total error number of UL QPSK TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.9 |
| 20149 | >>>>Total error number of UL 16QAM TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.9 |
| 20150 | >>>>Total error number of UL 64QAM TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.9 |
| 20151 | >>>Residual error number of DL TBs | STRUCTURE |  |  | TS 28.552 [28] Sec |
| 20152 | >>>>Residual error number of DL TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.5 |
| 20153 | >>>>Residual error number of DL QPSK TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.5 |
| 20154 | >>>>Residual error number of DL 16QAM TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.5 |
| 20155 | >>>>Residual error number of DL 64QAM TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.5 |
| 20156 | >>>Residual error number of UL TBs | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.7.10 |
| 20157 | >>>>Residual error number of UL TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.10 |
| 20158 | >>>>Residual error number of UL QPSK TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.10 |
| 20159 | >>>>Total error number of UL 16QAM TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.10 |
| 20160 | >>>>Total error number of UL 64QAM TBs | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.7.10 |
| 20201 | >>CQI-related measurements | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.11 |
| 20202 | >>>Distribution bins of CQI values | LIST |  |  | TS 28.552 [28] Sec 5.1.1.11 |
| 20203 | >>>>Distribution bin item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.11 |
| 20204 | >>>>>Bin value | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.11 |
| 20205 | >>>>>Number of samples | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.11 |
| 20206 | >>MCS-related measurements | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.12 |
| 20207 | >>>Distribution bins of PDSCH MCS values | LIST |  |  | TS 28.552 [28] Sec 5.1.1.12.1 |
| 20208 | >>>>Distribution bin item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.12.1 |
| 20209 | >>>>>Bin value | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.12.1 |
| 20210 | >>>>>Number of samples | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.12.1 |
| 20211 | >>>Distribution bins of PUSCH MCS values | LIST |  |  | TS 28.552 [28] Sec 5.1.1.12.2 |
| 20212 | >>>>Distribution bin item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.12.2 |
| 20213 | >>>>>Bin value | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.12.2 |
| 20214 | >>>>>Number of samples | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.12.2 |
| 20251 | >>Number of active UE measurements | STRUCTURE |  | INTEGER | TS 28.552 [28] Sec 5.1.1.23 |
| 20252 | >>>List of QoS levels | LIST |  |  | TS 28.552 [28] Sec 5.1.1.23 |
| 20253 | >>>>QoS level item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.23 |
| 20254 | >>>>>CHOICE QoS level | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.1.23 |
| 20255 | >>>>>>5QI | ELEMENT | TRUE | *5QI* IE in TS 38.413 [11] Section 9.3.1.28 |  |
| 20256 | >>>>>>S-NSSAI | STRUCTURE |  |  | *S-NSSAI* IE in TS 38.473 [19] Section 9.3.1.38 |
| 20257 | >>>>>>>SST | ELEMENT | TRUE | *SST* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 20258 | >>>>>>>SD | ELEMENT | FALSE | *SD* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 20259 | >>>>>Number of active UEs in the DL | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.23.1 |
| 20260 | >>>>>Maximum number of active UEs in the DL | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.23.2 |
| 20261 | >>>>>Number of active UEs in the UL | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.23.3 |
| 20262 | >>>>>Maximum number of active UEs in the UL | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.23.4 |
| 20271 | Packet level measurements | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.3 |
| 20272 | >List of QoS levels | LIST |  |  | TS 28.552 [28] Sec 5.1.3 |
| 20273 | >>QoS level item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.3 |
| 20274 | >>>CHOICE QoS level | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.3 |
| 20275 | >>>>5QI | ELEMENT | TRUE | *5QI* IE in TS 38.413 [11] Section 9.3.1.28 |  |
| 20276 | >>>>S-NSSAI | STRUCTURE |  |  | *S-NSSAI* IE in TS 38.473 [19] Section 9.3.1.38 |
| 20277 | >>>>>SST | ELEMENT | TRUE | *SST* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 20278 | >>>>>SD | ELEMENT | FALSE | *SD* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 20279 | >>>DL F1-U Packet Loss Rate | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.1.3 |
| 20280 | >>>DL RLC SDU Packet Drop Rate | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.2.2 |
| 20281 | >>>Average delay DL in gNB-DU | ELEMENT | FALSE | REAL | TS 28.552 [28] Sec 5.1.3.3.3 |
| 20282 | >>>Distribution bins of DL delay | LIST |  |  | TS 28.552 [28] Sec 5.1.3.3.6 |
| 20283 | >>>>Distribution bin item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.3.3.6 |
| 20284 | >>>>>Bin value | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.3.6 |
| 20285 | >>>>>Number of samples | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.1.3.6 |
| 20286 | >>>Average IP latency DL | ELEMENT | FALSE | REAL | TS 28.552 [28] Sec 5.1.3.4.2 |
| 20287 | >>>Distribution bins of DL IP latency | LIST |  |  | TS 28.552 [28] Sec 5.1.3.4.3 |
| 20288 | >>>>Distribution bin item | STRUCTURE |  |  | TS 28.552 [28] Sec 5.1.3.4.3 |
| 20289 | >>>>>Bin value | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.4.3 |
| 20290 | >>>>>Number of samples | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.4.3 |
| 20291 | Number of UE Context release requested from gNB-DU | ELEMENT | FALSE | INTEGER | TS 28.552 [28] Sec 5.1.3.5.1 |

#### 8.1.1.15 gNB Measurements

The following RAN Parameters are associated with the gNB measurements.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 20501 | gNB CU-CP Measurements | STRUCTURE |  | 8.1.1.12 | For both UE- and E2 node level measurements |
| 20502 | gNB CU-UP Measurements | STRUCTURE |  | 8.1.1.13 | For both UE- and E2 node level measurements |
| 20503 | gNB DU Measurements | STRUCTURE |  | 8.1.1.14 | For both UE- and E2 node level measurements |

#### 8.1.1.16 PDU Session

The following RAN Parameters are associated with PDU session.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 21001 | S-NSSAI | STRUCTURE |  |  | *S-NSSAI* IE in TS 38.473 [19] Section 9.3.1.38 |
| 21002 | >SST | ELEMENT | TRUE | *SST* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 21003 | >SD | ELEMENT | FALSE | *SD* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 21004 | PDU Session Aggregate Maximum Bit Rate | STRUCTURE |  |  | *PDU Session Aggregate Maximum Bit Rate* IE in TS 38.413 [11] Section 9.3.1.102 |
| 21005 | >PDU Session Aggregate Maximum Bit Rate Downlink | ELEMENT | FALSE | *PDU Session Aggregate Maximum Bit Rate Downlink* IE in TS 38.413 [11] Section 9.3.1.102 |  |
| 21006 | >PDU Session Aggregate Maximum Bit Rate Uplink | ELEMENT | FALSE | *PDU Session Aggregate Maximum Bit Rate Uplink* IE in TS 38.413 [11] Section 9.3.1.102 |  |
| 21008 | >Data Forwarding Not Possible | ELEMENT | FALSE | *Data Forwarding Not Possible* IE in TS 38.413 [11] Section 9.3.1.63 |  |
| 21009 | >PDU Session Type | ELEMENT | FALSE | *PDU Session Type* IE in TS 38.413 [11] Section 9.3.1.52 |  |
| 21010 | >Network Instance | ELEMENT | FALSE | *Network Instance* IE in TS 38.413 [11] Section 9.3.1.113 |  |
| 21011 | >Direct Forwarding Path Availability | ELEMENT | FALSE | *Direct Forwarding Path Availability* IE in TS 38.413 [11] Section 9.3.1.120 |  |
| 21012 | >Redundant Common Network Instance | ELEMENT | FALSE | *Redundant Common Network Instance* IE in TS 38.413 [11] Section 9.3.1.120 |  |
| 21013 | >Redundant PDU Session Information | ELEMENT | FALSE | *Redundant PDU Session Information* IE in TS 38.413 [11] Section 9.3.1.136 |  |

#### 8.1.1.17 UE Context Information

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | Semantics Description |
| 21501 | Master Node | STRUCTURE |  | 8.1.1.11 |  |
| 21502 | >gNB Measurements | STRUCTURE |  | 8.1.1.15 |  |
| 21503 | CHOICE Primary Cell of MCG | STRUCTURE |  |  |  |
| 21504 | >NR Cell | STRUCTURE |  | 8.1.1.1 | For NR SpCell |
| 21505 | >E-UTRA Cell | STRUCTURE |  | 8.1.1.2 | For E-UTRA PCell |
| 21506 | List of Secondary Cells of MCG | LIST |  |  | *Scell To Be Setup List* IE in TS 38.473 [19] clause 9.2.2.1 |
| 21507 | >SCell Item | STRUCTURE |  |  | *Scell To Be Setup Item* IEs IE in TS 38.473 [19] clause 9.2.2.1 |
| 21508 | >>CHOICE SCell | STRUCTURE |  |  |  |
| 21509 | >>>NR Cell | STRUCTURE |  | 8.1.1.1 | For NR SCell |
| 21510 | >>>E-UTRA Cell | STRUCTURE |  | 8.1.1.2 | For E-UTRA SCell |
| 21511 | Secondary Node | STRUCTURE |  | 8.1.1.11 |  |
| 21512 | >gNB Measurements | STRUCTURE |  | 8.1.1.15 |  |
| 21513 | CHOICE Primary Cell of SCG | STRUCTURE |  |  | *PSCell* IE as defined in TS 38.331 [22] or the structure defined in TS 38.473 [19] clause 9.2.2.1 |
| 21514 | >NR Cell | STRUCTURE |  | 8.1.1.1 |  |
| 21515 | >E-UTRA Cell | STRUCTURE |  | 8.1.1.2 |  |
| 21516 | List of Secondary Cells of SCG | LIST |  |  | *Scell To Be Setup List* IE in TS 38.473 [19] clause 9.2.2.1 |
| 21517 | >SCell Item | STRUCTURE |  |  | *Scell To Be Setup Item* IEs IE in TS 38.473 [19] clause 9.2.2.1 |
| 21518 | >>CHOICE SCell | STRUCTURE |  |  |  |
| 21519 | >>>NR Cell | STRUCTURE |  | 8.1.1.1 |  |
| 21520 | >>>E-UTRA Cell | STRUCTURE |  | 8.1.1.2 |  |
| 21521 | List of PDU Sessions | LIST |  |  | *PDU Session Resources To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 |
| 21522 | >PDU Session Item | STRUCTURE |  |  | *PDU Session Resources To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 |
| 21543 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.413 [11] Section 9.3.1.50 |  |
| 21523 | >>PDU Session | STRUCTURE |  | 8.1.1.16 |  |
| 21524 | >>List of DRBs | LIST |  |  | *DRB to Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 21525 | >>>DRB Item | STRUCTURE |  |  |  |
| 21546 | >>>>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.463 [21] clause 9.3.1.16 |  |
| 21547 | >>>>DRB | STRUCTURE |  | 8.1.1.5 |  |
| 21526 | >>>>List of QoS flows mapped to DRB | LIST |  |  | *QoS Flows Information To Be Setup* IE in TS 38.463 [21] Section 9.3.3.2 |
| 21527 | >>>>>QoS Flow Item | STRUCTURE |  |  |  |
| 21548 | >>>>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.413 [11] Section 9.3.1.51 |  |
| 21549 | >>>>>>QoS Flow | STRUCTURE |  | 8.1.1.6 |  |
| 21528 | List of Neighbor cells | LIST |  |  | *measResultNeighCells* IE in TS 38.331 [22] | |
| 21529 | >Neighbor Cell Item | STRUCTURE |  |  |  | |
| 21530 | >>CHOICE Neighbor Cell | STRUCTURE |  |  |  | |
| 21531 | >>>NR Cell | STRUCTURE |  | 8.1.1.1 | *MeasResultNR* IE in TS 38.331 [22] | |
| 21532 | >>>E-UTRA Cell | STRUCTURE |  | 8.1.1.2 | *MeasResultEUTRA* IE in TS 38.331 [22] | |

#### 8.1.1.18 eNB Measurements

*Editor’s Note: FFS*

### 8.1.2 RAN Parameters for Call Process Breakpoint

#### 8.1.2.0 Call process type IDs

The RAN Parameters for the Event Trigger style 2 are defined based on the following call process type.

|  |  |  |
| --- | --- | --- |
| **Call Process Type ID** | **Call Process Type** | **RAN Parameters** |
| 1 | UE Context Management | Defined in Section 8.1.2.1 |
| 2 | Bearer Context Management | Defined in Section 8.1.2.2 |
| 3 | Mobility Management | Defined in Section 8.1.2.3 |
| 4 | Multi-RAT Dual Connectivity Management | Defined in Section 8.1.2.4 |
| 5 | Radio Resource Control Management | Defined in Section 8.1.2.5 |
| 6 | PDU Session Management | Defined in Section 8.1.2.6 |

#### 8.1.2.1 UE Context Management

The RAN Parameters for the call process type of “UE Context Management” are defined as follows.

##### 8.1.2.1.1 UE Context Setup

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter xID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | ***Semantics Description*** |
| 25001 | Primary Cell ID | STRUCTURE |  |  | This is for the primary serving cell of the UE. The structuring of this parameter is based on *Target Cell Global ID* IE in TS 38.423 [15] clause 9.2.3.25 |
| 25002 | >CHOICE *Primary Cell* | STRUCTURE |  |  | The primary cell could either be an NR primary cell or an LTE primary cell. The structuring is based on*Target Cell* IE in TS 38.423 [15] clause 9.2.3.25 |
| 25003 | >>NR SpCell | STRUCTURE |  | 8.1.1.1 | *NR Cell* IE in TS 38.423 [15] clause 9.2.3.25 or *SpCell ID* IE in TS 38.473 [19] clause 9.2.2.1 |
| 25063 | >>E-UTRA PCell | STRUCTURE |  | 8.1.1.2 | *E-UTRA Cell* IE in TS 38.423 [15] clause 9.2.3.25 |
| 25004 | List of secondary cells to be setup | LIST |  |  | *Scell To Be Setup List* IE in TS 38.473 [19] clause 9.2.2.1 |
| 25005 | >Secondary cell to be setup Item | STRUCTURE |  |  | *Scell To Be Setup Item* IEs IE in TS 38.473 [19] clause 9.2.2.1 |
| 25006 | >>CHOICE Secondary cell | STRUCTURE |  |  | *Scell To Be Setup Item* IEs IE in TS 38.473 [19] clause 9.2.2.1 |
| 25007 | >>>NR SCell | STRUCTURE |  | 8.1.1.1 |  |
| 25008 | >>>E-UTRA SCell | STRUCTURE |  | 8.1.1.2 |  |
| 25009 | >>>Scell UL Configured | ELEMENT | FALSE | *Cell UL Configured* IE in TS 38.473 [19] clause 9.3.1.33 |  |
| 25010 | Number of secondary cells to be setup | ELEMENT | FALSE | INTEGER (1..32) | Count of list of secondary cells to be setup |
| 25011 | List of DRBs for setup | LIST |  |  | *DRB to Be Setup List* IE in TS 38.473 [19] clause 9.2.2.1 |
| 25012 | >DRB item for setup | STRUCTURE |  |  | *DRB to Be Setup Item* IE in TS 38.473 [19] clause 9.2.2.1 |
| 25033 | >>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.463 [21] clause 9.3.1.16 |  |
| 25034 | >>CHOICE *DRB Type* | STRUCTURE |  |  | The individual DRB could either be an NG-RAN DRB or a E-UTRA DRB |
| 25035 | >>>NG-RAN DRB | STRUCTURE |  | 8.1.1.5 |  |
| 25036 | >>>E-UTRA DRB | STRUCTURE |  | 8.1.1.9 |  |
| 25013 | >List of QoS flows for setup | LIST |  |  | This is the list of QoS flows multiplexed to an NG-RAN DRB. The structuring is based on *QoS Flow List* IE in TS 38.463 [21] Section 9.3.1.12 |
| 25014 | >>QoS flow Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.12 |
| 25045 | >>>QoS flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.463 [21] Section 9.3.1.12 |  |
| 25046 | >>>QoS flow | STRUCTURE |  | 8.1.1.6 |  |
| 25015 | List of PDU sessions for setup | LIST |  |  | ***PDU Session Resource Setup Request List* IE in TS 38.413 Section 9.2.1.1** |
| 25016 | >PDU Session Item | STRUCTURE |  |  | *PDU Session Resource Setup Item* IE in TS 38.413 Section 9.2.1.1 |
| 25057 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.413 [11] Section 9.3.1.50 |  |
| 25058 | >>PDU Session | STRUCTURE |  | 8.1.1.16 |  |
| 25017 | >>List of QoS flows for setup | LIST |  |  | *QoS Flow Setup Request Item* IE in TS 38.413 Section 9.3.4.1 |
| 25018 | >>>QoS flow Item | STRUCTURE |  |  | *QoS Flow Setup Request Item* IE in TS 38.413 Section 9.3.4.1 |
| 25019 | >>>>QoS flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.413 [11] Section 9.3.1.51 |  |
| 25020 | >>>>QoS flow | STRUCTURE |  | 8.1.1.6 |  |
| 25021 | Number of DRBs for setup | ELEMENT | FALSE | INTEGER (0..64) | Count of list of DRBs for setup |
| 25022 | UE Aggregate Maximum Bit Rate | STRUCTURE |  |  | *UE Aggregate Maximum Bit Rate* IE in TS 36.423 [17] Section 9.2.12 |
| 25023 | >UE Aggregate Maximum Bit Rate Downlink | ELEMENT | FALSE | *UE Aggregate Maximum Bit Rate Downlink* IE in TS 36.423 [17] clause 9.2.12 |  |
| 25024 | >UE Aggregate Maximum Bit Rate Uplink | ELEMENT | FALSE | *UE Aggregate Maximum Bit Rate Uplink* IE in TS 36.423 [17] clause 9.2.12 |  |

##### 8.1.2.1.2 UE Context Modification

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | ***Semantics Description*** |
| 25101 | Primary Cell ID | | STRUCTURE |  |  | This is for the primary serving cell of the UE. The structuring of this parameter is based on *Target Cell Global ID* IE in TS 38.423 [15] clause 9.2.3.25 |
| 25102 | >CHOICE *Primary Cell* | | STRUCTURE |  |  | The primary cell could either be an NR primary cell or an LTE primary cell. The structuring is based on *Target Cell* IE in TS 38.423 [15] clause 9.2.3.25 |
| 25103 | >>NR SpCell | | STRUCTURE |  | 8.1.1.1 | *NR* IE in TS 38.423 [15] clause 9.2.3.25 or *SpCell ID* IE in TS 38.473 [19] clause 9.2.2.1 |
| 25104 | >>E-UTRA PCell | | STRUCTURE |  | 8.1.1.2 | *E-UTRA* IE in TS 38.423 [15] clause 9.2.3.25 |
| 25105 | List of secondary cells to be setup | | LIST |  |  | *Scell To Be Setup List* IE in TS 38.473 [19] clause 9.2.2.1 |
| 25106 | >Secondary cell to be setup Item | | STRUCTURE |  |  | *Scell To Be Setup Item* IEs IE in TS 38.473 [19] clause 9.2.2.1 |
| 25107 | >>CHOICE Secondary cell | | STRUCTURE |  |  | *Scell To Be Setup Item* IEs IE in TS 38.473 [19] clause 9.2.2.1 |
| 25108 | >>>NR SCell | | STRUCTURE |  | 8.1.1.1 |  |
| 25109 | >>>E-UTRA SCell | | STRUCTURE |  | 8.1.1.2 |  |
| 25110 | >>>Scell UL Configured | | ELEMENT | FALSE | *Cell UL Configured* IEin TS 38.473 [19] [Q] clause 9.3.1.33 |  |
| 25111 | Number of secondary cells to be setup | | ELEMENT | FALSE | INTEGER (1..32) | Count of list of secondary cells to be setup |
| 25112 | List of Scells to be removed | | LIST |  |  | *SCell To Be Removed List* IE in TS 38.473 [19] clause 9.2.2.7 |
| 25113 | >Scell to be removed Item | | STRUCTURE |  |  | *SCell to Be Removed Item IEs* IE in TS 38.473 [19] clause 9.2.2.7 |
| 25114 | >>CHOICE Secondary cell | | STRUCTURE |  |  | A UE can have either NR Cells as secondary cells or E-UTRA cells as secondary cells. |
| 25115 | >>>NR SCell | | STRUCTURE |  | 8.1.1.1 |  |
| 25116 | >>>E-UTRA SCell | | STRUCTURE |  | 8.1.1.2 |  |
| 25117 | >>>Scell UL Configured | | ELEMENT | FALSE | *Cell UL Configured* IEin TS 38.473 [19] [Q] clause 9.3.1.33 |  |
| 25118 | Number of secondary cells to be removed | | ELEMENT | FALSE | INTEGER (1..32) | Count of list of secondary cells to be removed |
| 25119 | List of DRBs for setup | | LIST |  |  | DRB to Be Setup List IE in TS 38.473 [19] clause 9.2.2.1 |
| 25120 | >DRB item for setup | | STRUCTURE |  |  | DRB to Be Setup Item IE in TS 38.473 [19] clause 9.2.2.1 |
| 25161 | >>DRB ID | | ELEMENT | TRUE | *DRB ID* IE in TS 38.463 [21] clause 9.3.1.16 |  |
| 25162 | >>CHOICE *DRB Type* | | STRUCTURE |  |  | DRB could either be an NG-RAN DRB or a E-UTRA DRB |
| 25163 | >>>NG-RAN DRB | | STRUCTURE |  | 8.1.1.5 |  |
| 25164 | >>>E-UTRA DRB | | STRUCTURE |  | 8.1.1.9 |  |
| 25121 | >>List of QoS flows for setup | | LIST |  |  | This is the list of QoS flows multiplexed to an NG-RAN DRB for setup. The structuring is based on *QoS Flow List* IE in TS 38.463 [21] Section 9.3.1.12 |
| 25122 | >>>QoS flow Item | | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.12 |
| 25166 | >>>>QoS flow Identifier | | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.463 [21] Section 9.3.1.12 |  |
| 25167 | >>>>QoS flow | | STRUCTURE |  | 8.1.1.6 |  |
| 25123 | List of PDU sessions for setup | | LIST |  |  | *PDU Session Resource Setup Request List* IE in TS 38.413 Section 9.2.1.1 |
| 25124 | >PDU Session Item | | STRUCTURE |  |  | *PDU Session Resource Setup Item* IE in TS 38.413 Section 9.2.1.1 |
| 25175 | >>PDU Session ID | | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.413 [11] Section 9.3.1.50 |  |
| 25176 | >>PDU Session | | STRUCTURE |  | 8.1.1.16 |  |
| 25125 | >>List of QoS flows for setup | | LIST |  |  | *QoS Flow Setup Request Item* IE in TS 38.413 Section 9.3.4.1 |
| 25126 | >>>QoS flow Item | | STRUCTURE |  |  | *QoS Flow Setup Request Item* IE in TS 38.413 Section 9.3.4.1 |
| 25177 | >>>>QoS flow Identifier | | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.413 [11] Section 9.3.1.51 |  |
| 25178 | >>>>QoS flow | | STRUCTURE |  | 8.1.1.6 |  |
| 25127 | List of DRBs to be modified | | LIST |  |  | *DRB to Be Setup List* IE in TS 38.473 [19] clause 9.2.2.1 |
| 25128 | >DRB item for modification | | STRUCTURE |  | 8.1.1.5 | *DRB to Be Setup Item* IE in TS 38.473 [19] clause 9.2.2.1 |
| 25129 | >>List of QoS flows remapped | | LIST |  |  | This is the list of QoS flows remapped to an NG-RAN DRB. The structuring is based on *QoS Flow List* IE in TS 38.463 [21] Section 9.3.1.12 |
| 25130 | >>>QoS flow Item | | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.12 |
| 25181 | >>>>QoS flow Identifier | | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.463 [12] Section 9.3.1.12 |  |
| 25182 | >>>>QoS flow | | STRUCTURE |  | 8.1.1.6 |  |
| 25131 | List of PDU sessions for modification | | LIST |  |  | For modification of PDU sessions. The structuring is based on *PDU Session Resource Modify Request List* IE in TS 38.413 Section 9.2.1.5 |
| 25132 | >PDU Session Item | | STRUCTURE |  |  | *PDU Session Resource Modify Request Item* IE in TS 38.413 Section 9.2.1.5 |
| 25183 | >>PDU Session ID | | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.413 [11] Section 9.3.1.50 |  |
| 25184 | >>PDU Session | | STRUCTURE |  | 8.1.1.16 |  |
| 25133 | >>List of QoS flows remapped | | LIST |  |  | Modified list of QoS flows within the PDU Session. Structuring is based on *QoS Flow Add or Modify Request List* IE in TS 38,413 Section 9.3.4.3 |
| 25134 | >>>QoS flow Item | | STRUCTURE |  |  | *QoS Flow Add or Modify Request Item* IE in TS 38.413 Section 9.3.4.3 |
| 25185 | >>>>QoS flow identifier | | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.413 [11] Section 9.3.1.51 |  |
| 25186 | >>>>QoS flow | | STRUCTURE |  | 8.1.1.6 |  |
| 25135 | Number of DRBs to be modified | | ELEMENT | FALSE |  | Count of list of DRBs to be modified |
| 25136 | List of DRBs to be released | | LIST |  |  | *DRB To Be Released List* IE in TS 38.473 [19] Section 9.2.2.7 |
| 25137 | >DRB item for release | | STRUCTURE |  |  | *DRB To Be Released Item* IE in TS 38.473 [19] Section 9.2.2.7 |
| 25188 | >>DRB ID | | ELEMENT | TRUE | *DRB ID* IE in TS 38.463 [21] clause 9.3.1.16 |  |
| 25189 | >>CHOICE *DRB Type* | | STRUCTURE |  |  | DRB could either be an NG-RAN DRB or a E-UTRA DRB |
| 25190 | >>>NG-RAN DRB | | STRUCTURE |  | 8.1.1.5 |  |
| 25191 | >>>E-UTRA DRB | | STRUCTURE |  | 8.1.1.9 |  |
| 25138 | Number of DRBs to be released | | ELEMENT | FALSE |  | Count of list of DRBs to be released |
| 25139 | UE Aggregate Maximum Bit Rate | | STRUCTURE |  |  | *UE Aggregate Maximum Bit Rate* IE in TS 36.423 [17] Section 9.2.12 |
| 25140 | >UE Aggregate Maximum Bit Rate Downlink | | ELEMENT | FALSE | *UE Aggregate Maximum Bit Rate Downlink* IE in TS 36.423 [17] clause 9.2.12 |  |
| 25141 | >UE Aggregate Maximum Bit Rate Uplink | | ELEMENT | FALSE | *UE Aggregate Maximum Bit Rate Uplink* IE in TS 36.423 [17] clause 9.2.12 |  |
| 25151 | | Target Cell ID | STRUCTURE |  |  | This is for the target cell of the UE for HO. The structuring of this parameter is based on *Target Cell Global ID* IE in TS 38.423 [15] clause 9.2.3.25 |
| 25152 | | >CHOICE *Target Cell* | STRUCTURE |  |  | The target cell could either be a target NR primary cell or a target LTE primary cell. The structuring is based on *Target Cell* IE in TS 38.423 [15] clause 9.2.3.25 |
| 25153 | | >>Target NR SpCell | STRUCTURE |  | 8.1.1.1 | *NR* IE in TS 38.423 [15] clause 9.2.3.25 |
| 25154 | | >>Target E-UTRA PCell | STRUCTURE |  | 8.1.1.2 | *E-UTRA* IE in TS 38.423 [15] clause 9.2.3.25 |

##### 8.1.2.1.3 UE Context Release

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | ***Semantics Description*** |
| 25201 | List of candidate cells to be cancelled | LIST |  |  | *Candidate Cells To Be Cancelled List* IE in TS 38.473 [19] Section 9.2.2.4 |
| 25202 | >Candidate cell to be cancelled Item | STRUCTURE |  |  | *Candidate Cell to be Cancelled Item* IE in TS 38.473 [19] Section 9.2.2.4 |
| 25203 | >>CHOICE Candidate cell | STRUCTURE |  |  | *Candidate Cell to be Cancelled Item* IE in TS 38.473 [19] Section 9.2.2.4 |
| 25204 | >>>NR SCell | STRUCTURE |  | 8.1.1.1 |  |
| 25205 | >>>E-UTRA SCell | STRUCTURE |  | 8.1.1.2 |  |

#### 8.1.2.2 Bearer Context Management

The RAN Parameters for the call process type of “Bearer Context Management” are defined as follows.

##### 8.1.2.2.1 Bearer Context Setup

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 26101 | DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.463 [21] clause 9.3.1.16 |  |
| 26102 | CHOICE *DRB Type* | STRUCTURE |  |  | DRB could either be an NG-RAN DRB or a E-UTRA DRB |
| 26103 | >NG-RAN DRB | STRUCTURE |  | 8.1.1.5 |  |
| 26104 | >E-UTRA DRB | STRUCTURE |  | 8.1.1.9 |  |
| 26105 | List of QoS Flows to be setup in DRB | LIST |  |  | This is the list of QoS flows multiplexed to an NG-RAN DRB for setup. The structuring is based on *QoS Flow List* IE in TS 38.463 [21] Section 9.3.1.12 |
| 26106 | >QoS Flow Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.463 [21] clause 9.3.1.12 |
| 26107 | >>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.463 [21] clause 9.3.1.24 |  |
| 26108 | >>QoS Flow | STRUCTURE |  | 8.1.1.6 |  |
| 26109 | Count of list of QoS Flows to be setup in DRB | ELEMENT | FALSE | INTEGER (0..64) |  |
| 26110 | Cell Group List to Add | STRUCTURE |  |  | *CellGroupList* IE in TS 38.463 [21] Section 9.3.1.11 |
| 26111 | >Cell Group Item | STRUCTURE |  |  |  |
| 26122 | >>Cell Group ID | ELEMENT | TRUE | *cellGroup* IE in TS 38.331 [22] Section 6 |  |
| 26123 | >>Cell Group | STRUCTURE |  | 8.1.1.7 |  |
| 26112 | Logical Channel ID | ELEMENT | FALSE | *LogicalChannelIdentity* IE in TS 38.331 [22] clause 6 |  |
| 26113 | Channel Access Priority | ELEMENT | FALSE | *channelAccessPriority* IE in TS 38.331 [22] |  |
| 26114 | L2 Bearer State Information | STRUCTURE |  | 8.1.1.8 |  |
| 26115 | Count of cell group list to be added | ELEMENT | FALSE | INTEGER (0..4) |  |

##### 8.1.2.2.2 Bearer Context Modification

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | | **RAN Parameter Definition** | | **Semantics Description** |
| 26201 | DRB ID | ELEMENT | TRUE | | *DRB ID* IE in TS 38.463 [21] clause 9.3.1.16 | |  |
| 26202 | CHOICE *DRB Type* | STRUCTURE |  | |  | | DRB could either be an NG-RAN DRB or a E-UTRA DRB |
| 26203 | >NG-RAN DRB | STRUCTURE |  | | 8.1.1.1 | |  |
| 26204 | >E-UTRA DRB | STRUCTURE |  | | 8.1.1.2 | |  |
| 26205 | Logical Channel ID | ELEMENT | TRUE | | *LogicalChannelIdentity* IE in TS 38.331 [22] clause 6 | |  |
| 26206 | CHOICE RLC-Config | STRUCTURE |  | |  | | *RLC-Config* IE in TS 38.331 [22] |
| 26207 | >AM | STRUCTURE | |  | |  | *am* IE in TS 38.331 [22] |
| 26208 | >>UL AM RLC | STRUCTURE | |  | |  | *ul-AM-RLC* IE in TS 38.331 [22] |
| 26209 | >>>Poll Retransmit | ELEMENT | | FALSE | | *t-PollRetransmit* IE in TS 38.331 [22] |  |
| 26210 | >>>Max Retransmission Threshold | ELEMENT | | FALSE | | *maxRetxThreshold* IE in TS 38.331 [22] |  |
| 26211 | >>>Poll PDU | ELEMENT | | FALSE | | *pollPDU* IE in TS 38.331 [22] |  |
| 26212 | >>>Poll Byte | ELEMENT | | FALSE | | *pollByte* IE in TS 38.331 [22] |  |
| 26213 | >>DL AM RLC | STRUCTURE | |  | |  | *dl-AM-RLC* IE in TS 38.331 [22] |
| 26214 | >>>Reassembly | ELEMENT | | FALSE | | *t-Reassembly* IE in TS 38.331 [22] |  |
| 26215 | >>>Status Prohibit | ELEMENT | | FALSE | | *t-StatusProhibit* IE in TS 38.331 [22] |  |
| 26216 | >UM Bi-directional | STRUCTURE | |  | |  | *um-Bi-Directional* IE in TS 38.331 [22] |
| 26217 | >>UL UM RLC | ELEMENT | | FALSE | |  | *UL-UM-RLC* IE in TS 38.331 [22] |
| 26218 | >>DL UM RLC | STRUCTURE | |  | |  | *DL-UM-RLC* IE in TS 38.331 [22] |
| 26219 | >>>Reassembly | ELEMENT | | FALSE | | *t-Reassembly* IE in TS 38.331 [22] |  |
| 26220 | >UM Uni-directional UL | STRUCTURE | |  | |  | *um-Uni-Directional-UL* IE in TS 38.331 [22] |
| 26221 | >>UL UM RLC | ELEMENT | | FALSE | | *ul-UM-RLC* IE in TS 38.331 [22] |  |
| 26222 | >UM Uni-directional DL | ELEMENT | | FALSE | |  | *um-Uni-Directional-DL* IE in TS 38.331 [22] |
| 26223 | >DL UM RLC | STRUCTURE | |  | |  | *dl-UM-RLC* IE in TS 38.331 [22] |
| 26224 | >>Reassembly | ELEMENT | | FALSE | | *t-Reassembly* IE in TS 38.331 [22] |  |
| 26225 | List of QoS Flows to be setup in DRB | LIST |  | |  | | *Flow Mapping Information* IE in TS 38.463 [21] clause 9.3.1.26 |
| 26226 | >QoS Flow Item | STRUCTURE |  | |  | | *QoS Flow Item* IE in TS 38.463 [21] clause 9.3.1.12 |
| 26227 | >>QoS Flow Identifier | ELEMENT | TRUE | | *QoS Flow Identifier* IE in TS 38.463 [21] clause 9.3.1.24 | |  |
| 26228 | >>QoS Flow | STRUCTURE |  | | 8.1.1.6 | |  |
| 26229 | List of QoS Flows to be modified in DRB | LIST |  | |  | | *Flow Mapping Information* IE in TS 38.463 [21] clause 9.3.1.26 |
| 26230 | >QoS Flow Item | STRUCTURE |  | |  | | *QoS Flow Item* IE in TS 38.463 [21] clause 9.3.1.12 |
| 26231 | >>QoS Flow Identifier | ELEMENT | TRUE | | *QoS Flow Identifier* IE in TS 38.463 [21] clause 9.3.1.24 | |  |
| 26232 | >>QoS Flow | STRUCTURE |  | | 8.1.1.6 | |  |
| 26233 | List of Cell Groups to Add | LIST |  | |  | | *Cell Group List* IE in TS 38.463 [21] Section 9.3.1.11 |
| 26234 | >Cell Group Item | STRUCTURE |  | |  | |  |
| 26255 | >>Cell Group ID | ELEMENT | TRUE | | *cellGroup* IE in TS 38.331 [22] Section 6 | |  |
| 26256 | >>Cell Group | STRUCTURE |  | | 8.1.1.7 | |  |
| 26235 | List of Cell Groups To Modify/Update | LIST |  | |  | | *Cell Group List* IE in TS 38.463 [21] Section 9.3.1.11 |
| 26236 | >Cell Group Item | STRUCTURE |  | |  | |  |
| 26257 | >>Cell Group ID | ELEMENT | TRUE | | *cellGroup* IE in TS 38.331 [22] Section 6 | |  |
| 26258 | >>Cell Group | STRUCTURE |  | | 8.1.1.7 | |  |
| 26237 | List of Cell Groups To Delete | LIST |  | |  | | *Cell Group List* IE in TS 38.463 [21] Section 9.3.1.11 |
| 26238 | >Cell Group Item | STRUCTURE |  | |  | |  |
| 26259 | >>Cell Group ID | ELEMENT | TRUE | | *cellGroup* IE in TS 38.331 [22] Section 6 | |  |
| 26260 | >>Cell Group | STRUCTURE |  | | 8.1.1.7 | |  |
| 26239 | Logical Channel ID | ELEMENT | FALSE | | *LogicalChannelIdentity* IE in TS 38.331 [22] clause 6 | |  |
| 26240 | Channel Access Priority | ELEMENT | FALSE | | *channelAccessPriority* IE in TS 38.331 [22] | |  |
| 26241 | L2 State Information | STRUCTURE |  | | 8.1.1.8 | |  |
| 26242 | Data Report Usage List | LIST |  | |  | | *Data Usage Report List* IE in TS 38.463 [21] Section 9.3.1.44 |
| 26243 | >Data Report Usage Item | STRUCTURE |  | |  | | *Data Report Usage Item* IE in TS 38.463 [21] Section 9.3.1.44 |
| 26244 | >>Start Timestamp | ELEMENT | FALSE | | *Start timestamp* IE in TS 38.463 [21] Section 9.3.1.44 | |  |
| 26245 | >>End Timestamp | ELEMENT | FALSE | | *End timestamp* IE in TS 38.463 [21] Section 9.3.1.44 | |  |
| 26246 | >>Usage Count DL | ELEMENT | FALSE | | *Usage count DL* IE in TS 38.463 [21] Section 9.3.1.44 | |  |
| 26247 | >>Usage Count UL | ELEMENT | FALSE | | *Usage count DL* IE in TS 38.463 [21] Section 9.3.1.44 | |  |

##### 8.1.2.2.3 Bearer Context Release

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 26301 | DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.463 [21] clause 9.3.1.16 |  |
| 26302 | PDCP DL Count | ELEMENT | FALSE | *PDCP DL Count* IE in TS 38.463 [21] Section 9.2.2.11 |  |
| 26303 | PDCP UL Count | ELEMENT | FALSE | *PDCP UL Count* IE in TS 38.463 [21] Section 9.2.2.11 |  |
| 26304 | Release Cause | STRUCTURE |  |  | *Cause* IE in TS 38.463 [21] Section 9.3.1.2 |
| 26305 | >CHOICE Cause Group | STRUCTURE |  |  | *Cause Group* IE in TS 38.463 [21] Section 9.3.1.2 |
| 26306 | >>Radio Network Layer | STRUCTURE |  |  | *Radio Network Layer* IE in TS 38.463 [21] Section 9.3.1.2 |
| 26307 | >>>Radio Network Layer Cause | ELEMENT | FALSE | *Radio Network Layer Cause* IE in TS 38.463 [21] Section 9.3.1.2 |  |
| 26308 | >>Transport Layer | STRUCTURE |  |  | *Transport Layer* IE in TS 38.463 [21] Section 9.3.1.2 |
| 26309 | >>>Transport Layer Cause | ELEMENT | FALSE | *Transport Layer Cause* IE in TS 38.463 [21] Section 9.3.1.2 |  |
| 26310 | >>Protocol | STRUCTURE |  |  | *Protocol* IE in TS 38.463 [21] Section 9.3.1.2 |
| 26311 | >>>Protocol Cause | ELEMENT | FALSE | *Protocol Cause* IE in TS 38.463 [21] Section 9.3.1.2 |  |
| 26312 | >>Miscellaneous | STRUCTURE |  |  | *Misc* IE in TS 38.463 [21] Section 9.3.1.2 |
| 26313 | >>>Miscellaneous Cause | ELEMENT | FALSE | *Miscellaneous Cause* IE in TS 38.463 [21] Section 9.3.1.2 |  |

#### 8.1.2.3 Mobility Management

The RAN Parameters for the call process type of “Mobility Management” are defined as follows.

##### 8.1.2.3.1 Handover Preparation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 27101 | Event AN and inter-RAT B1 mobility thresholds | STRUCTURE |  | *Connectivity and Mobility Event Thresholds* IE in clause 8.1.1.10 |  |
| 27102 | List of Serving cells | LIST |  |  | *MeasResultServMOList* IE in TS 38.331 [22] |
| 27103 | >Serving Cell Item | STRUCTURE |  |  | *MeasResultServMO* IE in TS 38.331 [22] |
| 27104 | >>Serving Cell Index | ELEMENT | TRUE | *servCellID* IE in TS 38.331 [22] |  |
| 27105 | >>CHOICE Serving Cell | STRUCTURE |  |  | *MeasResultServMO* IE in TS 38.331 [22] |
| 27106 | >>>NR Cell | STRUCTURE |  | 8.1.1.1 |  |
| 27107 | >>>E-UTRA Cell | STRUCTURE |  | 8.1.1.2 |  |
| 27108 | >>CHOICE Best Neighboring Cell | STRUCTURE |  |  | *measResultBestNeighCell* IE in TS 38.331 [22] |
| 27109 | >>>NR Cell | STRUCTURE |  | 8.1.1.1 |  |
| 27110 | >>>E-UTRA Cell | STRUCTURE |  | 8.1.1.2 |  |
| 27113 | Primary Cell ID | STRUCTURE |  |  | This is for the primary serving cell of the UE. The structuring of this parameter is based on *Target Cell Global ID* IE in TS 38.423 [15] clause 9.2.3.25 |
| 27114 | >CHOICE *Primary Serving Cell* | STRUCTURE |  |  | The primary cell could either be an NR primary cell or an LTE primary cell. The structuring is based on*Target Cell* IE in TS 38.423 [15] clause 9.2.3.25 |
| 27115 | >>NR SpCell | STRUCTURE |  | 8.1.1.1 | *NR* IE in TS 38.423 [15] clause 9.2.3.25 or *SpCell ID* IE in TS 38.473 [19] clause 9.2.2.1 |
| 27116 | >>LTE E-UTRA PCell | STRUCTURE |  | 8.1.1.2 | *E-UTRA* IE in TS 38.423 [15] clause 9.2.3.25 |
| 27117 | List of Secondary cells | LIST |  |  | *SCell To Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 27118 | >Secondary Cell Item | STRUCTURE |  |  | *SCell To Be Setup Item IEs* IE in TS 38.473 [19] Section 9.2.2.1 |
| 27119 | >>Secondary Cell Index | ELEMENT | FALSE |  | SCellIndex IE in TS 38.473 [19] Section 9.2.2.1 |
| 27120 | >>CHOICE Secondary Cell | STRUCTURE |  |  | *SCell To Be Setup Item IEs* IE in TS 38.473 [19] Section 9.2.2.1 |
| 27121 | >>>NR Cell | STRUCTURE |  | 8.1.1.1 |  |
| 27122 | >>>E-UTRA Cell | STRUCTURE |  | 8.1.1.2 |  |
| 27123 | List of Neighbor cells | LIST |  |  | *measResultNeighCells* IE in TS 38.331 [22] |
| 27124 | >Neighbor Cell Item | STRUCTURE |  |  | *measResultNeighCells* IE in TS 38.331 [22] |
| 27125 | >>CHOICE Neighbor Cell | STRUCTURE |  |  | *measResultNeighCells* IE in TS 38.331 [22] |
| 27126 | >>>NR Cell | STRUCTURE |  | 8.1.1.1 | *MeasResultNR* IE in TS 38.331 [22] |
| 27127 | >>>E-UTRA Cell | STRUCTURE |  | 8.1.1.2 | *MeasResultEUTRA* IE in TS 38.331 [22] |
| 27128 | Target Primary Cell ID | STRUCTURE |  |  | *Target Cell Global ID* IE in TS 38.423 [15] Section 9.2.3.25 |
| 27129 | >CHOICE Target Cell | STRUCTURE |  |  | *Target Cell* IE in TS 38.423 [15] Section 9.2.3.25 |
| 27130 | >>NR SpCell | STRUCTURE |  | 8.1.1.1 | *NR* IE in TS 38.423 [15] Section 9.2.3.25 or *SpCell ID* IE in TS 38.473 [19] clause 9.2.2.1 |
| 27131 | >>LTE E-UTRA PCell | STRUCTURE |  | 8.1.1.2 | *E-UTRA* IE in TS 38.423 [15] Section 9.2.3.25 |
| 27132 | List of Candidate Target cells for conditional HO | LIST |  |  | *Candidate SpCell List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 27133 | >Candidate Target cell Item | STRUCTURE |  |  | *Candidate SpCell Item I****E****s* IE in TS 38.473 [19] Section 9.2.2.1 |
| 27134 | >>CHOICE Candidate Target Cell | STRUCTURE |  |  | *Target Cell* IE in TS 38.423 [15] Section 9.2.3.25 |
| 27135 | >>>NR SpCell candidate | STRUCTURE |  | 8.1.1.1 | *NR* IE in TS 38.423 [15] clause 9.2.3.25 or *SpCell ID* IE in TS 38.473 [19] clause 9.2.2.1 |
| 27136 | >>>LTE E-UTRA PCell candidate | STRUCTURE |  | 8.1.1.2 | *E-UTRA* IE in TS 38.423 [15] clause 9.2.3.25 |
| 27137 | >>Estimated Arrival Probability | ELEMENT | FALSE | *Estimated Arrival Probability* IE in TS 38.423 [15] Section 9.1.1.1 |  |
| 27138 | List of PDU Sessions for Handover | LIST |  |  | This is the list of PDU sessions of the UE that are subject to handover. The structuring is based on *PDU Session Resources To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 |
| 27139 | >PDU Session Item | STRUCTURE |  |  | *PDU Session Resources To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 |
| 27140 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.423 [15] Section 9.2.3.18 |  |
| 27141 | >>PDU Session | STRUCTURE |  | 8.1.1.16 |  |
| 27142 | >>List of QoS flows in the PDU Session | LIST |  |  | *QoS Flows To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 |
| 27143 | >>>QoS Flow Item | LIST |  |  | *QoS Flow To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 |
| 27144 | >>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 27145 | >>>>QoS Flow | STRUCTURE |  | 8.1.1.6 |  |
| 27146 | >>List of DRBs for Handover | LIST |  |  | This is the list of DRBs corresponding to the PDU session to be handed over. The structuring is based on *DRB to Be Setup List* IE in TS 38.473 [19] Section 9.2.2.7 |
| 27147 | >>>DRB Item for Handover | STRUCTURE |  |  | *DRB to Be Setup Item* IE in TS 38.473 [19] Section 9.2.2.7 |
| 27148 | >>>>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.473 [19] Section 9.3.1.8 |  |
| 27149 | >>>>CHOICE *DRB Type* | STRUCTURE |  |  |  |
| 27150 | >>>>>NG-RAN DRB | STRUCTURE |  | 8.1.1.5 |  |
| 27151 | >>>>>E-UTRA DRB | STRUCTURE |  | 8.1.1.9 |  |
| 27152 | >>>>List of QoS flows in the DRB | LIST |  |  | *QoS Flows Information To Be Setup* IE in TS 38.463 [21] Section 9.3.3.2 |
| 27153 | >>>>>QoS Flow Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.25 |
| 27154 | >>>>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.463 [21] Section 9.3.1.25 |  |
| 27155 | >>>>>>QoS Flow | STRUCTURE |  | 8.1.1.6 |  |
| 27175 | List of DRBs for Handover | LIST |  |  | *DRB to Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 27176 | >DRB Item for Handover | STRUCTURE |  |  | *DRB to Be Setup Item* IE in TS 38.473 [19] Section 9.2.2.1 |
| 27177 | >>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.473 [19] Section 9.3.1.8 |  |
| 27178 | >>CHOICE *DRB Type* | STRUCTURE |  |  |  |
| 27179 | >>>NG-RAN DRB | STRUCTURE |  | 8.1.1.5 |  |
| 27180 | >>>E-UTRA DRB | STRUCTURE |  | 8.1.1.9 |  |
| 27181 | >>List of QoS flows in the DRB | LIST |  |  | *QoS Flows Information To Be Setup* IE in TS 38.463 [21] Section 9.3.3.2 |
| 27182 | >>>QoS Flow Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.25 |
| 27183 | >>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.463 [21] Section 9.3.1.25 |  |
| 27184 | >>>>QoS Flow | STRUCTURE |  | 8.1.1.6 |  |

##### 8.1.2.3.2 Handover Cancel

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | Semantics Description |
| 27201 | Event AN and inter-RAT B1 mobility thresholds | STRUCTURE |  | *Connectivity and Mobility Event Thresholds* IE in clause 8.1.1.10 |  | |
| 27209 | List of candidate cells to be cancelled list | LIST |  |  | *Candidate Cells To Be Cancelled List* IE in TS 38.473 [19] Section 9.2.2.4 | |
| 27210 | >Candidate cell to be cancelled item | STRUCTURE |  |  | *Candidate Cells To Be Cancelled List* IE in TS 38.473 [19] Section 9.2.2.4 | |
| 27211 | >>Target cell ID | STRUCTURE |  |  | *Target Cell ID* IE in TS 38.473 [19] Section 9.2.2.4 | |
| 27212 | >>>CHOICE Target cell ID | STRUCTURE |  |  | *Target Cell ID* IE in TS 38.473 [19] Section 9.2.2.4 | |
| 27213 | >>>>NR Cell | STRUCTURE |  | 8.1.1.1 |  | |
| 27214 | >>>>LTE E-UTRA Cell | STRUCTURE |  | 8.1.1.2 |  | |
| 27215 | Cause for canceling HO or CHO | STRUCTURE |  |  | *Cause* IE in TS 38.423 [15] Section 9.1.1.6 | |
| 27216 | >CHOICE *Cause Group* | STRUCTURE |  |  | *Cause Group* IE in TS 38.423 [15] Section 9.2.3.2 | |
| 27217 | >>Radio Network Layer | STRUCTURE |  |  | *Radio Network Layer* IE in TS 38.423 [15] Section 9.2.3.2 | |
| 27218 | >>>Radio Network Layer Cause | ELEMENT | FALSE | *Radio Network Layer Cause* IE in TS 38.423 [15] Section 9.2.3.2 |  | |
| 27219 | >>Transport Layer | STRUCTURE |  |  | *Transport Layer* IE in TS 38.423 [15] Section 9.2.3.2 | |
| 27220 | >>>Transport Layer Cause | ELEMENT | FALSE | *Transport Layer Cause* IE in TS 38.423 [15] Section 9.2.3.2 |  | |
| 27221 | >>Protocol | STRUCTURE |  |  | *Protocol* IE in TS 38.423 [15] Section 9.2.3.2 | |
| 27222 | >>>Protocol Cause | ELEMENT | FALSE | *Protocol Cause* IE in TS 38.423 [15] Section 9.2.3.2 |  | |
| 27223 | >>Misc | STRUCTURE |  |  | *Misc* IE in TS 38.423 [15] Section 9.2.3.2 | |
| 27224 | >>>Miscellaneous Cause | ELEMENT | FALSE | *Miscellaneous Cause* IE in TS 38.423 [15] Section 9.2.3.2 |  | |

##### 8.1.2.3.3 Handover Resource Allocation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | Semantics Description |
| 27301 | Event AN and inter-RAT B1 mobility thresholds | STRUCTURE |  | *Connectivity and Mobility Event Thresholds* IE in clause 8.1.1.10 |  |
| 27302 | Handover Type | ELEMENT | FALSE | *Handover Type* IE in TS 38.413 [11] Section 9.3.1.22 |  |
| 27303 | List of PDU Sessions for Handover | LIST |  |  | *PDU Session Resources To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 |
| 27304 | >PDU Session Item | STRUCTURE |  |  | *PDU Session Resources To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 |
| 27305 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.423 [15] Section 9.2.3.18 |  |
| 27306 | >>PDU Session | STRUCTURE |  | 8.1.1.16 |  |
| 27307 | >>List of QoS flows in the PDU Session | LIST |  |  | *QoS Flows To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 |
| 27308 | >>>QoS Flow Item | LIST |  |  | *QoS Flow To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 |
| 27309 | >>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 27310 | >>>>QoS Flow | STRUCTURE |  | 8.1.1.6 |  |
| 27311 | >>List of DRBs for Handover | LIST |  |  | *DRB to Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 27312 | >>>DRB Item for Handover | STRUCTURE |  |  | *DRB to Be Setup Item* IE in TS 38.473 [19] Section 9.2.2.1 |
| 27313 | >>>>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.473 [19] Section 9.3.1.8 |  |
| 27314 | >>>>CHOICE *DRB Type* | STRUCTURE |  |  | *DRB to Be Setup Item* IE in TS 38.473 [19] Section 9.2.2.1 |
| 27315 | >>>>>NG-RAN DRB | STRUCTURE |  | 8.1.1.5 |  |
| 27316 | >>>>>E-UTRA DRB | STRUCTURE |  | 8.1.1.9 |  |
| 27317 | >>>>List of QoS flows in the DRB | LIST |  |  | *QoS Flows Information To Be Setup* IE in TS 38.463 [21] Section 9.3.3.2 |
| 27318 | >>>>>QoS Flow Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.25 |
| 27319 | >>>>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.463 [21] Section 9.3.1.25 |  |
| 27320 | >>>>>>QoS Flow | STRUCTURE |  | 8.1.1.6 |  |
| 27321 | List of DRBs for Handover | LIST |  |  | *DRB to Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 27322 | >DRB Item for Handover | STRUCTURE |  |  | *DRB to Be Setup Item* IE in TS 38.473 [19] Section 9.2.2.1 |
| 27323 | >>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.473 [19] Section 9.3.1.8 |  |
| 27324 | >>CHOICE *DRB Type* | STRUCTURE |  |  | *DRB to Be Setup Item* IE in TS 38.473 [19] Section 9.2.2.1 |
| 27325 | >>>NG-RAN DRB | STRUCTURE |  | 8.1.1.5 |  |
| 27326 | >>>E-UTRA DRB | STRUCTURE |  | 8.1.1.9 |  |
| 27327 | >>List of QoS flows in the DRB | LIST |  |  | *QoS Flows Information To Be Setup* IE in TS 38.463 [21] Section 9.3.3.2 |
| 27328 | >>>QoS Flow Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.25 |
| 27329 | >>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.463 [21] Section 9.3.1.25 |  |
| 27330 | >>>>QoS Flow | STRUCTURE |  | 8.1.1.6 |  |
| 27331 | Allowed S-NSSAI | LIST |  |  | *Allowed S-NSSAI* IE in TS 38.413 [11] Section 9.3.1.31 |
| 27332 | >Allowed S-NSSAI Item | STRUCTURE |  |  | *Allowed S-NSSAI Item* IE in TS 38.413 [11] Section 9.3.1.31 |
| 27333 | >>S-NSSAI | STRUCTURE |  |  | *S-NSSAI* IE in TS 38.413 [11] Section 9.3.1.24 |
| 27334 | >>>SST | ELEMENT | TRUE | *SST* IE in TS 38.413 [11] Section 9.3.1.24 |  |
| 27335 | >>>SD | ELEMENT | FALSE | *SD* IE in TS 38.413 [11] Section 9.3.1.24 |  |
| 27336 | Mobility Restriction List | STRUCTURE |  |  | *Mobility Restriction List* IE in TS 38.413 [11] Section 9.3.1.85 |
| 27337 | >Serving PLMN | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.413 [11] Section 9.3.3.5 |  |
| 27338 | >List of Equivalent PLMNs | LIST |  |  | *Equivalent PLMNs* IE in TS 38.413 [11] Section 9.3.1.85 |
| 27339 | >>Equivalent PLMN Item | STRUCTURE |  |  |  |
| 27340 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.413 [11] Section 9.3.3.5 |  |
| 27341 | >RAT Restrictions | LIST |  |  | *RAT Restrictions* IE in TS 38.413 [11] Section 9.3.1.85 |
| 27342 | >>RAT Restriction Item | STRUCTURE |  |  |  |
| 27343 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.413 [11] Section 9.3.3.5 |  |
| 27344 | >>>RAT Restriction Information | ELEMENT | FALSE | *RAT Restriction Information* IE in TS 38.413 [11] Section 9.3.1.85 |  |
| 27345 | >Forbidden Area Information | LIST |  |  | *Forbidden Area Information* IE in TS 38.413 [11] Section 9.3.1.85 |
| 27346 | >>Forbidden Area | STRUCTURE |  |  | *Forbidden Area Information* IE in TS 38.413 [11] Section 9.3.1.85 |
| 27347 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.413 [11] Section 9.3.3.5 |  |
| 27348 | >>>List of Forbidden TACs | LIST |  |  | *Forbidden TACs* IE in TS 38.413 [11] Section 9.3.1.85 |
| 27349 | >>>>Forbidden TAC Item | STRUCTURE |  |  | *Forbidden TACs* IE in TS 38.413 [11] Section 9.3.1.85 |
| 27350 | >>>>>TAC | ELEMENT | FALSE | *TAC* IE in TS 38.413 [11] Section 9.3.3.10 |  |
| 27351 | >Service Area Information | LIST |  |  | *Service Area Information* IE in TS 38.413 [11] Section 9.3.1.85 |
| 27352 | >>Service Area | STRUCTURE |  |  | *Service Area Information* IE in TS 38.413 [11] Section 9.3.1.85 |
| 27353 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.413 [11] Section 9.3.3.5 |  |
| 27364 | >>>List of allowed TACs | LIST |  |  | *Allowed TACs* IE in TS 38.413 [11] Section 9.3.1.85 |
| 27365 | >>>>Allowed TAC Item | STRUCTURE |  |  | *Allowed TACs* IE in TS 38.413 [11] Section 9.3.1.85 |
| 27366 | >>>>>TAC | ELEMENT | FALSE | *TAC* IE in TS 38.413 [11] Section 9.3.3.10 |  |
| 27367 | >>>List of Not allowed TACs | LIST |  |  | *Not Allowed TACs* IE in TS 38.413 [11] Section 9.3.1.85 |
| 27368 | >>>>Not Allowed TAC Item | STRUCTURE |  |  | *Not Allowed TACs* IE in TS 38.413 [11] Section 9.3.1.85 |
| 27369 | >>>>>TAC | ELEMENT | FALSE | *TAC* IE in TS 38.413 [11] Section 9.3.3.10 |  |

#### 8.1.2.4 Multi-RAT Dual Connectivity Management

The RAN Parameters for the call process type of “Multi-RAT Dual Connectivity Management” are defined as follows.

##### 8.1.2.4.1 SN Addition

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | Semantics Description |
| 28101 | Event AN and inter-RAT B1 mobility thresholds | STRUCTURE |  | *Connectivity and Mobility Event Thresholds* IE in clause 8.1.1.10 |  |
| 28102 | Secondary Node | STRUCTURE |  | 8.1.1.11 |  | |
| 28103 | CHOICE *PDCP Change Indication* | STRUCTURE |  |  | *PDCP Change Indication* IE in TS 38.423 [15] Section 9.2.3.74 | |
| 28104 | >From S-NG-RAN Node | STRUCTURE |  |  | *From S-NG-RAN Node* IE in TS 38.423 [15] Section 9.2.3.74 | |
| 28105 | >>Indication from S-NG-RAN node to M-NG-RAN node | ELEMENT | FALSE | *Indication from S-NG-RAN node to M-NG-RAN node* IE in TS 38.423 [15] Section 9.2.3.74 |  | |
| 28106 | >From M-NG-RAN Node | STRUCTURE |  |  | *From M-NG-RAN Node* IE in TS 38.423 [15] Section 9.2.3.74 | |
| 28107 | >>Indication from M-NG-RAN node to S-NG-RAN node | ELEMENT | FALSE | *Indication from M-NG-RAN node to S-NG-RAN node* IE in TS 38.423 [15] Section 9.2.3.74 |  | |
| 28108 | Secondary Node UE Aggregate Maximum Bit Rate | STRUCTURE |  |  | *UE Aggregate Maximum Bit Rate* IE in TS 36.423 [17] Section 9.2.12 | |
| 28109 | >UE Aggregate Maximum Bit Rate Downlink | ELEMENT | FALSE | *UE Aggregate Maximum Bit Rate Downlink* IE in TS 36.423 [17] clause 9.2.12 |  | |
| 28110 | >UE Aggregate Maximum Bit Rate Uplink | ELEMENT | FALSE | *UE Aggregate Maximum Bit Rate Uplink* IE in TS 36.423 [17] clause 9.2.12 |  | |
| 28111 | List of PDU sessions to be added | LIST |  |  | *PDU Session Resources To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 | |
| 28112 | >PDU Session Item | STRUCTURE |  |  | *PDU Session Resources To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 | |
| 28113 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.423 [15] Section 9.2.3.18 |  | |
| 28114 | >>PDU Session | STRUCTURE |  | 8.1.1.16 |  | |
| 28115 | >>CHOICE *PDU Session Setup Info* | STRUCTURE |  |  | *PDU Session Resource Setup Info – SN terminated* IE in TS 38.423 [15] Section 9.1.2.5 | |
| 28116 | >>>SN terminated PDU session | STRUCTURE |  |  | *PDU Session Resource Setup Info – SN terminated* IE in TS 38.423 [15] Section 9.1.2.5 | |
| 28118 | >>>>List of QoS flows to be setup | LIST |  |  | *QoS Flows To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 | |
| 28119 | >>>>>QoS flow Item to be setup | STRUCTURE |  |  | *QoS Flow To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 | |
| 28120 | >>>>>>QoS Flow Indicator | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  | |
| 28121 | >>>>>>QoS flow | STRUCTURE |  | 8.1.1.6 |  | |
| 28122 | >>>>Count of QoS flows to be setup | ELEMENT | FALSE | INTEGER (0..64) |  | |
| 28123 | >>>MN terminated PDU session | STRUCTURE |  |  | *PDU Session Resource Setup Info – MN terminated* IE in TS 38.423 [15] Section 9.1.2.5 | |
| 28125 | >>>>List of DRBs to be setup | LIST |  |  | *DRB to QoS Flow Mapping List* IE in TS 38.423 [15] Section 9.2.1.15 | |
| 28126 | >>>>>DRB Item to be setup | STRUCTURE |  |  | *DRB to QoS Flow Mapping Item* IE in TS 38.423 [15] Section 9.2.1.15 | |
| 28127 | >>>>>>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.423 [15] Section 9.2.3.33 |  | |
| 28128 | >>>>>>NG-RAN DRB | STRUCTURE |  | 8.1.1.5 |  | |
| 28129 | >>>>>>List of QoS flows to be setup | LIST |  |  | *QoS Flows List* IE in TS 38.423 [15] Section 9.2.1.15 | |
| 28130 | >>>>>>>QoS flow Item to be setup | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.423 [15] Section 9.2.1.15 | |
| 28131 | >>>>>>>>QoS Flow Indicator | ELEMENT | TRUE | *QoS Flow Indicator* IE in TS 38.423 [15] Section 9.2.3.10 |  | |
| 28132 | >>>>>>>>QoS Flow | STRUCTURE |  | 8.1.1.6 |  | |
| 28133 | >>>>>>Count of list of QoS flows to be setup | ELEMENT | FALSE | INTEGER (0..64) |  | |
| 28134 | >>>>Count of list of DRBs to be setup | ELEMENT | FALSE | INTEGER (0..64) |  | |
| 28135 | Count of list of PDU sessions to be added | ELEMENT | FALSE | INTEGER (0..256) |  | |
| 28136 | List of E-RABs to be added | LIST |  |  | *E-RABs To Be Added List* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28137 | >E-RAB Item | STRUCTURE |  |  | *E-RABs To Be Added Item* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28138 | >>E-RAB ID | ELEMENT | TRUE | *E-RAB ID* IE in TS 36.423 [17] Section 9.2.23 |  | |
| 28139 | >>E-RAB | STRUCTURE |  | 8.1.1.9 |  | |
| 28140 | >>EN-DC Resource Configuration | STRUCTURE |  |  | *EN-DC Resource Configuration* IE in TS 36.423 [17] Section 9.2.108 | |
| 28141 | >>>PDCP at SgNB | ELEMENT | FALSE | *PDCP at SgNB* IE in TS 36.423 [17] Section 9.2.108 |  | |
| 28142 | >>>MCG resources | ELEMENT | FALSE | *MCG resources* IE in TS 36.423 [17] Section 9.2.108 |  | |
| 28143 | >>>SCG resources | ELEMENT | FALSE | *SCG resources* IE in TS 36.423 [17] Section 9.2.108 |  | |
| 28144 | >>CHOICE Resource Configuration | STRUCTURE |  |  | *Resource Configuration* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28145 | >>>PDCP present in SN | STRUCTURE |  |  | *PDCP Present in SN* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28146 | >>>>Maximum MCG admittable E-RAB Level QoS parameters | STRUCTURE |  | 8.1.1.9 |  | |
| 28147 | >>>>RLC Mode | ELEMENT | FALSE | *RLC Mode* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28148 | >>>>UL Configuration | ELEMENT | FALSE | *UL Configuration* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28149 | >>>PDCP not present in SN | STRUCTURE |  |  | *PDCP Not Present in SN* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28150 | >>>>Requested SCG E-RAB Level QoS Parameters | STRUCTURE |  | 8.1.1.9 |  | |
| 28151 | >>>>RLC Mode | ELEMENT | FALSE | *RLC Mode* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28152 | >>>>UL Configuration | ELEMENT | FALSE | *UL Configuration* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28153 | Count of list of E-RABs to be added | ELEMENT | FALSE | INTEGER (0..256) |  | |
| 28154 | List of SN-terminated DRBs | LIST |  |  | *Available DRB IDs* IE in TS 38.423 [15] Section 9.1.2.1 | |
| 28155 | >SN-terminated DRB item | STRUCTURE |  |  |  | |
| 28156 | >>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.423 [15] Section 9.2.3.33 |  | |
| 28157 | >>CHOICE *DRB Type* | STRUCTURE |  |  |  | |
| 28158 | >>>NG-RAN DRB | STRUCTURE |  | 8.1.1.5 |  | |
| 28159 | >>>E-UTRA DRB | STRUCTURE |  | 8.1.1.9 |  | |
| 28160 | Count of list of SN-terminated DRBs | ELEMENT | FALSE | INTEGER (0..64) |  | |
| 28161 | Primary Cell ID | STRUCTURE |  |  | This is for the primary serving cell of the UE. The structuring of this parameter is based on *Target Cell Global ID* IE in TS 38.423 [15] clause 9.2.3.25 | |
| 28162 | >CHOICE Primary Cell | STRUCTURE |  |  | The primary cell could either be an NR primary cell or an LTE primary cell. The structuring is based on*Target Cell* IE in TS 38.423 [15] clause 9.2.3.25 | |
| 28163 | >>NR SpCell | STRUCTURE |  | 8.1.1.1 | *NR Cell* IE in TS 38.423 [15] clause 9.2.3.25 or *SpCell ID* IE in TS 38.473 [19] clause 9.2.2.1 | |
| 28164 | >>LTE PCell | STRUCTURE |  | 8.1.1.2 | *E-UTRA Cell* IE in TS 38.423 [15] clause 9.2.3.25 | |

##### 8.1.2.4.2 SN Modification and deletion

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 28201 | Event AN and inter-RAT B1 mobility thresholds | STRUCTURE |  | *Connectivity and Mobility Event Thresholds* IE in clause 8.1.1.10 | Event AN and inter-RAT B1 mobility thresholds | |
| 28202 | Secondary Node | STRUCTURE |  | 8.1.1.11 |  | |
| 28205 | CHOICE *PDCP Change Indication* | STRUCTURE |  |  | *PDCP Change Indication* IE in TS 38.423 [15] Section 9.2.3.74 | |
| 28206 | >From S-NG-RAN Node | STRUCTURE |  |  | *From S-NG-RAN Node* IE in TS 38.423 [15] Section 9.2.3.74 | |
| 28207 | >>Indication from S-NG-RAN node to M-NG-RAN node | STRUCTURE |  | *Indication from S-NG-RAN node to M-NG-RAN node* IE in TS 38.423 [15] Section 9.2.3.74 |  | |
| 28208 | >From M-NG-RAN Node | STRUCTURE |  |  | *From M-NG-RAN Node* IE in TS 38.423 [15] Section 9.2.3.74 | |
| 28209 | >>Indication from M-NG-RAN node to S-NG-RAN node | STRUCTURE |  | *Indication from M-NG-RAN node to S-NG-RAN node* IE in TS 38.423 [15] Section 9.2.3.74 |  | |
| 28210 | Secondary Node UE Aggregate Maximum Bit Rate | STRUCTURE |  |  | *UE Aggregate Maximum Bit Rate* IE in TS 36.423 [17] Section 9.2.12 | |
| 28211 | >UE Aggregate Maximum Bit Rate Downlink | ELEMENT | FALSE | *UE Aggregate Maximum Bit Rate Downlink* IE in TS 36.423 [17] clause 9.2.12 |  | |
| 28212 | >UE Aggregate Maximum Bit Rate Uplink | ELEMENT | FALSE | *UE Aggregate Maximum Bit Rate Uplink* IE in TS 36.423 [17] clause 9.2.12 |  | |
| 28213 | List of PDU sessions to be added | LIST |  |  | *PDU Session Resources To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 | |
| 28214 | >PDU Session Item | STRUCTURE |  |  | *PDU Session Resources To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 | |
| 28215 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.423 [15] Section 9.2.3.18 |  | |
| 28216 | >>PDU Session | STRUCTURE |  | 8.1.1.16 |  | |
| 28217 | >>CHOICE *PDU Session Setup Info* | STRUCTURE |  |  | *PDU Session Resource Setup Info – SN terminated* IE in TS 38.423 [15] Section 9.1.2.5 | |
| 28218 | >>>SN terminated PDU session | STRUCTURE |  |  | *PDU Session Resource Setup Info – SN terminated* IE in TS 38.423 [15] Section 9.1.2.5 | |
| 28219 | >>>>List of QoS flows to be setup | LIST |  |  | *QoS Flows To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 | |
| 28220 | >>>>>QoS flow Item to be setup | STRUCTURE |  |  | *QoS Flow To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 | |
| 28221 | >>>>>>QoS Flow Indicator | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  | |
| 28222 | >>>>>>QoS flow | STRUCTURE |  | 8.1.1.6 |  | |
| 28223 | >>>>Count of QoS flows to be setup | ELEMENT | FALSE | INTEGER (0..64) |  | |
| 28224 | >>>MN terminated PDU session | STRUCTURE |  |  | *PDU Session Resource Setup Info – MN terminated* IE in TS 38.423 [15] Section 9.1.2.5 | |
| 28225 | >>>>List of DRBs to be setup | LIST |  |  | *DRB to QoS Flow Mapping List* IE in TS 38.423 [15] Section 9.2.1.15 | |
| 28226 | >>>>>DRB Item to be setup | STRUCTURE |  |  | *DRB to QoS Flow Mapping Item* IE in TS 38.423 [15] Section 9.2.1.15 | |
| 28227 | >>>>>>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.423 [15] Section 9.2.3.33 |  | |
| 28228 | >>>>>>NG-RAN DRB | STRUCTURE |  | 8.1.1.5 |  | |
| 28229 | >>>>>>List of QoS flows to be setup | LIST |  |  | *QoS Flows List* IE in TS 38.423 [15] Section 9.2.1.15 | |
| 28230 | >>>>>>>QoS flow Item to be setup | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.423 [15] Section 9.2.1.15 | |
| 28231 | >>>>>>>>QoS Flow Indicator | ELEMENT | TRUE | *QoS Flow Indicator* IE in TS 38.423 [15] Section 9.2.3.10 |  | |
| 28232 | >>>>>>>>QoS Flow | STRUCTURE |  | 8.1.1.6 |  | |
| 28233 | >>>>>>Count of list of QoS flows to be setup | ELEMENT | FALSE | INTEGER (0..64) |  | |
| 28234 | >>>>Count of list of DRBs to be setup | ELEMENT | FALSE | INTEGER (0..64) |  | |
| 28235 | Count of list of PDU sessions to be added | ELEMENT | FALSE | INTEGER (0..256) |  | |
| 28236 | List of PDU sessions to be modified | LIST |  |  | *PDU Session Resources To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 | |
| 28237 | >PDU Session Item | STRUCTURE |  |  | *PDU Session Resources To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 | |
| 28238 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.423 [15] Section 9.2.3.18 |  | |
| 28239 | >>PDU Session | STRUCTURE |  | 8.1.1.16 |  | |
| 28240 | >>CHOICE *PDU Session Modification Info* | STRUCTURE |  |  |  | |
| 28241 | >>>SN terminated PDU session | STRUCTURE |  |  | *PDU Session Resource Setup Info – SN terminated* IE in TS 38.423 [15] Section 9.1.2.5 | |
| 28242 | >>>>List of QoS flows to be modified | LIST |  |  | *QoS Flows To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 | |
| 28243 | >>>>>QoS flow Item to be modified | STRUCTURE |  |  | *QoS Flow To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 | |
| 28244 | >>>>>>QoS Flow Indicator | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  | |
| 28245 | >>>>>>QoS flow | STRUCTURE |  | 8.1.1.6 |  | |
| 28246 | >>>>Count of QoS flows to be modified | ELEMENT | FALSE | INTEGER (0..64) |  | |
| 28247 | >>>MN terminated PDU session | STRUCTURE |  |  | *PDU Session Resource Setup Info – MN terminated* IE in TS 38.423 [15] Section 9.1.2.5 | |
| 28248 | >>>>List of DRBs to be modified | LIST |  |  | *DRB to QoS Flow Mapping List* IE in TS 38.423 [15] Section 9.2.1.15 | |
| 28249 | >>>>>DRB Item to be modified | STRUCTURE |  |  | *DRB to QoS Flow Mapping Item* IE in TS 38.423 [15] Section 9.2.1.15 | |
| 28250 | >>>>>>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.423 [15] Section 9.2.3.33 |  | |
| 28251 | >>>>>>NG-RAN DRB | STRUCTURE |  | 8.1.1.5 |  | |
| 28252 | >>>>>>List of QoS flows to be modified | LIST |  |  | *QoS Flows List* IE in TS 38.423 [15] Section 9.2.1.15 | |
| 28253 | >>>>>>>QoS flow Item to be setup | STRUCTURE |  |  | QoS Flow Item IE in TS 38.423 [15] Section 9.2.1.15 | |
| 28254 | >>>>>>>>QoS Flow Indicator | ELEMENT | TRUE | *QoS Flow Indicator* IE in TS 38.423 [15] Section 9.2.3.10 |  | |
| 28255 | >>>>>>>>QoS Flow | STRUCTURE |  | 8.1.1.6 |  | |
| 28256 | >>>>>>Count of list of QoS flows to be setup | ELEMENT | FALSE | INTEGER (0..64) |  | |
| 28257 | >>>>Count of list of DRBs to be modified | ELEMENT | FALSE | INTEGER (0..64) |  | |
| 28258 | >>MR-DC Usage Information | STRUCTURE |  |  | *MR-DC Usage Information* IE in TS 38.463 [21] Section 9.3.1.63 | |
| 28259 | >>>Secondary RAT Type | ELEMENT | FALSE | *Secondary RAT Type* IE in TS 38.463 [21] Section 9.3.1.63 |  | |
| 28260 | >>>PDU Session Timed Report List | LIST |  |  | *Data Usage Report List* IE in TS 38.463 [21] Section 9.3.1.64 | |
| 28261 | >>>>MR-DC Data Usage Report Item | STRUCTURE |  |  | *Data Report Usage Item* IE in TS 38.463 [21] Section 9.3.1.64 | |
| 28262 | >>>>>Start Timestamp | ELEMENT | FALSE | *Start timestamp* IE in TS 38.463 [21] Section 9.3.1.64 |  | |
| 28263 | >>>>>End Timestamp | ELEMENT | FALSE | *End timestamp* IE in TS 38.463 [21] Section 9.3.1.64 |  | |
| 28264 | >>>>>Usage Count UL | ELEMENT | FALSE | *Usage count DL* IE in TS 38.463 [21] Section 9.3.1.64 |  | |
| 28265 | >>>>>Usage Count DL | ELEMENT | FALSE | *Usage count DL* IE in TS 38.463 [21] Section 9.3.1.64 |  | |
| 28266 | >>MR-DC Usage for QoS flows | LIST |  |  | *Data Usage Per QoS Flow List* IE in TS 38.463 [21] Section 9.3.1.63 | |
| 28267 | >>>QoS Flow Item | STRUCTURE |  |  | *Data Usage Per QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.63 | |
| 28268 | >>>>QoS flow Indicator | ELEMENT | TRUE | *QoS Flow Indicator* IE in TS 38.463 [21] Section 9.3.1.24 |  | |
| 28269 | >>>>Secondary RAT Type | ELEMENT | FALSE | *Secondary RAT Type* IE in TS 38.463 [21] Section 9.3.1.63 |  | |
| 28270 | >>>>QoS Flow Timed Report List | LIST |  |  | *Data Usage Report List* IE in TS 38.463 [21] Section 9.3.1.64 | |
| 28271 | >>>>>MR-DC Data Usage Report Item | STRUCTURE |  |  | *Data Report Usage Item* IE in TS 38.463 [21] Section 9.3.1.64 | |
| 28272 | >>>>>>Start Timestamp | ELEMENT | FALSE | *Start timestamp* IE in TS 38.463 [21] Section 9.3.1.64 |  | |
| 28273 | >>>>>>End timestamp | ELEMENT | FALSE | *End timestamp* IE in TS 38.463 [21] Section 9.3.1.64 |  | |
| 28274 | >>>>>>Usage Count UL | ELEMENT | FALSE | *Usage count DL* IE in TS 38.463 [21] Section 9.3.1.64 |  | |
| 28275 | >>>>>>Usage Count DL | ELEMENT | FALSE | *Usage count DL* IE in TS 38.463 [21] Section 9.3.1.64 |  | |
| 28276 | Count of list of PDU sessions to be modified | ELEMENT | FALSE | INTEGER (0..256) |  | |
| 28277 | List of PDU sessions to be released | LIST |  |  | *PDU Session Resources To Be Released List* IE in TS 38.423 [15] Section 9.1.2.14 | |
| 28278 | >PDU Session Item | STRUCTURE |  |  | *PDU Session List With Cause* IE in TS 38.423 [15] Section 9.2.1.26 | |
| 28279 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.423 [15] Section 9.2.3.18 |  | |
| 28280 | >>PDU Session | STRUCTURE |  | 8.1.1.16 |  | |
| 26281 | >>Release Cause | STRUCTURE |  |  | *Cause* IE in TS 38.463 [21] Section 9.3.1.2 |
| 26282 | >>>CHOICE Cause Group | STRUCTURE |  |  | *Cause Group* IE in TS 38.463 [21] Section 9.3.1.2 |
| 26283 | >>>>Radio Network Layer | STRUCTURE |  |  | *Radio Network Layer* IE in TS 38.463 [21] Section 9.3.1.2 |
| 26284 | >>>>>Radio Network Layer Cause | ELEMENT | FALSE | *Radio Network Layer Cause* IE in TS 38.463 [21] Section 9.3.1.2 |  |
| 26285 | >>>>Transport Layer | STRUCTURE |  |  | *Transport Layer* IE in TS 38.463 [21] Section 9.3.1.2 |
| 26286 | >>>>>Transport Layer Cause | ELEMENT | FALSE | *Transport Layer Cause* IE in TS 38.463 [21] Section 9.3.1.2 |  |
| 26287 | >>>>Protocol | STRUCTURE |  |  | *Protocol* IE in TS 38.463 [21] Section 9.3.1.2 |
| 26288 | >>>>>Protocol Cause | ELEMENT | FALSE | *Protocol Cause* IE in TS 38.463 [21] Section 9.3.1.2 |  |
| 26289 | >>>>Miscellaneous | STRUCTURE |  |  | *Misc* IE in TS 38.463 [21] Section 9.3.1.2 |
| 26290 | >>>>>Miscellaneous Cause | ELEMENT | FALSE | *Miscellaneous Cause* IE in TS 38.463 [21] Section 9.3.1.2 |  |
| 28291 | Count of list of PDU sessions to be released | ELEMENT | FALSE | INTEGER (0..256) |  | |
| 28292 | List of E-RABs to be added | LIST |  |  | *E-RABs To Be Added List* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28293 | >E-RAB Item | STRUCTURE |  |  | *E-RABs To Be Added Item* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28294 | >>E-RAB ID | ELEMENT | TRUE | *E-RAB ID* IE in TS 36.423 [17] Section 9.2.23 |  | |
| 28295 | >>E-RAB | STRUCTURE |  | 8.1.1.9 |  | |
| 28296 | >>EN-DC Resource Configuration | STRUCTURE |  |  | *EN-DC Resource Configuration* IE in TS 36.423 [17] Section 9.2.108 | |
| 28297 | >>>PDCP at SgNB | STRUCTURE |  | *PDCP at SgNB* IE in TS 36.423 [17] Section 9.2.108 |  | |
| 28298 | >>>MCG resources | STRUCTURE |  | *MCG resources* IE in TS 36.423 [17] Section 9.2.108 |  | |
| 28299 | >>>SCG resources | STRUCTURE |  | *SCG resources* IE in TS 36.423 [17] Section 9.2.108 |  | |
| 28300 | >>CHOICE Resource Configuration | STRUCTURE |  |  | *Resource Configuration* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28301 | >>>PDCP present in SN | STRUCTURE |  |  | *PDCP Present in SN* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28302 | >>>>Maximum MCG admittable E-RAB Level QoS parameters | STRUCTURE |  | 8.1.1.9 |  | |
| 28303 | >>>>RLC Mode | ELEMENT | FALSE | *RLC Mode* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28304 | >>>>UL Configuration | ELEMENT | FALSE | *UL Configuration* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28305 | >>>PDCP not present in SN | STRUCTURE |  |  | *PDCP Not Present in SN* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28306 | >>>>Requested SCG E-RAB Level QoS Parameters | STRUCTURE |  | 8.1.1.9 |  | |
| 28307 | >>>>RLC Mode | ELEMENT | FALSE | *RLC Mode* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28308 | >>>>UL Configuration | ELEMENT | FALSE | *UL Configuration* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28309 | Count of list of E-RABs to be added | ELEMENT | FALSE | INTEGER (0..256) |  | |
| 28310 | List of E-RABs to be modified | LIST |  |  | *E-RABs To Be Modified List* IE in TS 36.423 [17] Section 9.1.4.5 | |
| 28311 | >E-RAB Item | STRUCTURE |  |  | *E-RABs To Be Modified Item* IE in TS 36.423 [17] Section 9.1.4.5 | |
| 28312 | >>E-RAB ID | ELEMENT | TRUE | *E-RAB ID* IE in TS 36.423 [17] Section 9.2.23 |  | |
| 28313 | >>E-RAB | STRUCTURE |  | 8.1.1.9 |  | |
| 28314 | >>EN-DC Resource Configuration | STRUCTURE |  |  | *EN-DC Resource Configuration* IE in TS 36.423 [17] Section 9.2.108 | |
| 28315 | >>>PDCP at SgNB | STRUCTURE |  | *PDCP at SgNB* IE in TS 36.423 [17] Section 9.2.108 |  | |
| 28316 | >>>MCG resources | STRUCTURE |  | *MCG resources* IE in TS 36.423 [17] Section 9.2.108 |  | |
| 28317 | >>>SCG resources | STRUCTURE |  | *SCG resources* IE in TS 36.423 [17] Section 9.2.108 |  | |
| 28318 | >>CHOICE Resource Configuration | STRUCTURE |  |  | *Resource Configuration* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28319 | >>>PDCP present in SN | STRUCTURE |  |  | *PDCP Present in SN* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28320 | >>>>Maximum MCG admittable E-RAB Level QoS parameters | STRUCTURE |  | 8.1.1.9 |  | |
| 28321 | >>>>RLC Mode | ELEMENT | FALSE | *RLC Mode* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28322 | >>>>UL Configuration | ELEMENT | FALSE | *UL Configuration* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28323 | >>>PDCP not present in SN | STRUCTURE |  |  | *PDCP Not Present in SN* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28324 | >>>>Requested SCG E-RAB Level QoS Parameters | STRUCTURE |  | 8.1.1.9 |  | |
| 28325 | >>>>RLC Mode | ELEMENT | FALSE | *RLC Mode* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28326 | >>>>UL Configuration | ELEMENT | FALSE | *UL Configuration* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28327 | Count of list of E-RABs to be modified | ELEMENT | FALSE | INTEGER (0..256) |  | |
| 28328 | List of E-RABs to be released | LIST |  |  | *E-RABs To Be Released List* IE in TS 36.423 [17] Section 9.1.4.5 | |
| 28329 | >E-RAB Item | STRUCTURE |  |  | *E-RABs To Be Released Item* IE in TS 36.423 [17] Section 9.1.4.5 | |
| 28330 | >>E-RAB ID | ELEMENT | TRUE | *E-RAB ID* IE in TS 36.423 [17] Section 9.2.23 |  | |
| 28331 | >>E-RAB | STRUCTURE |  | 8.1.1.9 |  | |
| 28332 | >>EN-DC Resource Configuration | STRUCTURE |  |  | *EN-DC Resource Configuration* IE in TS 36.423 [17] Section 9.2.108 | |
| 28333 | >>>PDCP at SgNB | ELEMENT | FALSE | *PDCP at SgNB* IE in TS 36.423 [17] Section 9.2.108 |  | |
| 28334 | >>>MCG resources | ELEMENT | FALSE | *MCG resources* IE in TS 36.423 [17] Section 9.2.108 |  | |
| 28335 | >>>SCG resources | ELEMENT | FALSE | *SCG resources* IE in TS 36.423 [17] Section 9.2.108 |  | |
| 28336 | >>CHOICE Resource Configuration | STRUCTURE |  |  | *Resource Configuration* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28337 | >>>PDCP present in SN | STRUCTURE |  |  | *PDCP Present in SN* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28338 | >>>>Maximum MCG admittable E-RAB Level QoS parameters | STRUCTURE |  | 8.1.1.9 |  | |
| 28339 | >>>>RLC Mode | ELEMENT | FALSE | *RLC Mode* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28340 | >>>>UL Configuration | ELEMENT | FALSE | *UL Configuration* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28341 | >>>PDCP not present in SN | STRUCTURE |  |  | *PDCP Not Present in SN* IE in TS 36.423 [17] Section 9.1.4.1 | |
| 28342 | >>>>Requested SCG E-RAB Level QoS Parameters | STRUCTURE |  | 8.1.1.9 |  | |
| 28343 | >>>>RLC Mode | ELEMENT | FALSE | *RLC Mode* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28344 | >>>>UL Configuration | ELEMENT | FALSE | *UL Configuration* IE in TS 36.423 [17] Section 9.1.4.1 |  | |
| 28345 | Count of list of E-RABs to be released | ELEMENT | FALSE | INTEGER (0..256) |  | |
| 28346 | List of SN-terminated DRBs to be modified or released | LIST |  |  | *Additional DRB IDs* IE in TS 38.423 [15] Section 9.1.2.5 | |
| 28347 | >SN-terminated DRB item | STRUCTURE |  |  | *Additional DRB IDs* IE in TS 38.423 [15] Section 9.1.2.5 | |
| 28358 | >>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.423 [15] Section 9.2.3.33 |  | |
| 28348 | >>CHOICE *DRB Type* | STRUCTURE |  |  | *Additional DRB IDs* IE in TS 38.423 [15] Section 9.1.2.5 | |
| 28349 | >>>NG-RAN DRB | STRUCTURE |  | 8.1.1.5 |  | |
| 28350 | >>>E-UTRA DRB | STRUCTURE |  | 8.1.1.9 |  | |
| 28351 | Count of list of SN-terminated DRBs | ELEMENT | FALSE | INTEGER (0..64) |  | |
| 28352 | Primary Cell ID | STRUCTURE |  |  | *SpCell ID IE* in TS 38.473 [19] clause 9.2.2.1 | |
| 28353 | >CHOICE Primary Cell | STRUCTURE |  |  | *SpCell ID IE* in TS 38.473 [19] clause 9.2.2.1 | |
| 28354 | >>NR SpCell | STRUCTURE |  | 8.1.1.1 |  | |
| 28355 | >>LTE PCell | STRUCTURE |  | 8.1.1.2 |  | |

#### 8.1.2.5 Radio Resource Control Management

The RAN Parameters for the call process type of “Radio Resource Control Management” are defined as follows.

##### 8.1.2.5.1 RRC CG-Config Information Transfer

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 29001 | CG-ConfigInfo | STRUCTURE |  |  | TS 38.473 [19] clause 9.3.1.25 | |
| 29011 | >MN Candidate Cell List Info | STRUCTURE |  |  | *candidateCellInfoListMN* IE in TS 38.331 [22] | |
| 29012 | >>List of NR Cell Measurements | LIST |  |  | *MeasResultList2NR* IE in TS 38.331 [22] | |
| 29013 | >>>NR Cell Measurement Item | STRUCTURE |  |  | *MeasResult2NR* *Item* IE in TS 38.331 [22] | |
| 29014 | >>>>SSB Frequency | ELEMENT | FALSE | *ssbFrequency* IE in TS 38.331 [22] |  | |
| 29015 | >>>>CSI-RS Reference Frequency | ELEMENT | FALSE | *refFreqCSI-RS* IE in TS 38.331 [22] |  | |
| 29016 | >>>>NR Serving Cell | STRUCTURE |  |  | *measResultServingCell* IE in TS 38.331 [22] | |
| 29017 | >>>>NR Neighbor Cell Measurement List | LIST |  |  | *measResultNeighCellListNR* IE in TS 38.331 [22] | |
| 29018 | >>>>>NR Neighbor Cell Measurement Item | STRUCTURE |  |  | *measResultNR* *Item* IE in TS 38.331 [22] | |
| 29019 | >>>>>>NR Neighbor Cell | STRUCTURE |  | *NR Cell* in 8.1.1.1 |  | |
| 29021 | >SN Candidate Cell List Info | STRUCTURE |  |  | *candidateCellInfoListMN* IE in TS 38.331 [22] | |
| 29022 | >>List of NR Cell Measurements | LIST |  |  | *MeasResultList2NR* IE in TS 38.331 [22] | |
| 29023 | >>>NR Cell Measurement Item | STRUCTURE |  |  | *MeasResult2NR Item* IE in TS 38.331 [22] | |
| 29024 | >>>>SSB Frequency | ELEMENT | FALSE | *ssbFrequency* IE in TS 38.331 [22] |  | |
| 29025 | >>>>CSI-RS Reference Frequency | ELEMENT | FALSE | *refFreqCSI-RS* IE in TS 38.331 [22] |  | |
| 29026 | >>>>NR Serving Cell | STRUCTURE |  |  | *measResultServingCell* IE in TS 38.331 [22] | |
| 29027 | >>>>NR Neighbor Cell Measurement List | LIST |  |  | *measResultNeighCellListNR* IE in TS 38.331 [22] | |
| 29028 | >>>>>NR Neighbor Cell Measurement Item | STRUCTURE |  |  | *measResultNR Item* IE in TS 38.331 [22] | |
| 29029 | >>>>>>NR Neighbor Cell | STRUCTURE |  | *NR Cell* in 8.1.1.1 |  | |
| 29031 | >SCG Failure Info | STRUCTURE |  |  | *FailureReportSCG* IE in TS 38.331 [22] | |
| 29032 | >>Failure Type | ELEMENT | FALSE | *failureType* IE in TS 38.331 [22] |  | |
| 29033 | >>Meas Result SCG Failure | STRUCTURE |  |  | *measResultSCG-Failure* IE in TS 38.331 [22] | |
| 29034 | >>>Measurement Result List Per Measurement Object | STRUCTURE |  |  | *measResultPerMOList* IE in TS 38.331 [22] | |
| 29035 | >>>>List of NR Cell Measurements | LIST |  |  | *MeasResultList2NR* IE in TS 38.331 [22] | |
| 29036 | >>>>>NR Cell Measurement Item | STRUCTURE |  |  | *MeasResult2NR Item* IE in TS 38.331 [22] | |
| 29037 | >>>>>>SSB Frequency | ELEMENT | FALSE | *ssbFrequency* IE in TS 38.331 [22] |  | |
| 29038 | >>>>>>CSI-RS Reference Frequency | ELEMENT | FALSE | *refFreqCSI-RS* IE in TS 38.331 [22] |  | |
| 29039 | >>>>>>NR Serving Cell | STRUCTURE |  |  | *measResultServingCell* IE in TS 38.331 [22] | |
| 29040 | >>>>>>>NR Neighbor Cell Measurement List | LIST |  |  | *measResultNeighCellListNR* IE in TS 38.331 [22] | |
| 29041 | >>>>>>>>NR Neighbor Cell Measurement Item | STRUCTURE |  |  | *measResultNR Item* IE in TS 38.331 [22] | |
| 29042 | >>>>>>>>NR Neighbor Cell | STRUCTURE |  | *NR Cell* in 8.1.1.1 |  | |
| 29051 | >DRX Info MCG | STRUCTURE |  |  | *drx-InfoMCG* IE in TS 38.331 [22] | |
| 29052 | >>DRX Long Cycle Start Offset | ELEMENT | FALSE | *drx-LongCycleStartOffset* IE in TS 38.331 [22] |  | |
| 29053 | >>Short DRX | STRUCTURE |  |  | *shortDRX* IE in TS 38.331 [22] | |
| 29054 | >>>DRX Short Cycle | ELEMENT | FALSE | *drx-ShortCycle* IE in TS 38.331 [22] |  | |
| 29055 | >>>DRX Short Cycle Timer | ELEMENT | FALSE | *drx-ShortCycleTimer* IE in TS 38.331 [22] |  | |
| 29061 | >Measurement Configuration MN | STRUCTURE |  |  | *MeasConfigMN* IE in TS 38.331 [22] | |
| 29062 | >>MN Measured Frequencies | LIST |  |  | *measuredFrequenciesMN* IE in TS 38.331 [22] | |
| 29063 | >>>NR Frequency Info Item | STRUCTURE |  | *NR-FreqInfo* IE in TS 38.331 [22] |  | |
| 29064 | >>>>NR ARFCN | ELEMENT | FALSE | *ARFCN-ValueNR* IE in TS 38.331 [22] |  | |
| 29065 | >Secondary Cell Group RB Config | STRUCTURE |  |  | *scg-RB-Config* IE in TS 38.331 [22] | |
| 29066 | >>Radio Bearer Config | STRUCTURE |  |  | *RadioBearerConfig* IE in TS 38.331 [22] | |
| 29067 | >>>DRB To Add Modify List | LIST |  |  | *Drb-ToAddModList* IE in TS 38.331 [22] | |
| 29068 | >>>>DRB To Add Modify Item | STRUCTURE |  |  | *DRB-ToAddMod* IE in TS 38.331 [22] | |
| 29069 | >>>>>CHOICE *CN Association* | STRUCTURE |  |  | *cnAssociation* IE in TS 38.331 [22] | |
| 29070 | >>>>>>EPS Bearer Identity | ELEMENT | FALSE | *eps-BearerIdentity* IE in TS 38.331 [22] |  | |
| 29071 | >>>>>>SDAP Config | STRUCTURE |  |  | *SDAP-Config* IE in TS 38.331 [22] | |
| 29072 | >>>>>>>PDU Session ID | ELEMENT | TRUE | *PDU-SessionID* IE in TS 38.331 [22] |  | |
| 29073 | >>>>>>>PDU Session | STRUCTURE |  | *PDU Session* in TS 38.331 [22] |  | |
| 29074 | >>>>>>>Default DRB | ELEMENT | FALSE | *defaultDRB* IE in TS 38.331 [22] |  | |
| 29075 | >>>>>DRB ID | ELEMENT | TRUE | *DRB-Identity* IE in TS 38.331 [22] |  | |
| 29076 | >>>>>CHOICE *DRB Type* | STRUCTURE |  |  | *DRB-ToAddMod* IE in TS 38.331 [22] | |
| 29077 | >>>>>>NG-RAN DRB | STRUCTURE |  | 8.1.1.5 |  | |
| 29078 | >>>>>>LTE E-UTRA DRB | STRUCTURE |  | 8.1.1.9 |  | |
| 29079 | >>>>>Reestablish PDCP | ELEMENT | FALSE | *reestablishPDCP* IE in TS 38.331 [22] |  | |
| 29080 | >>>>>Recover PDCP | ELEMENT | FALSE | *recoverPDCP* IE in TS 38.331 [22] |  | |
| 29081 | >>>>>PDCP Config | STRUCTURE |  | *PDCP Configuration* IE in 8.1.2.2.4 |  | |
| 29091 | >Master Cell Group RB Config | STRUCTURE |  |  | *scg-RB-Config* IE in TS 38.331 [22] | |
| 29092 | >>Radio Bearer Config | STRUCTURE |  |  | *RadioBearerConfig* IE in TS 38.331 [22] | |
| 29093 | >>>DRB To Add Modify List | LIST |  |  | *Drb-ToAddModList* IE in TS 38.331 [22] | |
| 29094 | >>>>DRB To Add Modify Item | STRUCTURE |  |  | *DRB-ToAddMod* IE in TS 38.331 [22] | |
| 29095 | >>>>>CHOICE *CN Association* | STRUCTURE |  |  | *cnAssociation* IE in TS 38.331 [22] | |
| 29096 | >>>>>>EPS Bearer Identity | ELEMENT | FALSE | *eps-BearerIdentity* IE in TS 38.331 [22] |  | |
| 29097 | >>>>>>SDAP Config | STRUCTURE |  |  | *SDAP-Config* IE in TS 38.331 [22] | |
| 29098 | >>>>>>>PDU Session ID | ELEMENT | FALSE | *PDU-SessionID* IE in TS 38.331 [22] |  | |
| 29099 | >>>>>>>PDU Session | STRUCTURE |  | *PDU Session* in TS 38.331 [22] |  | |
| 29100 | >>>>>>>Default DRB | ELEMENT | FALSE | *defaultDRB* IE in TS 38.331 [22] |  | |
| 29101 | >>>>>>>Reflective QoS | ELEMENT | FALSE | *as-reflectiveQoS* IE in TS 38.331 [22] |  | |
| 29102 | >>>>>DRB ID | ELEMENT | TRUE | *DRB-Identity* IE in TS 38.331 [22] |  | |
| 29103 | >>>>>CHOICE *DRB Type* | STRUCTURE |  |  | *DRB-ToAddMod* IE in TS 38.331 [22] | |
| 29104 | >>>>>>NG-RAN DRB | STRUCTURE |  | 8.1.1.5 |  | |
| 29105 | >>>>>>LTE E-UTRA DRB | STRUCTURE |  | 8.1.1.9 |  | |
| 29106 | >>>>>Reestablish PDCP | ELEMENT | FALSE | *reestablishPDCP* IE in TS 38.331 [22] |  | |
| 29107 | >>>>>Recover PDCP | ELEMENT | FALSE | *recoverPDCP* IE in TS 38.331 [22] |  | |
| 29108 | >>>>>PDCP Config | STRUCTURE |  | *PDCP Configuration* IE in 8.1.2.2.4 |  | |
| 29111 | >List of UE Capability RAT Containers | LIST |  |  | *UE-CapabilityRAT-ContainerList* IE in TS 38.331 [22] | |
| 29112 | >>UE Capability RAT Container Item | STRUCTURE |  |  | *UE-CapabilityRAT-Container* IE in TS 38.331 [22] | |
| 29113 | >>>RAT Type | ELEMENT | FALSE | *RAT-Type* IE in TS 38.331 [22] |  | |

##### 8.1.2.5.2 RRC Cell Group Config Transfer

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 29501 | CellGroupConfig | STRUCTURE |  |  | TS 38.473 [19] clause 9.3.1.25 | |
| 29502 | >Cell Group ID | STRUCTURE |  | 8.1.1.7 |  | |
| 29503 | >List of RLC Bearers to Add or Modify | LIST |  |  | *rlc-BearerToAddModList* IE in TS 38.331 [22] | |
| 29504 | >>RLC Bearer to Add or Modify Item | STRUCTURE |  |  | *rlc-BearerToAddModList* IE in TS 38.331 [22] | |
| 29505 | >>>Served RLC Radio Bearer | STRUCTURE |  | 8.1.1.5 |  | |
| 29506 | >>>RLC Bearer Config | STRUCTURE |  |  | *RLC-BearerConfig* IE in TS 38.331 [22] | |
| 29507 | >>>>Logical Channel Identity | ELEMENT | TRUE | *logicalChannelIdentity* IE in TS 38.331 [22] |  | |
| 29508 | >>>>Reestablish RLC | ELEMENT | FALSE | *reestablishRLC* IE in TS 38.331 [22] |  | |
| 29509 | >>>>CHOICE *RLC Config* | STRUCTURE |  |  | *RLC-Config* IE in TS 38.331 [22] | |
| 29510 | >>>>>AM | STRUCTURE |  |  | *am* IE in TS 38.331 [22] | |
| 29511 | >>>>>>UL AM RLC | STRUCTURE |  |  | *ul-AM-RLC* IE in TS 38.331 [22] | |
| 29512 | >>>>>>>Poll Retransmit | ELEMENT | FALSE | *t-PollRetransmit* IE in TS 38.331 [22] |  | |
| 29513 | >>>>>>>Max Retransmission Threshold | ELEMENT | FALSE | *maxRetxThreshold* IE in TS 38.331 [22] |  | |
| 29514 | >>>>>>>Poll PDU | ELEMENT | FALSE | *pollPDU* IE in TS 38.331 [22] |  | |
| 29515 | >>>>>>>Poll Byte | ELEMENT | FALSE | *pollByte* IE in TS 38.331 [22] |  | |
| 29516 | >>>>>>DL AM RLC | STRUCTURE |  |  | *dl-AM-RLC* IE in TS 38.331 [22] | |
| 29517 | >>>>>>>Reassembly | ELEMENT | FALSE | *t-Reassembly* IE in TS 38.331 [22] |  | |
| 29518 | >>>>>>>Status Prohibit | ELEMENT | FALSE | *t-StatusProhibit* IE in TS 38.331 [22] |  | |
| 29519 | >>>>>UM Bi-directional | STRUCTURE |  |  | *um-Bi-Directional* IE in TS 38.331 [22] | |
| 29521 | >>>>>>UL UM RLC | ELEMENT | FALSE |  | *UL-UM-RLC* IE in TS 38.331 [22] | |
| 29522 | >>>>>>DL UM RLC | STRUCTURE |  |  | *DL-UM-RLC* IE in TS 38.331 [22] | |
| 29523 | >>>>>>>Reassembly | ELEMENT | FALSE | *t-Reassembly* IE in TS 38.331 [22] |  | |
| 29530 | >>>>>UM Uni-directional UL | STRUCTURE |  |  | *um-Uni-Directional-UL* IE in TS 38.331 [22] | |
| 29531 | >>>>>>UL UM RLC | ELEMENT | FALSE | *ul-UM-RLC* IE in TS 38.331 [22] |  | |
| 29540 | >>>>>UM Uni-directional DL | STRUCTURE |  |  | *um-Uni-Directional-DL* IE in TS 38.331 [22] | |
| 29541 | >>>>>>DL UM RLC | STRUCTURE |  |  | *dl-UM-RLC* IE in TS 38.331 [22] | |
| 29542 | >>>>>>>Reassembly | ELEMENT | FALSE | *t-Reassembly* IE in TS 38.331 [22] |  | |
| 29551 | >>>>MAC Logical Channel Config | STRUCTURE |  |  |  | |
| 29552 | >>>>>Priority | ELEMENT | FALSE | *priority* IE in TS 38.331 [22] Section 6 |  | |
| 29553 | >>>>>Prioritized Bit Rate | ELEMENT | FALSE | *prioritisedBitRate* IE in TS 38.331 [22] Section 6 |  | |
| 29554 | >>>>>Bucket Size Duration | ELEMENT | FALSE | *bucketSizeDuration* IE in TS 38.331 [22] Section 6 |  | |
| 29555 | >>>>>List of allowed sub-carrier spacing | LIST |  |  | *allowedSCS-List* IE in TS 38.331 [22] Section 6 | |
| 29556 | >>>>>>Allowed sub-carrier spacing item | STRUCTURE |  |  |  | |
| 29557 | >>>>>>>Sub Carrier Spacing | ELEMENT | FALSE | *SubCarrierSpacing* IE in TS 38.331 [22] Section 6 |  | |
| 29558 | >>>>>Max PUSCH Duration | ELEMENT | FALSE | *maxPUSCH-Duration* IE in TS 38.331 [22] Sec 6 |  | |
| 29559 | >>>>>Configured Grant Type1 Allowed | STRUCTURE |  | *configuredGrantTypeAllowed* IE in TS 38.331 [22] Section 6 |  | |
| 29560 | >>>>>Logical Channel Group | ELEMENT | FALSE | *logicalChannelGroup* IE in TS 38.331 [22] |  | |
| 29561 | >>>>>Logical Channel SR – Mask | ELEMENT | FALSE | *logicalChannelSR-Mask* IE in TS 38.331 [22] Section 6 |  | |
| 29562 | >>>>>Logical Channel SR – Delay Timer Applied | ELEMENT | FALSE | *logicalChannelSR-DelayTimerApplied* IE in TS 38.331 [22] Sec 6 |  | |
| 29563 | >>>>>Bit Rate Query Prohibit Timer | ELEMENT | FALSE | *bitRateQueryProhibitTimer* IE in TS 38.331 [22] Section 6 |  | |
| 29564 | >>>>>Channel Access Priority | ELEMENT | FALSE | *reestablishRLC* IE in TS 38.331 [22] |  | |
| 29565 | >>>>>Bit Rate Multiplier | ELEMENT | FALSE | *logicalChannelGroup* IE in TS 38.331 [22] |  | |
| 29601 | >List of RLC Bearers to Release | LIST |  |  | *rlc-BearerToReleaseList* IE in TS 38.331 [22] | |
| 29602 | >>RLC Bearer to Release Item | STRUCTURE |  |  | *rlc-BearerToReleaseList* IE in TS 38.331 [22] | |
| 29603 | >>>Served RLC Radio Bearer | STRUCTURE |  | 8.1.1.5 |  | |
| 29604 | >>>Logical Channel Identity | ELEMENT | TRUE | *logicalChannelIdentity* IE in TS 38.331 [22] |  | |
| 29651 | >MAC Cell Group Config | STRUCTURE |  |  | *mac-CellGroupConfig* IE in TS 38.331 [22] | |
| 29652 | >>Scheduling Request Config | STRUCTURE |  |  | *schedulingRequestConfig* IE in TS 38.331 [22] | |
| 29654 | >>>List of Scheduling Requests to Add or Modify | LIST |  |  | *schedulingRequestToAddModList* IE in TS 38.331 [22] | |
| 29655 | >>>>Scheduling Request Item | STRUCTURE |  |  | *SchedulingRequestToAddMod* IE in TS 38.331 [22] | |
| 29656 | >>>>>Scheduling Request ID | ELEMENT | TRUE | *SchedulingRequestId* IE in TS 38.331 [22] |  | |
| 29657 | >>>>>SR Prohibit Timer | ELEMENT | FALSE | *sr-ProhibitTimer* IE in TS 38.331 [22] |  | |
| 29658 | >>>>>SR Transmission Max | ELEMENT | FALSE | *sr-TransMax* IE in TS 38.331 [22] |  | |
| 29659 | >>>List of Scheduling Requests for release | LIST |  |  | *schedulingRequestToReleaseList* IE in TS 38.331 [22] | |
| 29660 | >>>>Scheduling Request Item | STRUCTURE |  |  |  | |
| 29661 | >>>>>Scheduling Request ID | ELEMENT | TRUE | *SchedulingRequestId* IE in TS 38.331 [22] |  | |
| 29662 | >>>>>SR Prohibit Timer | ELEMENT | FALSE | *sr-ProhibitTimer* IE in TS 38.331 [22] |  | |
| 29663 | >>>>>SR Transmission Max | ELEMENT | FALSE | *sr-TransMax* IE in TS 38.331 [22] |  | |
| 29675 | >>BSR Config | STRUCTURE |  |  | *bsr-Config* IE in TS 38.331 [22] | |
| 29676 | >>>Periodic BSR Timer | ELEMENT | FALSE | *periodicBSR-Timer* IE in TS 38.331 [22] |  | |
| 29677 | >>>Retx BSR Timer | ELEMENT | FALSE | *retxBSR-Timer* IE in TS 38.331 [22] |  | |
| 29578 | >>>Logical Channel SR Delay Timer | ELEMENT | FALSE | *logicalChannelSR-DelayTimer* IE in TS 38.331 [22] |  | |

#### 8.1.2.6 PDU Session Management

The RAN Parameters for the call process type of “PDU Session Management” are defined as follows.

##### 8.1.2.6.1 PDU Session Resource Setup

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 30001 | PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.413 [11] Section 9.3.1.50 |  |
| 30002 | PDU Session | STRUCTURE |  | 8.1.1.16 |  |
| 30003 | List of QoS Flows to be setup | LIST |  |  | *QoS Flow Setup Request List* IE in TS 38.413 [11] Section 9.3.4.1 |
| 30004 | >QoS flow setup request item | STRUCTURE |  |  | *QoS Flow Setup Request Item* IE in TS 38.413 [11] Section 9.3.4.1 |
| 30005 | >>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.413 [11] Section 9.3.1.51 |  |
| 30006 | >>QoS flow | STRUCTURE |  | 8.1.1.6 |  |
| 30010 | List of QoS Flows failed to be setup | LIST |  |  | *QoS Flow Failed To Setup List* IE in TS 38.413 [11] Section 9.3.4.2 |
| 30011 | >QoS flow item failed for setup | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.413 [11] Section 9.3.1.13 |
| 30012 | >>QoS Flow Indicator | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.413 [11] Section 9.3.1.51 |  |
| 30013 | >>QoS flow | STRUCTURE |  | 8.1.1.6 |  |
| 30014 | >>Cause | STRUCTURE |  |  | *Cause* IE in TS 38.413 [11] Section 9.3.1.2 |
| 30015 | >>>CHOICE *Cause group* | STRUCTURE |  |  | *Cause Group* IE in TS 38.413 [11] Section 9.3.1.2 |
| 30016 | >>>>Radio Network Layer | STRUCTURE |  |  | *Radio Network Layer* IE in TS 38.413 [11] Section 9.3.1.2 |
| 30017 | >>>>>Radio Network Layer Cause | ELEMENT | FALSE | *Radio Network Layer Cause* IE in TS 38.413 [11] Section 9.3.1.2 |  |
| 30018 | >>>>Transport Layer | STRUCTURE |  |  | *Transport Layer* IE in TS 38.413 [11] Section 9.3.1.2 |
| 30019 | >>>>>Transport Layer Cause | ELEMENT | FALSE | *Transport Layer Cause* IE in TS 38.463 [21] Section 9.3.1.2 |  |
| 30020 | >>>>NAS | STRUCTURE |  |  | *NAS* IE in TS 38.413 [11] Section 9.3.1.2 |
| 30021 | >>>>>NAS Cause | ELEMENT | FALSE | *NAS Cause* IE in TS 38.413 [11] Section 9.3.1.2 |  |
| 30022 | >>>>Protocol | STRUCTURE |  |  | *Protocol* IE in TS 38.413 [11] Section 9.3.1.2 |
| 30023 | >>>>>Protocol Cause | ELEMENT | FALSE | *Protocol Cause* IE in TS 38.413 [11] Section 9.3.1.2 |  |
| 30024 | >>>>Miscellaneous | STRUCTURE |  |  | *Misc* IE in TS 38.413 [11] Section 9.3.1.2 |
| 30025 | >>>>>Miscellaneous Cause | ELEMENT | FALSE | *Miscellaneous Cause* IE in TS 38.413 [11] Section 9.3.1.2 |  |
| 30031 | Primary Cell ID | STRUCTURE |  |  | This is for the primary serving cell of the UE. The structuring of this parameter is based on *Target Cell Global ID* IE in TS 38.423 [15] clause 9.2.3.25 |
| 30032 | >CHOICE *Primary Cell* | STRUCTURE |  |  | The primary cell could either be an NR primary cell or an LTE primary cell. The structuring is based on*Target Cell* IE in TS 38.423 [15] clause 9.2.3.25 |
| 30033 | >>NR SpCell | STRUCTURE |  | 8.1.1.1 | *NR Cell* IE in TS 38.423 [15] clause 9.2.3.25 |
| 30034 | >>E-UTRA PCell | STRUCTURE |  | 8.1.1.2 | *E-UTRA Cell* IE in TS 38.423 [15] clause 9.2.3.25 |

##### 8.1.2.6.2 PDU Session Resource Modification

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 31001 | PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.413 [11] Section 9.3.1.50 |  |
| 31002 | PDU Session | STRUCTURE |  | 8.1.1.16 |  |
| 31003 | List of QoS Flows to add or modify | LIST |  |  | *QoS Flow Add or Modify Request List IE* in TS 38.413 [11] Section 9.3.4.3 |
| 31004 | >QoS flow add or modify request item | STRUCTURE |  |  | *QoS Flow Add or Modify Request Item* IE in TS 38.413 [11] Section 9.3.4.3 |
| 31005 | >QoS Flow Indicator | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.413 [11] Section 9.3.1.51 |  |
| 31006 | >>QoS flow | STRUCTURE |  | 8.1.1.6 |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| 31012 | List of QoS Flows failed to be added or modified | LIST |  |  | *QoS Flow Failed To Add or Modify List* IE in TS 38.413 [11] Section 9.3.4.2 |
| 31013 | >QoS flow item failed to be added or modified | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.413 [11] Section 9.3.1.13 |
| 31014 | >>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.413 [11] Section 9.3.1.51 |  |
| 31015 | >>QoS flow | STRUCTURE |  | 8.1.1.6 |  |
| 31016 | >>Cause | STRUCTURE |  |  | *Cause* IE in TS 38.413 [11] Section 9.3.1.2 |
| 31017 | >>>CHOICE *Cause group* | STRUCTURE |  |  | *Cause Group* IE in TS 38.413 [11] Section 9.3.1.2 |
| 31018 | >>>>Radio Network Layer | STRUCTURE |  |  | *Radio Network Layer* IE in TS 38.413 [11] Section 9.3.1.2 |
| 31019 | >>>>>Radio Network Layer Cause | ELEMENT | FALSE | *Radio Network Layer Cause* IE in TS 38.413 [11] Section 9.3.1.2 |  |
| 31020 | >>>>Transport Layer | STRUCTURE |  |  | *Transport Layer* IE in TS 38.413 [11] Section 9.3.1.2 |
| 31021 | >>>>>Transport Layer Cause | ELEMENT | FALSE | *Transport Layer Cause* IE in TS 38.463 [21] Section 9.3.1.2 |  |
| 31022 | >>>>NAS | STRUCTURE |  |  | *NAS* IE in TS 38.413 [11] Section 9.3.1.2 |
| 31023 | >>>>>NAS Cause | ELEMENT | FALSE | *NAS Cause* IE in TS 38.413 [11] Section 9.3.1.2 |  |
| 31024 | >>>>Protocol | STRUCTURE |  |  | *Protocol* IE in TS 38.413 [11] Section 9.3.1.2 |
| 31025 | >>>>>Protocol Cause | ELEMENT | FALSE | *Protocol Cause* IE in TS 38.413 [11] Section 9.3.1.2 |  |
| 31026 | >>>>Miscellaneous | STRUCTURE |  |  | *Misc* IE in TS 38.413 [11] Section 9.3.1.2 |
| 31027 | >>>>>Miscellaneous Cause | ELEMENT | FALSE | *Miscellaneous Cause* IE in TS 38.413 [11] Section 9.3.1.2 |  |
| 31031 | List of QoS Flows to be released | LIST |  |  | *QoS Flow To Release List* IE in TS 38.413 [11] Section 9.3.4.2 |
| 31032 | >QoS flow item to be released | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.413 [11] Section 9.3.1.13 |
| 31033 | >>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.413 [11] Section 9.3.1.51 |  |
| 31034 | >>QoS flow | STRUCTURE |  | 8.1.1.6 |  |
| 31035 | >>Cause | STRUCTURE |  |  | *Cause* IE in TS 38.413 [11] Section 9.3.1.2 |
| 31036 | >>>CHOICE *Cause group* | STRUCTURE |  |  | *Cause Group* IE in TS 38.413 [11] Section 9.3.1.2 |
| 31037 | >>>>Radio Network Layer | STRUCTURE |  |  | *Radio Network Layer* IE in TS 38.413 [11] Section 9.3.1.2 |
| 31038 | >>>>>Radio Network Layer Cause | ELEMENT |  | *Radio Network Layer Cause* IE in TS 38.413 [11] Section 9.3.1.2 |  |
| 31039 | >>>>Transport Layer | STRUCTURE |  |  | *Transport Layer* IE in TS 38.413 [11] Section 9.3.1.2 |
| 31040 | >>>>>Transport Layer Cause | ELEMENT | FALSE | *Transport Layer Cause* IE in TS 38.463 [21] Section 9.3.1.2 |  |
| 31041 | >>>>NAS | STRUCTURE |  |  | *NAS* IE in TS 38.413 [11] Section 9.3.1.2 |
| 31042 | >>>>>NAS Cause | ELEMENT | FALSE | *NAS Cause* IE in TS 38.413 [11] Section 9.3.1.2 |  |
| 31043 | >>>>Protocol | STRUCTURE |  |  | *Protocol* IE in TS 38.413 [11] Section 9.3.1.2 |
| 31044 | >>>>>Protocol Cause | ELEMENT | FALSE | *Protocol Cause* IE in TS 38.413 [11] Section 9.3.1.2 |  |
| 31045 | >>>>Miscellaneous | STRUCTURE |  |  | *Misc* IE in TS 38.413 [11] Section 9.3.1.2 |
| 31046 | >>>>>Miscellaneous Cause | ELEMENT | FALSE | *Miscellaneous Cause* IE in TS 38.413 [11] Section 9.3.1.2 |  |
| 31051 | MR-DC Usage Information | STRUCTURE |  |  | *MR-DC Usage Information* IE in TS 38.463 [21] Section 9.3.1.63 |
| 31052 | >Secondary RAT Type | ELEMENT | FALSE | *Secondary RAT Type* IE in TS 38.463 [21] Section 9.3.1.63 |  |
| 31053 | >PDU Session Timed Report List | LIST |  |  | *Data Usage Report List* IE in TS 38.463 [21] Section 9.3.1.64 |
| 31054 | >>MR-DC Data Usage Report Item | STRUCTURE |  |  | *Data Report Usage Item* IE in TS 38.463 [21] Section 9.3.1.64 |
| 31055 | >>>Start Timestamp | ELEMENT | FALSE | *Start timestamp* IE in TS 38.463 [21] Section 9.3.1.64 |  |
| 31075 | >>>End Timestamp | ELEMENT | FALSE | *End timestamp* IE in TS 38.463 [21] Section 9.3.1.64 |  |
| 31056 | >>>Usage Count UL | ELEMENT | FALSE | *Usage count DL* IE in TS 38.463 [21] Section 9.3.1.64 |  |
| 31057 | >>>Usage Count DL | ELEMENT | FALSE | *Usage count DL* IE in TS 38.463 [21] Section 9.3.1.64 |  |
| 31061 | MR-DC Usage for QoS flows | LIST |  |  | *Data Usage Per QoS Flow List* IE in TS 38.463 [21] Section 9.3.1.63 |
| 31062 | >QoS Flow Item | STRUCTURE |  |  | *Data Usage Per QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.63 |
| 31063 | >>QoS flow Indicator | ELEMENT | TRUE | *QoS Flow Indicator* IE in TS 38.463 [21] Section 9.3.1.24 |  |
| 31064 | >>Secondary RAT Type | ELEMENT | FALSE | *Secondary RAT Type* IE in TS 38.463 [21] Sec 9.3.1.63 |  |
| 31065 | >>QoS Flow Timed Report List | LIST |  |  | *Data Usage Report List* IE in TS 38.463 [21] Section 9.3.1.64 |
| 31066 | >>>MR-DC Data Usage Report Item | STRUCTURE |  |  | *Data Report Usage Item* IE in TS 38.463 [21] Section 9.3.1.64 |
| 31067 | >>>>Start Timestamp | ELEMENT | FALSE | *Start timestamp* IE in TS 38.463 [21] Section 9.3.1.64 |  |
| 31068 | >>>>End timestamp | ELEMENT | FALSE | *End timestamp* IE in TS 38.463 [21] Section 9.3.1.64 |  |
| 31069 | >>>>Usage Count UL | ELEMENT | FALSE | *Usage count DL* IE in TS 38.463 [21] Section 9.3.1.64 |  |
| 31070 | >>>>Usage Count DL | ELEMENT | FALSE | *Usage count DL* IE in TS 38.463 [21] Section 9.3.1.64 |  |
| 31081 | Primary Cell ID | STRUCTURE |  |  | This is for the primary serving cell of the UE. The structuring of this parameter is based on *Target Cell Global ID* IE in TS 38.423 [15] clause 9.2.3.25 |
| 31082 | >CHOICE Primary Cell | STRUCTURE |  |  | The primary cell could either be an NR primary cell or an LTE primary cell. The structuring is based on *Target Cell* IE in TS 38.423 [15] clause 9.2.3.25 |
| 31083 | >>NR SpCell | STRUCTURE |  | 8.1.1.1 | *NR Cell* IE in TS 38.423 [15] clause 9.2.3.25 |
| 31084 | >>E-UTRA PCell | STRUCTURE |  | 8.1.1.2 | *E-UTRA Cell* IE in TS 38.423 [15] clause 9.2.3.25 |

##### 8.1.2.6.3 PDU Session Resource Release

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | | **Semantics Description** |
| 32001 | PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.413 [11] Section 9.3.1.50 | |  |
| 32002 | PDU Session | STRUCTURE |  | 8.1.1.16 | |  |
| 32011 | Cause | STRUCTURE |  |  | | *Cause* IE in TS 38.413 [11] Section 9.3.1.2 |
| 32012 | >CHOICE *Cause group* | STRUCTURE |  |  | | *Cause Group* IE in TS 38.413 [11] Section 9.3.1.2 |
| 32013 | >>Radio Network Layer | STRUCTURE |  |  | | *Radio Network Layer* IE in TS 38.413 [11] Section 9.3.1.2 |
| 32014 | >>>Radio Network Layer Cause | ELEMENT | FALSE | *Radio Network Layer Cause* IE in TS 38.413 [11] Section 9.3.1.2 | |  |
| 32015 | >>Transport Layer | STRUCTURE |  |  | | *Transport Layer* IE in TS 38.413 [11] Section 9.3.1.2 |
| 32016 | >>>Transport Layer Cause | ELEMENT | FALSE | *Transport Layer Cause* IE in TS 38.463 [21] Section 9.3.1.2 | |  |
| 32017 | >>NAS | STRUCTURE |  |  | | *NAS* IE in TS 38.413 [11] Section 9.3.1.2 |
| 32018 | >>>NAS Cause | ELEMENT | FALSE | *NAS Cause* IE in TS 38.413 [11] Section 9.3.1.2 | |  |
| 32019 | >>Protocol | STRUCTURE |  |  | | *Protocol* IE in TS 38.413 [11] Section 9.3.1.2 |
| 32020 | >>>Protocol Cause | ELEMENT | FALSE | *Protocol Cause* IE in TS 38.413 [11] Section 9.3.1.2 | |  |
| 32021 | >>Miscellaneous | STRUCTURE |  |  | | *Misc* IE in TS 38.413 [11] Section 9.3.1.2 |
| 32022 | >>>Miscellaneous Cause | ELEMENT | FALSE | *Miscellaneous Cause* IE in TS 38.413 [11] Section 9.3.1.2 | |  |
| 32031 | MR-DC Usage Information | STRUCTURE |  |  | | *MR-DC Usage Information* IE in TS 38.463 [21] Section 9.3.1.63 |
| 32032 | >Secondary RAT Type | ELEMENT | FALSE | *Secondary RAT Type* IE in TS 38.463 [21] Section 9.3.1.63 | |  |
| 32033 | >PDU Session Timed Report List | LIST |  |  | | *Data Usage Report List* IE in TS 38.463 [21] Section 9.3.1.64 |
| 32034 | >>MR-DC Data Usage Report Item | STRUCTURE |  |  | | *Data Report Usage Item* IE in TS 38.463 [21] Section 9.3.1.64 |
| 32035 | >>>Start Timestamp | ELEMENT | FALSE | *Start timestamp* IE in TS 38.463 [21] Section 9.3.1.64 | |  |
| 32036 | >>>End Timestamp | ELEMENT | FALSE | *End timestamp* IE in TS 38.463 [21] Section 9.3.1.64 | |  |
| 32037 | >>>Usage Count UL | ELEMENT | FALSE | *Usage count DL* IE in TS 38.463 [21] Section 9.3.1.64 |  | |
| 32038 | >>>Usage Count DL | ELEMENT | FALSE | *Usage count DL* IE in TS 38.463 [21] Section 9.3.1.64 |  | |
| 32041 | MR-DC Usage for QoS flows | LIST |  |  | *Data Usage Per QoS Flow List* IE in TS 38.463 [21] Section 9.3.1.63 | |
| 32042 | >QoS Flow Item | STRUCTURE |  |  | *Data Usage Per QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.63 | |
| 32043 | >>QoS flow Indicator | ELEMENT | TRUE | *QoS Flow Indicator* IE in TS 38.463 [21] Sec 9.3.1.24 |  | |
| 32054 | >>QoS flow | STRUCTURE |  | 8.1.1.6 |  | |
| 32044 | >>Secondary RAT Type | ELEMENT | FALSE | *Secondary RAT Type* IE in TS 38.463 [21] Section 9.3.1.63 |  | |
| 32045 | >>QoS Flow Timed Report List | LIST |  |  | *Data Usage Report List* IE in TS 38.463 [21] Section 9.3.1.64 | |
| 32046 | >>>MR-DC Data Usage Report Item | STRUCTURE |  |  | *Data Report Usage Item* IE in TS 38.463 [21] Section 9.3.1.64 | |
| 32047 | >>>>Start Timestamp | ELEMENT | FALSE | *Start timestamp* IE in TS 38.463 [21] Section 9.3.1.64 |  | |
| 32048 | >>>>End timestamp | ELEMENT | FALSE | *End timestamp* IE in TS 38.463 [21] Section 9.3.1.64 |  | |
| 32049 | >>>>Usage Count UL | ELEMENT | FALSE | *Usage count DL* IE in TS 38.463 [21] Section 9.3.1.64 |  | |
| 32050 | >>>>Usage Count DL | ELEMENT | FALSE | *Usage count DL* IE in TS 38.463 [21] Section 9.3.1.64 |  | |
| 32061 | Primary Cell ID | STRUCTURE |  |  | This is for the primary serving cell of the UE. The structuring of this parameter is based on *Target Cell Global ID* IE in TS 38.423 [15] clause 9.2.3.25 | |
| 32062 | >CHOICE Primary Cell | STRUCTURE |  |  | The primary cell could either be an NR primary cell or an LTE primary cell. The structuring is based on *Target Cell* IE in TS 38.423 [15] clause 9.2.3.25 | |
| 32063 | >>NR SpCell | STRUCTURE |  | 8.1.1.1 | *NR Cell* IE in TS 38.423 [15] clause 9.2.3.25 | |
| 32064 | >>E-UTRA PCell | STRUCTURE |  | 8.1.1.2 | *E-UTRA Cell* IE in TS 38.423 [15] clause 9.2.3.25 | |

### 8.1.3 RAN Parameters for UE Identification

The following RAN Parameters are defined for identification of UEs.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 35001 | Cell Global ID | STRUCTURE |  |  | To identify UEs associated to a specific cell |
| 35002 | >NR CGI | STRUCTURE |  |  |  |
| 35003 | >>PLMN Identity | ELEMENT | FALSE | Defined in [4] clause 6.2.3.1. |  |
| 35004 | >>NR Cell Identity | ELEMENT | FALSE | Defined in [4] clause 6.2.3.7. |  |
| 35005 | >E-UTRA CGI | STRUCTURE |  |  |  |
| 35006 | >>PLMN Identity | ELEMENT | FALSE | Defined in [4] clause 6.2.3.1. |  |
| 35007 | >>E-UTRA Cell Identity | ELEMENT | FALSE | Defined in [4] clause 6.2.3.11. |  |
| 35010 | S-NSSAI | STRUCTURE |  |  | To identify UEs associated to a specific S-NSSAI |
| 35011 | >SST | ELEMENT | FALSE | Defined in [4] clause 6.2.3.12. |  |
| 35012 | >SD | ELEMENT | FALSE | Defined in [4] clause 6.2.3.12. |  |
| 35020 | Group ID | STRUCTURE |  |  | To identify UEs associated to a specific Group ID defined in [4] clause 6.2.2.7. |
| 35021 | >IRFSP | ELEMENT | FALSE | Defined in [4] clause 6.2.3.27. |  |
| 35022 | >SPID | ELEMENT | FALSE | Defined in [4] clause 6.2.3.28. |  |
| 35030 | Explicit UE List ID | ELEMENT | FALSE | Defined in Section 8.4.9.1. | To identify UEs associated to a specific Explicit UE List ID defined in Section 8.4.9.1. |
| 35040 | Core Control Plane ID | STRUCTURE |  |  | To identify UEs associated to a specific Core Control Plane ID (GUAMI/GUMMEI) defined in [4] clause 6.2.2.8. |
| 35041 | >GUAMI | STRUCTURE |  |  |  |
| 35042 | >>PLMN Identity | ELEMENT | FALSE | Defined in [4] clause 6.2.3.1. |  |
| 35043 | >>AMF Region ID | ELEMENT | FALSE | Defined in [4] clause 6.2.3.17. |  |
| 35044 | >>AMF Set ID | ELEMENT | FALSE | Defined in [4] clause 6.2.3.17. |  |
| 35045 | >>AMF Pointer | ELEMENT | FALSE | Defined in [4] clause 6.2.3.17. |  |
| 35046 | >GUMMEI | STRUCTURE |  |  |  |
| 35047 | >>PLMN Identity | ELEMENT | FALSE | Defined in [4] clause 6.2.3.1. |  |
| 35048 | >>MME Group ID | ELEMENT | FALSE | Defined in [4] clause 6.2.3.18. |  |
| 35049 | >>MME Code | ELEMENT | FALSE | Defined in [4] clause 6.2.3.18. |  |
| 35050 | QoS ID | STRUCTURE |  |  | To identify UEs associated to a specific QoS (QCI/5QI) defined in [4] clause 6.2.2.9. The criteria is for any EPS/PDU sessions assigned to a UE. |
| 35051 | >5QI | ELEMENT | FALSE | Defined in [4] clause 6.2.3.13. |  |
| 35052 | >QCI | ELEMENT | FALSE | Defined in [4] clause 6.2.3.14. |  |
| 35061 | UE Throughput (DL) | ELEMENT | FALSE | INTEGER | To identify UEs based on Average Total DL Thoughtput (kbit/s) as defined in TS 28.552 [28] clause 5.1.1.3.1 |
| 35062 | UE Throughput (UL) | ELEMENT | FALSE | INTEGER | To identify UEs based on Average Total UL Thoughtput (kbit/s) as defined in TS 28.552 [28] clause 5.1.1.3.3 |

### 8.1.4 RAN Parameters for Cell Identification

The following RAN Parameters are defined for identification of Cells.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 36001 | PLMN Identity | ELEMENT | FALSE | Defined in [4] clause 6.2.3.1. | To identify cells based on PLMN ID |
| 36010 | S-NSSAI | STRUCTURE |  |  | To identify cells based on supported S-NSSAI |
| 36011 | >SST | ELEMENT | FALSE | Defined in [4] clause 6.2.3.12. |  |
| 36012 | >SD | ELEMENT | FALSE | Defined in [4] clause 6.2.3.12. |  |

### 8.1.5 UE Events

The following UE Event IDs are defined.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE Event ID** | **UE Event Name** | **Message Event in Event Trigger Definition Format 1** | **If used in Event Trigger Definition Format 1** | **If used in Indication Message Format 1** |
| 1 | Carrier Aggregation Initiated | “F1” Network Interface message of “UE Context Setup Request”. | Event triggering is only when this message event is by initiating carrier aggregation. | Indicates that this message event happened due to carrier aggregation. |
| 2 | A3 Measurement Report Reception | “RRC” message of “Measurement Report”. | Event triggering is only when this message event is by A3 event. | Indicates that this message event happened due to A3 event. |

## 8.2 RAN parameters for REPORT services

### 8.2.1 RAN Parameters for Report Service Style 1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter Name | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | Semantics Description |
| 1 | UE Event ID | ELEMENT | FALSE | INTEGER | This shall be used to report the related UE Event ID described in Section 8.1.5. |
| 2 | NI Message | ELEMENT | FALSE | OCTET STRING | This shall be used to report Network Interface Message |
| 3 | RRC Message | ELEMENT | FALSE | OCTET STRING | This shall be used to report RRC Message |
| 4 | UE ID | ELEMENT | FALSE | OCTET STRING | Defined in Section 9.3.10. This shall be used to report UE ID when the message event configured by the Event Trigger Style 1 is set to “RRC Setup Complete message” (UE attach), or “Xn/NG Handover Request” or “F1 UE Context Setup Request” (Intra gNB HandOver). |
| 5 | Old AMF UE NGAP ID | ELEMENT | FALSE | Defined in [4] clause 6.2.3.16. | This shall be used to report Old AMF UE NGAP IDwhen the message event configured by Event Trigger Style 1 is set to “Xn Handover Request” and AMF UE NGAP ID is changed during HO. |
| 6 | Cell Global ID | ELEMENT | FALSE | OCTET STRING | Defined in Section 9.3.36  This shall be used to report the SpCell ID where the UE belongs to during reporting. |

### 8.2.2 RAN Parameters for Report Service Style 2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter Name | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | Semantics Description |
| 1 | Current UE ID | ELEMENT | FALSE | OCTET STRING | Defined in Section 9.3.10. This shall be used to report UE ID defined at the time of Call Process Outcome. |
| 2 | Old UE ID | ELEMENT | FALSE | OCTET STRING | Defined in Section 9.3.10. This shall be used to report the previously assigned UE ID prior to the call process. |
| 3 | Current RRC State | ELEMENT | FALSE | Defined in Section 9.3.37. | This shall be used to report the RRC state at the time of Call Process Outcome. |
| 4 | Old RRC State | ELEMENT | FALSE | Defined in Section 9.3.37. | This shall be used to report the previous RRC state prior to the Call Process Outcome. |
| 5 | UE Context Information  Container | ELEMENT | FALSE | OCTET STRING | The RETRIEVE UE CONTEXT RESPONSE message content in TS 38.423 [17] clause 9.1.1.9. This shall be used to report UE Context information. |
| 6 | Cell Global ID | ELEMENT | FALSE | OCTET STRING | Defined in Section 9.3.36  This shall be used to report the SpCell ID where the UE belongs to during reporting. |
| 7 | UE Information | Defined in Section 8.1.1.17 | | | |

### 8.2.3 RAN Parameters for Report Service Style 3

|  |  |  |
| --- | --- | --- |
| RAN Parameter ID | RAN Parameter Name | Semantics Description |
| 1 | Cell Context Information | *Served Cell Information* IE in TS 38.473 [19] clause 9.3.1.10. This shall be used to report Cell Context information. |
| 2 | Cell Deleted | This shall be used to report deleted cells. The value shall be set to “True” for the deleted Cell Global ID. |
| 3 | Neighbour Relation Table | This shall be used to report neighbour relation information of the serving cells. |

### 8.2.4 RAN Parameters for Report Service Style 4

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| RAN Parameter Category | RAN Parameter ID | RAN Parameter Name | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | Semantics Description |
| PDCP UE Variables | Defined in Section 8.1.1.8 L2 Bearer State Variables for PDCP State Variables | | | | | |
| RLC UM UE Variables | Defined in Section 8.1.1.8 L2 Bearer State Variables for RLC UM State Variables | | | | | |
| RLC AM UE Variables | Defined in Section 8.1.1.8 L2 Bearer State Variables for RLC AM State Variables | | | | | |
| MAC Variables | 100 | UL MAC CE | ELEMENT | FALSE | OCTET STRING | This shall be used to report MAC CE Structure as per TS 38.321 [26] clause 6.1.3 |
| 101 | DL MAC CE | ELEMENT | FALSE | OCTET STRING |
| 102 | DL Buffer Occupancy | ELEMENT | FALSE | INTEGER | DL Buffer Occupancy at RLC. Expressed as absolute values in terms of Number of Kilo Bytes (KB) |
| RRC State | 201 | Current RRC State | ELEMENT | FALSE | Defined in Section 9.3.37. | This shall be used to report the RRC state before RRC state change. |
| 202 | RRC State Changed To | ELEMENT | FALSE | Defined in Section 9.3.37. | This shall be used to report new RRC state upon RRC stage change |
| 203 | RRC Message | ELEMENT | FALSE | OCTET STRING | This shall be used to report the RRC message which triggered RRC state change |
| UE Identifier Change | 300 | Old UE ID | ELEMENT | FALSE | OCTET STRING | Defined in Section 9.3.10. This shall be used to report the old UE ID upon UE ID change  E2 Node shall report any available old NI or RRC interface UE identifier within the UEID structure. |
| 301 | Current UE ID | ELEMENT | FALSE | OCTET STRING | Defined in Section 9.3.10. This shall be used to report the UE ID available at the time of reporting. |
| 302 | NI Message | ELEMENT | FALSE | OCTET STRING | This shall be used to report the Network Interface message which triggered the UE ID change . |
| Cell Global ID | 400 | Cell Global ID | ELEMENT | FALSE | OCTET STRING | Defined in Section 9.3.36. This shall be used to report the SpCell ID where the UE belongs to during reporting. |

### 8.2.5 RAN Parameters for Report Service Style 5

|  |  |  |
| --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter Name** | **Semantics Description** |
| 1 | UE Context Information | The RETRIEVE UE CONTEXT RESPONSE message content in TS 38.423 [15] clause 9.1.1.9. This shall be used to report UE Context information. |
| 2 | Cell Context Information | *Served Cell Information* IE in TS 38.473 [19] clause 9.3.1.10. This shall be used to report Cell Context information. |
| 3 | Neighbour Relation Table | This shall be used to report neighbour relation information of the serving cells. |

## 8.3 RAN parameters for INSERT services

8.3.1 Approach

The approach for RAN parameters associated with Insert service is provided in Section 8.0.

### 8.3.2 Radio Bearer Control request

#### 8.3.2.1 DRB QoS Configuration request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.2.1.

#### 8.3.2.2 QoS flow mapping configuration request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.2.2.

#### 8.3.2.3 Logical channel configuration request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.2.3.

#### 8.3.2.4 Radio Bearer Admission Control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.2.4.

#### 8.3.2.5 DRB Termination Control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.2.5.

#### 8.3.2.6 DRB Split Ratio Control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.2.6.

#### 8.3.2.7 PDCP Duplication Control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.2.7.

### 8.3.3 Radio Resource Allocation request

#### 8.3.3.1 DRX Parameter Configuration request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.3.1.

#### 8.3.3.2 Scheduling Request Parameter Configuration request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.3.2.

#### 8.3.3.3 Semi-Persistent Scheduling Parameter Configuration request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.3.3.

#### 8.3.3.4 Configured Grant Configuration request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.3.4.

#### 8.3.3.5 CQI table configuration request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.3.5.

#### 8.3.3.6 Slice-level PRB quota allocation request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.3.6.

### 8.3.4 Connected Mode Mobility Control Request

#### 8.3.4.1 Handover Control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.4.1.

#### 8.3.4.2 Conditional Handover Control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.4.2.

#### 8.3.4.3 DAPS Handover Control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.4.3.

### 8.3.5 Radio Access Control request

#### 8.3.5.1 UE admission control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.5.1.

#### 8.3.5.2 RACH backoff control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.5.2.

#### 8.3.5.3 Access barring control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.5.3.

#### 8.3.5.4 RRC Connection Release request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.5.4.

#### 8.3.5.5 RRC Connection Reject request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.5.5.

### 8.3.6 Dual Connectivity Control request

#### 8.3.6.1 DC Secondary Node Addition Control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.6.1.

#### 8.3.6.2 DC Secondary Node Modification Control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.6.2.

#### 8.3.6.3 PSCell Change cell for Secondary Cell Group Control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.6.3.

#### 8.3.6.4 DC Secondary Node Change Control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.6.4.

### 8.3.7 Carrier Aggregation Control request

#### 8.3.7.1 Secondary cell Addition control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.7.1.

#### 8.3.7.2 Secondary cell Modification control request

The RAN parameters associated with this Insert Indication are listed in Section 8.4.7.2.

### 8.3.8 Idle Mode Mobility Control request

#### 8.3.8.1 Cell reselection priority control

The RAN parameters associated with this Insert Indication are listed in Section 8.4.8.1.

### 8.3.9 Common RAN Parameters for INSERT Service styles

The table below shows the set of RAN parameters that are common for all INSERT service styles.

#### 8.3.9.1 UE Context Information

The associated RAN parameters are given in Section 8.1.1.17.

#### 8.3.9.2 E2 Node Context Information

The associated RAN parameters are given in Section 8.1.1.11.

### 8.3.10 Indication Semantics Description for interpretation by the RIC

The E2 node requests the near-RT RIC for the following services as far as the radio bearer Control request is concerned.

(a) In the *RIC Indication Header* IE, the E2 node indicates the *Insert Indication* ID, that is associated with the *Insert Service Style* ID for the radio bearer control request, along with the UE ID, so as to enable the RIC to interpret which Insert Indication service pertaining to which UE is being requested by the E2 node.

(b) In the *RIC Indication Message* IE, the E2 node indicates the list of the RAN parameters in the Indication message that it wants to be controlled by the near-RT RIC. If the E2 node does not provide values for these parameters in the *RIC Indication message* IE, then the RIC would set the values for these parameters in the control action sent via the *RIC* *Control Request* message, along with its decision to accept/deny the request raised by the E2 node (indicated in the *RIC Indication* *Header* IE). If the RAN parameter indicated by the E2 node is an ELEMENT, the RIC would set the value for the parameter in its *RIC Control Request* message. If the indicated RAN parameter is a STRUCTURE but if the E2 node does not list any constitutent RAN parameter of the STRUCTURE, then the RIC would set the values for all the constitutent RAN parameters of the STRUCTURE. If the parameter is a LIST, then:

a. If the E2 node also indicates the *Key* RAN parameter pertaining to the itemized STRUCTURE in the LIST, then the RIC would set the values for all constituent RAN parameters within the structure, pointed by the key.

b. If the E2 node does not indicate the *Key* RAN parameter pertaining to the itemized STRUCTURE in the LIST, then the RIC would set the values for all constituent RAN parameters within each itemized STRUCTURE, whose *key* RAN parameter is identified by the RIC.

(c) If the E2 node provides values for these parameters in the *RIC Indication message* IE, then the RIC would set the values only for those indicated parameters for which it would choose to replace the values already set by the E2 node. It also communicates its decision to accept/deny the request raised by the E2 node for the DRB.

(d) Any RAN parameter identified as a *key* shall always carry a value set by the E2 node, if the E2 node expects the RIC to control the parameters pertaining to the STRUCTURE pointed by the E2 node. The value of this *key* RAN parameter is an index that points to the entire STRUCTURE, and hence the value of the *key* RAN parameter cannot be modified by the near-RT RIC. Without indicating the value for the *key* RAN parameter, the RIC would not control the parameters associated with the structure indexed by the *key*.

Note that the RIC can only set the values for those RAN parameters identified as ELEMENT when they are indicated by the E2 node; however, these RAN parameters can be contained with a STRUCTURE or within an itemized STRUCTURE in a LIST. Also, if the *DRB ID* key parameter is not present for any DRB in the *RIC Indication Message* IE, then the RIC would discard the *RIC Indication* message. And the E2 node would have to set values based on its default radio resource management policies upon time out, and continue with the ongoing call processing. Hence, indicating the *DRB ID* IE for the DRB(s) is a pre-requisite for the RIC to act on the Insert indication via its *RIC Control Request* message.

## 8.4 RAN Parameters for Control Actions

8.4.1 Approach

The approach for RAN parameters associated with Control service is provided in Section 8.0.

### 8.4.2 Radio Bearer Control

#### 8.4.2.1 DRB QoS Configuration

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to DRB QoS Configuration, such as *Bearer Context Management*, *UE Context Management*, *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages. If the *DRB ID* is missing in the *RIC Control Request* message, the E2 node will send a *RIC Control Failure*.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.463 [21] Section 9.3.1.16 |  |
| 2 | 5QI | ELEMENT | FALSE | *5QI* IE in TS 38.463 [21] Section 9.3.1.27 or TS 38.463 [21] Section 9.3.1.28 |  |
| 3 | Packet Delay Budget | ELEMENT | FALSE | *Packet Delay Budget* IE in TS 38.463 [21] Section 9.3.1.47 |  |
| 4 | Packet Error Rate | STRUCTURE |  |  | *Packet Error Rate* IE in TS 38.463 [21] Section 9.3.1.48 |
| 5 | >Scalar factor | ELEMENT | FALSE | *Scalar* IE in TS 38.463 [21] Section 9.3.1.48 |  |
| 6 | >Exponent factor | ELEMENT | FALSE | *Exponent* IE in TS 38.463 [21] Section 9.3.1.48 |  |
| 7 | NG-RAN DRB Allocation and Retention Priority | STRUCTURE |  |  | *NG-RAN Allocation and Retention Priority* IE in TS 38.463 [21] Section 9.3.1.29 |
| 8 | >Priority Level | ELEMENT | FALSE | *Priority Level* IE in TS 38.463 [21] Section 9.3.1.29 |  |
| 9 | >Pre-emption Capability | ELEMENT | FALSE | *Pre-emption Capability* IE in TS 38.463 [21] Section 9.3.1.29 |  |
| 10 | >Pre-emption Vulnerability | ELEMENT | FALSE | *Pre-emption Vulnerability* IE in TS 38.463 [21] Section 9.3.1.29 |  |
| 11 | Priority Level of the mapped QoS flows | ELEMENT | FALSE | *Priority Level* IE in TS 38.463 [21] Section 9.3.1.51 |  |
| 12 | QoS parameters for GBR flows in NG-RAN Bearer | STRUCTURE |  |  | *GBR QoS Flow Information* IE in TS 38.463 [21] Section 9.3.1.30 |
| 13 | >Maximum Flow Bit Rate Downlink | ELEMENT | FALSE | *Bit Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 14 | >Guaranteed Flow Bit Rate Downlink | ELEMENT | FALSE | *Bit Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 15 | >Maximum Packet Loss Rate Downlink | ELEMENT | FALSE | *Packet Loss Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 16 | >Maximum Flow Bit Rate Uplink | ELEMENT | FALSE | *Bit Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 17 | >Guaranteed Flow Bit Rate Uplink | ELEMENT | FALSE | *Bit Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 18 | >Maximum Packet Loss Rate Uplink | ELEMENT | FALSE | *Packet Loss Rate* IE in TS 38.463 [21] Section 9.3.1.30 |  |
| 19 | QoS Monitoring Enable Request | ELEMENT | FALSE | *QoS Monitoring Request* IE in TS 38.463 [21] Section 9.3.1.26 |  |
| 20 | QoS Monitoring Reporting Frequency | ELEMENT | FALSE | *QoS Monitoring Reporting Frequency* IE in TS 38.463 [21] Section 9.3.1.26 |  |
| 21 | QoS Monitoring Disabled | ELEMENT | FALSE | *QoS Monitoring Disabled* IE in TS 38.463 [21] Section 9.3.1.26 |  |
| 22 | Reflective QoS Mapping | ELEMENT | FALSE | *RDI* IE in TS 38.463 [21] Section 9.3.1.26 |  |

#### 8.4.2.2 QoS flow mapping configuration

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to QoS flow mapping Configuration, such as *Bearer Context Management*, *UE Context Management*, *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages. If the *DRB ID* is missing in the *RIC Control Request* message, the E2 node will send a *RIC Control Failure*.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | Semantics Description |
| 1 | DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.463 [21] Section 9.3.1.16 |  |
| 2 | List of QoS Flows to be modified in DRB | LIST |  |  | *Flow Mapping Information* IE in TS 38.463 [21] Section 9.3.1.26 |
| 3 | >QoS Flow Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.12 |
| 4 | >>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.463 [21] Section 9.3.1.24 |  |
| 5 | >>QoS Flow Mapping Indication | ELEMENT | FALSE | *QoS Flow Mapping Indication* IE in TS 38.463 [21] Section 9.3.1.60 |  |

#### 8.4.2.3 Logical channel configuration

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to Logical channel Configuration, such as *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related RRC messages. If the *DRB ID* is missing in the *RIC Control Request* message, the E2 node will send a *RIC Control Failure*.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | DRB ID | ELEMENT | TRUE | *DRB-Identity* IE in TS 38.331 [22] Section 6 |  |
| 2 | Logical Channel ID | ELEMENT | FALSE | *LogicalChannelIdentity* IE in TS 38.331 [22] Section 6 |  |
| 3 | List of cell groups to be added | LIST |  |  | *Cell Group To Add* IE in TS 38.463 [21] Section 9.3.3.11 |
| 4 | >Cell group item | STRUCTURE |  |  | *Cell Group Item* IE in TS 38.463 [21] Section 9.3.1.11 |
| 5 | >>Cell Group ID | ELEMENT | TRUE | *Cell Group ID* IE in TS 38.463 [21] Section 9.3.1.11 |  |
| 6 | >>UL Configuration | ELEMENT | FALSE | *UL Configuration* IE in TS 38.463 [21] Section 9.3.1.33 |  |
| 7 | List of cell groups to be modified | LIST |  |  | *Cell Group To Modify* IE in TS 38.463 [21] Section 9.3.1.11 |
| 8 | >Cell group item | STRUCTURE |  |  | *Cell Group Item* IE in TS 38.463 [21] Section 9.3.1.11 |
| 9 | >>Cell Group ID | ELEMENT | TRUE | *Cell Group ID* IE in TS 38.463 [21] Section 9.3.1.11 |  |
| 10 | >>UL Configuration | ELEMENT | FALSE | *UL Configuration* IE in TS 38.463 [21] Section 9.3.1.11 |  |
| 11 | List of cell groups to be removed | LIST |  |  | *Cell Group To Remove* IE in TS 38.463 [21] Section 9.3.1.11 |
| 12 | >Cell group item | STRUCTURE |  |  | *Cell Group Item* IE in TS 38.463 [21] Section 9.3.1.11 |
| 13 | >>Cell Group ID | ELEMENT | FALSE | *Cell Group ID* IE in TS 38.463 [21] Section 9.3.1.11 |  |
| 14 | Uplink Specific Parameters | STRUCTURE |  |  | *ul-SpecificParameters* IE in TS 38.331 [22] Section 6 |
| 15 | >Priority | ELEMENT | FALSE | *priority* IE in TS 38.331 [22] Section 6 |  |
| 16 | >Prioritized Bit rate | ELEMENT | FALSE | *prioritisedBitRate* IE in TS 38.331 [22] Section 6 |  |
| 17 | >Bucket Size Duration | ELEMENT | FALSE | *bucketSizeDuration* IE in TS 38.331 [22] Section 6 |  |
| 18 | >List of Allowed Serving Cells | LIST |  |  | *allowedServingCells* IE in TS 38.331 [22] Section 6 |
| 19 | >>Allowed Serving Cell Item | STRUCTURE |  |  |  |
| 20 | >>>Serving Cell Index | ELEMENT | FALSE | *ServCellIndex* IE in TS 38.331 [22] Section 6 |  |
| 21 | >List of Allowed SCS Configuration | LIST |  |  | *allowedSCS-List* IE in TS 38.331 [22] Section 6 |
| 22 | >>Allowed SCS Configuration Item | STRUCTURE |  |  |  |
| 23 | >>Subcarrier Spacing Configuration | ELEMENT | FALSE | *SubCarrierSpacing* IE in TS 38.331 [22] Section 6 |  |
| 24 | >Maximum PUSCH Duration | ELEMENT | FALSE | *maxPUSCH-Duration* IE in TS 38.331 [22] Sec 6 |  |
| 25 | >Configured Grant Type 1 Allowed | ELEMENT | FALSE | *configuredGrantTypeAllowed* IE in TS 38.331 [22] Section 6 |  |
| 26 | >Logical Channel SR – Mask | ELEMENT | FALSE | *logicalChannelSR-Mask* IE in TS 38.331 [22] Section 6 |  |
| 27 | >Logical Channel SR – Delay Timer Applied | ELEMENT | FALSE | *logicalChannelSR-DelayTimerApplied* IE in TS 38.331 [22] Sec 6 |  |
| 28 | >Bit Rate Query Prohibit Timer | ELEMENT | FALSE | *bitRateQueryProhibitTimer* IE in TS 38.331 [22] Section 6 |  |
| 29 | >RLC re-establishment | ELEMENT | FALSE | *reestablishRLC* IE in TS 38.331 [22] |  |
| 30 | >Logical Channel Group | ELEMENT | FALSE | *logicalChannelGroup* IE in TS 38.331 [22] |  |

#### 8.4.2.4 Radio Bearer Admission Control

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to Radio Bearer Admission Control, such as *Bearer Context Management*, *UE Context Management*, *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages. If the *DRB ID* is missing in the *RIC Control Request* message, the E2 node will send a *RIC Control Failure*.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics description** |
| 1 | DRB Identity | ELEMENT | TRUE | *DRB ID* IE in TS 38.463 [21] Section 9.3.1.16 |  |
| 2 | List of cell groups to be added | LIST |  |  | *Cell Group To Add* IE in TS 38.463 [21] Section 9.3.3.11 |
| 3 | >Cell group item | STRUCTURE |  |  | *Cell Group Item* IE in TS 38.463 [21] Section 9.3.1.11 |
| 4 | >>Cell Group ID | ELEMENT | TRUE | *Cell Group ID* IE in TS 38.463 [21] Section 9.3.1.11 |  |
| 5 | SDAP Configuration | STRUCTURE |  |  | *SDAP Configuration* IE in TS 38.463 [21] Section 9.3.1.39 |
| 6 | >PDU Session ID | ELEMENT | FALSE | *PDU-SessionID* IE in TS 38.331 [22] Sec 6 |  |
| 7 | >Default DRB | ELEMENT | FALSE | *Default DRB* IE in TS 38.463 [21] Section 9.3.1.39 |  |
| 8 | PDCP Configuration | STRUCTURE |  |  | *PDCP Configuration* IE in TS 38.463 [21] Section 9.3.1.38 |
| 9 | >RLC mode | ELEMENT | FALSE | *RLC mode* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 10 | >PDCP Duplication | ELEMENT | FALSE | *PDCP Duplication* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 11 | >UL Data Split Threshold | ELEMENT | FALSE | *UL Data Split Threshold* IE in TS 38.463 [21] Section 9.3.1.43 |  |
| 12 | >PDCP Re-establishment | ELEMENT | FALSE | *PDCP Re-establishment* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 13 | >PDCP Data Recovery | ELEMENT | FALSE | *PDCP Data Recovery* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 14 | >Out-of-Order Delivery | ELEMENT | FALSE | *Out of Order Delivery* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 15 | >PDCP Status Report Indication | ELEMENT | FALSE | *PDCP Status Report Indication* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 16 | >Number of PDCP duplication | ELEMENT | FALSE | *Additional PDCP duplication Information* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 17 | >UL More than one RLC | STRUCTURE |  |  | *moreThanOneRLC* IE in TS 38.331 [22] Section 6 |
| 18 | >>Primary Path | STRUCTURE |  |  | *primaryPath* IE in TS 38.331 [22] Section 6 |
| 19 | >>>Cell Group ID | ELEMENT | TRUE | *cellGroup* IE in TS 38.331 [22] Section 6 |  |
| 20 | >>>Logical Channel ID | ELEMENT | FALSE | *logicalChannel* IE in TS 38.331 [22] Sec 6 |  |
| 21 | >UL More than two RLC | STRUCTURE |  |  | *moreThanTwoRLC-DRB-r16* IE in TS 38.331 [22] Section 6 |
| 22 | >>Split Secondary Path | ELEMENT | FALSE | *splitSecondaryPath* IE in TS 38.331 [22] Sec 6 |  |
| 23 | >>Duplication State | ELEMENT | FALSE | *duplicationState* IE in TS 38.331 [22] Sec 6 |  |
| 17 | >DL More than one RLC | STRUCTURE |  |  | *moreThanOneRLC* IE in TS 38.331 [22] Section 6 |
| 18 | >>Primary Path | STRUCTURE |  |  | *primaryPath* IE in TS 38.331 [22] Section 6 |
| 19 | >>>Cell Group ID | ELEMENT | TRUE | *cellGroup* IE in TS 38.331 [22] Section 6 |  |
| 20 | >>>Logical Channel ID | ELEMENT | FALSE | *logicalChannel* IE in TS 38.331 [22] Sec 6 |  |
| 21 | >DL More than two RLC | STRUCTURE |  |  | *moreThanTwoRLC-DRB-r16* IE in TS 38.331 [22] Section 6 |
| 22 | >>Split Secondary Path | ELEMENT | FALSE | *splitSecondaryPath* IE in TS 38.331 [22] Sec 6 |  |
| 23 | >>Duplication State | ELEMENT | FALSE | *duplicationState* IE in TS 38.331 [22] Sec 6 |  |

#### 8.4.2.5 DRB Termination Control

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to DRB Termination change, such as *Dual Connectivity Secondary Node Modification (MN/SN initiated)*, *UE Context Management*, *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages. If the *DRB ID* is missing in the *RIC Control Request* message, the E2 node will send a *RIC Control Failure*.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Param** | **RAN Parameter definition** | **Semantics Description** |
| 1 | List of DRBs to be modified to SN-Termination | LIST |  |  | *DRBs To Be Modified* IE in TS 38.423 [15] Section 9.2.1.11 |
| 2 | >DRB Item to be modified to SN-Termination | STRUCTURE |  |  | *DRBs To Be Modified Item* IE in TS 38.423 [15] Section 9.2.1.11 |
| 3 | >>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.423 [15] Section 9.2.3.33 |  |
| 4 | >>Logical Channel ID | ELEMENT | FALSE | *LCID* IE in TS 38.423 [15] Section 9.2.3.70 |  |
| 5 | >>RLC Status | ELEMENT | FALSE | *RLC Status* IE in TS 38.423 [15] Section 9.2.3.80 |  |
| 6 | >>List of QoS flows to be modified to SN-Termination | LIST |  |  | *QoS Flows List* IE in TS 38.423 [15] Section 9.2.1.15 |
| 7 | >>>QoS flow item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.423 [15] Section 9.2.1.15 |
| 8 | >>>>QoS flow ID | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.1.15 |  |
| 9 | >>>>QoS Flow Mapping Indication | ELEMENT | FALSE | *QoS Flow Mapping Indication* IE in TS 38.423 [15] Section 9.2.1.15 |  |
| 10 | List of DRBs to be modified to MN-Termination | LIST |  |  | *DRBs To Be Modified* IE in TS 38.423 [15] Section 9.2.1.9 |
| 11 | >DRB Item to be modified to MN-Termination | STRUCTURE |  |  | *DRBs To Be Modified Item* IE in TS 38.423 [15] Section 9.2.1.9 |
| 12 | >>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.423 [15] Section 9.2.3.33 |  |
| 13 | >>Logical Channel ID | ELEMENT | FALSE | *LCID* IE in TS 38.423 [15] Section 9.2.3.70 |  |
| 14 | >>RLC Status | ELEMENT | FALSE | *RLC Status* IE in TS 38.423 [15] Section 9.2.3.80 |  |
| 15 | >>List of QoS flows to be modified to SN-Termination | LIST |  |  | *QoS Flows List* IE in TS 38.423 [15] Section 9.2.1.15 |
| 16 | >>>QoS flow item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.423 [15] Section 9.2.1.15 |
| 17 | >>>>QoS flow ID | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.1.15 |  |
| 18 | >>>>QoS Flow Mapping Indication | ELEMENT | FALSE | *QoS Flow Mapping Indication* IE in TS 38.423 [15] Section 9.2.1.15 |  |

#### 8.4.2.6 DRB Split Ratio Control

Upon receiving the *RIC Control Request* message, in the presence of *Downlink PDCP Data Split* IE, the E2 node shall split the downlink PDCP traffic between the Master Node and Secondary Node over the X2/Xn interface based on the recommended ratio. In the presence of *Uplink PDCP Data Split Threshold* IE, the E2 node shall invoke procedures related to DRB Split Ratio Control, such as *Bearer Context Management*, *UE Context Management*, *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages. If the *DRB ID* is missing in the *RIC Control Request* message, the E2 node will send a *RIC Control Failure*.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.463 [21] Section 9.3.1.16 |  |
| 2 | Uplink PDCP Data Split Threshold | ELEMENT | FALSE | *UL Data Split Threshold* IE in TS 38.463 [21] Section 9.3.1.43 |  |
| 3 | Downlink PDCP Data Split | ELEMENT | FALSE | INTEGER (0..100) Defined in Section 9.4.2 | Indicates the percentage of PDCP traffic that the MN has to split with the SN |

#### 8.4.2.7 PDCP Duplication Control

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to PDCP Duplication Control, such as *Bearer Context Management*, *UE Context Management*, *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages. If the *DRB ID* is missing in the *RIC Control Request* message, the E2 node will send a *RIC Control Failure*.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.463 [21] Section 9.3.1.16 |  |
| 2 | PDCP Duplication | ELEMENT | FALSE | *PDCP Duplication* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 3 | UL More Than One RLC | STRUCTURE |  |  | *moreThanOneRLC* IE in TS 38.331 [22] |
| 4 | >Primary Path | STRUCTURE |  |  | *primaryPath* IE in TS 38.331 [22] Section 6 |
| 5 | >>Cell Group ID | ELEMENT | TRUE | *cellGroup* IE in TS 38.331 [22] Section 6 |  |
| 6 | >>Logical Channel ID | ELEMENT | FALSE | *logicalChannel* IE in TS 38.331 [22] Sec 6 |  |
| 7 | UL More Than Two RLC | STRUCTURE |  |  | *moreThanTwoRLC-DRB-r16* IE in TS 38.331 [22] Section 6 |
| 8 | >Split Secondary Path | ELEMENT | FALSE | *splitSecondaryPath* IE in TS 38.331 [22] Sec 6 |  |
| 9 | >Duplication State | ELEMENT | FALSE | *duplicationState* IE in TS 38.331 [22] Sec 6 |  |
| 10 | PDCP Duplication Activation | ELEMENT | FALSE | *Duplication Activation* IE in TS 38.463 [21] Section 9.3.1.38 |  |
| 11 | Number of PDCP duplication | ELEMENT | FALSE | *Additional PDCP duplication Information* IE in TS 38.463 [21] Section 9.3.1.38 |  |

### 8.4.3 Radio Resource Allocation Control

#### 8.4.3.1 DRX Parameter Configuration

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to DRX Parameter Configuration, such as *UE Context Management*, *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | Long DRX Cycle Length | ELEMENT | FALSE | *Long DRX Cycle Length* IE in TS 38.473 [19] Section 9.3.1.24 |  |
| 2 | Short DRX Cycle Length | ELEMENT | FALSE | *Short DRX Cycle Length* IE in TS 38.473 [19] Section 9.3.1.24 |  |
| 3 | Short DRX Cycle Timer | ELEMENT | FALSE | *Short DRX Cycle Timer* IE in TS 38.473 [19] Section 9.3.1.24 |  |

#### 8.4.3.2 Scheduling Request Parameter Configuration

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to Scheduling Request Parameter Configuration, such as *UE Context Management*, *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages. If the *Scheduling Request ID* is missing in the *RIC Control Request* message, the E2 node will send a *RIC Control Failure*.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Param** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | List of Scheduling Requests for modification | LIST |  |  | *schedulingRequestToAddModList* IE in TS 38.331 [22] |
| 2 | >Scheduling Request Item | STRUCTURE |  |  | *SchedulingRequestToAddMod* IE in TS 38.331 [22] |
| 3 | >>Scheduling Request ID | ELEMENT | TRUE | *SchedulingRequestId* IE in TS 38.331 [22] |  |
| 4 | >>SR Prohibit Timer | ELEMENT | FALSE | *sr-ProhibitTimer* IE in TS 38.331 [22] |  |
| 5 | >>SR Transmission Max | ELEMENT | FALSE | *sr-TransMax* IE in TS 38.331 [22] |  |
| 6 | List of Scheduling Requests for release | LIST |  |  | *schedulingRequestToReleaseList* IE in TS 38.331 [22] |
| 7 | >Scheduling Request Item | STRUCTURE |  |  |  |
| 8 | >>Scheduling Request ID | ELEMENT | TRUE | *SchedulingRequestId* IE in TS 38.331 [22] |  |

#### 8.4.3.3 Semi-Persistent Scheduling Parameter Configuration

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to Scheduling Request Parameter Configuration, such as *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | SPS-Config | STRUCTURE |  |  | *SPS-Config* IE in TS 38.331 [22] Section |
| 2 | >SPS Periodicity | ELEMENT | FALSE | *periodicity* IE in TS 38.331 [22] Section |  |
| 3 | >Number of HARQ Processes | ELEMENT | FALSE | *nrofHARQ-Processes* IE in TS 38.331 [22] Section |  |
| 4 | >MCS Table | ELEMENT | FALSE | *mcs-Table* IE in TS 38.331 [22] Section |  |

#### 8.4.3.4 Configured Grant Configuration

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to Scheduling Request Parameter Configuration, such as *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | Grant Configuration | STRUCTURE |  |  | *ConfiguredGrantConfig* IE in 38.331 Section |
| 2 | >MCS Table | ELEMENT | FALSE | *mcs-Table* IE in TS 38.331 [22] Section |  |
| 3 | >MCS Table Without Transform Precoder | ELEMENT | FALSE | *Mcs-TableTransformPrecoder* IE in TS 38.331 [22] Section |  |
| 4 | >Resource Allocation | ELEMENT | FALSE | *resourceAllocation* IE in TS 38.331 [22] Section |  |
| 5 | >Number of HARQ processes | ELEMENT | FALSE | *nrofHARQ-Processes* IE in TS 38.331 [22] Section |  |
| 6 | >HARQ retransmissions | ELEMENT | FALSE | *nrofHARQ-Process* IE in TS 38.331 [22] Section |  |
| 7 | >Number of repetitions of HARQ PDU | ELEMENT | FALSE | *repK* IE in TS 38.331 [22] Section |  |
| 8 | >Redundancy Version Format | ELEMENT | FALSE | *repK-RV* IE in TS 38.331 [22] Section |  |
| 9 | >UL Transmission periodicity | ELEMENT | FALSE | *periodicity* IE in TS 38.331 [22] Section |  |
| 10 | >Configured grant timer | ELEMENT | FALSE | *configuredGrantTimer* IE in TS 38.331 [22] Section |  |
| 11 | >RRC Configured Uplink Grant | STRUCTURE |  |  | *rrc-ConfiguredUplinkGrant* IE in TS 38.331 [22] Section |
| 12 | >>Time Domain Offset | ELEMENT | FALSE | *timeDomainOffset* IE in TS 38.331 [22] Section |  |
| 13 | >>Time Domain Allocation | ELEMENT | FALSE | *timeDomainAllocation* IE in TS 38.331 [22] Section |  |
| 14 | >>Frequency Domain Allocation | ELEMENT | FALSE | *frequencyDomainAllocation* IE in TS 38.331 [22] Section |  |
| 15 | >>Antenna Port | ELEMENT | FALSE | *antennaPort* IE in TS 38.331 [22] Section |  |
| 16 | >>Precoding and number of layers | ELEMENT | FALSE | *precodingAndNumberOfLayers* IE in TS 38.331 [22] Section |  |
| 17 | >>MCS and TBS | ELEMENT | FALSE | *mcsAndTBS* IE in TS 38.331 [22] Section |  |
| 18 | >>Path Loss Reference Index | ELEMENT | FALSE | *pathlossReferenceIndex* IE in TS 38.331 [22] |  |

#### 8.4.3.5 CQI table configuration

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to Scheduling Request Parameter Configuration, such as *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages. If the *CSI Report Config ID* is missing in the *RIC Control Request* message, the E2 node will send a *RIC Control Failure*.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Param** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | List of CSI Report Configurations | LIST |  |  | *csi-ReportConfigToAddModList* IE in TS 38.331 [22] Section |
| 2 | >CSI Report Configuration Item | STRUCTURE |  |  | *CSI-ReportConfig* IE in TS 38.331 [22] Section |
| 3 | >>CSI Report Config ID | ELEMENT | TRUE | *CSI-ReportConfigID* IE in TS 38.331 [22] Section |  |
| 4 | >>Carrier | ELEMENT | FALSE | *ServCellIndex* IE in TS 38.331 [22] Section |  |
| 5 | >>CQI-FormatIndicator | ELEMENT | FALSE | *cqi-FormatIndicator* IE in TS 38.331 [22] Section |  |
| 6 | >>PMI-FormatIndicator | ELEMENT | FALSE | *pmi-FormatIndicator* IE in TS 38.331 [22] Section |  |
| 7 | >>CQI Table | ELEMENT | FALSE | *cqi-Table* IE in TS 38.331 [22] Section |  |
| 8 | >>Sub-band size | ELEMENT | FALSE | *subbandSize* IE in TS 38.331 [22] Section |  |

#### 8.4.3.6 Slice-level PRB quota

Upon receiving the *RIC Control Request* message, the E2 node allocates slice-specific PRB quota for the indicated S-NSSAI in terms of the maximum PRB allocation ratio, minimum PRB allocation ratio and dedicated PRB allocation ratio for the given slice among the available set of PRBs. If the *S-NSSAI* is missing in the *RIC Control Request* message, the E2 node will send a *RIC Control Failure*.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | ***Semantics Description*** |
| **1** | RRM Policy Ratio List | LIST |  | *0.. <maxnoofRRMPolicyRatioGroups>* | RRMPolicyRatioList in TS 28.541 |
| **2** | >RRM Policy Ratio Group | STRUCTURE |  |  | RRMPolicyRatio in TS 28.541 |
| 3 | >>RRM Policy | STRUCTURE |  |  | RRMPolicy in TS 28.541 |
| 5 | >>RRM Policy Member List | LIST |  | *0..<maxnoofRRMPolicyMembers>* | *RRMPolicyMemberList* in TS 28.541 |
| 6 | >>>>RRM Policy Member | STRUCTURE |  |  | *RRMPolicyMember* in TS 28.541 |
| 7 | >>>>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.473 [19] Section 9.3.1.14 |  |
| 8 | >>>>>S-NSSAI | STRUCTURE |  |  | *S-NSSAI* IE in TS 38.473 [19] Section 9.3.1.38 |
| 9 | >>>>>>SST | ELEMENT | FALSE | *SST* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 10 | >>>>>>SD | ELEMENT | FALSE | *SD* IE in TS 38.473 [19] Section 9.3.1.38 |  |
| 11 | >>Min PRB Policy Ratio | ELEMENT | FALSE | INTEGER (0..100) | rRMPolicyMinRatio IE in TS 28.541 |
| 12 | >>Max PRB Policy Ratio | ELEMENT | FALSE | INTEGER (0..100) | rRMPolicyMaxRatio IE in TS 28.541 |
| 13 | >>Dedicated PRB Policy Ratio | ELEMENT | FALSE | INTEGER (0..100) | rRMPolicyDedicatedRatio IE in TS 28.541 |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofRRMPolicyRatioGroups | Maximum no. of RAN parameters supported by RAN Function for a specific Control action. The value is <65535>. |
| maxnoofRRMPolicyMembers | Maximum no. of RAN parameters supported by RAN Function for a specific Control action. The value is <65535> |

### 8.4.4 Connected Mode Mobility Control

#### 8.4.4.1 Handover Control

Upon receiving the *RIC Control Request* message, in the case of Xn/X2 or NG or inter-RAT handovers, the E2 node shall invoke procedures, such as *Handover Preparation* related to UE Mobility Management, *Bearer Context Modification, UE Context Modification*, *RRC Message Transfer*, etc. In the case of intra-gNB or F1 handover, the E2 node shall invoke procedures, such as *UE Context Modification*, *RRC Message Transfer*, etc. The E2 node includes the IEs corresponding to one or more of parameters described below in the related interface messages. If the *Target Primary Cell ID* IE is missing in the *RIC Control Request* message, the E2 node will send a *RIC Control Failure* message.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | Semantics Description |
| 1 | Target Primary Cell ID | STRUCTURE |  |  | *Target Cell Global ID* IE in TS 38.423 [15] Section 9.2.3.25 |
| 2 | >CHOICE Target Cell | STRUCTURE |  |  | *Target Cell* IE in TS 38.423 [15] Section 9.2.3.25 |
| 3 | >>NR Cell | STRUCTURE |  |  | *NR* IE in TS 38.423 [15] Section 9.2.3.25 |
| 4 | >>>NR CGI | ELEMENT | FALSE | *NR CGI* IE in TS 38.423 [15] Section 9.2.2.7 |  |
| 5 | >>E-UTRA Cell | STRUCTURE |  |  | *E-UTRA* IE in TS 38.423 [15] Section 9.2.3.25 |
| 6 | >>>E-UTRA CGI | ELEMENT | FALSE | *E-UTRA CGI* IE in TS 38.423 [15] Section 9.2.2.8 |  |
| 7 | List of PDU sessions for handover | LIST |  |  | *PDU Session Resources To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 |
| 8 | >PDU session Item for handover | STRUCTURE |  |  | *PDU Session Resources To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 |
| 9 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.423 [15] Section 9.2.3.18 |  |
| 10 | >>List of QoS flows in the PDU session | LIST |  |  | *QoS Flows To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 |
| 11 | >>>QoS flow Item | STRUCTURE |  |  | *QoS Flow To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 |
| 12 | >>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 13 | List of DRBs for handover | LIST |  |  | *DRB to Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 14 | >DRB item for handover | STRUCTURE |  |  | *DRB to Be Setup Item* IE in TS 38.473 [19] Section 9.2.2.1 |
| 15 | >>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.473 [19] Section 9.3.1.8 |  |
| 16 | >>List of QoS flows in the DRB | LIST |  |  | *QoS Flows Information To Be Setup* IE in TS 38.463 [21] Section 9.3.3.2 |
| 17 | >>>QoS flow Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.25 |
| 18 | >>>>QoS flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.463 [21] Section 9.3.1.25 |  |
| 19 | List of Secondary cells to be setup | LIST |  |  | *Scell To Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 20 | >Secondary cell Item to be setup | STRUCTURE |  |  | *Scell To Be Setup Item Ies* IE in TS 38.473 [19] Section 9.2.2.1 |
| 21 | >>Secondary cell ID | ELEMENT | FALSE | *Scell ID* IE in TS 38.473 [19] Section 9.2.2.1 |  |

#### 8.4.4.2 Conditional Handover Control

Upon receiving the *RIC Control Request* message, in the case of Xn/X2 or NG or inter-RAT conditional handovers, the E2 node shall invoke procedures, such as *Handover Preparation* related to UE Mobility Management, *Bearer Context Modification, UE Context Modification*, *RRC Message Transfer*, etc. involving the candidate target cells (note that there is only one *Handover Preparation* in the case of NG or inter-RAT handovers). In the case of intra-gNB or F1 conditional handover, the E2 node shall invoke procedures, such as *UE Context Modification*, *RRC Message Transfer*, etc. The E2 node includes the IEs corresponding to one or more of parameters described below in the related interface messages. If the *Target Cell* IE is missing in the *RIC Control Request* message, the E2 node will send a *RIC Control Failure* message.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Param** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | List of Candidate target primary cells | LIST |  |  | *Candidate SpCell List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 2 | >Candidate target primary cell item | STRUCTURE |  |  | *Candidate SpCell Item IEs* IE in TS 38.473 [19] Section 9.2.2.1 |
| 3 | >>CHOICE Target Cell | STRUCTURE |  |  | *Target Cell* IE in TS 38.423 [15] Section 9.2.3.25 |
| 4 | >>>NR | STRUCTURE |  |  | *NR* IE in TS 38.423 [15] Section 9.2.3.25 |
| 5 | >>>>NR CGI | ELEMENT | FALSE | *NR CGI* IE in TS 38.423 [15] Section 9.2.2.7 |  |
| 6 | >>>E-UTRA | STRUCTURE |  |  | *E-UTRA* IE in TS 38.423 [15] Section 9.2.3.25 |
| 7 | >>>>E-UTRA CGI | ELEMENT | FALSE | *E-UTRA CGI* IE in TS 38.423 [15] Section 9.2.2.8 |  |
| 8 | >>Estimated Arrival Probability | ELEMENT | FALSE |  |  |
| 9 | List of PDU sessions for handover | LIST |  |  | *PDU Session Resources To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 |
| 10 | >PDU session Item for handover | STRUCTURE |  |  | *PDU Session Resources To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 |
| 11 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.423 [15] Section 9.2.3.18 |  |
| 12 | >>List of QoS flows in the PDU session | LIST |  |  | *QoS Flows To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 |
| 13 | >>>QoS flow Item | STRUCTURE |  |  | *QoS Flow To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 |
| 14 | >>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 15 | Candidate target primary cell global ID for NG handover | STRUCTURE |  |  | *Target Cell ID* IE in TS 38.413 [11] Section 9.3.1.73 |
| 16 | >CHOICE *Target Cell* | STRUCTURE |  |  | *Target Cell* IE in TS 38.423 [15] Section 9.2.3.25 |
| 17 | >>NR Cell | STRUCTURE |  |  | *NR* IE in TS 38.423 [15] Section 9.2.3.25 |
| 18 | >>>NR CGI | ELEMENT | FALSE | *NR CGI* IE in TS 38.423 [15] Section 9.2.2.7 |  |
| 19 | >>E-UTRA Cell | STRUCTURE |  |  | *E-UTRA* IE in TS 38.423 [15] Section 9.2.3.25 |
| 20 | >>>E-UTRA CGI | ELEMENT | FALSE | *E-UTRA CGI* IE in TS 38.423 [15] Section 9.2.2.8 |  |
| 21 | List of DRBs for handover | LIST |  |  | *DRB To Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 22 | >DRB item for handover | STRUCTURE |  |  | *DRB To Be Setup Item* IE in TS 38.473 [19] Section 9.2.2.1 |
| 23 | >>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.473 [19] Section 9.3.1.8 |  |
| 24 | >>List of QoS flows in the DRB | LIST |  |  | *Flows Mapped To DRB Item* IE in TS 38.473 [19] Section 9.2.2.1 |
| 25 | >>>QoS flow Item | STRUCTURE |  |  |  |
| 26 | >>>>QoS flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.473 [19] Section 9.3.1.63 |  |
| 27 | List of Secondary cells to be setup | LIST |  |  | *SCell To Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 28 | >Secondary cell Item to be setup | STRUCTURE |  |  | *SCell To Be Setup Item IEs* IE in TS 38.473 [19] Section 9.2.2.1 |
| 29 | >>Secondary cell ID | ELEMENT | FALSE | *SCell ID* IE in TS 38.473 [19] Section 9.2.2.1 |  |

#### 8.4.4.3 DAPS Handover Control

Upon receiving the *RIC Control Request* message, in the case of Xn/X2 DAPS handovers, the E2 node shall invoke procedures, such as *Handover Preparation* related to UE Mobility Management, *Bearer Context Modification, UE Context Modification*, *RRC Message Transfer*, etc. In the case of intra-gNB or F1 DAPS handover, the E2 node shall invoke procedures, such as *UE Context Modification*, *RRC Message Transfer*, etc. The E2 node includes the IEs corresponding to one or more of parameters described below in the related interface messages. If the *Target Primary Cell ID* IE is missing in the *RIC Control Request* message, the E2 node will send a *RIC Control Failure* message.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Param** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | Target Primary Cell ID | STRUCTURE |  |  | *Target Cell Global ID* IE in TS 38.423 [15] Section 9.2.3.25 |
| 2 | >CHOICE *Target Cell* | STRUCTURE |  |  | *Target Cell* IE in TS 38.423 [15] Section 9.2.3.25 |
| 3 | >>NR Cell | STRUCTURE |  |  | *NR* IE in TS 38.423 [15] Section 9.2.3.25 |
| 4 | >>>NR CGI | ELEMENT | FALSE | *NR CGI* IE in TS 38.423 [15] Section 9.2.2.7 |  |
| 5 | >>E-UTRA Cell | STRUCTURE |  |  | *E-UTRA* IE in TS 38.423 [15] Section 9.2.3.25 |
| 6 | >>>E-UTRA CGI | ELEMENT | FALSE | *E-UTRA CGI* IE in TS 38.423 [15] Section 9.2.2.8 |  |
| 7 | List of DRBs subject to DAPS handover | LIST |  |  | *Source DRB to QoS Flow Mapping List* IE in TS 38.423 [15] Section 9.2.1.17 |
| 8 | >DRB item for handover | STRUCTURE |  |  | *DRB to QoS Flow Mapping Item* IE in TS 38.423 [15] Section 9.2.1.15 |
| 9 | >>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.423 [15] Section 9.2.3.33 |  |
| 10 | >>List of QoS flows in the DRB | LIST |  |  | *QoS Flows List* IE in TS 38.423 [15] Section 9.2.1.15 |
| 11 | >>>QoS flow Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.423 [15] Section 9.2.1.15 |
| 12 | >>>>QoS flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 13 | >>>>QoS flow mapping indication | ELEMENT | FALSE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.79 |  |
| 14 | List of DRBs subject to handover without DAPS | LIST |  |  | *Source DRB to QoS Flow Mapping List* IE in TS 38.423 [15] Section 9.2.1.17 |
| 15 | >DRB item for handover | STRUCTURE |  |  | *DRB to QoS Flow Mapping Item* IE in TS 38.423 [15] Section 9.2.1.15 |
| 16 | >>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.423 [15] Section 9.2.3.33 |  |
| 17 | >>List of QoS flows in the DRB | LIST |  |  | *QoS Flows List* IE in TS 38.423 [15] Section 9.2.1.15 |
| 18 | >>>QoS flow Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.423 [15] Section 9.2.1.15 |
| 19 | >>>>QoS flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 20 | >>>>QoS flow mapping indication | ELEMENT | FALSE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.79 |  |
| 21 | List of PDU Sessions subject for handover | LIST |  |  | *PDU Session Resources To Setup List* IE in TS 38.423 [15] Section 9.2.1.1 |
| 22 | >PDU Session Item | STRUCTURE |  |  | *PDU Session Resources To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 |
| 23 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.423 [15] Section 9.2.1.1 |  |
| 24 | >>List of DRBs subject to DAPS handover | LIST |  |  | *Source DRB to QoS Flow Mapping List* IE in TS 38.423 [15] Section 9.2.1.17 |
| 25 | >>>DRB item for handover | STRUCTURE |  |  | *DRB to QoS Flow Mapping Item* IE in TS 38.423 [15] Section 9.2.1.15 |
| 26 | >>>>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.423 [15] Section 9.2.3.33 |  |
| 27 | >>>>List of QoS flows in the DRB | LIST |  |  | *QoS Flows List* IE in TS 38.423 [15] Section 9.2.1.15 |
| 28 | >>>>>QoS flow Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.423 [15] Section 9.2.1.15 |
| 29 | >>>>>>QoS flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 30 | >>>>>>QoS flow mapping indication | ELEMENT | FALSE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.79 |  |
| 31 | >>List of DRBs subject to handover without DAPS | LIST |  |  | *Source DRB to QoS Flow Mapping List* IE in TS 38.423 [15] Section 9.2.1.17 |
| 32 | >>>DRB item for handover | STRUCTURE |  |  | *DRB to QoS Flow Mapping Item* IE in TS 38.423 [15] Section 9.2.1.15 |
| 33 | >>>>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.423 [15] Section 9.2.3.33 |  |
| 34 | >>>>List of QoS flows in the DRB | LIST |  |  | *QoS Flows List* IE in TS 38.423 [15] Section 9.2.1.15 |
| 35 | >>>>>QoS flow Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.423 [15] Section 9.2.1.15 |
| 36 | >>>>>>QoS flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 37 | >>>>>>QoS flow mapping Indication | ELEMENT | FALSE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.79 |  |

### 8.4.5 Radio Access Control

#### 8.4.5.1 UE admission control

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to UE admission control, such as *PDU Session Management*, *Bearer Context Management*, *UE Context Management*, *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | | **RAN Parameter Definition** | **Semantics Description** |
| 1 | Primary Cell ID | STRUCTURE |  | |  | *Target Cell Global ID* IE in TS 38.423 [15] clause 9.2.3.25 |
| 2 | >CHOICE *Primary Cell* | STRUCTURE |  | |  | *Target Cell* IE in TS 38.423 [15] clause 9.2.3.25 |
| 3 | >>NR Cell | STRUCTURE |  | |  | *NR* IE in TS 38.423 [15] Section 9.2.3.25 |
| 4 | >>>NR CGI | ELEMENT | FALSE | | *NR CGI* IE in TS 38.423 [15] Section 9.2.2.7 |  |
| 5 | >>E-UTRA Cell | STRUCTURE |  | |  | *E-UTRA* IE in TS 38.423 [15] Section 9.2.3.25 |
| 6 | >>>E-UTRA CGI | ELEMENT | FALSE | | *E-UTRA CGI* IE in TS 38.423 [15] Section 9.2.2.8 |  |
| 7 | List of PDU sessions for admission | LIST |  | |  | *PDU Session Resources To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 |
| 8 | >PDU session Item for admission | STRUCTURE |  | |  | *PDU Session Resources To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 |
| 9 | >>PDU Session ID | ELEMENT | TRUE | | *PDU Session ID* IE in TS 38.423 [15] Section 9.2.3.18 |  |
| 10 | >>List of DRBs for admission | LIST |  | |  | *DRB to Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 11 | >>>DRB item for admission | STRUCTURE |  | |  | *DRB to Be Setup Item* IE in TS 38.473 [19] Section 9.2.2.1 |
| 12 | >>>>DRB ID | ELEMENT | TRUE | | *DRB ID* IE in TS 38.473 [19] Section 9.3.1.8 |  |
| 13 | >>>>List of QoS flows in the DRB | LIST |  | |  | *QoS Flows Information To Be Setup* IE in TS 38.463 [21] Section 9.3.3.2 |
| 14 | >>>>>QoS flow Item | STRUCTURE |  | |  | *QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.25 |
| 15 | >>>>>>QoS flow Identifier | ELEMENT | TRUE | | *QoS Flow Identifier* IE in TS 38.463 [21] Section 9.3.1.25 |  |
| 16 | >>>>>>QoS flow mapping indication | ELEMENT | TRUE | | *QoS Flow Mapping Indication* IE in TS 38.463 [21] Section 9.3.1.60 |  |
| 17 | >>>List of cell groups to be added | LIST |  |  | | *Cell Group To Add* IE in TS 38.463 [21] Section 9.3.3.11 | |
| 18 | >>>>Cell group item | STRUCTURE |  |  | | *Cell Group Item* IE in TS 38.463 [21] Section 9.3.1.11 | |
| 19 | >>>>>Cell Group ID | ELEMENT | TRUE | *Cell Group ID* IE in TS 38.463 [21] Section 9.3.1.11 | |  | |
| 20 | >>>SDAP Configuration | STRUCTURE |  |  | | *SDAP Configuration* IE in TS 38.463 [21] Section 9.3.1.39 | |
| 21 | >>>Default DRB | ELEMENT | FALSE | *Default DRB* IE in TS 38.463 [21] Section 9.3.1.39 | |  | |
| 22 | >>>PDCP Configuration | STRUCTURE |  |  | | *PDCP Configuration* IE in TS 38.463 [21] Section 9.3.1.38 | |
| 23 | >>>RLC mode | ELEMENT | FALSE | *RLC mode* IE in TS 38.463 [21] Section 9.3.1.38 | |  | |
| 24 | >>>PDCP Duplication | ELEMENT | FALSE | *PDCP Duplication* IE in TS 38.463 [21] Section 9.3.1.38 | |  | |
| 25 | >>>UL Data Split Threshold | ELEMENT | FALSE | *UL Data Split Threshold* IE in TS 38.463 [21] Section 9.3.1.43 | |  | |
| 26 | >>>PDCP Re-establishment | ELEMENT | FALSE | *PDCP Re-establishment* IE in TS 38.463 [21] Section 9.3.1.38 | |  | |
| 27 | >>>PDCP Data Recovery | ELEMENT | FALSE | *PDCP Data Recovery* IE in TS 38.463 [21] Section 9.3.1.38 | |  | |
| 28 | >>>Out-of-Order Delivery | ELEMENT | FALSE | *Out of Order Delivery* IE in TS 38.463 [21] Section 9.3.1.38 | |  | |
| 29 | >>>PDCP Status Report Indication | ELEMENT | FALSE | *PDCP Status Report Indication* IE in TS 38.463 [21] Section 9.3.1.38 | |  | |
| 30 | >>>Number of PDCP duplication | ELEMENT | FALSE | *Additional PDCP duplication Information* IE in TS 38.463 [21] Section 9.3.1.38 | |  | |
| 31 | >>>UL More than one RLC | STRUCTURE |  |  | | *moreThanOneRLC* IE in TS 38.331 [22] Section 6 | |
| 32 | >>>>Primary Path | STRUCTURE |  |  | | *primaryPath* IE in TS 38.331 [22] Section 6 | |
| 33 | >>>>>Cell Group ID | ELEMENT | TRUE | *cellGroup* IE in TS 38.331 [22] Section 6 | |  | |
| 34 | >>>>>Logical Channel ID | ELEMENT | FALSE | *logicalChannel* IE in TS 38.331 [22] Sec 6 | |  | |
| 35 | >>>UL More than two RLC | STRUCTURE |  |  | | *moreThanTwoRLC-DRB-r16* IE in TS 38.331 [22] Section 6 | |
| 36 | >>>>Split Secondary Path | ELEMENT | FALSE | *splitSecondaryPath* IE in TS 38.331 [22] Sec 6 | |  | |
| 37 | >>>>Duplication State | ELEMENT | FALSE | *duplicationState* IE in TS 38.331 [22] Sec 6 | |  | |
| 38 | >>>DL More than one RLC | STRUCTURE |  |  | | *moreThanOneRLC* IE in TS 38.331 [22] Section 6 | |
| 39 | >>>>Primary Path | STRUCTURE |  |  | | *primaryPath* IE in TS 38.331 [22] Section 6 | |
| 49 | >>>>>Cell Group ID | ELEMENT | TRUE | *cellGroup* IE in TS 38.331 [22] Section 6 | |  | |
| 50 | >>>>>Logical Channel ID | ELEMENT | FALSE | *logicalChannel* IE in TS 38.331 [22] Sec 6 | |  | |
| 51 | >>>DL More than two RLC | STRUCTURE |  |  | | *moreThanTwoRLC-DRB-r16* IE in TS 38.331 [22] Section 6 | |
| 52 | >>>>Split Secondary Path | ELEMENT | FALSE | *splitSecondaryPath* IE in TS 38.331 [22] Sec 6 | |  | |
| 53 | >>>>Duplication State | ELEMENT | FALSE | *duplicationState* IE in TS 38.331 [22] Sec 6 | |  | |
| 54 | List of Secondary cells to be setup | LIST |  | |  | *Scell To Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 55 | >Secondary cell Item to be setup | STRUCTURE |  | |  | *Scell To Be Setup Item Ies* IE in TS 38.473 [19] Section 9.2.2.1 |
| 56 | >>Secondary cell ID | ELEMENT | FALSE | | *Scell ID* IE in TS 38.473 [19] Section 9.2.2.1 |  |

#### 8.4.5.2 RACH backoff control

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to RACH backoff control, such as *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | Common RACH Config Parameters | STRUCTURE |  |  | *RACH-ConfigGeneric* IE in TS 38.331 [22] Section 6 |
| 2 | >PRACH Configuration Index | ELEMENT | FALSE | *prach-ConfigurationIndex* IE in TS 38.331 [22] Sec 6 |  |
| 3 | >Zero correlation Zone Config | ELEMENT | FALSE | *zeroCorrelationZoneConfig* IE in TS 38.331 [22] Sec 6 |  |
| 4 | >Preamble Received Target Power | ELEMENT | FALSE | *preambleReceivedTargetPower* IE in TS 38.331 [22] Section 6 |  |
| 5 | >Preamble Transmission Max | ELEMENT | FALSE | *preambleTransMax* IE in TS 38.331 [22] Sec 6 |  |
| 6 | >Power Ramping Step High Priority | ELEMENT | FALSE | *powerRampingStep* IE in TS 38.331 [22] Sec 6 |  |
| 7 | >Random Access Response Window | ELEMENT | FALSE | *ra-ResponseWindow* IE in TS 38.331 [22] Sec 6 |  |
| 8 | Dedicated RACH Config Parameters | STRUCTURE |  |  | *RACH-ConfigDedicated* IE in TS 38.331 [22] Section 6 |
| 9 | >Random Access Prioritization | STRUCTURE |  |  | *RA-Prioritization* IE in TS 38.331 [22] Sec 6 |
| 10 | >>Scaling Factor for Backoff Indicator | ELEMENT | FALSE | *scalingFactorBI* IE in TS 38.331 [22] Sec 6 |  |
| 11 | >>Power Ramping Step High Priority | ELEMENT | FALSE | *powerRampingStepHighPriority* IE in TS 38.331 [22] Section 6 |  |

#### 8.4.5.3 Access barring control

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to Access barring control, such as *UE Context Management*, *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Param** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | Unified Access Control Barring Info | STRUCTURE |  |  | *uac-BarringInfo* IE in TS 38.331 [22] Sec 6 |
| 2 | >UAC Barring for Common List | LIST |  |  | *uac-BarringForCommon* IE in TS 38.331 [22] Sec 6 |
| 3 | >>Barring Per Cat | STRUCTURE |  |  | *UAC-BarringPerCat* IE in TS 38.331 [22] Section 6 |
| 4 | >>>Access Category | ELEMENT | FALSE | *accessCategory* IE in TS 38.331 [22] Sec 6 |  |
| 5 | >>>Barring Info Set Index | ELEMENT | FALSE | *UAC-BarringInfoSetIndex* IE in TS 38.331 [22] Section 6 |  |
| 6 | >UAC Barring for PLMN List | LIST |  |  | *uac-BarringPerPLMN-List* IE in TS 38.331 [22] Section 6 |
| 7 | >>UAC-BarringPerPLMN | STRUCTURE |  |  | *UAC-BarringPerPLMN* IE in TS 38.331 [22] Sec 6 |
| 8 | >>>PLMN Identity Index | ELEMENT | TRUE | *plmn-IdentityIndex* IE in TS 38.331 [22] Sec 6 |  |
| 9 | >>>CHOICE UAC AC Barring List Type | STRUCTURE |  |  | *Uac-ACBarringListType* IE in TS 38.331 [22] Sec 6 |
| 10 | >>>>UAC Implicit AC Barring List | LIST |  |  | *uac-ImplicitACBarringList* IE in TS 38.331 [22] Section 6 |
| 11 | >>>>>UAC Implicit AC Barring Item | STRUCTURE |  |  |  |
| 12 | >>>>>>UAC Barring Info Set Index | ELEMENT | FALSE | *UAC-BarringInfoSetIndex* IE in TS 38.331 [22] Sec 6 |  |
| 13 | >>>>UAC Explicit AC Barring List | LIST |  |  | *uac-ExplicitACBarringList* IE in TS 38.331 [22] Section 6 |
| 14 | >>>>>Barring Per Cat | STRUCTURE |  |  | *UAC-BarringPerCat* IE in TS 38.331 [22] Section 6 |
| 15 | >>>>>>Access Category | ELEMENT | FALSE | *accessCategory* IE in TS 38.331 [22] Sec 6 |  |
| 16 | >>>>>>Barring Info Set Index | ELEMENT | FALSE | *UAC-BarringInfoSetIndex* IE in TS 38.331 [22] Section 6 |  |
| 17 | >UAC Barring Info Set List | LIST |  |  | *UAC-BarringInfoSetList* IE in TS 38.331 [22] Sec 6 |
| 18 | >>UAC Barring Info Set Item | STRUCTURE |  |  | *UAC-BarringInfoSet* IE in TS 38.331 [22] Section 6 |
| 19 | >>>UAC Barring Factor | ELEMENT | FALSE | *uac-BarringFactor* IE in TS 38.331 [22] Sec 6 |  |
| 20 | >>>UAC Barring Time | ELEMENT | FALSE | *uac-BarringTime* IE in TS 38.331 [22] Sec 6 |  |
| 21 | >>>UAC Barring For Access Identity | ELEMENT | FALSE | *uac-BarringForAccessIdentity* in TS 38.331 [22] Section 6 |  |
| 22 | >CHOICE Access Category 1 – Selection Assistance Info | STRUCTURE |  |  | *uac-AccessCategory1-SelectionAssistanceInfo* IE in TS 38.331 [22] Sec 6 |
| 23 | >>PLMN Common | ELEMENT | FALSE | *UAC-AccessCategory1-SelectAssistanceInfo* IE in TS 38.331 [22] Section 6 |  |
| 24 | >>Individual PLMN List | LIST |  |  | *individualPLMNList* IE in TS 38.331 [22] Section 6 |
| 25 | >>>PLMN Item | STRUCTURE |  |  |  |
| 26 | >>>>UAC Access Category 1 Selection Assistance Info | ELEMENT | FALSE | *UAC-AccessCategory1-SelectAssistanceInfo* IE in TS 38.331 [22] Section 6 |  |

#### 8.4.5.4 RRC Connection Release Control

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to RRC Connection Release control, such as *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | | Semantics Description | |
| 1 | CHOICE Redirected Carrier Info | STRUCTURE |  |  | | *redirectedCarrierInfo* IE in TS 36.331 [23] | |
| 2 | >E-UTRA | STRUCTURE |  | *eutra* IE in TS 36.331 [23] | |  | |
| 3 | >>EARFCN | ELEMENT | FALSE | *ARFCN-ValueEUTRA* IE in TS 36.331 [23] | |  | |
| 4 | >NR | STRUCTURE |  | *nr-r15* IE in TS 36.331 [23] | |  | |
| 5 | >>Carrier Info NR | STRUCTURE |  |  | | *CarrierInfoNR-r15* IE in TS 36.331 [23] | |
| 6 | >>>Carrier Frequency | ELEMENT | FALSE | *ARFCN-ValueNR-r15* IE in TS 36.331 [23] | |  | |
| 7 | >>>Subcarrier Spacing SSB | ELEMENT | FALSE | *subcarrierSpacingSSB-r15* IE in TS 36.331 [23] | |  | |
| 8 | Idle Mode Mobility Control Info | STRUCTURE |  |  | | *IdleModeMobilityControlInfo* IE in TS 36.331 [23] | |
| 9 | >Frequency Priority List E-UTRA | LIST |  |  | *FreqPriorityListEUTRA* IE in TS 36.331 [23] | |
| 10 | >>Frequency Priority Item E-UTRA | STRUCTURE |  |  | *FreqPriorityEUTRA* IE in TS 36.331 [23] | |
| 11 | >>>Carrier Frequency | ELEMENT | FALSE | carrierFreq IE in TS 38.331 [22] |  | |
| 12 | >>>Cell Reselection Priority | ELEMENT | FALSE | *cellReselectionPriority* IE in TS 38.331 [22] |  | |
| 13 | >>>Cell Reselection Sub Priority | ELEMENT | FALSE | *cellReselectionSubPriority* IE in TS 38.331 [22] |  | |
| 14 | >Frequency Priority List NR | LIST |  |  | *FreqPriorityListNR* IE in TS 38.331 [22] | |
| 15 | >>Frequency Priority Item NR | STRUCTURE |  |  | *FreqPriorityNR* IE in TS 38.331 [22] | |
| 16 | >>>Carrier Frequency | ELEMENT | FALSE | *carrierFreq* IE in TS 38.331 [22] |  | |
| 17 | >>>Cell Reselection Priority | ELEMENT | FALSE | *cellReselectionPriority* IE in TS 38.331 [22] |  | |
| 18 | >>>Cell Reselection Sub Priority | ELEMENT | FALSE | *cellReselectionSubPriority* IE in TS 38.331 [22] |  | |
| 19 | >T-320 timer expiry | ELEMENT | FALSE | *t320* IE in TS 38.331 [22] |  | |

#### 8.4.5.5 RRC Connection Reject Control

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to RRC Connection Reject, such as *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | Semantics Description |
| 1 | Wait Time | ELEMENT | FALSE | *waitTime* IE in TS 36.331 [23] |  |
| 2 | Deprioritization Requirement | STRUCTURE |  |  | *deprioritisationReq-r11* IE in TS 36.331 [23] |
| 3 | >Deprioritization Type | ELEMENT | FALSE | *deprioritisationType-r11* IE in TS 36.331 [23] |  |
| 4 | >Deprioritization Timer | ELEMENT | FALSE | *deprioritisationTimer-r11* IE in TS 36.331 [23] |  |
| 5 | RRC Suspend Indication | ELEMENT | FALSE | *rrc-SuspendIndication-r13* IE in TS 36.331 [23] |  |

### 8.4.6 Dual Connectivity Control

#### 8.4.6.1 DC Secondary Node Addition Control

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to DC Secondary Node Addition Control, such as *Dual Connectivity Secondary Node Addition*, *UE Context Management*, *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages. If the *Secondary Node ID* is missing in the *RIC Control Request* message, the E2 node will send a *RIC Control Failure*.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | Secondary Node ID | STRUCTURE |  |  | *Global NG-RAN Node ID* IE in TS 38.423 [15] Section 9.2.2.3 |
| 2 | >CHOICE Secondary Node Type | STRUCTURE |  |  |  |
| 3 | >>Secondary Node gNB | STRUCTURE |  |  | *Global ng-eNB ID* IE in TS 38.423 [15] Section 9.2.2.1 |
| 4 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.423 [15] Section 9.2.2.4 |  |
| 5 | >>>gNB ID | ELEMENT | FALSE | *gNB ID* IE in TS 38.423 [15] Section 9.2.2.1 |  |
| 6 | >>Secondary Node ng-eNB | STRUCTURE |  |  | *Global ng-eNB ID* IE in TS 38.423 [15] Section 9.2.2.2 |
| 7 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.423 [15] Section 9.2.2.4 |  |
| 8 | >>>ng-eNB ID | ELEMENT | FALSE | *Long Macro ng-eNB ID* IE in TS 38.423 [15] Section 9.2.2.2 |  |
| 9 | >>Secondary Node en-gNB | STRUCTURE |  |  | *en-gNB* IE in TS 36.423 [17] Sec |
| 10 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 36.423 [17] Section 9.2.4 |  |
| 11 | >>>en-gNB ID | ELEMENT | FALSE | *Global en-gNB ID* IE in TS 36.423 [17] Section 9.2.4 |  |
| 12 | List of PDU Sessions to be Added | LIST |  |  | *PDU Session Resources To Be Added List* IE in TS 38.423 [15] Section 9.1.2.1 |
| 13 | >PDU Session to be Added Item | STRUCTURE |  |  | *PDU Session Resources To Be Added Item* IE in TS 38.423 [15] Section 9.1.2.1 |
| 14 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.423 [15] Section 9.2.3.18 |  |
| 15 | >>PDU Session Resource Setup Info – SN-Terminated | STRUCTURE |  |  | *PDU Session Resource Setup Info – SN Terminated* IE in TS 38.423 [15] Section 9.2.1.5 |
| 16 | >>>QoS Flow To Be Setup List | LIST |  |  | *QoS Flows To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.5 |
| 17 | >>>>QoS Flow Item | STRUCTURE |  |  | *QoS Flows To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.5 |
| 18 | >>>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 19 | >>>>>QoS Flow Mapping Indication | ELEMENT | FALSE | *QoS Flow Mapping Indication* IE in TS 38.423 [15] Section 9.2.3.79 |  |
| 20 | >>>Default DRB allowed | ELEMENT | FALSE | *Default DRB Allowed* IE in TS 38.423 [15] Section 9.2.3.93 |  |
| 21 | >>PDU Session Resource Setup Info – MN-Terminated | STRUCTURE |  |  | *PDU Session Resource Setup Info – SN Terminated* IE in TS 38.423 [15] Section 9.2.1.7 |
| 22 | >>>DRBs To Be Setup List | STRUCTURE |  |  | *DRBs To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.7 |
| 23 | >>>>DRB To Be Setup Item | STRUCTURE |  |  | *DRBs To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.7 |
| 24 | >>>>>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.463 [21] Section 9.3.1.16 |  |
| 25 | >>>>>QoS Flow To Be Setup List | LIST |  |  | *QoS Flows To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.5 |
| 26 | >>>>>>QoS Flow Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.423 [15] Section 9.2.3.10 |
| 27 | >>>>>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 28 | >>>>>>>QoS Flow Mapping Indication | ELEMENT | FALSE | *QoS Flow Mapping Indication* IE in TS 38.423 [15] Section 9.2.3.79 |  |
| 29 | List of SN-terminated DRB IDs | LIST |  |  | *Additional DRB IDs* IE in TS 38.423 [15] Section 9.2.1.29 |
| 30 | >SN-Terminated DRB Item | STRUCTURE |  |  |  |
| 31 | >>DRB Identity | ELEMENT | TRUE | *DRB ID* IE in TS 38.473 [19] Section 9.3.1.8 |  |
| 32 | List of E-RABs to be Added | LIST |  |  | *E-RABs To Be Added List* IE in TS 36.423 [17] Section 9.1.4.1 |
| 33 | >E-RAB to be Added Item | STRUCTURE |  |  | *E-RABs To Be Added Item* IE in TS 36.423 [17] Section 9.1.4.1 |
| 34 | >>E-RAB ID | ELEMENT | TRUE | *E-RAB ID* IE in TS 36.423 [17] Section 9.2.23 |  |
| 35 | >>EN-DC Resource Configuration | STRUCTURE |  |  | *EN-DC Resource Configuration* IE in TS 36.423 [17] Section 9.2.108 |
| 36 | >>>PDCP at SgNB | ELEMENT | FALSE | *PDCP at SgNB* IE in TS 36.423 [17] Section 9.2.108 |  |
| 37 | >>>MCG Resources | ELEMENT | FALSE | *MCG resources* IE in TS 36.423 [17] Section 9.2.108 |  |
| 38 | >>>SCG Resources | ELEMENT | FALSE | *SCG resources* IE in TS 36.423 [17] Section 9.2.108 |  |

#### 8.4.6.2 DC Secondary Node Modification Control

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to DC Secondary Node Modification Control, such as *Dual Connectivity Secondary Node Modification*, *UE Context Management*, *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | Semantics Description |
| 1 | Secondary Node | STRUCTURE |  |  | *Global NG-RAN Node ID* IE in TS 38.423 [15] Section 9.2.2.3 |
| 2 | CHOICE Secondary Node Type | STRUCTURE |  |  |  |
| 3 | >Secondary Node gNB | STRUCTURE |  |  | *Global gNB ID* IE in TS 38.423 [15] Section 9.2.2.1 |
| 4 | >>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.423 [15] Section 9.2.2.4 |  |
| 5 | >>gNB ID | ELEMENT | FALSE | *gNB ID* IE in TS 38.423 [15] Section 9.2.2.1 |  |
| 6 | >Secondary Node ng-eNB | STRUCTURE |  |  | *Global ng-eNB ID* IE in TS 38.423 [15] Section 9.2.2.2 |
| 7 | >>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.423 [15] Section 9.2.2.4 |  |
| 8 | >>ng-eNB ID | ELEMENT | FALSE | *Long Macro ng-eNB ID* IE in TS 38.423 [15] Section 9.2.2.2 |  |
| 9 | >Secondary Node en-gNB | STRUCTURE |  |  | *en-gNB* IE in TS 36.423 [17] Sec |
| 10 | >>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 36.423 [17] Section 9.2.4 |  |
| 11 | >>en-gNB ID | ELEMENT | FALSE | *Global en-gNB ID* IE in TS 36.423 [17] Section 9.2.4 |  |
| 12 | List of PDU Session Resources to be modified | LIST |  |  | PDU Session Resources To Be Modified List IE in TS 38.423 [15] Section 9.1.2.5 |
| 13 | >PDU Session Resource to be Modified Item | STRUCTURE |  |  | PDU Session Resources To Be Modified Item IE in TS 38.423 [15] Section 9.1.2.5 |
| 14 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.423 [15] Section 9.2.3.18 |  |
| 15 | >>PDU Session Resource Modification Info – SN-Terminated | STRUCTURE |  |  | PDU Session Resource Modification Info – SN Terminated IE in TS 38.423 [15] Section 9.2.1.9 |
| 16 | >>>QoS Flows To Be Setup List | LIST |  |  | *QoS Flows To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.9 |
| 17 | >>>>QoS Flow Item | STRUCTURE |  |  | *QoS Flows To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.9 |
| 18 | >>>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 19 | >>>>>QoS Flow Mapping Indication | ELEMENT | FALSE | *QoS Flow Mapping Indication* IE in TS 38.423 [15] Section 9.2.3.79 |  |
| 20 | >>>>>Redundant QoS Flow Indicator | ELEMENT | FALSE |  |  |
| 21 | >>>QoS Flows To Be Modified List | LIST |  |  | *QoS Flows To Be Modified List* IE in TS 38.423 [15] Section 9.2.1.9 |
| 22 | >>>>QoS Flow Item | STRUCTURE |  |  | *QoS Flows To Be Modified Item* IE in TS 38.423 [15] Section 9.2.1.9 |
| 23 | >>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 24 | >>>>QoS Flow Mapping Indication | ELEMENT | FALSE | *QoS Flow Mapping Indication* IE in TS 38.423 [15] Section 9.2.3.79 |  |
| 25 | >>>>Redundant QoS Flow Indicator | ELEMENT | FALSE | *Redundant QoS Flow Indicator* IE in TS 38.423 [15] Section 9.2.3.118 |  |
| 26 | >>>QoS Flows To Be Released List | LIST |  |  | *QoS Flows To Be Released List* IE in TS 38.423 [15] Section 9.2.1.9 |
| 27 | >>>>QoS Flow Item | STRUCTURE |  |  | *QoS Flow With Cause Item* IE in TS 38.423 [15] Section 9.2.1.4 |
| 28 | >>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 29 | >>>Default DRB allowed | ELEMENT | FALSE | *Default DRB Allowed* IE in TS 38.423 [15] Section 9.2.3.93 |  |
| 30 | >>PDU Session Resource Modification Info – MN-Terminated | STRUCTURE |  |  | *PDU Session Resource Modification Info – MN Terminated* IE in TS 38.423 [15] Section 9.2.1.11 |
| 31 | >>>DRBs to be setup list | LIST |  |  | *DRBs To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.11 |
| 32 | >>>>DRBs to be setup item | STRUCTURE |  |  | *DRBs To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.11 |
| 33 | >>>>>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.463 [21] Section 9.3.1.16 |  |
| 34 | >>>>>DRB QoS | STRUCTURE |  |  |  |
| 35 | >>>>>PDCP Duplication Activation | ELEMENT | TRUE | *Duplication Activation* IE in TS 38.463 [21] Section 9.2.3.71 |  |
| 36 | >>>>>QoS Flows Mapped to DRB List | LIST |  |  | *QoS Flows Mapped to DRB List* IE in TS 38.463 [21] Section 9.2.1.11 |
| 37 | >>>>>>QoS Flows Mapped to DRB Item | STRUCTURE |  |  | *QoS Flows Mapped To DRB Item* IE in TS 38.463 [21] Section 9.2.1.11 |
| 38 | >>>>>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 39 | >>>>>>>QoS Flow Mapping Indication | ELEMENT | FALSE | *QoS Flow Mapping Indication* IE in TS 38.423 [15] Section 9.2.3.79 |  |
| 40 | >>>DRBs to be modified list | LIST |  |  | *DRBs To Be Modified List* IE in TS 38.463 [21] Section 9.2.1.11 |
| 41 | >>>>DRB to be modified item | STRUCTURE |  |  | *DRBs To Be Modified Item* IE in TS 38.463 [21] Section 9.2.1.11 |
| 42 | >>>>>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.463 [21] Section 9.3.1.16 |  |
| 43 | >>>>>DRB QoS | STRUCTURE |  |  |  |
| 44 | >>>>>PDCP Duplication Configuration | ELEMENT | FALSE | *PDCP Duplication Configuration* IE in TS 38.463 [21] Section 9.2.3.86 |  |
| 45 | >>>>>PDCP Duplication Activation | ELEMENT | FALSE | *Duplication Activation* IE in TS 38.463 [21] Section 9.2.3.71 |  |
| 46 | >>>>>QoS Flows Mapped to DRB List | LIST |  |  | *Flow Mapping Information* IE in TS 38.463 [21] Section 9.3.1.26 |
| 47 | >>>>>>QoS Flows Mapped to DRB Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.25 |
| 48 | >>>>>>>QoS Flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 49 | >>>>>>>QoS Flow Mapping Indication | ELEMENT | FALSE | *QoS Flow Mapping Indication* IE in TS 38.423 [15] Section 9.2.3.79 |  |
| 50 | >>>DRBs to be released list | LIST |  |  | *DRBs To Be Released List* IE in TS 38.423 [15] Section 9.2.1.28 |
| 51 | >>>>DRB to be released item | STRUCTURE |  |  | *DRBs To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.11 |
| 52 | >>>>>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.463 [21] Section 9.3.1.16 |  |
| 53 | List of PDU Session Resources to be deleted | LIST |  |  | *PDU Session Resources To Be Released List* IE in TS 38.423 [15] Section 9.1.2.5 |
| 54 | >PDU Session Resource to be deleted Item | STRUCTURE |  |  | *PDU Session Resource To Be Released Item* IE |
| 55 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.423 [15] Section 9.2.3.18 |  |
| 56 | List of E-RABs to be Modified | LIST |  |  | *E-RABs To Be Modified List* IE in TS 36.423 [17] Section 9.1.4.5 |
| 57 | >E-RAB to be Modified Item | STRUCTURE |  |  | *E-RAB To Be Modified Item* IE in TS 36.423 [17] Section 9.1.4.5 |
| 58 | >>E-RAB ID | ELEMENT | TRUE | *E-RAB ID* IE in TS 36.423 [17] Section 9.2.23 |  |
| 59 | >>EN-DC Resource Configuration | STRUCTURE |  |  | *EN-DC Resource Configuration* IE in TS 36.423 [17] Section 9.2.108 |
| 60 | >>>PDCP at SgNB | ELEMENT | FALSE | *PDCP at SgNB* IE in TS 36.423 [17] Section 9.2.108 |  |
| 61 | >>>MCG Resources | ELEMENT | FALSE | *MCG resources* IE in TS 36.423 [17] Section 9.2.108 |  |
| 62 | >>>SCG Resources | ELEMENT | FALSE | *SCG resources* IE in TS 36.423 [17] Section 9.2.108 |  |
| 63 | List of E-RABs to be Released | LIST |  |  | *E-RABs To Be Released List* IE in TS 36.423 [17] Section 9.1.4.5 |
| 64 | >E-RAB to be Released Item | STRUCTURE |  |  | *E-RABs To Be Released Item* IE in TS 36.423 [17] Section 9.1.4.5 |
| 65 | >>E-RAB ID | ELEMENT | TRUE | *E-RAB ID* IE in TS 36.423 [17] Section 9.2.23 |  |

#### 8.4.6.3 PSCell Change control for Secondary Cell Group

Upon receiving the *RIC Control Request* message, in the case of intra-SN PSCell change, the E2 node shall invoke procedures related to PSCell Change Control, such as *Dual Connectivity Secondary Node Modification*, *UE Context Modification*, *RRC Message Transfer*, etc. In the case of inter-SN PSCell change, the E2 node shall invoke procedures such as *Dual Connectivity Secondary Node Release* (MN/SN-initiated) or *SN Change* (only SN-initiated), *Bearer Context Modification*, *UE Context Modification*, *RRC Message Transfer*, etc. The E2 node then includes the IEs corresponding to one or more of parameters described below in the related interface messages.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | | Semantics Description |
| 1 | Target PSCell ID | STRUCTURE |  |  | | *Target Cell Global ID* IE in TS 38.423 [15] Section 9.2.3.25 |
| 2 | >CHOICE Target Cell | STRUCTURE |  |  | | *Target Cel*l IE in TS 38.423 [15] Section 9.2.3.25 |
| 3 | >>NR Cell | STRUCTURE |  |  | | *NR* IE in TS 38.423 [15] Section 9.2.3.25 |
| 4 | >>>NR CGI | ELEMENT | FALSE | *NR CGI* IE in TS 38.423 [15] Section 9.2.2.7 | |  |
| 5 | >>E-UTRA Cell | STRUCTURE |  |  | | *E-UTRA* IE in TS 38.423 [15] Section 9.2.3.25 |
| 6 | >>>E-UTRA CGI | ELEMENT | FALSE | *E-UTRA CGI* IE in TS 38.423 [15] Section 9.2.2.8 | |  |
| 7 | Secondary Node ID | STRUCTURE |  |  | | *Global NG-RAN Node ID* IE in TS 38.423 [15] Section 9.2.2.3 |
| 8 | >CHOICE Secondary Node Type | STRUCTURE |  |  | |  |
| 9 | >>Secondary Node gNB | STRUCTURE |  |  | | *Global gNB ID* IE in TS 38.423 [15] Section 9.2.2.1 |
| 10 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.423 [15] Section 9.2.2.4 | |  |
| 11 | >>>gNB ID | ELEMENT | FALSE | *gNB ID* IE in TS 38.423 [15] Section 9.2.2.1 | |  |
| 12 | >>Secondary Node ng-eNB | STRUCTURE |  |  | | *Global ng-eNB ID* IE in TS 38.423 [15] Section 9.2.2.2 |
| 13 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.423 [15] Section 9.2.2.4 | |  |
| 14 | >>>ng-eNB ID | ELEMENT | FALSE | *Long Macro ng-eNB ID* IE in TS 38.423 [15] Section 9.2.2.2 | |  |
| 15 | >>Secondary Node en-gNB | STRUCTURE |  |  | | *en-gNB* IE in TS 36.423 [17] Sec |
| 16 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 36.423 [17] Section 9.2.4 | |  |
| 17 | >>>en-gNB ID | ELEMENT | FALSE | *Global en-gNB ID* IE in TS 36.423 [17] Section 9.2.4 | |  |
| 18 | PDU Session SN Change Required List | LIST |  |  | | *PDU Session SN Change Required List* IE in TS 38.423 [15] Section 9.1.2.11 |
| 19 | >PDU Session SN Change Required Item | STRUCTURE |  |  | | *PDU Session SN Change Required Item* IE in TS 38.423 [15] Section 9.1.2.11 |
| 20 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.423 [15] Section 9.2.3.18 | |  |
| 21 | >>List of QoS flows in the PDU session | LIST |  | |  | *QoS Flows To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 |
| 22 | >>>QoS flow Item | STRUCTURE |  | |  | *QoS Flow To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 |
| 23 | >>>>QoS Flow Identifier | ELEMENT | TRUE | | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 |  |
| 24 | List of DRBs for PSCell handover | LIST |  |  | | *DRB to Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 25 | >DRB item for PSCell handover | STRUCTURE |  |  | | *DRB to Be Setup Item* IE in TS 38.473 [19] Section 9.2.2.1 |
| 26 | >>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.473 [19] Section 9.3.1.8 | |  |
| 27 | >>List of QoS flows in the DRB | LIST |  |  | | *QoS Flows Information To Be Setup* IE in TS 38.463 [21] Section 9.3.3.2 |
| 28 | >>>QoS flow Item | STRUCTURE |  |  | | *QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.25 |
| 29 | >>>>QoS flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.463 [21] Section 9.3.1.25 | |  |

#### 8.4.6.4 DC Secondary Node Change Control

Upon receiving the RIC Control Request message, the E2 node shall invoke procedures such as Dual Connectivity Secondary Node Release (MN/SN-initiated) or SN Change (only SN-initiated), Bearer Context Modification, UE Context Modification, RRC Message Transfer, etc. and includes the IEs corresponding to one or more of parameters described below in the related interface messages.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | | Semantics Description | |
| 1 | Target PSCell ID | STRUCTURE |  |  | | *Target Cell Global ID* IE in TS 38.423 [15] Section 9.2.3.25 | |
| 2 | >CHOICE Target Cell | STRUCTURE |  |  | | *Target Cell* IE in TS 38.423 [15] Section 9.2.3.25 | |
| 3 | >>NR Cell | STRUCTURE |  |  | | *NR* IE in TS 38.423 [15] Section 9.2.3.25 | |
| 4 | >>>NR CGI | ELEMENT | FALSE | *NR CGI* IE in TS 38.423 [15] Section 9.2.2.7 | |  | |
| 5 | >>E-UTRA Cell | STRUCTURE |  |  | | *E-UTRA* IE in TS 38.423 [15] Section 9.2.3.25 | |
| 6 | >>>E-UTRA CGI | ELEMENT | FALSE | *E-UTRA CGI* IE in TS 38.423 [15] Section 9.2.2.8 | |  | |
| 7 | Target Secondary Node ID | STRUCTURE |  |  | | *Target S-NG-RAN node ID* IE in TS 38.423 [15] Section 9.1.2.11 | |
| 8 | >CHOICE Target Secondary Node Type | STRUCTURE |  |  | |  | |
| 9 | >>Secondary Node gNB | STRUCTURE |  |  | | *Global gNB ID* IE in TS 38.423 [15] Section 9.2.2.1 | |
| 10 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.423 [15] Section 9.2.2.4 | |  | |
| 11 | >>>gNB ID | ELEMENT | FALSE | *gNB ID* IE in TS 38.423 [15] Section 9.2.2.1 | |  | |
| 12 | >>Secondary Node ng-eNB | STRUCTURE |  |  | | *Global ng-eNB ID* IE in TS 38.423 [15] Section 9.2.2.2 | |
| 13 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 38.423 [15] Section 9.2.2.4 | |  | |
| 14 | >>>ng-eNB ID | ELEMENT | FALSE | *Long Macro ng-eNB ID* IE in TS 38.423 [15] Section 9.2.2.2 | |  | |
| 15 | >>Secondary Node en-gNB | STRUCTURE |  |  | | *en-gNB* IE in TS 36.423 [17] Sec | |
| 16 | >>>PLMN Identity | ELEMENT | FALSE | *PLMN Identity* IE in TS 36.423 [17] Section 9.2.4 | |  | |
| 17 | >>>en-gNB ID | ELEMENT | FALSE | *Global en-gNB ID* IE in TS 36.423 [17] Section 9.2.4 | |  | |
| 18 | PDU Session SN Change Required List | LIST |  |  | | *PDU Session SN Change Required List* IE in TS 38.423 [15] Section 9.1.2.11 | |
| 19 | >PDU Session SN Change Required Item | STRUCTURE |  |  | | *PDU Session SN Change Required Item* IE in TS 38.423 [15] Section 9.1.2.11 | |
| 20 | >>PDU Session ID | ELEMENT | TRUE | *PDU Session ID* IE in TS 38.423 [15] Section 9.2.3.18 | |  | |
| 21 | >>List of QoS flows in the PDU session | LIST |  | |  | | *QoS Flows To Be Setup List* IE in TS 38.423 [15] Section 9.2.1.1 |
| 22 | >>>QoS flow Item | STRUCTURE |  | |  | | *QoS Flow To Be Setup Item* IE in TS 38.423 [15] Section 9.2.1.1 |
| 23 | >>>>QoS Flow Identifier | ELEMENT | TRUE | | *QoS Flow Identifier* IE in TS 38.423 [15] Section 9.2.3.10 | |  |
| 24 | List of DRBs for PSCell handover | LIST |  |  | | *DRB to Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 | |
| 25 | >DRB item for PSCell handover | STRUCTURE |  |  | | *DRB to Be Setup Item* IE in TS 38.473 [19] Section 9.2.2.1 | |
| 26 | >>DRB ID | ELEMENT | TRUE | *DRB ID* IE in TS 38.473 [19] Section 9.3.1.8 | |  | |
| 27 | >>List of QoS flows in the DRB | LIST |  |  | | *QoS Flows Information To Be Setup* IE in TS 38.463 [21] Section 9.3.3.2 | |
| 28 | >>>QoS flow Item | STRUCTURE |  |  | | *QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.25 | |
| 29 | >>>>QoS flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.463 [21] Section 9.3.1.25 | |  | |

### 8.4.7 Carrier Aggregation Control

#### 8.4.7.1 Secondary cell Addition control

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to Secondary cell Addition Control, such as *UE Context Management*, *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | Semantics Description |
| 1 | List of secondary cells to be setup | LIST |  |  | *Scell To Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 2 | >Secondary cell to be setup Item | STRUCTURE |  |  | *Scell To Be Setup Item Ies* IE in TS 38.473 [19] Section 9.2.2.1 |
| 3 | >>Scell Cell Global ID | ELEMENT | FALSE | *Scell ID* IE in TS 38.473 [19] Section 9.2.2.1 |  |
| 4 | >>Scell UL Configured | ELEMENT | FALSE | *Cell UL Configured* IE in TS 38.473 [19] Section 9.3.1.33 |  |
| 5 | List of DRBs to be served using SCells | LIST |  |  | *DRB to Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 6 | >DRB item | STRUCTURE |  |  | *DRB to Be Setup Item* IE in TS 38.473 [19] Section 9.2.2.1 |
| 7 | >>DRB ID | ELEMENT | TRUE | DRB ID IE in TS 38.473 [19] Section 9.3.1.8 |  |
| 8 | >>List of QoS flows in the DRB | LIST |  |  | *QoS Flows Information To Be Setup* IE in TS 38.463 [21] Section 9.3.3.2 |
| 9 | >>>QoS flow Item | STRUCTURE |  |  | *QoS Flow Item* IE in TS 38.463 [21] Section 9.3.1.25 |
| 10 | >>>>QoS flow Identifier | ELEMENT | TRUE | *QoS Flow Identifier* IE in TS 38.463 [21] Section 9.3.1.25 |  |

#### 8.4.7.2 Secondary cell Modification control

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to Secondary cell Modification Control, such as *UE Context Management*, *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | List of secondary cells to be setup | LIST |  |  | *Scell To Be Setup List* IE in TS 38.473 [19] Section 9.2.2.1 |
| 2 | >Secondary cell to be setup Item | STRUCTURE |  |  | *Scell To Be Setup Item Ies* IE in TS 38.473 [19] Section 9.2.2.1 |
| 3 | >>Scell Global ID | ELEMENT | FALSE | *Scell ID* IE in TS 38.473 [19] Section 9.2.2.1 |  |
| 4 | >>Scell UL Configured | ELEMENT | FALSE | *Cell UL Configured* IE in TS 38.473 [19] Section 9.3.1.33 |  |
| 5 | List of Scells to be removed | LIST |  |  | *SCell To Be Removed List* IE in TS 38.473 [19] Section 9.2.2.7 |
| 6 | >Scell to be removed Item | STRUCTURE |  |  | *SCell to Be Removed Item IEs* IE in TS 38.473 [19] Section 9.2.2.7 |
| 7 | >>Scell Global ID | ELEMENT | FALSE | *Scell ID* IE in TS 38.473 [19] Section 9.2.2.1 |  |

### 8.4.8 Idle Mode Mobility Control

#### 8.4.8.1 Cell reselection priority control

Upon receiving the *RIC Control Request* message, the E2 node shall invoke procedures related to cell reselection priority control, such as *RRC Message Transfer*, etc. and include the IEs corresponding to one or more of parameters described below in the related interface messages.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | *Semantics Description* |
| 1 | Cell Reselection Priorities | STRUCTURE |  |  | *IdleModeMobilityControlInfo* IE in TS 36.331 [23] |
| 2 | >Frequency Priority List E-UTRA | LIST |  |  | *FreqPriorityListEUTRA* IE in TS 38.331 [22] |
| 3 | >>Frequency Priority Item E-UTRA | STRUCTURE |  |  | *FreqPriorityEUTRA* IE in TS 38.331 [22] |
| 4 | >>>Carrier Frequency | ELEMENT | FALSE | *carrierFreq* IE in TS 38.331 [22] |  |
| 5 | >>>Cell Reselection Priority | ELEMENT | FALSE | *cellReselectionPriority* IE in TS 38.331 [22] |  |
| 6 | >>>Cell Reselection Sub Priority | ELEMENT | FALSE | *cellReselectionSubPriority* IE in TS 38.331 [22] |  |
| 7 | >Frequency Priority List NR | LIST |  |  | *FreqPriorityListNR* IE in TS 38.331 [22] |
| 8 | >>Frequency Priority Item NR | STRUCTURE |  |  | *FreqPriorityNR* IE in TS 38.331 [22] |
| 9 | >>>Carrier Frequency | ELEMENT | FALSE | *carrierFreq* IE in TS 38.331 [22] |  |
| 10 | >>>Cell Reselection Priority | ELEMENT | FALSE | *cellReselectionPriority* IE in TS 38.331 [22] |  |
| 11 | >>>Cell Reselection Sub Priority | ELEMENT | FALSE | *cellReselectionSubPriority* IE in TS 38.331 [22] |  |
| 12 | >T-320 timer expiry | ELEMENT | FALSE | *t320* IE in TS 38.331 [22] |  |

### 8.4.9 UE identification and assignment

#### 8.4.9.1 UE to Explicit UE list assignment command

This Control action uses the following RAN Parameters.

*RIC Control Message* IE contents:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | *Explicit UE list* identifier | ELEMENT | FALSE | INTEGER | Identifier previously announced by E2 Node Set to 0 when used with assignment command = 3 |
| 2 | Assignment command | ELEMENT | FALSE | INTEGER | 1= Add UE, 2= Remove UE, 3= Send list of supported *Explicit UE list* |

*RIC Control Outcome* IE contents (success case):

Only used for the special case of Assignment command = 3

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1001 | List of supported *Explicit UE list* | LIST |  |  |  |
| 1002 | >*Explicit UE list* information | STRUCTURE |  |  |  |
| 1003 | >>*Explicit UE list* identifier | ELEMENT | TRUE | INTEGER | Identifier of Explicit UE List |
| 1004 | >>*Explicit UE list* name | ELEMENT | FALSE | PRINTABLE STRING | Name of Explicit UE List |
| 1005 | >>*Explicit UE list* description | ELEMENT | FALSE | PRINTABLE STRING | Text description of Explicit UE list |

*RIC Control Outcome* IE contents (failure case):

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1010 | Failure Cause | ELEMENT | FALSE | INTEGER | 0= reserved, 1= UE already assigned to Explicit UE list, 2 = Explicit UE list not known, 3= UEID not known, 4 = Other |

### 8.4.10 Measurement Reporting Configuration Control

#### 8.4.10.1 Add MR Configuration

Upon receiving the *RIC Control Request* message with the *Measurement Report Configuration Control* Service Style and the *Add MR Configuration* control action, the E2 node shall invoke relevant RRC procedures to configure Measurement Report to the UE. E2 Node shall include the IEs corresponding to one or more of RAN parameters described below in the related RRC or NI interface messages.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | List of Measurement Objects to Add | LIST |  |  | *measObjectToAddModList* IE in TS 38.331 Sec 6 |
| 2 | 1>Measurement Object to Add Item | STRUCTURE |  |  | *MeasObjectToAddMod* IE in TS 38.331 Sec 6 |
| 3 | 2>MO Sequence ID | ELEMENT | TRUE | INTEGER (1..64) | This is the unique ID used by the RIC for the measurement object it seeks to add via the control service style. |
| 4 | 2>CHOICE  *MO Type* | STRUCTURE |  |  | *measObject* IE in TS 38.331 Sec 6 |
| 11 | 3>*NR MO* | STRUCTURE |  |  | *MeasObjectNR* IE in TS 38.331 Sec 6 |
| 12 | 4>SSB Frequency | ELEMENT | TRUE | *ARFCN-ValueNR* IE in TS 38.331 Sec 6 |  |
| 13 | 4>SSB Subcarrier spacing | ELEMENT | FALSE | *subcarrierSpacing* IE in TS 38.331 Sec 6 |  |
| 14 | 4>SSB Primary MTC | STRUCTURE |  |  | *smtc1* IE in TS 38.331 Sec 6 |
| 15 | 5>CHOICE *Periodicity and Offset* | STRUCTURE |  |  | *periodicityAndOffset* IE in TS 38.331 Sec 6 |
| 16 | 6>Sub-frame 5 | ELEMENT | FALSE | *sf5* IE in TS 38.331 Sec 6 |  |
| 17 | 6>Sub-frame 10 | ELEMENT | FALSE | *sf10* IE in TS 38.331 Sec 6 |  |
| 18 | 6>Sub-frame 20 | ELEMENT | FALSE | *sf20* IE in TS 38.331 Sec 6 |  |
| 19 | 6>Sub-frame 40 | ELEMENT | FALSE | *sf40* IE in TS 38.331 Sec 6 |  |
| 20 | 6>Sub-frame 80 | ELEMENT | FALSE | *sf80* IE in TS 38.331 Sec 6 |  |
| 21 | 6>Sub-frame 160 | ELEMENT | FALSE | *sf160* IE in TS 38.331 Sec 6 |  |
| 22 | 5>Duration | ELEMENT | FALSE | *duration* IE in TS 38.331 Sec 6 |  |
| 31 | 4>SSB Secondary MTC | STRUCTURE |  |  | *smtc2* IE in TS 38.331 Sec 6 |
| 32 | 5>List of cells | LIST |  |  | *pci-List* IE in TS 38.331 Sec 6 |
| 33 | 6>Cell Item | STRUCTURE |  |  | *physCellID* IE in TS 38.331 Sec 6 |
| 34 | 7>PCI | ELEMENT | TRUE | *physCelIID* IE in TS 38.331 Sec 6 |  |
| 35 | 5>Periodicity | ELEMENT | FALSE | *periodicity* IE in TS 38.331 Sec 6 |  |
| 36 | 4>Reference Frequency CSI – RS | ELEMENT | TRUE | *refFreqCSI-RS* IE in TS 38.331 Sec 6 |  |
| 37 | 4>Reference Signal Config | STRUCTURE |  |  | *referenceSignalConfig* IE in TS 38.331 Sec 6 |
| 38 | 5>SSB Configuration Mobility | STRUCTURE |  |  | *SSB-ConfigMobility* IE in TS 38.331 Sec 6 |
| 40 | 6>CHOICE *SSB To Measure for setup* | STRUCTURE |  |  | *SSB-ToMeasure* IE in TS 38.331 Sec 6 |
| 41 | 7>Short Bitmap | ELEMENT | FALSE | *shortBitmap* IE in TS 38.331 Sec 6 |  |
| 42 | 7>Medium Bitmap | ELEMENT | FALSE | *mediumBitmap* IE in TS 38.331 Sec 6 |  |
| 43 | 7>Long Bitmap | ELEMENT | FALSE | *longBitmap* IE in TS 38.331 Sec 6 |  |
| 44 | 6>Derive SSB Index From Cell | ELEMENT | FALSE | *deriveSSB-IndexFromCell* IE in TS 38.331 Sec 6 |  |
| 45 | 6>SS RSSI Measurement | STRUCTURE |  |  | *ss-RSSI-Measurement* IE in TS 38.331 Sec 6 |
| 46 | 7>Measurement Slots | ELEMENT | FALSE | *measurementSlots* IE in TS 38.331 Sec 6 |  |
| 47 | 7>End Symbol | ELEMENT | FALSE | *endSymbol* IE in TS 38.331 Sec 6 |  |
| 50 | 6>CSI RS Resource Config Mobility for setup | STRUCTURE |  |  | *csi-rs-ResourceConfigMobility* IE in TS 38.331 Sec 6 |
| 51 | 7>Reference Serving cell Index | ELEMENT | TRUE | *refServellIndex* IE in TS 38.331 Sec 6 |  |
| 52 | 7>Sub carrier spacing | ELEMENT | FALSE | *subcarrierSpacing* IE in TS 38.331 Sec 6 |  |
| 53 | 7>CSI RS Cell List Mobility | LIST |  |  | *csi-RS-CellList-Mobility* IE in TS 38.331 Sec 6 |
| 54 | 8>CSI RS Cell Mobility | STRUCTURE |  |  | *CSI-RS-CellMobility* IE in TS 38.331 Sec 6 |
| 55 | 9>Physical Cell ID | ELEMENT | TRUE | *PhysCellID* IE in TS 38.331 Sec 6 |  |
| 56 | 9>CSI RS Measurement Bandwidth | STRUCTURE |  |  | *csi-rs-MeasurementBW* IE in TS 38.331 Sec 6 |
| 57 | 10>Number of PRBs | ELEMENT | FALSE | *nrofPRBs* IE in TS 38.331 Sec 6 |  |
| 58 | 10>Start PRB | ELEMENT | FALSE | *startPRB* IE in TS 38.331 Sec 6 |  |
| 59 | 9>Density | ELEMENT | FALSE | *density* IE in TS 38.331 Sec 6 |  |
| 60 | 9>CSI RS Resource List Mobility | LIST |  |  | *csi-rs-ResourceList-Mobility* IE in TS 38.331 Sec 6 |
| 61 | 10>CSI RS Resource Item Mobility | STRUCTURE |  |  | *CSI-RS-Resource-Mobility* IE in TS 38.331 Sec 6 |
| 62 | 11>CSI RS Index | ELEMENT | TRUE | *csi-RS-Index* IE in TS 38.331 Sec 6 |  |
| 63 | 11>CHOICE *Slot Config* | STRUCTURE |  |  | *slotConfig* IE in TS 38.331 Sec 6 |
| 64 | 12>ms4 | ELEMENT | FALSE | *ms4* IE in TS 38.331 Sec 6 |  |
| 65 | 12>ms5 | ELEMENT | FALSE | *ms5* IE in TS 38.331 Sec 6 |  |
| 66 | 12>ms10 | ELEMENT | FALSE | *ms10* IE in TS 38.331 Sec 6 |  |
| 67 | 12>ms20 | ELEMENT | FALSE | *ms20* IE in TS 38.331 Sec 6 |  |
| 68 | 12>ms40 | ELEMENT | FALSE | *ms40* IE in TS 38.331 Sec 6 |  |
| 69 | 11>Associated SSB | STRUCTURE |  |  | *assoiatedSSB* IE in TS 38.331 Sec 6 |
| 70 | 12>SSB Index | ELEMENT | TRUE | *ssb-Index* IE in TS 38.331 Sec 6 |  |
| 71 | 12>Is Quasi colocolo | ELEMENT | FALSE | *isQuasiColocated* IE in TS 38.331 Sec 6 |  |
| 72 | 11>CHOICE *Frequency Domain Allocation* | STRUCTURE |  |  | *frequencyDomainAllocation* IE in TS 38.331 Sec 6 |
| 73 | 12>Frequency Domain Allocation Row 1 | ELEMENT | FALSE | *row1* IE in TS 38.331 Sec 6 |  |
| 74 | 12>Frequency Domain Allocation Row 2 | ELEMENT | FALSE | *row2* IE in TS 38.331 Sec 6 |  |
| 75 | 11>First OFDM Symbol in Time Domain | ELEMENT | FALSE | *firstOFDMSymbolInTimeDomain* IE in TS 38.331 Sec 6 |  |
| 76 | 11>Sequence Generation Config | ELEMENT | FALSE | *sequenecGenerationConfig* IE in TS 38.331 Sec 6 |  |
| 77 | 4>Absolute Threshold SSB – Block Consolidation | STRUCTURE |  |  | *absThreshSS-BlocksConsolidation* IE in TS 38.331 Sec 6 |
| 78 | 5>Block Consolidation Threshold RSRP | ELEMENT | FALSE | *RSRP-Range* IE in TS 38.331 Sec 6 |  |
| 79 | 5>Block Consolidation Threshold RSRQ | ELEMENT | FALSE | *RSRQ-Range* IE in TS 38.331 Sec 6 |  |
| 80 | 5>Block Consolidation Threshold SINR | ELEMENT | FALSE | *SINR-Range* IE in TS 38.331 Sec 6 |  |
| 81 | 4>Absolute Threshold CSI RS Consolidation | STRUCTURE |  |  | *absThreshCSI-RS-Consolidation* IE in TS 38.331 Sec 6 |
| 82 | 5>RS Consolidation Threshold RSRP | ELEMENT | FALSE | *RSRP-Range* IE in TS 38.331 Sec 6 |  |
| 83 | 5>RS Consoldation Threshold RSRQ | ELEMENT | FALSE | *RSRQ-Range* IE in TS 38.331 Sec 6 |  |
| 84 | 5>RS Consolidated Threshold SINR | ELEMENT | FALSE | *SINR-Range* IE in TS 38.331 Sec 6 |  |
| 91 | 4>Number of SS blocks to average | ELEMENT | FALSE | *nrofSS-BlocksToAverage* IE in TS 38.331 Sec 6 |  |
| 92 | 4>Number of CSI RS Resources to average | ELEMENT | FALSE | *nrofCSI-RS-ResouresToAverage* IE in TS 38.331 Sec 6 |  |
| 93 | 4>Quantity Config Index | ELEMENT | TRUE | *quantityConfigIndex* IE in TS 38.331 Sec 6 |  |
| 100 | 4>Q-Offset MO Range Sequence | STRUCTURE |  |  | *offsetMO* IE in TS 38.331 Sec 6 |
| 101 | 5>RSRP Offset SSB | ELEMENT | FALSE | *rsrpOffsetSSB* IE in TS 38.331 Sec 6 |  |
| 102 | 5>RSRQ Offset SSB | ELEMENT | FALSE | *rsrqOffsetSSB* IE in TS 38.331 Sec 6 |  |
| 103 | 5>SINR Offset SSB | ELEMENT | FALSE | *sinrOffsetSSB* IE in TS 38.331 Sec 6 |  |
| 104 | 5>RSRP Offset CSI RS | ELEMENT | FALSE | *rsrpOffsetCSI-RS* IE in TS 38.331 Sec 6 |  |
| 105 | 5>RSRQ Offset CSI RS | ELEMENT | FALSE | *rsrqOffsetCSI-RS* IE in TS 38.331 Sec 6 |  |
| 106 | 5>SINR Offset CSI RS | ELEMENT | FALSE | *sinrOffsetCSI-RS* IE in TS 38.331 Sec 6 |  |
| 110 | 4>Cells to Add List | LIST |  |  | *CellsToAddModList* IE in TS 38.331 Sec 6 |
| 111 | 5>Cell to Add Item | STRUCTURE |  |  | *CellsToAdd* IE in TS 38.331 Sec 6 |
| 112 | 6>Cell to Add - Physical Cell ID | ELEMENT | TRUE | *physCellID* IE in TS 38.331 Sec 6 |  |
| 113 | 6>Cell Individual Offset | STRUCTURE |  |  | *cellIndividualOffset* IE in TS 38.331 Sec 6 |
| 115 | 7>RSRP Offset SSB | ELEMENT | FALSE | *rsrpOffsetSSB* IE in TS 38.331 Sec 6 |  |
| 116 | 7>RSRQ Offset SSB | ELEMENT | FALSE | *rsrqOffsetSSB* IE in TS 38.331 Sec 6 |  |
| 117 | 7>SINR Offset SSB | ELEMENT | FALSE | *sinrOffsetSSB* IE in TS 38.331 Sec 6 |  |
| 118 | 7>RSRP Offset CSI RS | ELEMENT | FALSE | *rsrpOffsetCSI-RS* IE in TS 38.331 Sec 6 |  |
| 119 | 7>RSRQ Offset CSI RS | ELEMENT | FALSE | *rsrqOffsetCSI-RS* IE in TS 38.331 Sec 6 |  |
| 120 | 7>SINR Offset CSI RS | ELEMENT | FALSE | *sinrOffsetCSI-RS* IE in TS 38.331 Sec 6 |  |
| 125 | 4>Black cells to Add List | LIST |  |  | *blackCellsToAddModList* IE in TS 38.331 Sec 6 |
| 126 | 5>Black cell to Add Item | STRUCTURE |  |  | *PCI-RangeElement* IE in TS 38.331 Sec 6 |
| 127 | 6>Black cell to Add – Physical Cell Range Index | ELEMENT | TRUE | *PCI-RangeIndex* IE in TS 38.331 Sec 6 |  |
| 128 | 6>Physical Cell ID - Range | STRUCTURE |  |  | *PCI-Range* IE in TS 38.331 Sec 6 |
| 129 | 7>Physical Cell ID Start | ELEMENT | TRUE | *physCellId* IE in TS 38.331 Sec 6 |  |
| 130 | 7>Physical Cell ID Range | ELEMENT | FALSE | *range* IE in TS 38.331 Sec 6 |  |
| 135 | 4>White cells to Add List | LIST |  |  | *whiteCellsToAddModList* IE in TS 38.331 Sec 6 |
| 136 | 5>White cell to Add Item | STRUCTURE |  |  | *PCI-RangeElement* IE in TS 38.331 Sec 6 |
| 137 | 6>White cell to Add – Physical Cell Range Index | ELEMENT | TRUE | *PCI-RangeIndex* IE in TS 38.331 Sec 6 |  |
| 138 | 6>Physical Cell ID - Range | STRUCTURE |  |  | *PCI-Range* IE in TS 38.331 Sec 6 |
| 129 | 7>Physical Cell ID Start | ELEMENT | TRUE | *PhysCellId* IE in TS 38.331 Sec 6 |  |
| 130 | 7>Physical Cell ID Range | ELEMENT | FALSE | *range* IE in TS 38.331 Sec 6 |  |
| 141 | 4>Frequency Band Indicator NR | ELEMENT | TRUE | *freqBandIndicatorNR* IE in TS 38.331 Sec 6 |  |
| 142 | 4>Measurement Cycle Secondary cell | ELEMENT | FALSE | *measCycleSCell* IE in TS 38.331 Sec 6 |  |
| 151 | 3>*E-UTRA MO* | STRUCTURE |  |  | *MeasObjectEUTRA* IE in TS 38.331 Sec 6 |
| 152 | 4>E-UTRA Carrier Frequency | ELEMENT | TRUE | *carrierFreq* IE in TS 38.331 Sec 6 |  |
| 153 | 4>E-UTRA Allowed Measurement Bandwidth | ELEMENT | FALSE | *allowedMeasBandwidth* IE in TS 38.331 Sec 6 |  |
| 171 | 4>List of E-UTRA cells to add | LIST |  |  | *cellsToAddModListEUTRAN* IE in TS 38.331 Sec 6 |
| 172 | 5>E-UTRA Cell to add Item | STRUCTURE |  |  |  |
| 173 | 6>E-UTRA Cell to add | STRUCTURE |  |  | *EUTRA-Cell* IE in TS 38.331 Sec 6 |
| 174 | 7>E-UTRA PCI to add | ELEMENT | TRUE | *EUTRA-PhysCellId* IE in TS 38.331 Sec 6 |  |
| 175 | 7>E-UTRA Cell Individual Offset | ELEMENT | FALSE | *cellIndividualOffset* IE in TS 38.331 Sec 6 |  |
| 191 | 4>List of E-UTRA black cells to add | LIST |  |  | *blackCellsToAddModList* IE in TS 38.331 Sec 6 |
| 192 | 5>E-UTRA black cell to add item | STRUCTURE |  |  |  |
| 193 | 6>E-UTRA black cell to add | STRUCTURE |  |  | *EUTRA-BlackCell* IE in TS 38.331 Sec 6 |
| 194 | 7>E-UTRA Physical Cell ID Range | STRUCTURE |  |  | *EUTRA-PhysCellIdRange* IE in TS 38.331 Sec 6 |
| 195 | 8>E-UTRA PCI Start | ELEMENT | TRUE | *EUTRA-PhysCellId* IE in TS 38.331 Sec 6 |  |
| 196 | 8>E-UTRA PCI Range | ELEMENT | FALSE | *range* IE in TS 38.331 Sec 6 |  |
| 201 | 4>E-UTRA Presence Antenna Port 1 | ELEMENT | FALSE | *eutra-PresenceAntennaPort1* IE in TS 38.331 Sec 6 |  |
| 205 | 4>E-UTRA Q Offset Range | ELEMENT | FALSE | *eutra-Q-OffsetRange* IE in TS 38.331 Sec 6 |  |
| 210 | 4>Wideband RSRQ Measurement | ELEMENT | FALSE | *widebandRSRQ-Meas* IE in TS 38.331 Sec 6 |  |
| 301 | List of Report Config Objects to Add | LIST |  |  | *ReportConfigToAddModList* IE in TS 38.331 Sec 6 |
| 302 | 1>Report Config Object to Add Item | STRUCTURE |  |  | *ReportConfigToAddMod* IE in TS 38.331 Sec 6 |
| 303 | 2>Report Config Sequence ID | ELEMENT | TRUE | INTEGER (1..64) | This is the unique ID used by the RIC for the measurement object it seeks to add via the control service style. |
| 304 | 2>CHOICE *Report Config Type* | STRUCTURE |  |  | *reportConfig* IE in TS 38.331 Sec 6 |
| 311 | 3>*NR Report Config* | STRUCTURE |  |  | *ReportConfigNR* IE in TS 38.331 Sec 6 |
| 312 | 4>CHOICE *Report Type* | STRUCTURE |  |  | *reportType* IE in TS 38.331 Sec 6 |
| 313 | 5>Periodical Report Config | STRUCTURE |  |  | *PeriodicalReportConfig* IE in TS 38.331 Sec 6 |
| 314 | 6>NR RS Type | ELEMENT | FALSE | *NR-RS-Type* IE in TS 38.331 Sec 6 |  |
| 315 | 6>NR Report Interval | ELEMENT | FALSE | *ReportInterval* IE in TS 38.331 Sec 6 |  |
| 316 | 6>NR Report Amount | ELEMENT | FALSE | *reportAmount* IE in TS 38.331 Sec 6 |  |
| 317 | 6>Measurement Report Quantity | STRUCTURE |  |  | *MeasReportQuantity* IE in TS 38.331 Sec 6 |
| 318 | 7>MR RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 |  |
| 319 | 7>MR RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 |  |
| 320 | 7>MR SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 |  |
| 321 | 6>Maximum number of Report cells | ELEMENT | FALSE | *maxReportCells* IE in TS 38.331 Sec 6 |  |
| 322 | 6>Report Quantity Reference Signal – Indexes | STRUCTURE |  |  | *reportQuantityRS-Indexes* IE in TS 38.331 Sec 6 |
| 323 | 7>Report Qty RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 |  |
| 324 | 7>Report Qty RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 |  |
| 325 | 7>Report Qty SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 |  |
| 326 | 6>Maximum number of reference signals – Indexes to Report | ELEMENT | FALSE | *maxNrofRS-IndexesToReport* IE in TS 38.331 Sec 6 |  |
| 327 | 6>Include Beam Measurements | ELEMENT | FALSE | *includeBeamMeasuremetns* IE in TS 38.331 Sec 6 |  |
| 328 | 6>Use WhiteCellList | ELEMENT | FALSE | *useWhiteCellList* IE in TS 38.331 Sec 6 |  |
| 331 | 5>Event Trigger Config | STRUCTURE |  |  | *EventTriggerConfig* IE in TS 38.331 Sec 6 |
| 332 | 6>CHOICE *Event ID* | STRUCTURE |  |  | *eventide* IE in TS 38.331 Sec 6 |
| 333 | 7>Event A1 | STRUCTURE |  |  | *eventA1* IE in TS 38.331 Sec 6 |
| 334 | 8>A1 Threshold | STRUCTURE |  |  | *a1-Threshold* IE in TS 38.331 Sec 6 |
| 335 | 9>CHOICE *A1 Threshold Type* | STRUCTURE |  |  | *MeasTriggerQuantity* IE in TS 38.331 Sec 6 |
| 336 | 10>A1 Threshold RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 | *RSRP-Range* IE |
| 337 | 10>A1 Threshold RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 | *RSRQ-Range* IE |
| 338 | 10>A1 Threshold SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 | *SINR-Range* IE |
| 339 | 9>A1 Report On Leave | ELEMENT | FALSE | *reportOnLeave* IE in TS 38.331 Sec 6 |  |
| 340 | 9>A1 Hysteresis | ELEMENT | FALSE | *hysteresis* IE in TS 38.331 Sec 6 |  |
| 341 | 9>A1 Time to Trigger | ELEMENT | FALSE | *timeToTrigger* IE in TS 38.331 Sec 6 |  |
| 343 | 7>Event A2 | STRUCTURE |  |  | *eventA2* IE in TS 38.331 Sec 6 |
| 344 | 8>A2 Threshold | STRUCTURE |  |  | *A2-Threshold* IE in TS 38.331 Sec 6 |
| 345 | 9>CHOICE *A2 Threshold Type* | STRUCTURE |  |  | *MeasTriggerQuantity* IE in TS 38.331 Sec 6 |
| 346 | 10>A2 Threshold RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 | *RSRP-Range* IE |
| 347 | 10>A2 Threshold RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 | *RSRQ-Range* IE |
| 348 | 10>A2 Threshold SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 | *SINR-Range* IE |
| 349 | 9>A2 Report On Leave | ELEMENT | FALSE | *reportOnLeave* IE in TS 38.331 Sec 6 |  |
| 350 | 9>A2 Hysteresis | ELEMENT | FALSE | *hysteresis* IE in TS 38.331 Sec 6 |  |
| 351 | 9>A2 Time to Trigger | ELEMENT | FALSE | *timeToTrigger* IE in TS 38.331 Sec 6 |  |
| 353 | 7>Event A3 | STRUCTURE |  |  | *eventA3* IE in TS 38.331 Sec 6 |
| 354 | 8>A3 Offset | STRUCTURE |  |  | *a3-Threshold* IE in TS 38.331 Sec 6 |
| 355 | 9>CHOICE *A3 Offset Type* | STRUCTURE |  |  | *MeasTriggerQuantityOffset* IE in TS 38.331 Sec 6 |
| 356 | 10>A3 Threshold RSRP Offset | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 |  |
| 357 | 10>A3 Threshold RSRQ Offset | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 |  |
| 358 | 10>A3 Threshold SINR Offset | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 |  |
| 359 | 9>A3 Report On Leave | ELEMENT | FALSE | *reportOnLeave* IE in TS 38.331 Sec 6 |  |
| 360 | 9>A3 Hysteresis | ELEMENT | FALSE | *hysteresis* IE in TS 38.331 Sec 6 |  |
| 361 | 9>A3 Time to Trigger | ELEMENT | FALSE | *timeToTrigger* IE in TS 38.331 Sec 6 |  |
| 362 | 9>Use White Cell List | ELEMENT | FALSE | *useWhiteCellList* IE in TS 38.331 Sec 6 |  |
| 363 | 7>Event A4 | STRUCTURE |  |  | *eventA4* IE in TS 38.331 Sec 6 |
| 364 | 8>A4 Threshold | STRUCTURE |  |  | *A4-Threshold* IE in TS 38.331 Sec 6 |
| 365 | 9>CHOICE *A4 Threshold Type* | STRUCTURE |  |  | *MeasTriggerQuantity* IE in TS 38.331 Sec 6 |
| 366 | 10>A4 Threshold RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 | *RSRP-Range* IE |
| 367 | 10>A4 Threshold RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 | *RSRQ-Range* IE |
| 368 | 10>A4 Threshold SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 | *SINR-Range* IE |
| 369 | 9>A4 Report On Leave | ELEMENT | FALSE | *reportOnLeave* IE in TS 38.331 Sec 6 |  |
| 370 | 9>A4 Hysteresis | ELEMENT | FALSE | *hysteresis* IE in TS 38.331 Sec 6 |  |
| 371 | 9>A4 Time to Trigger | ELEMENT | FALSE | *timeToTrigger* IE in TS 38.331 Sec 6 |  |
| 372 | 9>Use White Cell List | ELEMENT | FALSE | *useWhiteCellList* IE in TS 38.331 Sec 6 |  |
| 375 | 7>Event A5 | STRUCTURE |  |  | *eventA5* IE in TS 38.331 Sec 6 |
| 376 | 8>A5 Threshold 1 | STRUCTURE |  |  | *a5-Threshold1* IE in TS 38.331 Sec 6 |
| 377 | 9>CHOICE *A5 Threshold1 Type* | STRUCTURE |  |  | *MeasTriggerQuantity* IE in TS 38.331 Sec 6 |
| 378 | 10>A5 Threshold1 RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 | *RSRP-Range* IE |
| 379 | 10>A5 Threshold1 1 RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 | *RSRQ-Range* IE |
| 380 | 10>A5 Threshold1 SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 | *SINR-Range* IE |
| 381 | 9>CHOICE *A5 Threshold2 Type* | STRUCTURE |  |  | *a5-Threshold2* IE in TS 38.331 Sec 6 |
| 382 | 10>A5 Threshold2 RSRP | ELEMENT | FALSE | *MeasTriggerQuantity* IE in TS 38.331 Sec 6 |  |
| 379 | 10>A5 Threshold2 RSRQ | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 | *RSRP-Range* IE |
| 380 | 10>A5 Threshold2 SINR | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 | *RSRQ-Range* IE |
| 381 | 9>A5 Report On Leave | ELEMENT | FALSE | *reportOnLeave* IE in TS 38.331 Sec 6 |  |
| 382 | 9>A5 Hysteresis | ELEMENT | FALSE | *hysteresis* IE in TS 38.331 Sec 6 |  |
| 383 | 9>A5 Time to Trigger | ELEMENT | FALSE | *timeToTrigger* IE in TS 38.331 Sec 6 |  |
| 384 | 9>Use White Cell List | ELEMENT | FALSE | *useWhiteCellList* IE in TS 38.331 Sec 6 |  |
| 391 | 7>Event A6 | STRUCTURE |  |  | *eventA6* IE in TS 38.331 Sec 6 |
| 392 | 8>A6 Threshold | STRUCTURE |  |  | *A6-Threshold* IE in TS 38.331 Sec 6 |
| 393 | 9>CHOICE *A6 Threshold Type* | STRUCTURE |  |  | *MeasTriggerQuantityOffset* IE in TS 38.331 Sec 6 |
| 394 | 10>A6 Threshold RSRP Offset | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 |  |
| 395 | 10>A6 Threshold RSRQ Offset | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 |  |
| 396 | 10>A6 Threshold SINR Offset | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 |  |
| 397 | 9>A6 Report On Leave | ELEMENT | FALSE | *reportOnLeave* IE in TS 38.331 Sec 6 |  |
| 398 | 9>A6 Hysteresis | ELEMENT | FALSE | *hysteresis* IE in TS 38.331 Sec 6 |  |
| 399 | 9>A6 Time to Trigger | ELEMENT | FALSE | *timeToTrigger* IE in TS 38.331 Sec 6 |  |
| 400 | 9>Use White Cell List | ELEMENT | FALSE | *useWhiteCellList* IE in TS 38.331 Sec 6 |  |
| 405 | 5>Report CGI | STRUCTURE |  |  | *ReportCGI* IE in TS 38.331 Sec 6 |
| 406 | 6>Cell to Report CGI | ELEMENT | TRUE | *PhysCellId* IE in TS 38.331 Sec 6 |  |
| 411 | 5>Report SFTD – NR | STRUCTURE |  |  | *ReportSFTD-NR* IE in TS 38.331 Sec 6 |
| 412 | 6>Report SFTD – Measurement | ELEMENT | FALSE | *reportSFTD-Meas* IE in TS 38.331 Sec 6 |  |
| 413 | 6>Report RSRP | ELEMENT | FALSE | *reportRSRP* IE in TS 38.331 Sec 6 |  |
| 414 | 6>Report SFTD Neigh Meas | ELEMENT | FALSE | *reportSFTD-NeighMeas* IE in TS 38.331 Sec 6 |  |
| 415 | 6>DRX SFTD Neigh Meas | ELEMENT | FALSE | *drx-SFTD-NeighMeas* IE in TS 38.331 Sec 6 |  |
| 416 | 6>List of cells for which to report SFTD | LIST |  |  | *cellsForWhichToReportSFTD* IE in TS 38.331 Sec 6 |
| 417 | 7>Cell Item for reporting SFTD | STRUCTURE |  |  |  |
| 418 | 8>Physical Cell Identity | ELEMENT | TRUE | *PhyCellId* IE in TS 38.331 Sec 6 |  |
| 421 | 3>Report Config Inter RAT | STRUCTURE |  |  | *ReportConfigInterRAT* IE in TS 38.331 Sec 6 |
| 422 | 4>CHOICE *Report Type* | STRUCTURE |  |  | *reportType* IE in TS 38.331 Sec 6 |
| 423 | 5>Periodical Report Config Inter RAT | STRUCTURE |  |  | *PeriodicalReportConfigInterRAT* IE in TS 38.331 Sec 6 |
| 431 | 6>Periodical Inter-RAT Report Interval | ELEMENT | FALSE | *reportInterval* IE in TS 38.331 Sec 6 |  |
| 432 | 6>Periodical Inter-RAT Report Amount | ELEMENT | FALSE | *reportAmount* IE in TS 38.331 Sec 6 |  |
| 435 | 6>Periodical Inter-RAT Report Quantity | STRUCTURE |  |  | *reportQuantity* IE in TS 38.331 Sec 6 |
| 436 | 7>Inter-RAT RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 |  |
| 437 | 7>Inter-RAT RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 |  |
| 438 | 7>Inter-RAT SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 |  |
| 439 | 6>Maximum number of cells for reporting | ELEMENT | FALSE | *maxReportCells* IE in TS 38.331 Sec 6 |  |
| 441 | 5>Event Trigger Config Inter RAT | STRUCTURE |  |  | *EventTriggerConfigInterRAT* IE in TS 38.331 Sec 6 |
| 442 | 6>CHOICE *Event ID* | STRUCTURE |  |  | *eventId* IE in TS 38.331 Sec 6 |
| 451 | 7>Event B1 | STRUCTURE |  |  | *eventB1* IE in TS 38.331 Sec 6 |
| 452 | 8>B1 Threshold EUTRA | STRUCTURE |  |  | *b1-ThresholdEUTRA* IE in TS 38.331 Sec 6 |
| 453 | 9>E-UTRA RSRP | ELEMENT | FALSE | *RSRP-RangeEUTRA* IE in TS 38.331 Sec 6 |  |
| 454 | 9>E-UTRA RSRQ | ELEMENT | FALSE | *RSRQ-RangeEUTRA* IE in TS 38.331 Sec 6 |  |
| 455 | 9>E-UTRA SINR | ELEMENT | FALSE | *SINR-RangeEUTRA* IE in TS 38.331 Sec 6 |  |
| 456 | 8>Event B1 Report On Leave | ELEMENT | FALSE | *reportOnLeave* IE in TS 38.331 Sec 6 |  |
| 457 | 8>E-UTRA Hysteresis | ELEMENT | FALSE | *hystereisis* IE in TS 38.331 Sec 6 |  |
| 458 | 8>E-UTRA Time To Trigger | ELEMENT | FALSE | *timeToTrigger* IE in TS 38.331 Sec 6 |  |
| 471 | 7>Event B2 | STRUCTURE |  |  | *eventB2* IE in TS 38.331 Sec 6 |
| 472 | 8>B2 Threshold1 NR | STRUCTURE |  |  | *b2-Threshold1* IE in TS 38.331 Sec 6 |
| 475 | 9>B2 Threshold1 NR RSRP | ELEMENT | FALSE | *RSRP-Range* IE in TS 38.331 Sec 6 |  |
| 476 | 9>B2 Threshold1 NR RSRQ | ELEMENT | FALSE | *RSRQ-Range* IE in TS 38.331 Sec 6 |  |
| 477 | 9>B2 Threshold1 NR SINR | ELEMENT | FALSE | *SINR-Range* IE in TS 38.331 Sec 6 |  |
| 481 | 8>B2 Threshold2 E-UTRA | STRUCTURE |  |  | *b2-Threshold2EUTRA* IE in TS 38.331 Sec 6 |
| 482 | 9>B2 Threshold2 E-UTRA RSRP | ELEMENT | FALSE | *RSRP-RangeEUTRA* IE in TS 38.331 Sec 6 |  |
| 483 | 9>B2 Threshold2 E-UTRA RSRQ | ELEMENT | FALSE | *RSRQ-RangeEUTRA* IE in TS 38.331 Sec 6 |  |
| 484 | 9>B2 Threshold2 E-UTRA SINR | ELEMENT | FALSE | *SINR-RangeEUTRA* IE in TS 38.331 Sec 6 |  |
| 491 | 6>Inter-RAT Reference Signal Type | ELEMENT | FALSE | *rsType* IE in TS 38.331 Sec 6 |  |
| 492 | 6>Inter-RAT Report Interval | ELEMENT | FALSE | *reportInterval* IE in TS 38.331 Sec 6 |  |
| 493 | 6>Inter-RAT Report Amount | ELEMENT | FALSE | *reportAmount* IE in TS 38.331 Sec 6 |  |
| 501 | 6>Inter-RAT Report Quantity | STRUCTURE |  |  | *reportQuantity* IE in TS 38.331 Sec 6 |
| 502 | 7>Inter-RAT Report Quantity RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 |  |
| 503 | 7>Inter-RAT Report Quantity RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 |  |
| 504 | 7>Inter-RAT Report Quantity SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 |  |
| 510 | 6>Maximum number of cells to be reported | ELEMENT | FALSE | *maxReportCells* IE in TS 38.331 Sec 6 |  |
| 519 | *CHOICE* NR SpCell RSRP Measurement Controlling | STRUCTURE |  |  | *s-MeasureConfig* IE in TS 38.331 Sec 6 |
| 520 | 1>SSB RSRP | ELEMENT | FALSE | *ssb-RSRP* IE in TS 38.331 Sec 6 |  |
| 521 | 1>CSI RSRP | ELEMENT | FALSE | *csi-RSRP* IE in TS 38.331 Sec 6 |  |
| 525 | Quantity Config | STRUCTURE |  |  | *QuantityConfig* IE in TS 38.331 Sec 6 |
| 526 | 1>Quantity Config NR List | LIST |  |  | *quantityConfigNR-List* IE in TS 38.331 Sec 6 |
| 527 | 2>Quantity Config NR | STRUCTURE |  |  | *quantityConfigNR* IE in TS 38.331 Sec 6 |
| 528 | 3>Quantity Config NR Cell | STRUCTURE |  |  | *quantityConfigCell* IE in TS 38.331 Sec 6 |
| 529 | 4>SSB Filter Config | STRUCTURE |  |  | *ssb-FilterConfig* IE in TS 38.331 Sec 6 |
| 530 | 5>SSB Filter Coefficient RSRP | ELEMENT | FALSE | *filterCoefficientRSRP* IE in TS 38.331 Sec 6 |  |
| 531 | 5>SSB Filter Coefficient RSRQ | ELEMENT | FALSE | *filterCoefficientRSRQ* IE in TS 38.331 Sec 6 |  |
| 532 | 5>SSB Filter Coefficient RS-SINR | ELEMENT | FALSE | *filterCoefficientSINR* IE in TS 38.331 Sec 6 |  |
| 533 | 4>CSI RS Filter Config | STRUCTURE |  |  | *csi-RS-FilterConfig* IE in TS 38.331 Sec 6 |
| 534 | 5>CSI RS Filter Coefficient RSRP | ELEMENT | FALSE | *filterCoefficientRSRP* IE in TS 38.331 Sec 6 |  |
| 535 | 5>CSI RS Filter Coefficient RSRQ | ELEMENT | FALSE | *filterCoefficientRSRQ* IE in TS 38.331 Sec 6 |  |
| 536 | 5>CSI RS Filter Coefficient RS-SINR | ELEMENT | FALSE | *filterCoefficientSINR* IE in TS 38.331 Sec 6 |  |
| 541 | 1>Quantity Config E-UTRA | STRUCTURE |  |  | *quantityConfigEUTRA* IE in TS 38.331 Sec 6 |
| 542 | 2>E-UTRA Filter Coefficient RSRP | ELEMENT | FALSE | *filterCoefficientRSRP* IE in TS 38.331 Sec 6 |  |
| 543 | 2>E-UTRA Filter Coefficient RSRQ | ELEMENT | FALSE | *filterCoefficientRSRQ* IE in TS 38.331 Sec 6 |  |
| 544 | 2>E-UTRA Filter Coefficient RS-SINR | ELEMENT | FALSE | *filterCoefficientSINR* IE in TS 38.331 Sec 6 |  |
| 551 | Measurement Gap Config | STRUCTURE |  |  | *MeasGapConfig* IE in TS 38.331 Sec 6 |
| 552 | 1>Gap FR2 for setup | STRUCTURE |  |  | *gapFR2* IE in TS 38.331 Sec 6 |
| 553 | 2>FR2 Gap Offset | ELEMENT | FALSE | *gapOffset* IE in TS 38.331 Sec 6 |  |
| 554 | 2>FR2 Measurement Gap Length | ELEMENT | FALSE | *mgl* IE in TS 38.331 Sec 6 |  |
| 555 | 2>FR2 Measurement Gap Repetition Period | ELEMENT | FALSE | *mgrp* IE in TS 38.331 Sec 6 |  |
| 556 | 2>FR2 Measurement Gap Timing Analysis | ELEMENT | FALSE | *mgta* IE in TS 38.331 Sec 6 |  |
| 557 | 2>FR2 Reference Serving Cell Indicator | ELEMENT | TRUE | *refServCellIndicator* IE in TS 38.331 Sec 6 |  |
| 560 | 1>Gap FR1 for setup | STRUCTURE |  |  | *gapFR1* IE in TS 38.331 Sec 6 |
| 561 | 2>FR1 Gap Offset | ELEMENT | FALSE | *gapOffset* IE in TS 38.331 Sec 6 |  |
| 562 | 2>FR1 Measurement Gap Length | ELEMENT | FALSE | *mgl* IE in TS 38.331 Sec 6 |  |
| 563 | 2>FR1 Measurement Gap Repetition Period | ELEMENT | FALSE | *mgrp* IE in TS 38.331 Sec 6 |  |
| 564 | 2>FR1 Measurement Gap Timing Analysis | ELEMENT | FALSE | *mgta* IE in TS 38.331 Sec 6 |  |
| 565 | 2>FR1 Reference Serving Cell Indicator | ELEMENT | TRUE | *refServCellIndicator* IE in TS 38.331 Sec 6 |  |
| 570 | 1>Gap UE for setup | STRUCTURE |  |  | *gapUE* IE in TS 38.331 Sec 6 |
| 571 | 2>UE Gap Offset | ELEMENT | FALSE | *gapOffset* IE in TS 38.331 Sec 6 |  |
| 572 | 2>UE Measurement Gap Length | ELEMENT | FALSE | *mgl* IE in TS 38.331 Sec 6 |  |
| 573 | 2>UE Measurement Gap Reptition Period | ELEMENT | FALSE | *mgrp* IE in TS 38.331 Sec 6 |  |
| 574 | 2>UE Measurement Gap Timing Analysis | ELEMENT | FALSE | *mgta* IE in TS 38.331 Sec 6 |  |
| 575 | 2>UE Reference Serving Cell Indicator | ELEMENT | TRUE | *refServCellIndicator* IE in TS 38.331 Sec 6 |  |
| 581 | Measurement Gap Sharing Config | STRUCTURE |  |  | *MeasGapSharingConfig* IE in TS 38.331 Sec 6 |
| 582 | 1>Gap Sharing FR2 for setup | ELEMENT | FALSE | *gapFR2* IE in TS 38.331 Sec 6 |  |
| 583 | 1>Gap Sharing FR1 for setup | ELEMENT | FALSE | *gapFR1* IE in TS 38.331 Sec 6 |  |
| 584 | 1>Gap Sharing UE for setup | ELEMENT | FALSE | *gapUE* IE in TS 38.331 Sec 6 |  |

#### 8.4.10.2 Modify MR Configuration

Upon receiving the *RIC Control Request* message with the *Measurement Report Configuration Control* Service Style and the *Modify MR Configuration* control action, the E2 node shall invoke RRC procedures related to MR Configuration, include the IEs corresponding to one or more of parameters described below in the related NI interface messages or RRC message.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | List of Measurement Objects to modify or add for modification | LIST |  |  | *measObjectToAddModList* IE in TS 38.331 Sec 6 |
| 2 | 1>Measurement Object to modify or add for modification Item | STRUCTURE |  |  | *MeasObjectToAddMod* IE in TS 38.331 Sec 6 |
| 3 | 2>Measurement Object ID | ELEMENT | TRUE | *MeasObjectID* IE in TS 38.331 Sec 6 | This is the ID used by the E2 node for the measurement object for the UE via *RRCReconfiguration* message |
| 4 | 2>CHOICE  *MO Type* | STRUCTURE |  |  | *measObject* IE in TS 38.331 Sec 6 |
| 11 | 3>*NR MO* | STRUCTURE |  |  | *MeasObjectNR* IE in TS 38.331 Sec 6 |
| 12 | 4>SSB Frequency | ELEMENT | TRUE | *ARFCN-ValueNR* IE in TS 38.331 Sec 6 |  |
| 13 | 4>SSB Subcarrier spacing | ELEMENT | FALSE | *SubcarrierSpacing* IE in TS 38.331 Sec 6 |  |
| 14 | 4>SSB Primary MTC | STRUCTURE |  |  | *smtc1* IE in TS 38.331 Sec 6 |
| 15 | 5>CHOICE *Periodicity and Offset* | STRUCTURE |  |  | *periodicityAndOffset* IE in TS 38.331 Sec 6 |
| 16 | 6>Sub-frame 5 | ELEMENT | FALSE | *sf5* IE in TS 38.331 Sec 6 |  |
| 17 | 6>Sub-frame 10 | ELEMENT | FALSE | *sf10* IE in TS 38.331 Sec 6 |  |
| 18 | 6>Sub-frame 20 | ELEMENT | FALSE | *sf20* IE in TS 38.331 Sec 6 |  |
| 19 | 6>Sub-frame 40 | ELEMENT | FALSE | *sf40* IE in TS 38.331 Sec 6 |  |
| 20 | 6>Sub-frame 80 | ELEMENT | FALSE | *sf80* IE in TS 38.331 Sec 6 |  |
| 21 | 6>Sub-frame 160 | ELEMENT | FALSE | *sf160* IE in TS 38.331 Sec 6 |  |
| 22 | 5>Duration | ELEMENT | FALSE | *duration* IE in TS 38.331 Sec 6 |  |
| 31 | 4>SSB Secondary MTC | STRUCTURE |  |  | *smtc2* IE in TS 38.331 Sec 6 |
| 32 | 5>List of cells | LIST |  |  | *pci-List* IE in TS 38.331 Sec 6 |
| 33 | 6>Cell Item | STRUCTURE |  |  | *PhysCellID* IE in TS 38.331 Sec 6 |
| 34 | 7>PCI | ELEMENT | TRUE | *physCelIID* IE in TS 38.331 Sec 6 |  |
| 35 | 5>Periodicity | ELEMENT | FALSE | *periodicity* IE in TS 38.331 Sec 6 |  |
| 36 | 4>Reference Frequency CSI – RS | ELEMENT | TRUE | *refFreqCSI-RS* IE in TS 38.331 Sec 6 |  |
| 37 | 4>Reference Signal Config | STRUCTURE |  |  | *referenceSignalConfig* IE in TS 38.331 Sec 6 |
| 38 | 5>SSB Configuration Mobility | STRUCTURE |  |  | *SSB-ConfigMobility* IE in TS 38.331 Sec 6 |
| 39 | 6>Setup or Release SSB to Measure | ELEMENT | FALSE | ENUMERATED (setup,release,…) | *SetupRelease* IE in TS 38.331 Sec 6 |
| 40 | 6>CHOICE *SSB To Measure for setup* | STRUCTURE |  |  | *SSB-ToMeasure* IE in TS 38.331 Sec 6 |
| 41 | 7>Short Bitmap | ELEMENT | FALSE | *shortBitmap* IE in TS 38.331 Sec 6 |  |
| 42 | 7>Medium Bitmap | ELEMENT | FALSE | *mediumBitmap* IE in TS 38.331 Sec 6 |  |
| 43 | 7>Long Bitmap | ELEMENT | FALSE | *longBitmap* IE in TS 38.331 Sec 6 |  |
| 44 | 6>Derive SSB Index From Cell | ELEMENT | FALSE | *deriveSSB-IndexFromCell* IE in TS 38.331 Sec 6 |  |
| 45 | 6>SS RSSI Measurement | STRUCTURE |  |  | *ss-RSSI-Measurement* IE in TS 38.331 Sec 6 |
| 46 | 7>Measurement Slots | ELEMENT | FALSE | *measurementSlots* IE in TS 38.331 Sec 6 |  |
| 47 | 7>End Symbol | ELEMENT | FALSE | *endSymbol* IE in TS 38.331 Sec 6 |  |
| 49 | 6>Setup or Release CSI RS Resource Config Mobility | ELEMENT | FALSE | ENUMERATED (setup, release,…) | *SetupRelease* IE in TS 38.331 Sec 6 |
| 50 | 6>CSI RS Resource Config Mobility for Setup | STRUCTURE |  |  | *csi-rs-ResourceConfigMobility* IE in TS 38.331 Sec 6 |
| 51 | 7>Reference Serving cell Index | ELEMENT | TRUE | *refServCellIndex* IE in TS 38.331 Sec 6 |  |
| 52 | 7>Sub carrier spacing | ELEMENT | FALSE | *subcarrierSpacing* IE in TS 38.331 Sec 6 |  |
| 53 | 7>CSI RS Cell List Mobility | LIST |  |  | *csi-RS-CellList-Mobility* IE in TS 38.331 Sec 6 |
| 54 | 8>CSI RS Cell Mobility | STRUCTURE |  |  | *CSI-RS-CellMobility* IE in TS 38.331 Sec 6 |
| 55 | 9>Physical Cell ID | ELEMENT | TRUE | *PhysCellID* IE in TS 38.331 Sec 6 |  |
| 56 | 9>CSI RS Measurement Bandwidth | STRUCTURE |  |  | *csi-rs-MeasurementBW* IE in TS 38.331 Sec 6 |
| 57 | 10>Number of PRBs | ELEMENT | FALSE | *nrofPRBs* IE in TS 38.331 Sec 6 |  |
| 58 | 10>Start PRB | ELEMENT | FALSE | *startPRB* IE in TS 38.331 Sec 6 |  |
| 59 | 9>Density | ELEMENT | FALSE | *Density* IE in TS 38.331 Sec 6 |  |
| 60 | 9>CSI RS Resource List Mobility | LIST |  |  | *csi-rs-ResourceList-Mobility* IE in TS 38.331 Sec 6 |
| 61 | 10>CSI RS Resource Item Mobility | STRUCTURE |  |  | *CSI-RS-Resource-Mobility* IE in TS 38.331 Sec 6 |
| 62 | 11>CSI RS Index | ELEMENT | TRUE | *csi-RS-Index* IE in TS 38.331 Sec 6 |  |
| 63 | 11>CHOICE *Slot Config* | STRUCTURE |  |  | *slotConfig* IE in TS 38.331 Sec 6 |
| 64 | 12>ms4 | ELEMENT | FALSE | *ms4* IE in TS 38.331 Sec 6 |  |
| 65 | 12>ms5 | ELEMENT | FALSE | *ms5* IE in TS 38.331 Sec 6 |  |
| 66 | 12>ms10 | ELEMENT | FALSE | *ms10* IE in TS 38.331 Sec 6 |  |
| 67 | 12>ms20 | ELEMENT | FALSE | *ms20* IE in TS 38.331 Sec 6 |  |
| 68 | 12>ms40 | ELEMENT | FALSE | *ms40* IE in TS 38.331 Sec 6 |  |
| 69 | 11>Associated SSB | STRUCTURE |  |  | *assoiatedSSB* IE in TS 38.331 Sec 6 |
| 70 | 12>SSB Index | ELEMENT | TRUE | *ssb-Index* IE in TS 38.331 Sec 6 |  |
| 71 | 12>Is Quasi colocolo | ELEMENT | FALSE | *isQuasiColocated* IE in TS 38.331 Sec 6 |  |
| 72 | 11>CHOICE *Frequency Domain Allocation* | STRUCTURE |  |  | *frequencyDomainnAllocation* IE in TS 38.331 Sec 6 |
| 73 | 12>Frequency Domain Allocation Row 1 | ELEMENT | FALSE | *row1* IE in TS 38.331 Sec 6 |  |
| 74 | 12>Frequency Domain Allocation Row 2 | ELEMENT | FALSE | *row2* IE in TS 38.331 Sec 6 |  |
| 75 | 11>First OFDM Symbol in Time Domain | ELEMENT | FALSE | *firstOFDMSymbolInTimeDomain* IE in TS 38.331 Sec 6 |  |
| 76 | 11>Sequence Generation Config | ELEMENT | FALSE | *sequenecGenerationConfig* IE in TS 38.331 Sec 6 |  |
| 77 | 4>Absolute Threshold SSB – Block Consolidation | STRUCTURE |  |  | *absThreshSS-BlocksConsolidation* IE in TS 38.331 Sec 6 |
| 78 | 5>Block Consolidation Threshold RSRP | ELEMENT | FALSE | *RSRP-Range* IE in TS 38.331 Sec 6 |  |
| 79 | 5>Block Consolidation Threshold RSRQ | ELEMENT | FALSE | *RSRQ-Range* IE in TS 38.331 Sec 6 |  |
| 80 | 5>Block Consolidation Threshold SINR | ELEMENT | FALSE | *SINR-Range* IE in TS 38.331 Sec 6 |  |
| 81 | 4>Absolute Threshold CSI RS Consolidation | STRUCTURE |  |  | *absThreshCSI-RS-Consolidation* IE in TS 38.331 Sec 6 |
| 82 | 5>RS Consolidation Threshold RSRP | ELEMENT | FALSE | *RSRP-Range* IE in TS 38.331 Sec 6 |  |
| 83 | 5>RS Consoldation Threshold RSRQ | ELEMENT | FALSE | *RSRQ-Range* IE in TS 38.331 Sec 6 |  |
| 84 | 5>RS Consolidated Threshold SINR | ELEMENT | FALSE | *SINR-Range* IE in TS 38.331 Sec 6 |  |
| 91 | 4>Number of SS blocks to average | ELEMENT | FALSE | *nrofSS-BlocksToAverage* IE in TS 38.331 Sec 6 |  |
| 92 | 4>Number of CSI RS Resources to average | ELEMENT | FALSE | *nrofCSI-RS-ResouresToAverage* IE in TS 38.331 Sec 6 |  |
| 93 | 4>Quantity Config Index | ELEMENT | TRUE | *quantityConfigIndex* IE in TS 38.331 Sec 6 |  |
| 100 | 4>Q-Offset MO Range Sequence | STRUCTURE |  |  | *offsetMO* IE in TS 38.331 Sec 6 |
| 101 | 5>RSRP Offset SSB | ELEMENT | FALSE | *rsrpOffsetSSB* IE in TS 38.331 Sec 6 |  |
| 102 | 5>RSRQ Offset SSB | ELEMENT | FALSE | *rsrqOffsetSSB* IE in TS 38.331 Sec 6 |  |
| 103 | 5>SINR Offset SSB | ELEMENT | FALSE | *sinrOffsetSSB* IE in TS 38.331 Sec 6 |  |
| 104 | 5>RSRP Offset CSI RS | ELEMENT | FALSE | *rsrpOffsetCSI-RS* IE in TS 38.331 Sec 6 |  |
| 105 | 5>RSRQ Offset CSI RS | ELEMENT | FALSE | *rsrqOffsetCSI-RS* IE in TS 38.331 Sec 6 |  |
| 106 | 5>SINR Offset CSI RS | ELEMENT | FALSE | *sinrOffsetCSI-RS* IE in TS 38.331 Sec 6 |  |
| 107 | 4>Cells to Remove List | LIST |  |  | *cellsToRemoveList* IE in TS 38.331 Sec 6 |
| 108 | 5>Cell to Remove Item | STRUCTURE |  |  |  |
| 109 | 6>Cell to Remove - Physical Cell ID | ELEMENT | TRUE | *PhysCellID* IE in TS 38.331 Sec 6 |  |
| 110 | 4>Cells to modify or add for modification List | LIST |  |  | *CellsToAddModList* IE in TS 38.331 Sec 6 |
| 111 | 5>Cell to modify or add for modification Item | STRUCTURE |  |  | *CellsToAdd* IE in TS 38.331 Sec 6 |
| 112 | 6>Cell to modify or add for modification - Physical Cell ID | ELEMENT | TRUE | *PhysCellID* IE in TS 38.331 Sec 6 |  |
| 113 | 6>Cell Individual Offset | STRUCTURE |  |  | *cellIndividualOffset* IE in TS 38.331 Sec 6 |
| 115 | 7>RSRP Offset SSB | ELEMENT | FALSE | *rsrpOffsetSSB* IE in TS 38.331 Sec 6 |  |
| 116 | 7>RSRQ Offset SSB | ELEMENT | FALSE | *rsrqOffsetSSB* IE in TS 38.331 Sec 6 |  |
| 117 | 7>SINR Offset SSB | ELEMENT | FALSE | *sinrOffsetSSB* IE in TS 38.331 Sec 6 |  |
| 118 | 7>RSRP Offset CSI RS | ELEMENT | FALSE | *rsrpOffsetCSI-RS* IE in TS 38.331 Sec 6 |  |
| 119 | 7>RSRQ Offset CSI RS | ELEMENT | FALSE | *rsrqOffsetCSI-RS* IE in TS 38.331 Sec 6 |  |
| 120 | 7>SINR Offset CSI RS | ELEMENT | FALSE | *sinrOffsetCSI-RS* IE in TS 38.331 Sec 6 |  |
| 121 | 4>Black cells to Remove List | LIST |  |  | *blackCellsToRemoveList* IE in TS 38.331 Sec 6 |
| 122 | 5>Black cell to Remove Item | STRUCTURE |  |  |  |
| 123 | 6>Black cell to Remove – Physical Cell Range Index | ELEMENT | TRUE | *PCI-RangeIndex* IE in TS 38.331 Sec 6 |  |
| 125 | 4>Black cells to modify or add for modification List | LIST |  |  | *blackCellsToAddModList* IE in TS 38.331 Sec 6 |
| 126 | 5>Black cell to modify or add for modification Item | STRUCTURE |  |  | *PCI-RangeElement* IE in TS 38.331 Sec 6 |
| 127 | 6>Black cell to modify or add for modification – Physical Cell Range Index | ELEMENT | TRUE | *PCI-RangeIndex* IE in TS 38.331 Sec 6 |  |
| 128 | 6>Physical Cell ID - Range | STRUCTURE |  |  | *PCI-Range* IE in TS 38.331 Sec 6 |
| 129 | 7>PCI Range Start | ELEMENT | TRUE | *PhysCellId* IE in TS 38.331 Sec 6 |  |
| 130 | 7>PCI Range | ELEMENT | FALSE | *range* IE in TS 38.331 Sec 6 |  |
| 131 | 4>White cells to Remove List | LIST |  |  | *whiteCellsToRemoveList* IE in TS 38.331 Sec 6 |
| 132 | 5>White cell to Remove Item | STRUCTURE |  |  | *whiteCellsToRemoveList* IE in TS 38.331 Sec 6 |
| 133 | 6>White cell to Remove – Physical Cell Range Index | ELEMENT | TRUE | *PCI-RangeIndex* IE in TS 38.331 Sec 6 |  |
| 135 | 4>White cells to modify or add for modification List | LIST |  |  | *whiteCellsToAddModList* IE in TS 38.331 Sec 6 |
| 136 | 5>White cell to modify or add for modification Item | STRUCTURE |  |  | *PCI-RangeElement* IE in TS 38.331 Sec 6 |
| 137 | 6>White cell to modify or add for modification – Physical Cell Range Index | ELEMENT | TRUE | *PCI-RangeIndex* IE in TS 38.331 Sec 6 |  |
| 138 | 6>Physical Cell ID - Range | STRUCTURE |  |  | *PCI-Range* IE in TS 38.331 Sec 6 |
| 139 | 7>PCI Range Start | ELEMENT | TRUE | *physCellId* IE in TS 38.331 Sec 6 |  |
| 140 | 7>PCI Range | ELEMENT | FALSE | *range* IE in TS 38.331 Sec 6 |  |
| 141 | 4>Frequency Band Indicator NR | ELEMENT | TRUE | *freqBandIndicatorNR* IE in TS 38.331 Sec 6 |  |
| 142 | 4>Measurement Cycle Secondary cell | ELEMENT | FALSE | *measCycleSCell* IE in TS 38.331 Sec 6 |  |
| 151 | 3>*E-UTRA MO* | STRUCTURE |  |  | *MeasObjectEUTRA* IE in TS 38.331 Sec 6 |
| 152 | 4>E-UTRA Carrier Frequency | ELEMENT | TRUE | *carrierFreq* IE in TS 38.331 Sec 6 |  |
| 153 | 4>E-UTRA Allowed Measurement Bandwidth | ELEMENT | FALSE | *allowedMeasBandwidth* IE in TS 38.331 Sec 6 |  |
| 161 | 4>List of E-UTRA cells to remove | LIST |  |  | *cellsToRemoveListEUTRAN* IE in TS 38.331 Sec 6 |
| 162 | 5>E-UTRA Cell to remove Item | STRUCTURE |  |  |  |
| 164 | 6>E-UTRA PCI to remove | ELEMENT | TRUE | *EUTRA-PhysCellID* IE in TS 38.331 Sec 6 | Note that RIC cannot use the Cell Index unless informed by the E2 node, so PCI is used here. |
| 171 | 4>List of E-UTRA cells to modify or add for modification | LIST |  |  | *cellsToAddModListEUTRAN* IE in TS 38.331 Sec 6 |
| 172 | 5>E-UTRA Cell to modify or add for modification Item | STRUCTURE |  |  |  |
| 173 | 6>E-UTRA Cell to modify or add for modification | STRUCTURE |  |  | *EUTRA-Cell* IE in TS 38.331 Sec 6 |
| 174 | 7>E-UTRA PCI to modify or add for modification | ELEMENT | TRUE | *EUTRA-PhysCellId* IE in TS 38.331 Sec 6 |  |
| 175 | 7>E-UTRA Cell Individual Offset | ELEMENT | FALSE | *cellIndividualOffset* IE in TS 38.331 Sec 6 |  |
| 181 | 4>List of E-UTRA black cells to remove | LIST |  |  | *blackCellsToRemoveListEUTRAN* IE in TS 38.331 Sec 6 |
| 182 | 5>E-UTRA black cell to remove Item | STRUCTURE |  |  |  |
| 184 | 6>E-UTRA PCI to remove | ELEMENT | TRUE | *EUTRA-PhysCellId* IE in TS 38.331 Sec 6 |  |
| 191 | 4>List of E-UTRA black cells to modify or add for modification | LIST |  |  | *blackCellsToAddModList* IE in TS 38.331 Sec 6 |
| 192 | 5>E-UTRA black cell to modify or add for modification item | STRUCTURE |  |  |  |
| 193 | 6>E-UTRA black cell to modify or add for modification | STRUCTURE |  |  | *EUTRA-BlackCell* IE in TS 38.331 Sec 6 |
| 194 | 7>E-UTRA Physical Cell ID Range | STRUCTURE |  |  | *EUTRA-PhysCellIdRange* IE in TS 38.331 Sec 6 |
| 195 | 8>E-UTRA PCI Start | ELEMENT | TRUE | *EUTRA-PhysCellId* IE in TS 38.331 Sec 6 |  |
| 196 | 8>E-UTRA PCI Range | ELEMENT | FALSE | *range* IE in TS 38.331 Sec 6 |  |
| 201 | 4>E-UTRA Presence Antenna Port 1 | ELEMENT | FALSE | *eutra-PresenceAntennaPort1* IE in TS 38.331 Sec 6 |  |
| 205 | 4>E-UTRA Q Offset Range | ELEMENT | FALSE | *eutra-Q-OffsetRange* IE in TS 38.331 Sec 6 |  |
| 210 | 4>Wideband RSRQ Measurement | ELEMENT | FALSE | *widebandRSRQ-Meas* IE in TS 38.331 Sec 6 |  |
| 301 | List of Report Config Objects to modify or add for modification | LIST |  |  | *ReportConfigToAddModList* IE in TS 38.331 Sec 6 |
| 302 | 1>Report Config Object to modify or add for modification Item | STRUCTURE |  |  | *ReportConfigToAddMod* IE in TS 38.331 Sec 6 |
| 303 | 2>Report Config Object ID | ELEMENT | TRUE | *ReportConfigID* IE in TS 38.331 Sec 6 | This is the ID used by the E2 node for the report config object for the UE via *RRCReconfiguration* message |
| 304 | 2>CHOICE *Report Config Type* | STRUCTURE |  |  | *reportConfig* IE in TS 38.331 Sec 6 |
| 311 | 3>*NR Report Config* | STRUCTURE |  |  | *ReportConfigNR* IE in TS 38.331 Sec 6 |
| 312 | 4>CHOICE *Report Type* | STRUCTURE |  |  | *reportType* IE in TS 38.331 Sec 6 |
| 313 | 5>Periodical Report Config | STRUCTURE |  |  | *PeriodicalReportConfig* IE in TS 38.331 Sec 6 |
| 314 | 6>NR RS Type | ELEMENT | FALSE | *NR-RS-Type* IE in TS 38.331 Sec 6 |  |
| 315 | 6>NR Report Interval | ELEMENT | FALSE | *ReportInterval* IE in TS 38.331 Sec 6 |  |
| 316 | 6>NR Report Amount | ELEMENT | FALSE | *reportAmount* IE in TS 38.331 Sec 6 |  |
| 317 | 6>Measurement Report Quantity | STRUCTURE |  |  | *MeasReportQuantity* IE in TS 38.331 Sec 6 |
| 318 | 7>MR RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 |  |
| 319 | 7>MR RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 |  |
| 320 | 7>MR SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 |  |
| 321 | 6>Maximum number of Report cells | ELEMENT | FALSE | *maxReportells* IE in TS 38.331 Sec 6 |  |
| 322 | 6>Report Quantity Reference Signal – Indexes | STRUCTURE |  |  | *reportQuantityRS-Indexes* IE in TS 38.331 Sec 6 |
| 323 | 7>Report Qty RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 |  |
| 324 | 7>Report Qty RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 |  |
| 325 | 7>Report Qty SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 |  |
| 326 | 6>Maximum number of reference signals – Indexes to Report | ELEMENT | FALSE | *maxNrofRS-IndexesToReport* IE in TS 38.331 Sec 6 |  |
| 327 | 6>Include Beam Measurements | ELEMENT | FALSE | *includeBeamMeasuremetns* IE in TS 38.331 Sec 6 |  |
| 328 | 6>Use WhiteCellList | ELEMENT | FALSE | *useWhiteCellList* IE in TS 38.331 Sec 6 |  |
| 331 | 5>Event Trigger Config | STRUCTURE |  |  | *EventTriggerConfig* IE in TS 38.331 Sec 6 |
| 332 | 6>CHOICE *Event ID* | STRUCTURE |  |  | *eventide* IE in TS 38.331 Sec 6 |
| 333 | 7>Event A1 | STRUCTURE |  |  | *eventA1* IE in TS 38.331 Sec 6 |
| 334 | 8>A1 Threshold | STRUCTURE |  |  | *a1-Threshold* IE in TS 38.331 Sec 6 |
| 335 | 9>CHOICE *A1 Threshold Type* | STRUCTURE |  |  | *MeasTriggerQuantity* IE in TS 38.331 Sec 6 |
| 336 | 10>A1 Threshold RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 | *RSRP-Range* IE |
| 337 | 10>A1 Threshold RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 | *RSRQ-Range* IE |
| 338 | 10>A1 Threshold SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 | *SINR-Range* IE |
| 339 | 9>A1 Report On Leave | ELEMENT | FALSE | *reportOnLeave* IE in TS 38.331 Sec 6 |  |
| 340 | 9>A1 Hysteresis | ELEMENT | FALSE | *hysteresis* IE in TS 38.331 Sec 6 |  |
| 341 | 9>A1 Time to Trigger | ELEMENT | FALSE | *timeToTrigger* IE in TS 38.331 Sec 6 |  |
| 343 | 7>Event A2 | STRUCTURE |  |  | *eventA2* IE in TS 38.331 Sec 6 |
| 344 | 8>A2 Threshold | STRUCTURE |  |  | *A2-Threshold* IE in TS 38.331 Sec 6 |
| 345 | 9>CHOICE *A2 Threshold Type* | STRUCTURE |  |  | *MeasTriggerQuantity* IE in TS 38.331 Sec 6 |
| 346 | 10>A2 Threshold RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 | *RSRP-Range* IE |
| 347 | 10>A2 Threshold RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 | *RSRQ-Range* IE |
| 348 | 10>A2 Threshold SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 | *SINR-Range* IE |
| 349 | 9>A2 Report On Leave | ELEMENT | FALSE | *reportOnLeave* IE in TS 38.331 Sec 6 |  |
| 350 | 9>A2 Hysteresis | ELEMENT | FALSE | *hysteresis* IE in TS 38.331 Sec 6 |  |
| 351 | 9>A2 Time to Trigger | ELEMENT | FALSE | *timeToTrigger* IE in TS 38.331 Sec 6 |  |
| 353 | 7>Event A3 | STRUCTURE |  |  | *eventA3* IE in TS 38.331 Sec 6 |
| 354 | 8>A3 Offset | STRUCTURE |  |  | *a3-Threshold* IE in TS 38.331 Sec 6 |
| 355 | 9>CHOICE *A3 Offset Type* | STRUCTURE |  |  | *MeasTriggerQuantityOffset* IE in TS 38.331 Sec 6 |
| 356 | 10>A3 Threshold RSRP Offset | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 |  |
| 357 | 10>A3 Threshold RSRQ Offset | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 |  |
| 358 | 10>A3 Threshold SINR Offset | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 |  |
| 359 | 9>A3 Report On Leave | ELEMENT | FALSE | *reportOnLeave* IE in TS 38.331 Sec 6 |  |
| 360 | 9>A3 Hysteresis | ELEMENT | FALSE | *hysteresis* IE in TS 38.331 Sec 6 |  |
| 361 | 9>A3 Time to Trigger | ELEMENT | FALSE | *timeToTrigger* IE in TS 38.331 Sec 6 |  |
| 362 | 9>Use White Cell List | ELEMENT | FALSE | *useWhiteCellList* IE in TS 38.331 Sec 6 |  |
| 363 | 7>Event A4 | STRUCTURE |  |  | *eventA4* IE in TS 38.331 Sec 6 |
| 364 | 8>A4 Threshold | STRUCTURE |  |  | *A4-Threshold* IE in TS 38.331 Sec 6 |
| 365 | 9>CHOICE *A4 Threshold Type* | STRUCTURE |  |  | *MeasTriggerQuantity* IE in TS 38.331 Sec 6 |
| 366 | 10>A4 Threshold RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 | *RSRP-Range* IE |
| 367 | 10>A4 Threshold RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 | *RSRQ-Range* IE |
| 368 | 10>A4 Threshold SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 | *SINR-Range* IE |
| 369 | 9>A4 Report On Leave | ELEMENT | FALSE | *reportOnLeave* IE in TS 38.331 Sec 6 |  |
| 370 | 9>A4 Hysteresis | ELEMENT | FALSE | *hysteresis* IE in TS 38.331 Sec 6 |  |
| 371 | 9>A4 Time to Trigger | ELEMENT | FALSE | *timeToTrigger* IE in TS 38.331 Sec 6 |  |
| 372 | 9>Use White Cell List | ELEMENT | FALSE | *useWhiteCellList* IE in TS 38.331 Sec 6 |  |
| 375 | 7>Event A5 | STRUCTURE |  |  | *eventA5* IE in TS 38.331 Sec 6 |
| 376 | 8>A5 Threshold 1 | STRUCTURE |  |  | *a5-Threshold1* IE in TS 38.331 Sec 6 |
| 377 | 9>CHOICE *A5 Threshold1 Type* | STRUCTURE |  |  | *MeasTriggerQuantity* IE in TS 38.331 Sec 6 |
| 378 | 10>A5 Threshold1 RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 | *RSRP-Range* IE |
| 379 | 10>A5 Threshold1 1 RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 | *RSRQ-Range* IE |
| 380 | 10>A5 Threshold1 SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 | *SINR-Range* IE |
| 381 | 9>CHOICE *A5 Threshold2 Type* | STRUCTURE |  |  | *a5-Threshold2* IE in TS 38.331 Sec 6 |
| 382 | 10>A5 Threshold2 RSRP | ELEMENT | FALSE | *MeasTriggerQuantity* IE in TS 38.331 Sec 6 |  |
| 379 | 10>A5 Threshold2 RSRQ | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 | *RSRP-Range* IE |
| 380 | 10>A5 Threshold2 SINR | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 | *RSRQ-Range* IE |
| 381 | 9>A5 Report On Leave | ELEMENT | FALSE | *reportOnLeave* IE in TS 38.331 Sec 6 |  |
| 382 | 9>A5 Hysteresis | ELEMENT | FALSE | *hysteresis* IE in TS 38.331 Sec 6 |  |
| 383 | 9>A5 Time to Trigger | ELEMENT | FALSE | *timeToTrigger* IE in TS 38.331 Sec 6 |  |
| 384 | 9>Use White Cell List | ELEMENT | FALSE | *useWhiteCellList* IE in TS 38.331 Sec 6 |  |
| 391 | 7>Event A6 | STRUCTURE |  |  | *eventA6* IE in TS 38.331 Sec 6 |
| 392 | 8>A6 Threshold | STRUCTURE |  |  | *A6-Threshold* IE in TS 38.331 Sec 6 |
| 393 | 9>CHOICE *A6 Threshold Type* | STRUCTURE |  |  | *MeasTriggerQuantityOffset* IE in TS 38.331 Sec 6 |
| 394 | 10>A6 Threshold RSRP Offset | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 |  |
| 395 | 10>A6 Threshold RSRQ Offset | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 |  |
| 396 | 10>A6 Threshold SINR Offset | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 |  |
| 397 | 9>A6 Report On Leave | ELEMENT | FALSE | *reportOnLeave* IE in TS 38.331 Sec 6 |  |
| 398 | 9>A6 Hysteresis | ELEMENT | FALSE | *hysteresis* IE in TS 38.331 Sec 6 |  |
| 399 | 9>A6 Time to Trigger | ELEMENT | FALSE | *timeToTrigger* IE in TS 38.331 Sec 6 |  |
| 400 | 9>Use White Cell List | ELEMENT | FALSE | *useWhiteCellList* IE in TS 38.331 Sec 6 |  |
| 405 | 5>Report CGI | STRUCTURE |  |  | *ReportCGI* IE in TS 38.331 Sec 6 |
| 406 | 6>Cell to Report CGI | ELEMENT | TRUE | *physCellId* IE in TS 38.331 Sec 6 |  |
| 411 | 5>Report SFTD – NR | STRUCTURE |  |  | *ReportSFTD-NR* IE in TS 38.331 Sec 6 |
| 412 | 6>Report SFTD – Measurement | ELEMENT | FALSE | *reportSFTD-Meas* IE in TS 38.331 Sec 6 |  |
| 413 | 6>Report RSRP | ELEMENT | FALSE | *reportRSRP* IE in TS 38.331 Sec 6 |  |
| 414 | 6>Report SFTD Neigh Meas | ELEMENT | FALSE | *reportSFTD-NeighMeas* IE in TS 38.331 Sec 6 |  |
| 415 | 6>DRX SFTD Neigh Meas | ELEMENT | FALSE | *drx-SFTD-NeighMeas* IE in TS 38.331 Sec 6 |  |
| 416 | 6>List of cells for which to report SFTD | LIST |  |  | *cellsForWhichToReportSFTD* IE in TS 38.331 Sec 6 |
| 417 | 7>Cell Item for reporting SFTD | STRUCTURE |  |  |  |
| 418 | 8>Physical Cell Identity | ELEMENT | TRUE | *physCellId* IE in TS 38.331 Sec 6 |  |
| 421 | 3>Report Config Inter RAT | STRUCTURE |  |  | *ReportConfigInterRAT* IE in TS 38.331 Sec 6 |
| 422 | 4>CHOICE *Report Type* | STRUCTURE |  |  | *reportType* IE in TS 38.331 Sec 6 |
| 423 | 5>Periodical Report Config Inter RAT | STRUCTURE |  |  | *PeriodicalReportConfigInterRAT* IE in TS 38.331 Sec 6 |
| 431 | 6>Periodical Inter-RAT Report Interval | ELEMENT | FALSE | *reportInterval* IE in TS 38.331 Sec 6 |  |
| 432 | 6>Periodical Inter-RAT Report Amount | ELEMENT | FALSE | *reportAmount* IE in TS 38.331 Sec 6 |  |
| 435 | 6>Periodical Inter-RAT Report Quantity | STRUCTURE |  |  | *reportQuantity* IE in TS 38.331 Sec 6 |
| 436 | 7>Inter-RAT RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 |  |
| 437 | 7>Inter-RAT RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 |  |
| 438 | 7>Inter-RAT SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 |  |
| 439 | 6>Maximum number of cells for reporting | ELEMENT | FALSE | *maxReportCells* IE in TS 38.331 Sec 6 |  |
| 441 | 5>Event Trigger Config Inter RAT | STRUCTURE |  |  | *EventTriggerConfigInterRAT* IE in TS 38.331 Sec 6 |
| 442 | 6>CHOICE *Event ID* | STRUCTURE |  |  | *eventId* IE in TS 38.331 Sec 6 |
| 451 | 7>Event B1 | STRUCTURE |  |  | *eventB1* IE in TS 38.331 Sec 6 |
| 452 | 8>B1 Threshold EUTRA | STRUCTURE |  |  | *b1-ThresholdEUTRA* IE in TS 38.331 Sec 6 |
| 453 | 9>E-UTRA RSRP | ELEMENT | FALSE | *RSRP-RangeEUTRA* IE in TS 38.331 Sec 6 |  |
| 454 | 9>E-UTRA RSRQ | ELEMENT | FALSE | *RSRQ-RangeEUTRA* IE in TS 38.331 Sec 6 |  |
| 455 | 9>E-UTRA SINR | ELEMENT | FALSE | *SINR-RangeEUTRA* IE in TS 38.331 Sec 6 |  |
| 456 | 8>Event B1 Report On Leave | ELEMENT | FALSE | *reportOnLeave* IE in TS 38.331 Sec 6 |  |
| 457 | 8>E-UTRA Hysteresis | ELEMENT | FALSE | *hystereisis* IE in TS 38.331 Sec 6 |  |
| 458 | 8>E-UTRA Time To Trigger | ELEMENT | FALSE | *timeToTrigger* IE in TS 38.331 Sec 6 |  |
| 471 | 7>Event B2 | STRUCTURE |  |  | *eventB2* IE in TS 38.331 Sec 6 |
| 472 | 8>B2 Threshold1 NR | STRUCTURE |  |  | *b2-Threshold1* IE in TS 38.331 Sec 6 |
| 475 | 9>B2 Threshold1 NR RSRP | ELEMENT | FALSE | *RSRP-Range* IE in TS 38.331 Sec 6 |  |
| 476 | 9>B2 Threshold1 NR RSRQ | ELEMENT | FALSE | *RSRQ-Range* IE in TS 38.331 Sec 6 |  |
| 477 | 9>B2 Threshold1 NR SINR | ELEMENT | FALSE | *SINR-Range* IE in TS 38.331 Sec 6 |  |
| 481 | 8>B2 Threshold2 E-UTRA | STRUCTURE |  |  | *b2-Threshold2EUTRA* IE in TS 38.331 Sec 6 |
| 482 | 9>B2 Threshold2 E-UTRA RSRP | ELEMENT | FALSE | *RSRP-RangeEUTRA* IE in TS 38.331 Sec 6 |  |
| 483 | 9>B2 Threshold2 E-UTRA RSRQ | ELEMENT | FALSE | *RSRQ-RangeEUTRA* IE in TS 38.331 Sec 6 |  |
| 484 | 9>B2 Threshold2 E-UTRA SINR | ELEMENT | FALSE | *SINR-RangeEUTRA* IE in TS 38.331 Sec 6 |  |
| 491 | 6>Inter-RAT Reference Signal Type | ELEMENT | FALSE | *rsType* IE in TS 38.331 Sec 6 |  |
| 492 | 6>Inter-RAT Report Interval | ELEMENT | FALSE | *reportInterval* IE in TS 38.331 Sec 6 |  |
| 493 | 6>Inter-RAT Report Amount | ELEMENT | FALSE | *reportAmount* IE in TS 38.331 Sec 6 |  |
| 501 | 6>Inter-RAT Report Quantity | STRUCTURE |  |  | *reportQuantity* IE in TS 38.331 Sec 6 |
| 502 | 7>Inter-RAT Report Quantity RSRP | ELEMENT | FALSE | *rsrp* IE in TS 38.331 Sec 6 |  |
| 503 | 7>Inter-RAT Report Quantity RSRQ | ELEMENT | FALSE | *rsrq* IE in TS 38.331 Sec 6 |  |
| 504 | 7>Inter-RAT Report Quantity SINR | ELEMENT | FALSE | *sinr* IE in TS 38.331 Sec 6 |  |
| 510 | 6>Maximum number of cells to be reported | ELEMENT | FALSE | *maxReportCells* IE in TS 38.331 Sec 6 |  |
| 519 | *CHOICE* NR SpCell RSRP Measurement Controlling | STRUCTURE |  |  | *s-MeasureConfig* IE in TS 38.331 Sec 6 |
| 520 | 1>SSB RSRP | ELEMENT | FALSE | *ssb-RSRP* IE in TS 38.331 Sec 6 |  |
| 521 | 1>CSI RSRP | ELEMENT | FALSE | *csi-RSRP* IE in TS 38.331 Sec 6 |  |
| 525 | Quantity Config | STRUCTURE |  |  | *QuantityConfig* IE in TS 38.331 Sec 6 |
| 526 | 1>Quantity Config NR List | LIST |  |  | *quantityConfigNR-List* IE in TS 38.331 Sec 6 |
| 527 | 2>Quantity Config NR | STRUCTURE |  |  | *quantityConfigNR* IE in TS 38.331 Sec 6 |
| 528 | 3>Quantity Config NR Cell | STRUCTURE |  |  | *quantityConfigCell* IE in TS 38.331 Sec 6 |
| 529 | 4>SSB Filter Config | STRUCTURE |  |  | *ssb-FilterConfig* IE in TS 38.331 Sec 6 |
| 530 | 5>SSB Filter Coefficient RSRP | ELEMENT | FALSE | *filterCoefficientRSRP* IE in TS 38.331 Sec 6 |  |
| 531 | 5>SSB Filter Coefficient RSRQ | ELEMENT | FALSE | *filterCoefficientRSRQ* IE in TS 38.331 Sec 6 |  |
| 532 | 5>SSB Filter Coefficient RS-SINR | ELEMENT | FALSE | *filterCoefficientSINR* IE in TS 38.331 Sec 6 |  |
| 533 | 4>CSI RS Filter Config | STRUCTURE |  |  | *csi-RS-FilterConfig* IE in TS 38.331 Sec 6 |
| 534 | 5>CSI RS Filter Coefficient RSRP | ELEMENT | FALSE | *filterCoefficientRSRP* IE in TS 38.331 Sec 6 |  |
| 535 | 5>CSI RS Filter Coefficient RSRQ | ELEMENT | FALSE | *filterCoefficientRSRQ* IE in TS 38.331 Sec 6 |  |
| 536 | 5>CSI RS Filter Coefficient RS-SINR | ELEMENT | FALSE | *filterCoefficientSINR* IE in TS 38.331 Sec 6 |  |
| 541 | 1>Quantity Config E-UTRA | STRUCTURE |  |  | *quantityConfigEUTRA* IE in TS 38.331 Sec 6 |
| 542 | 2>E-UTRA Filter Coefficient RSRP | ELEMENT | FALSE | *filterCoefficientRSRP* IE in TS 38.331 Sec 6 |  |
| 543 | 2>E-UTRA Filter Coefficient RSRQ | ELEMENT | FALSE | *filterCoefficientRSRQ* IE in TS 38.331 Sec 6 |  |
| 544 | 2>E-UTRA Filter Coefficient RS-SINR | ELEMENT | FALSE | *filterCoefficientSINR* IE in TS 38.331 Sec 6 |  |
| 551 | Measurement Gap Config | STRUCTURE |  |  | *MeasGapConfig IE in TS 38.331 Sec 6* |
| 552 | 1>Setup or Release Gap FR2 | ELEMENT | FALSE | ENUMERATED (setup, release,…) | *SetupRelease* IE in TS 38.331 Sec 6 |
| 553 | 1>Gap FR2 to Setup | STRUCTURE |  |  | *gapFR2 IE in TS 38.331 Sec 6* |
| 554 | 2>FR2 Gap Offset | ELEMENT | FALSE | *gapOffset* IE *in TS 38.331 Sec 6* |  |
| 555 | 2>FR2 Measurement Gap Length | ELEMENT | FALSE | *mgl* IE *in TS 38.331 Sec 6* |  |
| 556 | 2>FR2 Measurement Gap Repetition Period | ELEMENT | FALSE | *mgrp* IE *in TS 38.331 Sec 6* |  |
| 557 | 2>FR2 Measurement Gap Timing Analysis | ELEMENT | FALSE | *mgta* IE *in TS 38.331 Sec 6* |  |
| 558 | 2>FR2 Reference Serving Cell Indicator | ELEMENT | TRUE | *refServCellIndicator* IE *in TS 38.331 Sec 6* |  |
| 560 | 1>Setup or Release Gap FR1 | ELEMENT | FALSE | ENUMERATED (setup, release,…) | *SetupRelease* IE in TS 38.331 Sec 6 |
| 561 | 1>Gap FR1 to Setup | STRUCTURE |  |  | *gapFR1 IE in TS 38.331 Sec 6* |
| 562 | 2>FR1 Gap Offset | ELEMENT | FALSE | *gapOffset* IE *in TS 38.331 Sec 6* |  |
| 563 | 2>FR1 Measurement Gap Length | ELEMENT | FALSE | *mgl* IE *in TS 38.331 Sec 6* |  |
| 564 | 2>FR1 Measurement Gap Repetition Period | ELEMENT | FALSE | *mgrp* IE *in TS 38.331 Sec 6* |  |
| 565 | 2>FR1 Measurement Gap Timing Analysis | ELEMENT | FALSE | *mgta* IE *in TS 38.331 Sec 6* |  |
| 566 | 2>FR1 Reference Serving Cell Indicator | ELEMENT | TRUE | *refServCellIndicator* IE *in TS 38.331 Sec 6* |  |
| 570 | 1>Setup or Release Gap UE | ELEMENT | FALSE | ENUMERATED (setup, release,…) | *SetupRelease* IE in TS 38.331 Sec 6 |
| 571 | 1>Gap UE to Setup | STRUCTURE |  |  | *gapUE IE in TS 38.331 Sec 6* |
| 572 | 2>UE Gap Offset | ELEMENT | FALSE | *gapOffset* IE *in TS 38.331 Sec 6* |  |
| 573 | 2>UE Measurement Gap Length | ELEMENT | FALSE | *mgl* IE *in TS 38.331 Sec 6* |  |
| 574 | 2>UE Measurement Gap Reptition Period | ELEMENT | FALSE | *mgrp* IE *in TS 38.331 Sec 6* |  |
| 575 | 2>UE Measurement Gap Timing Analysis | ELEMENT | FALSE | *mgta* IE *in TS 38.331 Sec 6* |  |
| 576 | 2>UE Reference Serving Cell Indicator | ELEMENT | TRUE | *refServCellIndicator* IE *in TS 38.331 Sec 6* |  |
| 581 | Measurement Gap Sharing Config | STRUCTURE |  |  | *MeasGapSharingConfig IE in TS 38.331 Sec 6* |
| 582 | 1>Setup or Release Gap Sharing FR2 | ELEMENT | FALSE | ENUMERATED(setup,release,…) | *SetupRelease* IE in TS 38.331 Sec 6 |
| 583 | 1>Gap Sharing FR2 for setup | ELEMENT | FALSE | *gapFR2* IE *in TS 38.331 Sec 6* |  |
| 584 | 1>Setup or Release Gap Sharing FR1 | ELEMENT | FALSE | ENUMERATED (setup,release,…) | *SetupRelease* IE in TS 38.331 Sec 6 |
| 585 | 1>Gap Sharing FR1 for setup | ELEMENT | FALSE | *gapFR1* IE *in TS 38.331 Sec 6* |  |
| 586 | 1>Setup or Release Gap Sharing UE | ELEMENT | FALSE | ENUMERATED (setup,release,…) | *SetupRelease* IE in TS 38.331 Sec 6 |
| 587 | 1>Gap Sharing UE | ELEMENT | FALSE | *gapUE* IE *in TS 38.331 Sec 6* |  |

#### 8.4.10.3 Delete MR Configuration

Upon receiving the *RIC Control Request* message with the *Measurement Report Configuration Control* Service Style and the *Modify MR Configuration* control action, the E2 node shall invoke RRC procedures related to deletion of MR Configuration and include the IEs corresponding to one or more of parameters described below in the related interface or RRC messages.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | List of Measurement Objects to Remove | LIST |  |  | *measObjectToRemoveList* IE in TS 38.331 Sec 6 |
| 2 | 1>Measurement Object to Remove Item | STRUCTURE |  |  | *MeasObjectToRemove* IE in TS 38.331 Sec 6 |
| 3 | 2>Measurement Object ID | ELEMENT | TRUE | *MeasObjectID* IE in TS 38.331 Sec 6 |  |
| 4 | List of Report Config Objects to Remove | LIST |  |  | *ReportConfigToRemoveList* IE in TS 38.331 Sec 6 |
| 5 | 1>Report Config Object to Remove Item | STRUCTURE |  |  | *ReportConfigToRemove* IE in TS 38.331 Sec 6 |
| 6 | 2>Report Config Object ID | ELEMENT | TRUE | *ReportConfigID* IE in TS 38.331 Sec 6 |  |
| 7 | List of Measurement IDs to Remove | LIST |  |  | *measIdToRemoveList* IE in TS 38.331 Sec 6 |
| 8 | 1>Measurement ID Item to Remove | STRUCTURE |  |  |  |
| 9 | 2>Measurement ID | ELEMENT | TRUE | *MeasID* IE in TS 38.331 Sec 6 |  |

#### 8.4.10.4 Control Outcome parameters

Upon processing the *RRCReconfiguration* message with the control action parameters sent by the RIC, the E2 node shall report the call processing outcome to the RIC as a response to the control action based on the following parameters.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 1 | List of Measurement Objects successfully added | LIST |  | *0..1* | *MeasObjectToAddModList* IE in TS 38.331 Sec 6 |
| 2 | >Measurement Object successfully added Item | STRUCTURE |  | *1..<maxMeasObjects>* | *MeasObjectId* IE in TS 38.331 Sec 6 |
| 3 | >>Measurement Object sequence ID | ELEMENT | TRUE | INTEGER (1..maxMeasObject,…) | This is the ID used by the RIC for the measurement object it seeks to add via the control service style |
| 4 | >>Measurement Object ID | ELEMENT | TRUE | *MeasObjectID* IE in TS 38.331 Sec 6 | This is the ID used by the E2 node for the measurement object for the UE via *RRCReconfiguration* message |
| 11 | List of Measurement Objects failed to be added | LIST |  | *0..1* | *MeasObjectToAddModList* IE in TS 38.331 Sec 6 |
| 12 | >Measurement Object failed to be added Item | STRUCTURE |  | *1..<maxMeasObjects>* | *MeasObjectId* IE in TS 38.331 Sec 6 |
| 14 | >>Measurement Object sequence ID | ELEMENT | TRUE | INTEGER (1..maxMeasObject,…) | This is the ID used by the RIC for the measurement object it seeks to add via the control service style |
| 15 | >>Addition failure cause | ELEMENT | FALSE | PrintableString(SIZE(1.. 150, ...)) | Failure cause string |
| 21 | List of Measurement Objects successfully modified | LIST |  | *0..1* | *MeasObjectToAddModList* IE in TS 38.331 Sec 6 |
| 22 | >Measurement Object successfully modified Item | STRUCTURE |  | *1..<maxMeasObjects>* | *MeasObjectId* IE in TS 38.331 Sec 6 |
| 24 | >>Measurement Object ID | ELEMENT | TRUE | *MeasObjectID* IE in TS 38.331 Sec 6 | This is the ID used by the E2 node for the measurement object for the UE via *RRCReconfiguration* message |
| 31 | List of Measurement Objects failed to be modified | LIST |  | *0..1* | *MeasObjectToAddModList* IE in TS 38.331 Sec 6 |
| 32 | >Measurement Object failed to be modified Item | STRUCTURE |  | *1..<maxMeasObjects>* | *MeasObjectId* IE in TS 38.331 Sec 6 |
| 34 | >>Measurement Object ID | ELEMENT | TRUE | *MeasObjectID* IE in TS 38.331 Sec 6 | This is the ID used by the E2 node for the measurement object for the UE via *RRCReconfiguration* message |
| 35 | >>Modification Failure Cause | ELEMENT | FALSE | PrintableString(SIZE(1.. 150, ...)) | Failure cause string |
| 41 | List of Measurement Objects successfully deleted | LIST |  | *0..1* | *MeasObjectToRemoveList* IE in TS 38.331 Sec 6 |
| 42 | >Measurement Object successfully deleted Item | STRUCTURE |  | *1..<maxMeasObjects>* | *MeasObjectId* IE in TS 38.331 Sec 6 |
| 44 | >>Measurement Object ID | ELEMENT | TRUE | *MeasObjectID* IE in TS 38.331 Sec 6 | This is the ID used by the E2 node for the measurement object for the UE via *RRCReconfiguration* message |
| 51 | List of Measurement Objects failed to be deleted | LIST |  | *0..1* | *MeasObjectToRemoveList* IE in TS 38.331 Sec 6 |
| 52 | >Measurement Object failed to be deleted Item | STRUCTURE |  | *1..<maxMeasObjects>* | *MeasObjectId* IE in TS 38.331 Sec 6 |
| 54 | >>Measurement Object ID | ELEMENT | TRUE | *MeasObjectID* IE in TS 38.331 Sec 6 | This is the ID used by the E2 node for the measurement object for the UE via *RRCReconfiguration* message |
| 55 | >>Delete Failure Cause | ELEMENT | FALSE | PrintableString(SIZE(1.. 150, ...)) | Failure cause string |
| 61 | List of Report Config Objects successfully added | LIST |  | *0..1* | *ReportConfigToAddModList* IE in TS 38.331 Sec 6 |
| 62 | >Report Config Object successfully added Item | STRUCTURE |  | *1..<maxReportConfigObjects>* | *maxReportConfigId* IE in TS 38.331 Sec 6 |
| 63 | >>Report Config Object sequence ID | ELEMENT | TRUE | INTEGER (1..maxReportConfigObjects,…) | This is the ID used by the RIC for the report config object it seeks to add via the control service style |
| 64 | >>Report Config Object ID | ELEMENT | TRUE | *ReportConfigID* IE in TS 38.331 Sec 6 | This is the ID used by the E2 node for the report config object for the UE via *RRCReconfiguration* message |
| 71 | List of Report Config Objects failed to be added | LIST |  | *0..1* | *ReportConfigToAddModList* IE in TS 38.331 Sec 6 |
| 72 | >Report Config Object failed to be added Item | STRUCTURE |  | *1..<maxReportConfigObjects>* | *maxReportConfigId* IE in TS 38.331 Sec 6 |
| 74 | >>Report Config Object sequence ID | ELEMENT | TRUE | INTEGER (1..maxReportConfigObjects,…) | This is the ID used by the RIC for the report config object it attempts to add via the control service style |
| 75 | >>Addition failure cause | ELEMENT | FALSE | PrintableString(SIZE(1.. 150, ...)) | Failure cause string |
| 81 | List of Report Config Objects successfully modified | LIST |  | *0..1* | *ReportConfigToAddModList* IE in TS 38.331 Sec 6 |
| 82 | >Report Config Object successfully modified Item | STRUCTURE |  | *1..<maxReportConfigObjects>* | *maxReportConfigId* IE in TS 38.331 Sec 6 |
| 84 | >>Report Config Object ID | ELEMENT | TRUE | *ReportConfigID* IE in TS 38.331 Sec 6 | This is the ID used by the E2 node for the report config object for the UE via *RRCReconfiguration* message |
| 91 | List of Report Config Objects failed to be modified | LIST |  | *0..1* | *ReportConfigToAddModList* IE in TS 38.331 Sec 6 |
| 92 | >Report Config Object failed to be modified Item | STRUCTURE |  | *1..<maxReportConfigObjects>* | *maxReportConfigId* IE in TS 38.331 Sec 6 |
| 94 | >>Report Config Object ID | ELEMENT | TRUE | *ReportConfigID* IE in TS 38.331 Sec 6 | This is the ID used by the E2 node for the report config object for the UE via *RRCReconfiguration* message |
| 95 | >>Modification Failure Cause | ELEMENT | FALSE | PrintableString(SIZE(1.. 150, ...)) | Failure cause string |
| 101 | List of Report Config Objects successfully deleted | LIST |  | *0..1* | *ReportConfigToRemoveList* IE in TS 38.331 Sec 6 |
| 102 | >Report Config Object successfully deleted Item | STRUCTURE |  | *1..<maxReportConfigObjects>* | *maxReportConfigId* IE in TS 38.331 Sec 6 |
| 104 | >>Report Config Object ID | ELEMENT | TRUE | *ReportConfigID* IE in TS 38.331 Sec 6 | This is the ID used by the E2 node for the report config object for the UE via *RRCReconfiguration* message |
| 111 | List of Report Config Objects failed to be deleted | LIST |  | *0..1* | *ReportConfigToRemoveList* IE in TS 38.331 Sec 6 |
| 112 | >Report Config Object failed to be deleted Item | STRUCTURE |  | *1..<maxReportConfigObjects>* | *maxReportConfigId* IE in TS 38.331 Sec 6 |
| 114 | >>Report Config Object ID | ELEMENT | TRUE | *ReportConfigID* IE in TS 38.331 Sec 6 | This is the ID used by the E2 node for the report config object for the UE via *RRCReconfiguration* message |
| 115 | >>Delete Failure Cause | ELEMENT | FALSE | PrintableString(SIZE(1.. 150, ...)) | Failure cause string |
| 116 | List of Measurement IDs successfully added | LIST |  | *0..1* | *MeasIdToAddModList* IE in TS 38.331 Sec 6 |
| 117 | >Meaasurement ID successfully added Item | STRUCTURE |  | *1..<maxMeasId>* | *maxNrofMeasId* IE in TS 38.331 Sec 6 |
| 118 | >>Measurement ID | ELEMENT | TRUE | *MeasId* IE in TS 38.331 Sec 6 |  |
| 119 | >>Measurement Object ID | ELEMENT | TRUE | *MeasObjectID* IE in TS 38.331 Sec 6 |  |
| 120 | >>Report Config Object ID | ELEMENT | TRUE | *ReportConfigID* IE in TS 38.331 Sec 6 |  |
| 125 | List of Measurement IDs successfully removed | LIST |  | *0..1* | *measIdToRemoveList* IE in TS 38.331 Sec 6 |
| 126 | >Measurement ID successfully removed Item | STRUCTURE |  | *1..<maxMeasID>* | *maxNrofMeasId* IE in TS 38.331 Sec 6 |
| 127 | >>Measurement ID | ELEMENT | TRUE | *MeasId* IE in TS 38.331 Sec 6 |  |
| 129 | List of Measurement IDs failed to be removed | LIST |  | *0..1* | *measIdToRemoveList* IE in TS 38.331 Sec 6 |
| 130 | >Measurement ID failed to be removed Item | STRUCTURE |  | *1..<maxMeasID>* | *maxNrofMeasId* IE in TS 38.331 Sec 6 |
| 131 | >>Measurement ID | ELEMENT | TRUE | *MeasId* IE in TS 38.331 Sec 6 |  |
| 132 | >>Removal failure Cause | ELEMENT | FALSE | PrintableString(SIZE(1.. 150, ...)) | Failure cause string |
| 135 | Received Timestamp | ELEMENT | FALSE | OCTET STRING (SIZE(8)) | Time RIC Control Request message received by RAN Function over E2 interface.  Carries UTC time encoded as the 64-bit timestamp format as defined in section Section 6 of IETF RFC 5905 [30] containing both seconds and fraction parts. |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxMeasObjects | Maximum no. of measurement objects supported by the RAN function. The value is <*64*>. |
| maxReportConfigObjects | Maximum no. of report configuration objects supported by the RAN function. The value is <*64*>. |
| maxMeasID | Maximum no. of measurement IDs supported by the RAN function. The value is *<64>* |

## 8.5 RAN parameters for POLICY services

8.5.1 Approach

The RAN parameters associated with each policy action being controlled by Near-RT RIC described in Section 7.7 are listed.

There are two types of E2 policies:

i) **Control action policy**: In this type, the near-RT RIC tells the E2 node on the specific per-UE control action that needs to be performed, upon meeting a given policy condition for a given UE or a group of UEs, for a given cell and/or for a given E2 node. This policy type is descriptive in nature. The control action is defined with respect to individual UEs and UE-specific bearers, flows, PDU sessions, etc.

ii) **Offset based policy**: In this type, the near-RT RIC offers a generic prescriptive guidance to the E2 node on how it shall deviate from default behaviour via the application of offset parameters provided in the POLICY Action IE. Different POLICY Action IEs are associated with different POLICY conditions described in terms of UE and E2 Node characteristics. As defined in section 6.6.3, offset parameters are to be applied to default parameters according to the following rules:

- INTEGER and REAL default parameters: Offset parameter have the same data type as default parameter and is added to default parameter with positive offset parameter values increasing default value and negative offset parameter values decreasing default value. That is, policy modifies the target call process such that:  
Value to be applied = (Default Parameter) + (Offset Parameter)- ENUMERATED parameters: Offset parameter are of data type INTEGER and are used to select a different item in the ENUMERATED list, positive offset parameter values used to select items that are further on in the list, zero offset parameter values used to select the default value, negative offset parameter values used to select items that are earlier on in the list. When and if the offset parameter value results in the selection of an item in the ENUMERATED list that exceeds the ENUMERATED list length then the last item in the list is selected. When and if the offset parameter value results in the selection of an item in the ENUMERATED list that prior to the first item in the ENUMERATED list then the first item in the list is selected. That is, policy modifies the target call process such that:  
ENUMERATED List index = MIN [List length-1, MAX [0, (Default Parameter) + (Offset Parameter)] ]

8.5.1A Common RAN Parameters for POLICY services

The common set of RAN Parameters that can be used across all POLICY service styles is given in the table below.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 5001 | Measurement Object | ELEMENT | FALSE | ENUMERATED (UE, E2 Node,…) | If the value is *UE*, then the rest of the ensuing parameters related to PMs have UE-specific values for the UE ID. Else if the value is E2 Node, then the rest of the parameters shall have node-specific measurements | |
| 5002 | gNB DU Measurements | Refer to *gNB DU Measurements* structure in Section 8.1.1.14 | | | | |
| 5003 | >UE Throughput Measurements |
| 5004 | >Packet level measurements |
| 5005 | >Packet delay measurements |
| 5011 | gNB CU-UP Measurements | Refer to *gNB CU-UP Measurements* structure in Section 8.1.1.13 | | | | |
| 5012 | >PDCP data volume measurement |
| 5013 | >Packet delay measurements |
| 5021 | gNB CU-CP Measurements | Refer to *gNB CU-CP Measurements* structure in Section 8.1.1.12 | | | | |
| 5022 | >Inter-gNB handovers |
| 5023 | >Intra-gNB handovers |
| 5024 | >RRC connection related measurements |
| 5025 | >QoS flow-related measurements |
| 5026 | >DRB related measurements |
| 5027 | >PDU Session Management |
| 5028 | >Inter-system mobility measurements between 5GS and EPS |

In addition to using the above RAN Parameters, POLICY conditions may also use RAN parameters defined in Section 8.1 for RIC *Event Trigger* definition.

### 8.5.2 Radio Bearer Control

#### 8.5.2.0 Common RAN Parameters for Radio Bearer Control

The RAN Parameters pertaining to POLICY Conditions for the “Radio Bearer Control” policy service style used across all POLICY actions of the policy service style are listed in the below table.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 501 | DRB related measurements | Refer to *gNB CU-CP Measurements* structure in Section 8.1.1.12 where these parameters are defined. | | | | |
| 502 | List of QoS levels |
| 503 | >QoS level item |
| 504 | >>CHOICE QoS level |
| 505 | >>>5QI |
| 506 | >>>S-NSSAI |
| 507 | >>>>SST |
| 508 | >>>>SD |
| 509 | >>Number of DRBs successfully setup per QoS level |
| 510 | Total number of DRBs successfully setup for UE | ELEMENT | FALSE | INTEGER (0..64) | Total number of DRBs across all QoS levels for a UE. Maximum 64 DRBs can be setup for a UE. Refer to TS 38.473 [19] Section 9.2.2.1 | |
| 511 | UE DL Aggregate Maximum Bit Rate | ELEMENT | FALSE | *UE Aggregate Maximum Bit Rate Downlink* IE in TS 36.423 [17] clause 9.2.12 |  | |
| 512 | gNB CU-UP capacity | Refer to *E2 Node* structure in Section 8.1.1.11 where these parameters are defined | | | | |

In addition to using the above RAN Parameters for POLICY conditions, this service style also uses RAN parameters defined in Section 8.1. Accordingly, this service style supports Policy Conditions using the RAN parameters defined in Sections 8.1, 8.5.1 and those covered in the above table.

#### 8.5.2.1 DRB QoS Configuration

##### 8.5.2.1.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.2.1 Table 1.

##### 8.5.2.1.2 Offset

Editor’s Note: FFS

#### 8.5.2.2 QoS flow mapping configuration

##### 8.5.2.2.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.2.2 Table 1.

##### 8.5.2.2.2 Offset

Editor’s Note: FFS

#### 8.5.2.3 Logical channel configuration

##### 8.5.2.3.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.2.3 Table 1.

##### 8.5.2.3.2 Offset

Editor’s Note: FFS

#### 8.5.2.4 Radio Bearer Admission Control

##### 8.5.2.4.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.2.4 Table 1.

##### 8.5.2.4.2 Offset

#### 8.5.2.5 DRB Termination Control

##### 8.5.2.5.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.2.5 Table 1.

##### 8.5.2.5.2 Offset

Editor’s Note: FFS

#### 8.5.2.6 DRB Split Ratio Control

##### 8.5.2.6.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.2.6 Table 1.

##### 8.5.2.6.2 Offset

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 101 | Uplink PDCP Data Split Threshold offset | ELEMENT | FALSE | INTEGER | *UL Data Split Threshold* IE in TS 38.463 [21] Section 9.3.1.43 |
| 102 | Downlink PDCP Data Split | ELEMENT | FALSE | INTEGER | *Downlink PDCP Data Split* IE in 8.4.2.6 |

#### 8.5.2.7 PDCP Duplication Control

##### 8.5.2.7.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.2.7 Table 1.

##### 8.5.2.7.2 Offset

Editor’s Note: FFS

### 8.5.3 Radio Resource Allocation Control

#### 8.5.3.0 Common RAN Parameters for Radio Resource Allocation Control

The RAN Parameters pertaining to POLICY Conditions for the “Radio Resource Allocation Control” policy service style used across all POLICY actions of the policy service style are listed in the below table.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | Semantics Description |
| 501 | SPS Config | STRUCTURE |  |  | *SPS-Config* IE in TS 38.331 [22] |
| 502 | >Number of HARQ Processes | ELEMENT | FALSE | *nrofHARQ-Processes* IE in TS 38.331 [22] |  |
| 503 | Grant Configuration | STRUCTURE |  |  | *ConfiguredGrantConfig* IE in TS 38.331 [22] |
| 504 | >Number of HARQ Processes | ELEMENT | FALSE | *nrofHARQ-Processes* IE in TS 38.331 [22] |  |
| 505 | PDSCH Serving Cell Config Setup | STRUCTURE |  |  | *PDSCH-ServingCellConfig* IE in TS 38.331 [22] |
| 506 | >Number of HARQ Processes | ELEMENT | FALSE | *nrofHARQ-ProcessesForPDSCH* IE in TS 38.331 [22] |  |

In addition to using the above RAN Parameters for POLICY conditions, this service style also uses RAN parameters defined in Section 8.1. Accordingly, this service style supports Policy Conditions using the RAN parameters defined in Sections 8.1, 8.5.1 and those covered in the above table.

#### 8.5.3.1 DRX Parameter Configuration

##### 8.5.3.1.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.3.1 Table 1.

##### 8.5.3.1.2 Offset

Editor’s Note: FFS

#### 8.5.3.2 Scheduling Request Parameter Configuration

##### 8.5.3.2.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.3.2 Table 1.

##### 8.5.3.2.2 Offset

Editor’s Note: FFS

#### 8.5.3.3 Semi-Persistent Scheduling Parameter Configuration

##### 8.5.3.3.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.3.3 Table 1.

##### 8.5.3.3.2 Offset

Editor’s Note: FFS

#### 8.5.3.4 Configured Grant Configuration

##### 8.5.3.4.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.3.4 Table 1.

##### 8.5.3.4.2 Offset

Editor’s Note: FFS

#### 8.5.3.5 CQI table configuration

##### 8.5.3.5.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.3.5 Table 1.

##### 8.5.3.5.2 Offset

Editor’s Note: FFS

#### 8.5.3.6 Slice-level PRB quota

##### 8.5.3.6.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.3.6 Table 1.

##### 8.5.3.6.2 Offset

Editor’s Note: FFS

### 8.5.4 Connected Mode Mobility Control

#### 8.5.4.0 Common RAN Parameters for Connected Mode Mobility Control

The RAN Parameters pertaining to POLICY Conditions for the “Connected Mode Mobility Control” policy service style used across all POLICY actions of the policy service style are listed in the below table.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | | **RAN Parameter Name** | | **RAN Parameter Value Type** | **Key flag** | **RAN Parameter Definition** | |
| 501 | | List of Serving Cells | | LIST |  | Refer to *Handover Preparation* structure in 8.1.2.3.1 where this parameter is defined. | |
| 502 | | >Serving Cell Item | | STRUCTURE |  | Refer to *Handover Preparation* structure in 8.1.2.3.1 where this parameter is defined. | |
| 503 | | >>CHOICE *Cell Type* | | STRUCTURE |  | Refer to *Handover Preparation* structure in 8.1.2.3.1 where this parameter is defined. | |
| 504 | | >>>NR Cell | | STRUCTURE |  | Refer to *Handover Preparation* structure in 8.1.2.3.1 where this parameter is defined | |
| 505 | | >>>>NR CGI | | ELEMENT | TRUE | Refer to *NR Cell* structure in 8.1.1.1 where this parameter is defined | |
| 506 | | >>>>NR PCI | | ELEMENT | FALSE | Refer to *NR Cell* structure in 8.1.1.1 where this parameter is defined | |
| 507 | | >>>>PLMN Identity | | ELEMENT | FALSE | Refer to *NR Cell* structure in 8.1.1.1 where this parameter is defined | |
| 508 | >>>>Reported NR RRC Measurements | | | STRUCTURE |  | Refer to *Reported NR RRC Measurements* in 8.1.1.1 where this parameter is defined |
| 509 | >>>>>Cell Results | | | STRUCTURE |  | Refer to *Cell Results* structure in 8.1.1.1 where this parameter is defined |
| 510 | >>>>>>SSB Results | | | STRUCTURE |  | Refer to *SSB Results* structure in 8.1.1.1 where this parameter is defined |
| 511 | >>>>>>CSI-RS Results | | | STRUCTURE |  | Refer to *CSI-RS Results* structure in 8.1.1.1 where this parameter is defined |
| 512 | | >>>E-UTRA Cell | | STRUCTURE |  | Refer to *E-UTRA Cell* structure in 8.1.1.2 where this parameter is defined | |
| 513 | | >>>>ECGI | | ELEMENT | TRUE | Refer to *E-UTRA Cell* structure in 8.1.1.2 where this parameter is defined | |
| 514 | | >>>>PCI | | ELEMENT | FALSE | Refer to *E-UTRA Cell* structure in 8.1.1.2 where this parameter is defined | |
| 515 | | >>>>PLMN Identity | | ELEMENT | FALSE | Refer to *E-UTRA Cell* structure in 8.1.1.2where this parameter is defined | |
| 516 | | >>>>Reported LTE RRC Measurements | | STRUCTURE |  | Refer to *Reported LTE RRC Measurements* in 8.1.1.2 where this parameter is defined | |
| 521 | | List of Neighboring Cells | | LIST |  | Refer to *Handover Preparation* structure in 8.1.2.3.1 where this parameter is defined. | |
| 522 | | >Neighboring Cell Item | | STRUCTURE |  | Refer to *Handover Preparation* structure in 8.1.2.3.1 where this parameter is defined. | |
| 523 | | >>CHOICE *Cell Type* | | STRUCTURE |  | Refer to *Handover Preparation* structure in 8.1.2.3.1 where this parameter is defined. | |
| 524 | | >>>NR Cell | | STRUCTURE |  | Refer to *NR Cell* structure in 8.1.1.12 where this parameter is defined | |
| 525 | | >>>>NR CGI | | ELEMENT | TRUE | Refer to *NR Cell* structure in 8.1.1.12 where this parameter is defined | |
| 526 | | >>>>NR PCI | | ELEMENT | FALSE | Refer to *NR Cell* structure in 8.1.1.12 where this parameter is defined | |
| 527 | | >>>>PLMN Identity | | ELEMENT | FALSE | Refer to *NR Cell* structure in 8.1.1.12 where this parameter is defined | |
| 528 | | >>>>Reported NR RRC Measurements | | STRUCTURE |  | Refer to *Reported NR RRC Measurements* in 8.1.1.1 where this parameter is defined | |
| 529 | | >>>>>Cell Results | | STRUCTURE |  | Refer to *Cell Results* structure in 8.1.1.1 where this parameter is defined | |
| 530 | | >>>>>>SSB Results | | STRUCTURE |  | Refer to *SSB Results* structure in 8.1.1.1 where this parameter is defined | |
| 531 | | >>>>>>CSI-RS Results | | STRUCTURE |  | Refer to *CSI-RS Results* structure in 8.1.1.1 where this parameter is defined | |
| 532 | | >>>E-UTRA Cell | | STRUCTURE |  | Refer to *E-UTRA Cell* structure in 8.1.1.2 where this parameter is defined | |
| 533 | | >>>>ECGI | | STRUCTURE |  | Refer to *E-UTRA Cell* structure in 8.1.1.2 where this parameter is defined | |
| 534 | | >>>>PCI | | STRUCTURE |  | Refer to *E-UTRA Cell* structure in 8.1.1.2 where this parameter is defined | |
| 535 | | >>>>PLMN Identity | | ELEMENT | FALSE | Refer to *E-UTRA Cell* structure in 8.1.1.11 where this parameter is defined | |
| 536 | | >>>>Reported LTE RRC Measurements | | STRUCTURE |  | Refer to *Reported LTE RRC Measurements* in 8.1.1.2 where this parameter is defined | |
| 541 | | gNB Handover measurements | STRUCTURE | |  |  | |
| 542 | | >Inter-gNB handover measurements | STRUCTURE | |  | Refer to *Inter-gNB Handovers* structure in 8.1.1.12 where this parameter is defined | |
| 543 | | >Intra-gNB handover measurements | STRUCTURE | |  | Refer to *Intra-gNB Handovers* structure in 8.1.1.12 where this parameter is defined | |
| 544 | | >Inter-system mobility measurements | STRUCTURE | |  | Refer to *Inter-system mobility measurements between 5GS and EPS* structure in 8.1.1.12 where this parameter is defined | |
| 545 | | NR Composite Available Capacity Group | | STRUCTURE |  | Refer to *Composite Available Capacity Group* in 8.1.1.1 where this parameter is defined | |
| 546 | | E-UTRA Composite Available Capacity Group | | STRUCTURE |  | Refer to *Composite Available Capacity Group* in 8.1.1.2 where this parameter is defined | |

In addition to using the above RAN Parameters for POLICY conditions and all RAN Parameters identified in 8.5.1.this service style also uses RAN parameters defined in Section 8.1Accordingly, this service style supports Policy Conditions using the RAN parameters defined in Sections 8.1, 8.5.1 and those covered in the above table.

#### 8.5.4.1 Handover Control

##### 8.5.4.1.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.4.1 Table 1.

##### 8.5.4.1.2 Offset

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** |
| 101 | A1 Event Threshold offset | STRUCTURE |  |  | *EventA1* IE in 8.1.1.10 |
| 102 | >RSRP Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, i.e. RSRP threshold to be used is default RSRP+RSRP Offset |
| 103 | >RSRQ Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, i.e. RSRP threshold to be used is default RSRQ+RSRQ Offset |
| 104 | >SINR Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, i.e. RSRP threshold to be used is default SINR+SINR Offset |
| 105 | >Hysteresis | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 111 | A2 Event Threshold offset | STRUCTURE |  |  | *EventA2* IE in 8.1.1.10 |
| 112 | >RSRP Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 113 | >RSRQ Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 114 | >SINR Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 115 | >Hysteresis | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 121 | A3 Event Threshold offset | STRUCTURE |  |  | *EventA3* IE in 8.1.1.10 |
| 122 | >RSRP Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 123 | >RSRQ Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 124 | >SINR Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 125 | >Hysteresis | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 131 | A4 Event Threshold offset | STRUCTURE |  |  | *EventA4* IE in 8.1.1.10 |
| 132 | >RSRP Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 133 | >RSRQ Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 134 | >SINR Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 135 | >Hysteresis | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 140 | A5 Event Threshold offset | STRUCTURE |  |  | *EventA5* IE in 8.1.1.10 |
| 141 | >A5-Threshold1 offset | STRUCTURE |  |  | *EventA5* IE in 8.1.1.10 |
| 142 | >>RSRP Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 143 | >>RSRQ Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 144 | >>SINR Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 145 | >>Hysteresis | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 146 | >A5-Threshold2 offset | STRUCTURE |  |  | *EventA5* IE in 8.1.1.10 |
| 147 | >>RSRP Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 148 | >>RSRQ Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 149 | >>SINR Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 150 | >>Hysteresis Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 151 | A6 Event Threshold Offset | STRUCTURE |  |  | *EventA6* IE in 8.1.1.10 |
| 152 | >RSRP Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 153 | >RSRQ Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 154 | >SINR Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 155 | >Hysteresis Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 161 | B1 Event Threshold Offset | STRUCTURE |  |  | *EventB1* IE in 8.1.1.10 |
| 162 | >RSRP Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 163 | >RSRQ Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 164 | >SINR Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 165 | >Hysteresis Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 170 | B2 Event Threshold offset | STRUCTURE |  |  | *EventB2* IE in 8.1.1.10 |
| 171 | >B2-Threshold-NR offset | STRUCTURE |  |  | *EventB2* IE in 8.1.1.10 |
| 172 | >>RSRP Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 173 | >>RSRQ Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 174 | >>SINR Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 175 | >>Hystersis Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 176 | >B2-Threshold-EUTRA offset | STRUCTURE |  |  | *EventB2* IE in 8.1.1.10 |
| 177 | >>RSRP Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 178 | >>RSRQ Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 179 | >>SINR Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |
| 180 | >>Hysteresis Offset | ELEMENT | FALSE | INTEGER | Offsets to be applied to default values, |

#### 8.5.4.2 Conditional Handover Control

##### 8.5.4.2.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.4.2 Table 1.

##### 8.5.4.2.2 Offset

The RAN parameters associated with this policy type are listed in Section 8.5.4.1.2.

#### 8.5.4.3 DAPS Handover Control

##### 8.5.4.3.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.4.3 Table 1.

##### 8.5.4.3.2 Offset

The RAN parameters associated with this policy type are listed in Section 8.5.4.1.2.

### 8.5.5 Radio Access Control

#### 8.5.5.0 Common RAN Parameters for Radio Access Control

The RAN Parameters pertaining to POLICY Conditions for the “Radio Access Control” policy service style used across all POLICY actions of the policy service style are listed in the below table.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter Name** | **RAN Parameter Value Type** | **Key flag** | **Parameter description** |
| 501 | E2 Node | STRUCTURE |  | Refer to *E2 Node* structure in 8.1.1.11 |
| 502 | >CHOICE E2 Node Component Type | STRUCTURE |  | Refer to *E2 Node* structure in 8.1.1.11 where this parameter is defined |
| 503 | >>NG-RAN gNB DU | STRUCTURE |  | Refer to *E2 Node* structure in 8.1.1.11 where this parameter is defined |
| 504 | >>>gNB DU Measurements | STRUCTURE |  | Refer to *E2 Node* structure in 8.1.1.11 where this parameter is defined |
| 505 | >>>List of NR cells | LIST |  | Refer to *gNB DU Measurements* structure in 8.1.1.14 where this parameter is defined |
| 506 | >>>>NR Cell Item | STRUCTURE |  | Refer to *gNB DU Measurements* structure in 8.1.1.14 where this parameter is defined |
| 507 | >>>>>Radio Resource Utilization | STRUCTURE |  | Refer to *Radio Resource Utilization* structure in 8.1.1.14 where this parameter is defined. This has load measurements in terms of PRB usage. |
| 508 | >>>>>Number of active UE measurements | STRUCTURE |  | Refer to *Number of active UE measurements* structure in 8.1.1.14 where this parameter is defined. This has load measurements in terms of number of active UEs. |
| 509 | >>>>>Slice Available Capacity List | STRUCTURE |  | Refer to *Slice Available Capacity List* in 8.1.1.1 |
| 511 | >>NG-RAN gNB CU-CP | STRUCTURE |  | Refer to *E2 Node* structure in 8.1.1.11 where this parameter is defined |
| 512 | >>>RRC connection related measurements | STRUCTURE |  | Refer to *gNB CU-CP Measurements* structure in 8.1.1.12 where this parameter is defined |
| 521 | >>NG-RAN gNB | STRUCTURE |  | Refer to E2 Node structure in 8.1.1.11 where this parameter is defined |
| 522 | >>>gNB DU Measurements | STRUCTURE |  | Refer to E2 Node structure in 8.1.1.11 where this parameter is defined |
| 523 | >>>List of NR cells | LIST |  | Refer to gNB DU Measurements structure in 8.1.1.14 where this parameter is defined |
| 524 | >>>>NR Cell Item | STRUCTURE |  | Refer to gNB DU Measurements structure in 8.1.1.14 where this parameter is defined |
| 525 | >>>>>Radio Resource Utilization | STRUCTURE |  | Refer to Radio Resource Utilization structure in 8.1.1.14 where this parameter is defined. This has load measurements in terms of PRB usage. |
| 526 | >>>>>Number of active UE measurements | STRUCTURE |  | Refer to Number of active UE measurements structure in 8.1.1.14 where this parameter is defined. This has load measurements in terms of number of active UEs. |
| 527 | >>>>>Slice Available Capacity List | STRUCTURE |  | Refer to *Slice Available Capacity List* in 8.1.1.1 |
| 531 | >>>gNB CU-CP Measurements | STRUCTURE |  | Refer to *E2 Node* structure in 8.1.1.11 where this parameter is defined |
| 532 | >>>>RRC connection related measurements | STRUCTURE |  | Refer to *gNB CU-CP Measurements* structure in 8.1.1.12 where this parameter is defined |

In addition to using the above RAN Parameters for POLICY conditions, this service style also uses RAN parameters defined in Section 8.1. Accordingly, this service style supports Policy Conditions using the RAN parameters defined in Sections 8.1, 8.5.1 and those covered in the above table.

#### 8.5.5.1 UE admission control request

##### 8.5.5.1.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.5.1 Table 1.

##### 8.5.5.1.2 Offset

Editor’s Note: FFS

#### 8.5.5.2 RACH backoff control request

##### 8.5.5.2.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.5.2 Table 1.

##### 8.5.5.2.2 Offset

Editor’s Note: FFS

#### 8.5.5.3 Access barring control request

##### 8.5.5.3.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.5.3 Table 1.

##### 8.5.5.3.2 Offset

Editor’s Note: FFS

#### 8.5.5.4 RRC Connection Release request

##### 8.5.5.4.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.5.3 Table 1.

##### 8.5.5.4.2 Offset

Editor’s Note: FFS

#### 8.5.5.5 RRC Connection Reject request

##### 8.5.5.5.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.5.3 Table 1.

##### 8.5.5.5.2 Offset

Editor’s Note: FFS

### 8.5.6 Dual Connectivity Control

#### 8.5.6.0 Common RAN Parameters for Dual Connectivity Control

The RAN Parameters pertaining to POLICY Conditions for the “Dual Connectivity Control” policy service style used across all POLICY actions of the policy service style are listed in the below table.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter Name | RAN Parameter Value Type | Key flag | Parameter description |
| 501 | Target Secondary Node | STRUCTURE |  | Refer to *E2 Node* structure in 8.1.1.11 |
| 502 | >CHOICE E2 Node Component Type | STRUCTURE |  | Refer to *E2 Node* structure in 8.1.1.11 where this parameter is defined |
| 503 | >>NG-RAN gNB DU | STRUCTURE |  | Refer to *E2 Node* structure in 8.1.1.11 where this parameter is defined |
| 504 | >>>gNB DU Measurements | STRUCTURE |  | Refer to *E2 Node* structure in 8.1.1.11 where this parameter is defined |
| 505 | >>>List of NR cells | LIST |  | Refer to *gNB DU Measurements* structure in 8.1.1.14 where this parameter is defined |
| 506 | >>>>NR Cell Item | STRUCTURE |  | Refer to *gNB DU Measurements* structure in 8.1.1.14 where this parameter is defined |
| 507 | >>>>>Radio Resource Utilization | STRUCTURE |  | Refer to *Radio Resource Utilization* structure in 8.1.1.14 where this parameter is defined. This has load measurements in terms of PRB usage. |
| 508 | >>>>>Number of active UE measurements | STRUCTURE |  | Refer to *Number of active UE measurements* structure in 8.1.1.14 where this parameter is defined. This has load measurements in terms of number of active UEs. |
| 509 | >>>>>Slice Available Capacity List | STRUCTURE |  | Refer to *Slice Available Capacity List* in 8.1.1.1 |
| 510 | >>>List of logical channels | LIST |  |  |
| 511 | >>>>Logical Channel Item | STRUCTURE |  |  |
| 512 | >>>>>Buffer Occupancy | ELEMENT | FALSE | Refer to *L2 MAC State Variables* structure in 8.1.1.4 where this parameter is defined. |
| 511 | >>NG-RAN gNB CU-CP | STRUCTURE |  | Refer to *E2 Node* structure in 8.1.1.11 where this parameter is defined |
| 512 | >>>RRC connection related measurements | STRUCTURE |  | Refer to *gNB CU-CP Measurements* structure in 8.1.1.12 where this parameter is defined |
| 521 | >>NG-RAN gNB | STRUCTURE |  | Refer to E2 Node structure in 8.1.1.11 where this parameter is defined |
| 522 | >>>gNB DU Measurements | STRUCTURE |  | Refer to E2 Node structure in 8.1.1.11 where this parameter is defined |
| 523 | >>>List of NR cells | LIST |  | Refer to gNB DU Measurements structure in 8.1.1.14 where this parameter is defined |
| 524 | >>>>NR Cell Item | STRUCTURE |  | Refer to gNB DU Measurements structure in 8.1.1.14 where this parameter is defined |
| 525 | >>>>>Radio Resource Utilization | STRUCTURE |  | Refer to Radio Resource Utilization structure in 8.1.1.14 where this parameter is defined. This has load measurements in terms of PRB usage. |
| 526 | >>>>>Number of active UE measurements | STRUCTURE |  | Refer to Number of active UE measurements structure in 8.1.1.14 where this parameter is defined. This has load measurements in terms of number of active UEs. |
| 527 | >>>>>Slice Available Capacity List | STRUCTURE |  | Refer to *Slice Available Capacity List* in 8.1.1.1 |
| 528 | >>>List of logical channels | LIST |  | Buffer Occupancy (BO) in number of bytes as defined in TS 25.321 [27] clause 8.2.2(c).LCID indicates logical channel ID. |
| 529 | >>>>Logical Channel Item | STRUCTURE |  | Buffer Ocupancy (BO) in number of bytes as defined in TS 25.321 [27] clause 8.2.2(c).LCID indicates logical channel ID. |
| 530 | >>>>>Buffer Occupancy | ELEMENT | FALSE | Refer to *L2 MAC State Variables* structure in 8.1.1.4 where this parameter is defined. |
| 531 | >>>gNB CU-CP Measurements | STRUCTURE |  | Refer to *E2 Node* structure in 8.1.1.11 where this parameter is defined |
| 532 | >>>>RRC connection related measurements | STRUCTURE |  | Refer to *gNB CU-CP Measurements* structure in 8.1.1.12 where this parameter is defined |

In addition to using the above RAN Parameters for POLICY conditions, this service style also uses RAN parameters defined in Section 8.1. Accordingly, this service style supports Policy Conditions using the RAN parameters defined in Sections 8.1, 8.5.1 and those covered in the above table.

#### 8.5.6.1 DC Secondary Node Addition Control

##### 8.5.6.1.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.6.1 Table 1.

##### 8.5.6.1.2 Offset

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter** | **RAN Parameter Value Type** | | **Key Flag** | **RAN Parameter Definition** | **Semantics Description** | |
| 161 | B1 Event Threshold Offset | STRUCTURE |  | |  | *EventB1* IE in 8.1.1.10 |
| 162 | >RSRP Offset | ELEMENT | FALSE | | INTEGER | Offsets to be applied to default values, |
| 163 | >RSRQ Offset | ELEMENT | FALSE | | INTEGER | Offsets to be applied to default values, |
| 164 | >SINR Offset | ELEMENT | FALSE | | INTEGER | Offsets to be applied to default values, |
| 165 | >Hysteresis Offset | ELEMENT | FALSE | | INTEGER | Offsets to be applied to default values, |
| 170 | B2 Event Threshold offset | STRUCTURE |  | |  | *EventB2* IE in 8.1.1.10 |
| 171 | >B2-Threshold-NR offset | STRUCTURE |  | |  | *EventB2* IE in 8.1.1.10 |
| 172 | >>RSRP Offset | ELEMENT | FALSE | | INTEGER | Offsets to be applied to default values, |
| 173 | >>RSRQ Offset | ELEMENT | FALSE | | INTEGER | Offsets to be applied to default values, |
| 174 | >>SINR Offset | ELEMENT | FALSE | | INTEGER | Offsets to be applied to default values, |
| 175 | >>Hystersis Offset | ELEMENT | FALSE | | INTEGER | Offsets to be applied to default values, |
| 176 | >B2-Threshold-EUTRA offset | STRUCTURE |  | |  | *EventB2* IE in 8.1.1.10 |
| 177 | >>RSRP Offset | ELEMENT | FALSE | | INTEGER | Offsets to be applied to default values, |
| 178 | >>RSRQ Offset | ELEMENT | FALSE | | INTEGER | Offsets to be applied to default values, |
| 179 | >>SINR Offset | ELEMENT | FALSE | | INTEGER | Offsets to be applied to default values, |
| 180 | >>Hysteresis Offset | ELEMENT | FALSE | | INTEGER | Offsets to be applied to default values, |

#### 8.5.6.2 DC Secondary Node Modification Control

##### 8.5.6.2.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.6.2 Table 1.

##### 8.5.6.2.2 Offset

The RAN parameters associated with this policy type are listed in Section 8.5.4.1.2 Table 1.

#### 8.5.6.3 PSCell Change cell for Secondary Cell Group

##### 8.5.6.3.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.6.3 Table 1.

##### 8.5.6.3.2 Offset

The RAN parameters associated with this policy type are listed in Section 8.5.4.1.2 Table 1.

#### 8.5.6.4 DC Secondary Node Change Control

##### 8.5.6.4.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.6.4 Table 1.

##### 8.5.6.4.2 Offset

The RAN parameters associated with this policy type are listed in Section 8.5.4.1.2 Table 1.

### 8.5.7 Carrier Aggregation Control

#### 8.5.7.0 Common RAN Parameters for Carrier Aggregation Control

The RAN Parameters pertaining to POLICY Conditions for the “Carrier Aggregation Control” policy service style used across all POLICY actions of the policy service style are listed in the below table.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter Name** | | **RAN Parameter Value Type** | **Key flag** | **Parameter description** | |
| 501 | | List of secondary cells setup | LIST |  | *Scell To Be Setup List* IE in TS 38.473 [19] clause 9.2.2.1 |
| 502 | | >Secondary cell setup Item | STRUCTURE |  | *Scell To Be Setup Item* IEs IE in TS 38.473 [19] clause 9.2.2.1 |
| 503 | | >>CHOICE Secondary cell | STRUCTURE |  |  |
| 504 | | >>>NR SCell | STRUCTURE |  | 8.1.1.1 |
| 505 | | >>>>PM Measurements | STRUCTURE |  | Refer to *PM Measurements* structure in 8.1.1.1 |
| 506 | | >>>>>Radio Resource Status | STRUCTURE |  | Refer to *Radio Resource Utilization* structure in 8.1.1.1 where this parameter is defined. This has load measurements in terms of PRB usage. |
| 507 | | >>>>>Number of active UEs in the cell | ELEMENT | FALSE | Refer to *Number of active UE measurements* structure in 8.1.1.1 where this parameter is defined. This has load measurements in terms of number of active UEs. |
| 508 | | >>>>>Composite available capacity group | STRUCTURE |  | Refer to *Composite Available Capacity Group* structure in 8.1.1.1 |
| 509 | | >>>>>Slice available capacity list | STRUCTURE |  | Refer to *Slice Available Capacity List* in 8.1.1.1 |
| 511 | | >>>E-UTRA SCell | STRUCTURE |  | 8.1.1.2 |
| 512 | | >>>>PM Measurements | STRUCTURE |  | Refer to *PM Measurements* structure in 8.1.1.2 |
| 513 | | >>>>>Radio Resource Status | STRUCTURE |  | Refer to *Radio Resource Utilization* structure in 8.1.1.2 where this parameter is defined. This has load measurements in terms of PRB usage. |
| 514 | | >>>>>Composite Available capacity group | STRUCTURE |  | Refer to *Composite Available Capacity Group* structure in 8.1.1.2 |
| 515 | | >>>>>Number of active UEs in the cell | ELEMENT | FALSE | Refer to *Number of active UE measurements* structure in 8.1.1.12 where this parameter is defined. This has load measurements in terms of number of active UEs. |
| 516 | | List of logical channels | LIST |  | Buffer Occupancy (BO) in number of bytes as defined in TS 25.321 [27] clause 8.2.2(c).LCID indicates logical channel ID. |
| 517 | | >Logical Channel Item | STRUCTURE |  | Buffer Occupancy (BO) in number of bytes as defined in TS 25.321 [27] clause 8.2.2(c).LCID indicates logical channel ID. |
| 518 | | >>LCID | ELEMENT | TRUE | *logicalChannelIdentity* IEin TS 38.331 [22] Sec 6 |
| 519 | | >>Buffer Occupancy | ELEMENT | FALSE | Refer to *L2 MAC State Variables* structure where this parameter is defined |

In addition to using the above RAN Parameters for POLICY conditions, this service style also uses RAN parameters defined in Section 8.1. Accordingly, this service style supports Policy Conditions using the RAN parameters defined in Sections 8.1, 8.5.1 and those covered in the above table.

#### 8.5.7.1 Secondary cell Addition control

##### 8.5.7.1.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.7.1 Table 1.

##### 8.5.7.1.2 Offset

The RAN parameters associated with this policy type are listed in Section 8.5.4.1.2 Table 1.

#### 8.5.7.2 Secondary cell Modification control

##### 8.5.7.2.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.7.2 Table 1.

##### 8.5.7.2.2 Offset

The RAN parameters associated with this policy type are listed in Section 8.5.4.1.2 Table 1.

### 8.5.8 Idle Mode Mobility Control

#### 8.5.8.0 Common RAN Parameters for Idle Mode Mobility Control

The RAN Parameters pertaining to POLICY Conditions for the “Idle Mode Mobility Control” policy service style used across all POLICY actions of the policy service style are listed in the below table.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **RAN Parameter Name** | **RAN Parameter Value Type** | **Key flag** | **Parameter description** |
| 501 |  |  |  |  |

In addition to using the above RAN Parameters for POLICY conditions, this service style also uses RAN parameters defined in Section 8.1. Accordingly, this service style supports Policy Conditions using the RAN parameters defined in Sections 8.1, 8.5.1 and those covered in the above table.

#### 8.5.8.1 Cell reselection priority control

##### 8.5.8.1.1 Control action

The RAN parameters associated with this policy type are listed in Section 8.4.8.1 Table 1.

##### 8.5.8.1.2 Offset

The RAN parameters associated with this policy type are listed in Section 8.4.5.4 Table 1. For the priority and sub priority parameters, values are used to set offsets with respect to the default behaviour, i.e. carrier frequency with fourth priority and an offset of +1 shall be considered as third priority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RAN Parameter ID | RAN Parameter | RAN Parameter Value Type | Key Flag | RAN Parameter Definition | *Semantics Description* |
| 1 | Cell Reselection Priorities | STRUCTURE |  |  | *IdleModeMobilityControlInfo* IE in TS 36.331 [23] |
| 2 | >Frequency Priority List E-UTRA | LIST |  |  | *FreqPriorityListEUTRA* IE in TS 38.331 [22] |
| 3 | >>Frequency Priority Item E-UTRA | STRUCTURE |  |  | *FreqPriorityEUTRA* IE in TS 38.331 [22] |
| 4 | >>>Carrier Frequency | ELEMENT | FALSE | *carrierFreq* IE in TS 38.331 [22] |  |
| 5 | >>>Cell Reselection Priority offset | ELEMENT | FALSE | INTEGER | *cellReselectionPriority* IE in TS 38.331 [22] |
| 6 | >>>Cell Reselection Sub Priority offset | ELEMENT | FALSE | INTEGER | *cellReselectionSubPriority* IE in TS 38.331 [22] |
| 7 | >Frequency Priority List NR | LIST |  |  | *FreqPriorityListNR* IE in TS 38.331 [22] |
| 8 | >>Frequency Priority Item NR | STRUCTURE |  |  | *FreqPriorityNR* IE in TS 38.331 [22] |
| 9 | >>>Carrier Frequency | ELEMENT | FALSE | carrierFreq IE in TS 38.331 [22] |  |
| 10 | >>>Cell Reselection Priority offset | ELEMENT | FALSE | INTEGER | *cellReselectionPriority* IE in TS 38.331 [22] |
| 11 | >>>Cell Reselection Sub Priority ofset | ELEMENT | FALSE | INTEGER | *cellReselectionSubPriority* IE in TS 38.331 [22] |
| 12 | >T-320 timer expiry offset | ELEMENT | FALSE | INTEGER | *t320* IE in TS 38.331 [22] |

### 8.5.9 Measurement Reporting Configuration Control

The RAN Parameters pertaining to POLICY Conditions for the “Measurement Report Configuration Control” policy service style are FFS.

In addition, this service style also uses RAN parameters defined in Section 8.1. Thus, this service style currently supports Policy Conditions using the RAN parameters defined in Sections 8.1 and 8.5.1.

#### 8.5.9.1 Add MR Configuration

##### 8.5.9.1.1 Control Action

The RAN parameters associated with this policy type are listed in Section 8.4.10.1 Table 1

##### 8.5.9.1.2 Offset

Editor’s Note: FFS

#### 8.5.9.2 Modify MR Configuration

##### 8.5.9.2.1 Control Action

The RAN parameters associated with this policy type are listed in Section 8.4.10.2 Table 1

##### 8.5.9.2.2 Offset

Editor’s Note: FFS

#### 8.5.9.3 Delete MR Configuration

##### 8.5.9.3.1 Control Action

The RAN parameters associated with this policy type are listed in Section 8.4.10.3 Table 1

##### 8.5.9.3.2 Offset

Editor’s Note: FFS

# 9 Elements for E2SM Service Model

## 9.1 General

## 9.2 Message Functional Definition and Content

### 9.2.1 Messages for RIC Functional procedures

#### 9.2.1.1 RIC Event Trigger Definition IE

This information element is part of the RIC SUBSCRIPTION REQUEST message sent by the Near-RT RIC to an E2 Node and is required for event triggers used to initiate REPORT, INSERT and POLICY actions.

Direction: NEAR-RT RIC → E2 Node.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| **CHOICE** *Event Trigger Format* |  |  |  |  |
| >E2SM-RC Event Trigger Definition Format 1 | M |  | 9.2.1.1.1 | Used for Event Trigger Style 1 |
| >E2SM-RC Event Trigger Definition Format 2 | M |  | 9.2.1.1.2 | Used for Event Trigger Style 2 |
| >E2SM-RC Event Trigger Definition Format 3 | M |  | 9.2.1.1.3 | Used for Event Trigger Style 3 |
| >E2SM-RC Event Trigger Definition Format 4 | M |  | 9.2.1.1.4 | Used for Event Trigger Style 4 |
| >E2SM-RC Event Trigger Definition Format 5 | M |  | 9.2.1.1.5 | Used for Event Trigger Style 5 |

##### 9.2.1.1.1 E2SM-RC Event Trigger Definition Format 1: Message Event

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Sequence of Messages for Event Trigger |  | *1..<maxnoofMessages>* |  |  |
| >Event Trigger Condition ID | M |  | 9.3.21 |  |
| *>***CHOICE** *Message Type* | M |  |  |  |
| **>>*Network Interface*** |  |  |  |  |
| >>>NI Type | M |  | 9.3.32 | 3GPP Network Interface Type |
| >>>NI Identifier | O |  | 9.3.33 | “Any” Network Interface instance to be used if absent. |
| >>>NI Message | O |  | 9.3.34 | Network Interface Message ID. This can indicate whether NUA (Non-UE Associated) or UA (UE-Associated). |
| ***>>RRC*** |  |  |  |  |
| >>>RRC Message ID | M |  | 9.3.35 | RRC Message ID |
| >Message Direction | O |  | ENUMERATED (incoming, outgoing, …) | Indicates message arrival or departure for event triggering ("Any” direction if not included). |
| >Associated UE Info | O |  | 9.3.26 | Indicates applicable UE(s) for event triggering associated to each message event ("Any" UE if not included).  Shall not be included in case of NUA type NI message. |
| >Associated UE Event | O |  | 9.3.28 | Indicates specific UE event(s) defined in Section 8.1.5 for event triggering associated to each message event. |
| >Logical OR | O |  | 9.3.25 |  |
| Global Associated UE Info | O |  | 9.3.26 | Indicates applicable UE(s) for event triggering, applied to all the message events uniformly.  This IE shall override any *Associated UE Info* IE included for some message events.  Shall not be included in case a NUA type NI message event is configured. |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofMessages | Maximum number of Messages in a given E2 node for which event trigger can be defined. The value is *<65535>.* |

##### 9.2.1.1.2 E2SM-RC Event Trigger Definition Format 2: Call Process Breakpoint

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Call Process Type ID | M |  | 9.3.15 |  |
| Call Breakpoint ID | M |  | 9.3.49 |  |
| Associated E2 Node Info | O |  | 9.3.29 | Used to set optional E2 Node related information for event triggering. RAN Parameters in Section 8.1.2 shall only be used. |
| Associated UE Info | O |  | 9.3.26 | Indicates applicable UE(s) for event triggering ("Any" UE if not included). |

9.2.1.1.3 E2SM-RC Event Trigger Definition Format 3: E2 Node Information Change

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Sequence of E2 Node Information Change |  | *1..<maxnoofE2InfoChanges>* |  |  |
| >Event Trigger Condition ID | M |  | 9.3.21 |  |
| >E2 Node Information Change ID | M |  | INTEGER (1..512, ...) | Defined in 7.3.4. |
| >Associated Cell Info | O |  | 9.3.27 | "Any” cell if not included. |
| >Logical OR | O |  | 9.3.25 |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofE2InfoChanges | Maximum number of E2 Node information changes for which event trigger can be defined. The value is *<65535>.* |

9.2.1.1.4 E2SM-RC Event Trigger Definition Format 4: UE Information Change

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Sequence of UE Information Change |  | *1..<maxnoofUEInfoChanges>* |  |  |
| >Event Trigger Condition ID | M |  | 9.3.21 |  |
| **>CHOICE** *Trigger Type* | M |  |  |  |
| **>>*RRC State*** |  |  |  |  |
| >>>RRC State List |  | *1..<maxnoofRRCstate>* |  |  |
| >>>>State Changed To | M |  | 9.3.37 |  |
| >>>>Logical OR | O |  | 9.3.25 |  |
| **>>*UE Identifier*** |  |  |  |  |
| >>>UE Identifier Change ID | M |  | INTEGER (1..512, ...) | Defined in 7.3.5. |
| **>>*L2 State*** |  |  |  | Used to set conditions for PDCP, RLC and MAC state variable reporting |
| >>>Associated L2 Variables | M |  | 9.3.29 | RAN Parameters in Sections 8.1.1.4 and 8.1.1.8 shall only be used. |
| >Associated UE Info | O |  | 9.3.26 | Indicates applicable UE(s) for event triggering ("Any" UE if not included). |
| >Logical OR | O |  | 9.3.25 |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofUEInfoChanges | Maximum number of UE information changes for which event trigger can be defined. The value is *<65535>.* |
| maxnoofRRCstate | Maximum number of RRC states for which event trigger can be defined. The value is *<*8*>.* |

##### 9.2.1.1.5 E2SM-RC Event Trigger Definition Format 5: On Demand

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| On Demand | M |  | ENUMERATED (true, …) |  |
| Associated UE Info | O |  | 9.3.26 | Indicates applicable UE(s) for event triggering ("Any" UE if not included). |
| Associated Cell Info | O |  | 9.3.27 | "Any” cell if not included. |

#### 9.2.1.2 RIC ACTION DEFINITION IE

This information element is part of the RIC SUBSCRIPTION REQUEST message sent by the Near-RT RIC to an E2 Node. In this service model, this information element provides additional information for the nominated RIC Action.

Direction: NEAR-RT RIC → E2 Node.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | |
| RIC Style Type | M |  | 9.3.3 |  | |
| **CHOICE** *Action Definition Format* |  |  |  |  | |
| >E2SM-RC Action Definition Format 1 | M |  | 9.2.1.2.1 | Used by REPORT service | |
| >E2SM-RC Action Definition Format 2 | M |  | 9.2.1.2.2 | Used by POLICY service when encoding a list of Policy Conditions | |
| >E2SM-RC Action Definition Format 3 | M |  | 9.2.1.2.3 | Used by INSERT service except style 255 |
| >E2SM-RC Action Definition Format 4 | M |  | 9.2.1.2.4 | Used only by INSERT service style 255 |

##### 9.2.1.2.1 E2SM-RC Action Definition Format 1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Parameters to be Reported List |  | *1..<maxnoofParametersToReport>* |  |  |
| >RAN Parameter ID | M |  | 9.3.8 | Only the RAN Parameter ID values declared in RAN Function Definition may be included. |
| >RAN Parameter Definition | O |  | 9.3.51 | To define the parameter along with its constituent parameters, if any (for a structure), and itemized members, if any (for a list).  If not included for the RAN Parameter ID of a STRUCTURE type or a LIST type, then all the constituent RAN parameters under this RAN Parameter ID are assumed to be supported.  Only the RAN Parameter ID values declared in RAN Function Definition may be included. |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofParametersToReport | Maximum no. of RAN parameters supported by Action Definition Format 1. The value is <*65535*>. |

##### 9.2.1.2.2 E2SM-RC Action Definition Format 2: Policy with Conditions

The *E2SM-RC Action Definition* IE Format 2 supports a POLICY services encoded as a list of Policy Conditions, each with a Policy Condition definition described using *Conditional Criteria Definition* IE in terms of a list of RAN parameters with test conditions and a *Policy Action* IE command described in terms of a list of RAN parameters. The meaning of the RAN Parameter ID/Value pairs for each list is defined in Section 8.5.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Sequence of Policy Conditions |  | *1..<maxnoofPolicyConditions>* |  |  |
| >Policy Action Definition | M |  | 9.3.20 | Defines policy to be applied for specific Policy Condition |
| >Policy Condition Definition | O |  | 9.3.29 | Defines conditional test. |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofPolicyConditions | Maximum no. of Policy Condition in action definition supported by RAN Function. Value is <*65535*>. |

##### 9.2.1.2.3 E2SM-RC Action Definition Format 3

The E2SM-RC Action Definition Format 3 supports an INSERT service of the indicated *RIC Style Type* IE and is encoded by the Insert Indication ID and a list of RAN parameters. The meaning of the RAN Parameter ID(s) in the list is defined in Section 8.3.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Insert Indication ID | M |  | 9.3.16 | Refer to Section 7.5 |
| List of RAN parameters for Insert Indication | M | *1..<maxnoofAssociatedRANParameters*> |  | Refer to Section 8.3 |
| >RAN Parameter ID | M |  | 9.3.8 | Refer to Section 8.3  Only the RAN Parameter ID values declared in RAN Function Definition may be included. |
| >RAN Parameter Definition | O |  | 9.3.51 | To define the parameter along with its constituent parameters, if any (for a structure), and itemized members, if any (for a list).  If not included for the RAN Parameter ID of a STRUCTURE type or a LIST type, then all the constituent RAN parameters under this RAN Parameter ID are assumed to be supported.  Only the RAN Parameter ID values declared in RAN Function Definition may be included. |
| UE ID | O |  | 9.3.10 | If included, indicates that the subscribed INSERT service, upon the associated event trigger occurs, shall be executed for this UE only.  In case of UE-related event triggers, the subscribed INSERT service shall not be executed unless the triggered event is related to this UE. |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofAssociatedRANParameters | Maximum no. of RAN parameters supported by Action Definition Format 3 for INSERT Indication. The value is <*65535*>. |

##### 9.2.1.2.4 E2SM-RC Action Definition Format 4

The E2SM-RC Action Definition Format 4 supports multiple Insert Indication actions of one or more requested INSERT services, where each Insert Indication action is encoded by Insert Indication ID and a list of RAN parameters. The meaning of the RAN Parameter ID/Value pairs for each list is defined in Section 8.3.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Sequence of Insert Styles for Multiple Actions |  | *1..<maxnoofRICStyles*> |  |  |
| >Requested Insert Style | M |  | 9.3.3 |  |
| >Sequence of Insert Indication Action Definition |  | *1..<maxnoofInsertIndicationActions*> |  |  |
| >>Insert Indication ID | M |  | 9.3.16 | Refer to Section 7.5 |
| >>List of RAN parameters for Insert Indication |  | *1..<maxnoofAssociatedRANParameters*> |  | Refer to Section 8.3 |
| >>>RAN Parameter ID | M |  | 9.3.8 | Refer to Section 8.3  Only the RAN Parameter ID values declared in RAN Function Definition may be included. |
| >>>RAN Parameter Definition | O |  | 9.3.51 | To define the parameter along with its constituent parameters, if any (for a structure), and itemized members, if any (for a list).  If not included for the RAN Parameter ID of a STRUCTURE type or a LIST type, then all the constituent RAN parameters under this RAN Parameter ID are assumed to be supported.  Only the RAN Parameter ID values declared in RAN Function Definition may be included. |
| UE ID | O |  | 9.3.10 | If included, indicates that the subscribed INSERT service, upon the associated event trigger occurs, shall be executed for this UE only.  In case of UE-related event triggers, the subscribed INSERT service shall not be executed unless the triggered event is related to this UE. |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofRICStyles | Maximum no. of Insert Styles supported by Action Definition Format 4 for INSERT Indication. The value is <63>. |
| maxnoofInsertIndicationActions | Maximum no. of Insert indication actions supported by RAN Function. The value is <63>. |
| maxnoofAssociatedRANParameters | Maximum no. of RAN parameters supported by Action Definition Format 4 for INSERT Indication. The value is <*65535*>. |

#### 9.2.1.3 RIC INDICATION HEADER IE

This information element is part of the RIC INDICATION message sent by the E2 Node to the Near-RT RIC and is required for REPORT action.

Direction: E2 Node → NEAR-RT RIC.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CHOICE *Indication Header Format* |  |  |  |  |
| >E2SM-RC Indication Header Format 1 | M |  | 9.2.1.3.1 |  |
| >E2SM-RC Indication Header Format 2 | M |  | 9.2.1.3.2 |  |
| >E2SM-RC Indication Header Format 3 | M |  | 9.2.1.3.3 |  |

##### 9.2.1.3.1 E2SM-RC Indication Header Format 1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Event Trigger Condition ID | O |  | 9.3.21 | Event Trigger Condition ID |

##### 9.2.1.3.2 E2SM-RC Indication Header Format 2

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| UE ID | M |  | 9.3.10 |  |
| RIC Insert Style Type | M |  | 9.3.3 |  |
| Insert Indication ID | M |  | 9.3.16 | Refer to Section 7.5 |

9.2.1.3.3 E2SM-RC Indication Header Format 3

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Event Trigger Condition ID | O |  | 9.3.21 |  |
| UE ID | O |  | 9.3.10 |  |

#### 9.2.1.4 RIC INDICATION MESSAGE IE

This information element is part of the RIC INDICATION message sent by the E2 Node to the Near-RT RIC and is required for REPORT action.

Direction: E2 Node → NEAR-RT RIC.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **CHOICE** *Indication Message* *Format* | M |  |  |  |
| >E2SM-RC Indication Message Format 1 |  |  | 9.2.1.4.1 |  |
| >E2SM-RC Indication Message Format 2 |  |  | 9.2.1.4.2 |  |
| >E2SM-RC Indication Message Format 3 |  |  | 9.2.1.4.3 |  |
| >E2SM-RC Indication Message Format 4 |  |  | 9.2.1.4.4 |  |
| >E2SM-RC Indication Message Format 5 |  |  | 9.2.1.4.5 |  |
| >E2SM-RC Indication Message Format 6 |  |  | 9.2.1.4.6 |  |

##### 9.2.1.4.1 E2SM-RC Indication Message Format 1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of RAN Parameters |  | *1..<maxnoofAssociatedRANParameters>* |  |  |
| >RAN Parameter ID | M |  | 9.3.8 |  |
| >RAN Parameter Value | M |  | 9.3.11 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofAssociatedRANParameters | Maximum number of RAN Parameters supported by Indication Message Format 1. The value is <*65535*>. |

##### 9.2.1.4.2 E2SM-RC Indication Message Format 2

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of UE Identifiers |  | *1..<maxnoofUEID>* |  |  |
| >UE ID | M |  | 9.3.10 |  |
| >Sequence of RAN Parameters |  | *1..<maxnoofAssociatedRANParameters>* |  |  |
| >>RAN Parameter ID | M |  | 9.3.8 |  |
| >>RAN Parameter Value | M |  | 9.3.11 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofUEID | Maximum number of UE Identifiers supported by Indication Message Format 2 to be reported. The value is <*65535*>. |
| maxnoofAssociatedRANParameters | Maximum number of RAN Parameters supported by Indication Message Format 2 to be reported. The value is <*65535*>. |

##### 9.2.1.4.3 E2SM-RC Indication Message Format 3

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of Cell Information |  | *1..<maxnoofCellID>* |  |  |
| >Cell Global ID | M |  | 9.3.36 |  |
| >Cell Context Information | O |  | OCTET STRING | *Served Cell Information* IE in TS 38.473 [19] clause 9.3.1.10. This IE shall be reported if RAN Parameter ID is set to “1” as described in Section 7.4.4. |
| >Cell Deleted | O |  | BOOLEAN | This IE shall be used to report deleted cells. The value shall be set to “True” for the deleted Cell Global ID. This IE shall be reported if RAN Parameter ID is set to “2” as described in Section 7.4.4. |
| >Neighbour Relation Table | O |  | 9.3.38 | Provides information on neighbours of serving cell. This IE shall be reported if RAN Parameter ID is set to “3” as described in Section 7.4.4. |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofCellID | Maximum number of Cell Identifiers supported by Indication Message Format 3 to be reported. The value is <*65535*>. |

##### 9.2.1.4.4 E2SM-RC Indication Message Format 4

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of UE Information |  | *0..<maxnoofUEID>* |  |  |
| >UE ID | M |  | 9.3.10 |  |
| >UE Context Information | O |  | OCTET STRING | The RETRIEVE UE CONTEXT RESPONSE message content in TS 38.423 [15] clause 9.1.1.9. This IE shall be reported if RAN Parameter ID is set to “1” as described in Section 7.4.6. |
| >Cell Global ID | M |  | 9.3.36 | This IE indicates the SpCell ID where the UE belongs to. |
| Sequence of Cell Information |  | *0..<maxnoofCellID>* |  |  |
| >Cell Global ID | M |  | 9.3.36 |  |
| >Cell Context Information | O |  | OCTET STRING | *Served Cell Information* IE in TS 38.473 [19] clause 9.3.1.10. This IE shall be reported if RAN Parameter ID is set to “2” as described in Section 7.4.6. |
| >Neighbour Relation Table | O |  | 9.3.38 | Provides information on neighbours of serving cell. This IE shall be reported if RAN Parameter ID is set to “3” as described in Section 7.4.6. |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofUEID | Maximum number of UE Identifiers supported by Indication Message Format 4 to be reported. The value is <*65535*>. |
| maxnoofCellID | Maximum number of Cell Identifiers supported by Indication Message Format 4 to be reported. The value is <*65535*>. |

##### 9.2.1.4.5 E2SM-RC Indication Message Format 5

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| List of RAN parameters requested |  | *0..<maxnoofAssociatedRANParameters>* |  |  |
| >RAN Parameter ID | M |  | 9.3.8 | Refer to table in Section 8.3 |
| >RAN Parameter Value Type | M |  | 9.3.11 | Refer to table in Section 8.3 |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofAssociatedRANParameters | Maximum no. of RAN parameters supported by RAN Function for a specific Control action. The value is <*65535*>. |

9.2.1.4.6 E2SM-RC Indication Message Format 6

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of Insert Styles for Multiple Actions |  | *1..<maxnoofRICStyles*> |  |  |
| >Indicated Insert Style | M |  | 9.3.3 |  |
| >Sequence of Insert Indication Actions |  | *1..<maxnoofInsertIndicationActions>* |  |  |
| >>Insert Indication ID | M |  | 9.3.16 | Refer to Section 7.5 |
| >>List of RAN parameters requested |  | *0..<maxnoofAssociatedRANParameters>* |  |  |
| >>>RAN Parameter ID | M |  | 9.3.8 | Refer to table in Section 8.3 |
| >>>RAN Parameter Value Type | M |  | 9.3.11 | Refer to table in Section 8.3 |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofRICStyles | Maximum no. of Insert Styles supported for multiple actions. The value is <63>. |
| maxnoofInsertIndicationActions | Maximum no. of Insert indication actions supported by RAN Function. The value is <*63*>. |
| maxnoofAssociatedRANParameters | Maximum no. of RAN parameters supported by RAN Function for a specific Insert indication action. The value is <*65535*>. |

#### 9.2.1.5 RIC CALL PROCESS ID IE

This information element is part of the RIC INDICATION message sent by the E2 Node to a Near-RT RIC node and is required for INSERT action. The same information element is used in RIC Control procedure

Direction: E2 Node → Near-RT RIC (when carried in RIC INDICATION) and Near-RT RIC → E2 Node (when carried in RIC CONTROL REQUEST).

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **CHOICE** *Call Process ID Format* |  |  |  |  |
| >E2SM-RC Call Process ID Format 1 | M |  | 9.2.1.5.1 |  |

##### 9.2.1.5.1 E2SM-RC Call Process ID Format 1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| RIC Call Process ID | M |  | 9.3.18 |  |

#### 9.2.1.6 RIC CONTROL HEADER IE

This information element is part of the RIC CONTROL message sent by the Near-RT RIC to an E2 Node and is required for RIC Control Procedure.

Direction: Near-RT RIC → E2 Node.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **CHOICE** *Control Header Format* | M |  |  |  |
| >E2SM-RC Control Header Format 1 |  |  | 9.2.1.6.1 |  |
| >E2SM-RC Control Header Format 2 |  |  | 9.2.1.6.2 |  |

##### 9.2.1.6.1 E2SM-RC Control Header Format 1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| UE ID | M |  | 9.3.10 |  |
| RIC Style Type | M |  | 9.3.3 |  |
| Control Action ID | M |  | 9.3.6 | Refer to Section 7.6 |
| RIC Control decision | O |  | ENUMERATED (accept, reject, …) | Used only when a CONTROL action is sent as a response to an Insert Indication |

##### 9.2.1.6.2 E2SM-RC Control Header Format 2

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| UE ID | O |  | 9.3.10 |  |
| RIC Control decision | O |  | ENUMERATED (accept, reject, …) | Used only when RIC Control Request message is sent as a response to the INSERT indication message from E2 Node. |

#### 9.2.1.7 RIC CONTROL MESSAGE IE

This information element is part of the RIC CONTROL message sent by the Near-RT RIC to an E2 Node and is required for RIC Control Procedure.

Direction: Near-RT RIC → E2 Node.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **CHOICE** *Control Message Format* | M |  |  |  |
| >E2SM-RC Control Message Format 1 |  |  | 9.2.1.7.1 |  |
| >E2SM-RC Control Message Format 2 |  |  | 9.2.1.7.2 |  |

##### 9.2.1.7.1 E2SM-RC Control Message Format 1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| List of RAN parameters |  | *0..<maxnoofAssociatedRANParameters>* |  |  |
| >RAN Parameter ID | M |  | 9.3.8 | Refer to table in Section 8.4 |
| >RAN Parameter Value Type | M |  | 9.3.11 | Refer to table in Section 8.4 |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofAssociatedRANParameters | Maximum no. of RAN parameters supported by RAN Function for a specific Control action. The value is <*65535*>. |

9.2.1.7.2 E2SM-RC Control Message Format 2

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of Control Styles for Multiple Actions |  | *1..<maxnoofRICStyles>* |  |  |
| >Indicated Control Style | M |  | 9.3.3 |  |
| >Sequence of Control Actions |  | *1..<maxnoofMulCtrlActions>* |  |  |
| >>Control Action ID | M |  | 9.3.6 | Refer to Section 7.6 |
| >>Control Action Parameters | O |  | 9.2.1.7.1  E2SM-RC Control Message Format 1 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofRICStyles | Maximum no. of Control Styles supported by RAN Function. The value is <63>. |
| maxnoofMulCtrlActions | Maximum no. of Control actions supported by RAN Function. The value is <*63*>. |

#### 9.2.1.8 RIC CONTROL OUTCOME IE

This information element is part of the RIC CONTROL ACKOWLEDGEMENT and RIC CONTROL FAILURE messages and is sent by the E2 Node to the Near-RT RIC and is required for RIC Control Procedure.

Direction: E2 Node → Near-RT RIC.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **CHOICE** *Control Outcome Format* | M |  |  |  |
| >E2SM-RC Control Outcome Format 1 |  |  | 9.2.1.8.1 |  |
| >E2SM-RC Control Outcome Format 2 |  |  | 9.2.1.8.2 |  |
| >E2SM-RC Control Outcome Format 3 |  |  | 9.2.1.8.3 |  |

##### 9.2.1.8.1 E2SM-RC Control Outcome Format 1

The *E2SM-RC Control Outcome* IE Format 1 supports a sequence of RAN Parameters sent as ID/Value pairs. The meaning of the ID/Value pairs is defined in Section 7.6.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of RAN Parameters |  | *0..<maxnoofRANOutcomeParameters>* |  |  |
| >RAN Parameter ID | M |  | 9.3.8 |  |
| >RAN Parameter Value | M |  | 9.3.14 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofRANOutcomeParameters | Maximum no. of RAN Parameters. Value is <*255*> |

##### 9.2.1.8.2 E2SM-RC Control Outcome Format 2

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of Control Styles for Multiple Outcomes |  | *1..<maxnoofRICStyles>* |  |  |
| >Indicated Control Style | M |  | 9.3.3 |  |
| >Sequence of Control Actions Outcome |  | *1..<maxnoofMulCtrlActions>* |  |  |
| >>Control Action ID | M |  | 9.3.6 |  |
| >>Sequence of RAN Parameters |  | *1..<maxnoofRANOutcomeParameters>* |  |  |
| >>>RAN Parameter ID | M |  | 9.3.8 |  |
| >>>RAN Parameter Value | M |  | 9.3.14 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofRICStyles | Maximum no. of Control Styles supported by RAN Function. The value is <63>. |
| maxnoofMulCtrlActions | Maximum no. of Control actions supported by RAN Function. The value is <*63*>. |
| maxnoofRANOutcomeParameters | Maximum no. of RAN Parameters. Value is <*255*> |

##### 9.2.1.8.3 E2SM-RC Control Outcome Format 3

The *E2SM-RC Control Outcome* IE Format 3 supports a sequence of RAN Parameters sent as ID and RAN parameter value types, where each RAN parameter value type is based on the categorization of the parameters into *ELEMENT with Key Value TRUE*, *ELEMENT with Key Value FALSE*, *STRUCTURE* and *LIST*.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of RAN Parameters |  | *0..<maxnoofRANOutcomeParameters>* |  |  |
| >RAN Parameter ID | M |  | 9.3.8 |  |
| >RAN Parameter Value Type | M |  | 9.3.11 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofRANOutcomeParameters | Maximum no. of RAN Parameters. Value is <*255*> |

### 9.2.2 Messages for RIC Global Procedures

#### 9.2.2.1 RAN Function Definition IE

This information element is part of the E2 SETUP REQUEST, and RIC SERVICE UPDATE message sent by the E2 Node to the Near-RT RIC and is used to provide all required information for the Near-RT RIC to determine how a given E2 Node has been configured to support a given RAN Function specific E2SM.

Direction: E2 Node → NEAR-RT RIC.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| RAN Function Name | M |  | 9.3.2 |  |
| RAN Function Definition for EVENT TRIGGER | O |  | 9.2.2.2 |  |
| RAN Function Definition for REPORT | O |  | 9.2.2.3 |  |
| RAN Function Definition for INSERT | O |  | 9.2.2.4 |  |
| RAN Function Definition for CONTROL | O |  | 9.2.2.5 |  |
| RAN Function Definition for POLICY | O |  | 9.2.2.6 |  |

#### 9.2.2.2 RAN Function Definition for EVENT TRIGGER

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of EVENT TRIGGER styles |  | *1.. <maxnoofRICStyles>* |  |  |
| >RIC Event Trigger Style Type | M |  | 9.3.3 |  |
| >RIC Event Trigger Style Name | M |  | 9.3.4 |  |
| >RIC Event Trigger Format Type | M |  | 9.3.5 |  |
| Sequence of RAN Parameters for L2 Variables |  | *0.. <maxnoofAssociatedRANParameters>* |  | RAN Parameters defined in Sections 8.1.1.4 and 8.1.1.8. Only included if L2 variables for Event Trigger Style 4 is supported. |
| >RAN Parameter ID | M |  | 9.3.8 |  |
| >RAN Parameter Name | M |  | 9.3.9 |  |
| >RAN Parameter Definition | O |  | 9.3.51 | To define the parameter along with its constituent parameters, if any (for a structure), and itemized members, if any (for a list).  If not included for the RAN Parameter ID of a STRUCTURE type or a LIST type, then all the constituent RAN parameters under this RAN Parameter ID are assumed to be supported. |
| Sequence of Call Process Types |  | *0.. <maxnoofCallProcessTypes>* |  | Only included if Event Trigger Style 2 is supported. |
| >Call Process Type ID | M |  | 9.3.15 |  |
| >Call Process Type Name | M |  | 9.3.19 |  |
| >Sequence of Call Process Breakpoints |  | *1.. <maxnoofCallProcessBreakpoints>* |  |  |
| >>Call Process Breakpoint ID | M |  | 9.3.49 |  |
| >>Call Process Breakpoint Name | M |  | 9.3.50 |  |
| >>Sequence of Associated RAN Parameters |  | *0.. <maxnoofAssociatedRANParameters>* |  | RAN Parameters defined in Section 8.1.2. Only included if Associated E2 Node Info for Event Trigger style 2 is supported |
| >>>RAN Parameter ID | M |  | 9.3.8 |  |
| >>>RAN Parameter Name | M |  | 9.3.9 |  |
| >>>RAN Parameter Definition | O |  | 9.3.51 | To define the parameter along with its constituent parameters, if any (for a structure), and itemized members, if any (for a list).  If not included for the RAN Parameter ID of a STRUCTURE type or a LIST type, then all the constituent RAN parameters under this RAN Parameter ID are assumed to be supported. |
| Sequence of RAN Parameters for Identifying UEs |  | *0.. <maxnoofAssociatedRANParameters>* |  | RAN Parameters defined in Section 8.1.3.  Only included if Associated UE Info for any of Event Trigger Styles 1, 2, 4, 5 is supported. |
| >RAN Parameter ID | M |  | 9.3.8 |  |
| >RAN Parameter Name | M |  | 9.3.9 |  |
| >RAN Parameter Definition | O |  | 9.3.51 | To define the parameter along with its constituent parameters, if any (for a structure), and itemized members, if any (for a list).  If not included for the RAN Parameter ID of a STRUCTURE type or a LIST type, then all the constituent RAN parameters under this RAN Parameter ID are assumed to be supported. |
| Sequence of RAN Parameters for Identifying Cells |  | *0.. <maxnoofAssociatedRANParameters>* |  | RAN Parameters defined in Section 8.1.4.  Only included if Associated Cell Info for any of Event Trigger Styles 3, 5 is supported. |
| >RAN Parameter ID | M |  | 9.3.8 |  |
| >RAN Parameter Name | M |  | 9.3.9 |  |
| >RAN Parameter Definition | O |  | 9.3.51 | To define the parameter along with its constituent parameters, if any (for a structure), and itemized members, if any (for a list).  If not included for the RAN Parameter ID of a STRUCTURE type or a LIST type, then all the constituent RAN parameters under this RAN Parameter ID are assumed to be supported. |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofRICStyles | Maximum no. of styles supported by RAN Function. The value is <*63*>. |
| maxnoofAssociatedRANParameters | Maximum no. of RAN parameters supported by RAN Function. The value is <*65535*>. |
| maxnoofCallProcessTypes | Maximum no. of Call Process types supported by RAN Function. The value is <*65535*>. |
| maxnoofCallProcessBreakpoints | Maximum no. of Call Process breakpoints supported by RAN Function. The value is <*65535*>. |

#### 9.2.2.3 RAN Function Definition for REPORT

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of REPOT styles |  | *1.. <maxnoofRICStyles>* |  |  |
| >RIC Report Style Type | M |  | 9.3.3 |  |
| >RIC Report Style Name | M |  | 9.3.4 |  |
| >Supported RIC Event Trigger Style Type | M |  | 9.3.3 |  |
| >RIC Report Action Format Type | M |  | 9.3.5 | Action Definition type used by Report style |
| >RIC Indication Header Format Type | M |  | 9.3.5 | Indication Header type used by Report style |
| >RIC Indication Message Format Type | M |  | 9.3.5 | Indication Message type used by Report style |
| >Sequence of RAN Parameters Supported |  | *0.. <maxnoofAssociatedRANParameters>* |  | Only included if RAN parameters for corresponding Report style are supported. |
| >>RAN Parameter ID | M |  | 9.3.8 | RAN Parameter IDs for the corresponding Report Style defined in Section 7.4. |
| >>RAN Parameter Name | M |  | 9.3.9 | RAN Parameter Names for the corresponding Report Style defined in Section 7.4. |
| >>RAN Parameter Definition | O |  | 9.3.51 | To define the parameter along with its constituent parameters, if any (for a structure), and itemized members, if any (for a list).  If not included for the RAN Parameter ID of a STRUCTURE type or a LIST type, then all the constituent RAN parameters under this RAN Parameter ID are assumed to be supported. |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofRICstyles | Maximum no. of styles supported by RAN Function. The value is <*63*>. |
| maxnoofAssociatedRANParameters | Maximum no. of RAN parameters supported by RAN Function. The value is <*65535*>. |

#### 9.2.2.4 RAN Function Definition for INSERT

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of INSERT styles |  | *1.. <maxnoofRICStyles>* |  |  |
| >RIC Insert Style Type | M |  | 9.3.3 |  |
| >RIC Insert Style Name | M |  | 9.3.4 |  |
| >Supported RIC Event Trigger Style Type | M |  | 9.3.3 |  |
| >RIC Action Definition Format Type | M |  | 9.3.5 |  |
| >Sequence of Insert Indications |  | *0.. <**maxnoofInsertIndication>* |  |  |
| >>Insert Indication ID | M |  | 9.3.16 | Refer to Section 7.5. |
| >>Insert Indication Name | M |  | 9.3.17 | Refer to Section 7.5. |
| >>Sequence of Associated RAN Parameters |  | *0.. <maxnoofAssociatedRANParameters>* |  | Only included if RAN parameters for corresponding Insert style and Insert indication ID are supported |
| >>>RAN Parameter ID | M |  | 9.3.8 |  |
| >>>RAN Parameter Name | M |  | 9.3.9 |  |
| >>>RAN Parameter Definition | O |  | 9.3.51 | To define the parameter along with its constituent parameters, if any (for a structure), and itemized members, if any (for a list).  If not included for the RAN Parameter ID of a STRUCTURE type or a LIST type, then all the constituent RAN parameters under this RAN Parameter ID are assumed to be supported. |
| >RIC Indication Header Format Type | M |  | 9.3.5 |  |
| >RIC Indication Message Format Type | M |  | 9.3.5 |  |
| >RIC Call Process ID Format Type | M |  | 9.3.5 |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofRICstyles | Maximum no. of styles supported by RAN Function. The value is <*63*>. |
| maxnoofInsertIndication | Maximum no. of Insert indications supported by RAN Function. The value is <*65535*> |
| maxnoofAssociatedRANParameters | Maximum no. of RAN parameters supported by RAN Function. The value is <*65535*>. |

#### 9.2.2.5 RAN Function Definition for CONTROL

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of CONTROL styles |  | *1.. <maxnoofRICStyles>* |  |  |
| >RIC Control Style Type | M |  | 9.3.3 |  |
| >RIC Control Style Name | M |  | 9.3.4 |  |
| >Sequence of Control Actions |  | *0.. <**maxnoofControlAction>* |  |  |
| >>Control Action ID | M |  | 9.3.6 |  |
| >>Control Action Name | M |  | 9.3.7 |  |
| >>Sequence of Associated RAN Parameters |  | *0.. <maxnoofAssociatedRANParameters>* |  | Only included if Control message RAN parameters for corresponding Control style and Control Action ID are supported |
| >>>RAN Parameter ID | M |  | 9.3.8 |  |
| >>>RAN Parameter Name | M |  | 9.3.9 |  |
| >>>RAN Parameter Definition | O |  | 9.3.51 | To define the parameter along with its constituent parameters, if any (for a structure), and itemized members, if any (for a list).  If not included for the RAN Parameter ID of a STRUCTURE type or a LIST type, then all the constituent RAN parameters under this RAN Parameter ID are assumed to be supported. |
| >RIC Control Header Format Type | M |  | 9.3.5 |  |
| >RIC Control Message Format Type | M |  | 9.3.5 |  |
| >RIC Call Process ID Format Type | O |  |  |  |
| >RIC Control Outcome Format Type | M |  | 9.3.5 |  |
| >Sequence of Associated RAN Parameters for Control Outcome |  | *0..<maxnoofRANOutcomeParameters>* |  | Only included if Control Outcome RAN parameters for corresponding Control style are supported |
| >>RAN Parameter ID | M |  | 9.3.8 |  |
| >>RAN Parameter Name | M |  | 9.3.9 |  |
| >>RAN Parameter Definition | O |  | 9.3.51 | To define the parameter along with its constituent parameters, if any (for a structure), and itemized members, if any (for a list).  If not included for the RAN Parameter ID of a STRUCTURE type or a LIST type, then all the constituent RAN parameters under this RAN Parameter ID are assumed to be supported. |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofRICstyles | Maximum no. of styles supported by RAN Function. The value is <*63*>. |
| maxnoofControlAction | Maximum no. of Control actions supported by RAN Function. The value is <*65535*>. |
| maxnoofAssociatedRANParameters | Maximum no. of RAN parameters supported by RAN Function. The value is <*65535*>. |
| maxnoofRANOutcomeParameters | Maximum no. of parameters in RAN Control Outcome supported by RAN Function. The value is <*255*> |

#### 9.2.2.6 RAN Function Definition for POLICY

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of POLICY styles |  | *1.. <maxnoofRICStyles>* |  |  |
| >RIC Policy Style Type | M |  | 9.3.3 |  |
| >RIC Policy Style Name | M |  | 9.3.4 |  |
| >Supported RIC Event Trigger Style Type | M |  | 9.3.3 |  |
| >Sequence of Policy Actions |  | *0.. <**maxnoofPolicyAction>* |  |  |
| >>Policy Action ID | M |  | 9.3.6 |  |
| >>Policy Action Name | M |  | 9.3.7 |  |
| >>RIC Action Definition Format Type | M |  | 9.3.5 |  |
| >>Sequence of Associated RAN Parameters for Policy Action |  | *0.. <maxnoofAssociatedRANParameters>* |  | Only included if RAN parameters for the Policy action of the corresponding Policy style and Policy Action ID are supported |
| >>>RAN Parameter ID | M |  | 9.3.8 |  |
| >>>RAN Parameter Name | M |  | 9.3.9 |  |
| >>>RAN Parameter Definition | O |  | 9.3.51 | To define the parameter along with its constituent parameters, if any (for a structure), and itemized members, if any (for a list).  If not included for the RAN Parameter ID of a STRUCTURE type or a LIST type, then all the constituent RAN parameters under this RAN Parameter ID are assumed to be supported. |
| >>Sequence of Associated RAN Parameters for Policy Condition |  | *0.. <maxnoofAssociatedRANParameters>* |  | Only included if RAN parameters for the Policy condition of the corresponding Policy style and Policy Action ID are supported |
| >>>RAN Parameter ID | M |  | 9.3.8 |  |
| >>>RAN Parameter Name | M |  | 9.3.9 |  |
| >>>RAN Parameter Definition | O |  | 9.3.51 | To define the parameter along with its constituent parameters, if any (for a structure), and itemized members, if any (for a list).  If not included for the RAN Parameter ID of a STRUCTURE type or a LIST type, then all the constituent RAN parameters under this RAN Parameter ID are assumed to be supported. |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofRICstyles | Maximum no. of styles supported by RAN Function. The value is <*63*>. |
| maxnoofPolicyAction | Maximum no. of Policy actions supported by RAN Function. The value is <*65535*>. |
| maxnoofAssociatedRANParameters | Maximum no. of RAN parameters supported by RAN Function. The value is <*65535*>. |

## 9.3 Information Element definitions

### 9.3.1 General

When specifying information elements which are to be represented by bit strings, if not otherwise specifically stated in the semantics description of the concerned IE or elsewhere, the following principle applies with regards to the ordering of bits:

- The first bit (leftmost bit) contains the most significant bit (MSB);

- The last bit (rightmost bit) contains the least significant bit (LSB);

- When importing bit strings from other specifications, the first bit of the bit string contains the first bit of the concerned information.

### 9.3.2 RAN Function Name

This IE is defined in [4] clause 6.2.2.1.

### 9.3.3 RIC Style Type

This IE is defined in [4] clause 6.2.2.2.

### 9.3.4 RIC Style Name

This IE is defined in [4] clause 6.2.2.3.

### 9.3.5 RIC Format Type

This IE is defined in [4] clause 6.2.2.4.

### 9.3.6 Control Action ID

This IE uniquely identifies an action of a given RIC Control style.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Control Action ID | M |  | INTEGER (1.. 65535, …) |  |

### 9.3.7 Control Action Name

This IE defines the name of a given control action.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Control Action Name | M |  | PrintableString(SIZE(1.. 150, ...)) |  |

### 9.3.8 RAN Parameter ID

This IE uniquely identifies a specific RAN parameter of a given RIC Control style.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| RAN Parameter ID | M |  | INTEGER (1.. 4294967295, …) |  |

### 9.3.9 RAN Parameter Name

This IE defines the name of a given RAN parameter.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| RAN Parameter Name | M |  | PrintableString(SIZE(1.. 150, ...)) |  |

### 9.3.10 UE ID

This IE is defined in [4] clause 6.2.2.6.

### 9.3.11 RAN Parameter Value Type

This IE specifies the RAN parameters controlled by the RIC. The parameters can be individual elements, or structures containing constituent elements or a list of structures. The parameters and their types are given in Section 8.4.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **CHOICE** *RAN Parameter Value Type* | M |  |  | A RAN Parameter can either be an ELEMENT or a STRUCTURE or a LIST. |
| ***>ELEMENT with Key Flag TRUE*** |  |  |  | If the RAN parameter is singular variable and if it is a key parameter with key flag set to TRUE as in Section 8. |
| >>RAN Parameter Value | M |  | 9.3.14 | This IE must be filled for both INSERT and CONTROL if the key flag is TRUE so as to reference the proper structure within the list. |
| ***>ELEMENT with Key Flag FALSE*** |  |  |  | If the RAN parameter is singular variable and if it is NOT a key parameter (key flag set to FALSE). as in Section 8. |
| >>RAN Parameter Value | C-ifControl |  | 9.3.14 | This IE must be filled if this structure is part of a RIC Control Request message; else, if it is part of a RIC Indication message, this IE is optional. |
| ***>STRUCTURE*** |  |  |  | If the RAN parameter is a structure, in turn containing a set of RAN parameters. |
| >>RAN Parameter Structure | M |  | 9.3.12 |  |
| ***>LIST*** |  |  |  | If the RAN parameter is a list containing individual items, each of which has an index. |
| >>RAN Parameter List | M |  | 9.3.13 |  |

|  |  |
| --- | --- |
| Condition | Explanation |
| ifControl | This IE shall be present if it is part of a RIC Control Request message. Otherwise, it is optional. |

### 9.3.12 RAN Parameter Structure

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of RAN Parameters |  | *0..<maxnoofParametersinStructure>* |  | The size must be at least 1 in the case of CONTROL. |
| >RAN Parameter ID | M |  | 9.3.8 |  |
| >RAN Parameter Value Type | M |  | 9.3.11 | Each parameter in the structure can in turn be an individual ELEMENT or another STRUCTURE or a LIST |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofParametersinStructure | Maximum no. of RAN parameters supported in a structure. The value is <*65535*>. |

### 9.3.13 RAN Parameter List

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| List of RAN Parameter Structures |  | *0..<maxnoofItemsinList>* |  | The size must be at least 1 in the case of CONTROL |
| >RAN Parameter ID | M |  | 9.3.8 |  |
| >RAN Parameter Structure | M |  | 9.3.12 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofItemsinList | Maximum no. of RAN parameters supported in a structure. The value is <*65535*>. |

### 9.3.14 RAN Parameter Value

This IE defines the target value type for a RAN parameter ELEMENT.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **CHOICE** *RAN Parameter Value* | M |  |  |  |
| >BOOLEAN |  |  | BOOLEAN |  |
| >INTEGER |  |  | INTEGER |  |
| >REAL |  |  | REAL |  |
| >BIT STRING |  |  | BIT STRING |  |
| >OCTET STRING |  |  | OCTET STRING |  |
| >PrintableString |  |  | PrintableString |  |

### 9.3.15 Call Process Type ID

This IE uniquely identifies a call Process Type for a call process breakpoint event trigger.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Call Process Type ID | M |  | INTEGER (1.. 65535, …) |  |

### 9.3.16 Insert Indication ID

This IE uniquely identifies an action of a given RIC Control style.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Insert Indication ID | M |  | INTEGER (1.. 65535, …) |  |

### 9.3.17 Insert Indication Name

This IE defines the name of a given control action.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Insert Indication Name | M |  | PrintableString(SIZE(1.. 150, ...)) |  |

### 9.3.18 RAN Call Process ID

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Call Process ID |  |  | INTEGER (1.. 4294967295, …) | To be used to match an INSERT Indication request with a following CONTROL action |

### 9.3.19 Call Process Type Name

This IE defines the name of a given call Process Type.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Call Process Type Name | M |  | PrintableString (SIZE(1..150, …)) |  |

### 9.3.20 Policy Action

This IE defines the *Policy Action* IE

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Policy Action ID | M |  | 9.3.6 | Combined with RIC Style to define Policy type |
| Sequence of RAN Parameters |  | *0..<maxnoofAssociatedRANParameters>* |  |  |
| >RAN Parameter ID | M |  | 9.3.8 |  |
| >RAN Parameter Value Type | M |  | 9.3.11 |  |
| RIC Policy decision | O |  | ENUMERATED (accept, reject, …) | Used to indicate accept or reject a RRM function as Policy Action |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofAssociatedRANParameters | Maximum no. of RAN Parameter types in action definition supported by RAN Function. Value is <*65535*>. |

9.3.21 Event Trigger Condition ID

This IE defines an identifier for event trigger conditions configured for a specific Event Trigger style.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Event Trigger Condition ID | M |  | INTEGER (1..65535, …) |  |

9.3.22 Event Trigger ID for UE

This IE defines an identifier for a specific UE related condition configured for event triggering.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Event Trigger ID for UE | M |  | INTEGER (1..65535, …) |  |

9.3.23 Event Trigger ID for UE Event

This IE defines an identifier for a specific UE event configured for event triggering.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Event Trigger ID for UE Event | M |  | INTEGER (1..65535, …) |  |

9.3.24 Event Trigger ID for Cell

This IE defines an identifier for a specific cell related condition configured for event triggering.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Event Trigger ID for Cell | M |  | INTEGER (1..65535, …) |  |

### 9.3.25 Logical OR

This IE indicates a logical ("and” or “or”) connection of the current condition to the next condition in a given sequence of conditions.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Logical OR | M |  | ENUMERATED (true, false, …) | If set to “true”, logical connection to the next condition is “or”. Otherwise, “and”. |

### 9.3.26 Event Trigger UE Information

This IE defines a set of applicable UEs for event triggering.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of Associated UE Information |  | *1..<maxnoofUEInfo>* |  |  |
| >Event Trigger UE ID | M |  | 9.3.22 |  |
| >**CHOICE** *UE Type* |  |  |  |  |
| ***>>Individual UE*** |  |  |  |  |
| >>>UE ID | M |  | 9.3.10 |  |
| >>>RAN Parameter Testing for Individual UE | O |  | 9.3.29 | To test a set of RAN Parameter conditions for a given UE. RAN Parameters defined in Section 8.1.3 shall be used. |
| ***>>UE Group*** |  |  |  |  |
| >>>RAN Parameter Testing for UE Group | M |  | 9.3.29 | To test a set of RAN Parameter conditions for defining a given UE group RAN Parameters defined in Section 8.1.3 shall be used. |
| >Logical OR | O |  | 9.3.25 |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofUEInfo | Maximum number of UE information in a given E2 node for which event trigger can be defined. The value is *<65535>* |

### 9.3.27 Event Trigger Cell Information

This IE defines a set of applicable cells for event triggering.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of Associated Cell Information |  | *1..<maxnoofCellInfo>* |  |  |
| >Event Trigger Cell ID | M |  | 9.3.24 |  |
| >**CHOICE** *Cell Type* | M |  |  |  |
| ***>>Individual Cell*** |  |  |  |  |
| >>>Cell Global ID | M |  | 9.3.36 |  |
| ***>>Cell Group*** |  |  |  |  |
| >>>RAN Parameter Testing for Cell Group | M |  | 9.3.29 | To test a set of RAN Parameter conditions for defining a given Cell group RAN Parameters defined in Section 8.1.4 shall be used. |
| >Logical OR | O |  | 9.3.25 |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofCellInfo | Maximum number of cells in a given E2 node for which event trigger can be defined. The value is *<65535>* |

### 9.3.28 Event Trigger UE Event Information

This IE defines a set of UE events for event triggering.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Sequence of UE Event for Event Triggering |  | *1..<maxnoofUEeventInfo>* |  |  |
| >UE Event ID | M |  | 9.3.23 | UE Events defined in Section 8.1.5 shall be used. |
| >Logical OR | O |  | 9.3.25 |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofUEeventInfo | Maximum number of UE Event information in a given E2 node for which event trigger can be defined. The value is *<65535>* |

### 9.3.29 RAN Parameter Conditional Criteria Definition

This IE defines the generic test conditions based on RAN parameters.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | **IE type and reference** | **Semantics description** |
| Sequence of RAN Parameter Testings |  | *1..<maxnoofRANparamTest>* |  |  |
| >RAN Parameter Testing | M |  | 9.3.30 |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofRANparamTest | Maximum no. of RAN Parameter Testing. Value is <*255*> |

### 9.3.30 RAN Parameter Test

This IE defines a set of test conditions for RAN parameters nested under a given RAN parameter through recursions. Only “ELEMENT” type of RAN parameter with Key Flag set to “False” is tested.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| RAN Parameter ID | M |  | 9.3.9 |  |
| **CHOICE** *RAN Parameter Type* | M |  |  | A RAN Parameter can either be an ELEMENT or a STRUCTURE or a LIST. An ELEMENT type RAN Parameter is with Key Flag set to either “True” or “False”. |
| ***>LIST*** |  |  |  |  |
| >>List of RAN Parameter Structures |  | *1*..*<maxnoofItemsinList>* |  |  |
| >>>RAN Parameter Testing | M |  | 9.3.30 |  |
| ***>STRUCTURE*** |  |  |  |  |
| >>Sequence of RAN Parameters |  | *1..<maxnoofParametersinStructure>* |  |  |
| >>>RAN Parameter Testing | M |  | 9.3.30 |  |
| ***>ELEMENT with Key Flag True*** |  |  |  |  |
| >>RAN Parameter Value | M |  | 9.3.14 |  |
| ***>ELEMENT with Key Flag False*** |  |  |  |  |
| >>RAN Parameter Test Condition | M |  | 9.3.31 |  |
| >>RAN Parameter Value | O |  | 9.3.14 |  |
| >>Logical OR | O |  | 9.3.25 |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofItemsinList | Maximum no. of RAN parameters supported in a structure. The value is <65535>. |
| maxnoofParametersinStructure | Maximum no. of RAN parameters supported in a structure. The value is <65535>. |

### 9.3.31 RAN Parameter Test Condition

This IE compares the particular value of a given RAN parameter with the target value.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| **CHOICE** *RAN Parameter Test Condition* |  |  |  |  |
| >Comparison | M |  | ENUMERATED (equal, difference, greaterthan, lessthan, contains, starts with, …) | Applies only when RAN Parameter Value is present in 9.3.30. |
| >Presence | M |  | ENUMERATED (present, configured, rollover, non-zero, …) | Applies only when RAN Parameter Value is not present in 9.3.30. |

For the choice type of “Comparison”, the test condition is Value (*RAN Parameter ID*) (*RAN Parameter Test Condition*) (*RAN Parameter Value*).

|  |  |
| --- | --- |
| **RAN Parameter Test condition** | **Test condition** |
| Equal | Value (RAN Parameter ID) = (RAN Parameter Value) |
| Difference | Value (RAN Parameter ID) <> (RAN Parameter Value) |
| Greaterthan | Value (RAN Parameter ID) => (RAN Parameter Value) |
| lessthan | Value (RAN Parameter ID) < (RAN Parameter Value) |
| contains | Value (RAN Parameter ID) contains (RAN Parameter Value) |
| Starts with | Value (RAN Parameter ID) has the same initial part as (RAN Parameter Value) |

For the choice type of “Presence”, the test condition is applied to Value (*RAN Parameter ID*)

|  |  |
| --- | --- |
| **RAN Parameter Test condition** | **Test condition** |
| present | Value (RAN Parameter ID) is defined (i.e. memory allocated) |
| configured | Value (RAN Parameter ID) has been set (i.e. not NULL) |
| rollover | Value (RAN Parameter ID) was max defined value and now 0 |
| non-zero | Value (RAN Parameter ID) <> 0 |
| Length (Value (RAN Parameter ID)) > 0 |

### 9.3.32 Network Interface Type

This IE is defined in [4] clause 6.2.2.10.

### 9.3.33 Network Interface Identifier

This IE is defined in [4] clause 6.2.2.11.

### 9.3.34 Network Interface Message ID

This IE is defined in [4] clause 6.2.2.12.

### 9.3.35 RRC Message ID

This IE is defined in [4] clause 6.2.2.13.

### 9.3.36 Cell Global ID

This IE is defined in [4] clause 6.2.2.5.

### 9.3.37 RRC State

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| RRC State | M |  | ENUMERATED (RRC\_Connected, RRC\_Inactive, RRC\_Idle, Any, …) | Value ‘any’ indicates RRC state shall be any of the values in the enumeration. |

### 9.3.38 Neighbour Relation Information

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Serving Cell PCI | M |  | 9.3.39 |  |
| Serving Cell ARFCN | M |  | 9.3.40 | DL Frequency Info for FDD Mode. |
| Neighbour Cell List |  | *1..<maxnoofNeighbourCell>* |  |  |
| >**CHOICE** *RAN Type* | M |  |  |  |
| ***>>NR*** | M |  |  |  |
| >>>NR CGI | M |  | 9.3.41 |  |
| >>>NR PCI | M |  | 9.3.42 |  |
| >>>5GS TAC | M |  | 9.3.43 |  |
| >>>NR Mode Info | M |  | ENUMERATED (FDD, TDD, …) |  |
| >>>NR Frequency Info | M |  | 9.3.44 | DL Frequency Info for FDD Mode.  NR Frequency Info IE in TS 38.473 9.3.1.17 |
| >>>Xn X2 Established | M |  | ENUMERATED (True, False, …) | Value “True” shall indicate that Xn or X2 Interface Setup with the neighbour is successful. |
| >>>HO Validated | M |  | ENUMERATED (True, False, …) | Value “True” if at least one successful HO is executed with the neighbour. |
| >>>Version | M |  | INTEGER  (1..65535, …) | For every neighbour information, the value is incremented by 1. When there is a change in the existing neighbour information, a new incremented version number is used. The deleted neighbours are not sent. |
| ***>>E-UTRA*** | M |  |  |  |
| >>>E-UTRA CGI | M |  | 9.3.45 |  |
| >>>E-UTRA PCI | M |  | 9.3.46 |  |
| >>>E-UTRA ARFCN | M |  | 9.3.47 |  |
| >>>E-UTRA TAC | M |  | 9.3.48 |  |
| >>>Xn X2 Established | M |  | ENUMERATED (True, False, …) | Value “True” shall indicate that Xn or X2 Interface Setup with the neighbour is successful. |
| >>>HO Validated | M |  | ENUMERATED (True, False, …) | Value “True” if at least one successful HO is executed with this neighbour. |
| >>>Version | M |  | INTEGER (1..65535, …) | For every neighbour information, the value is incremented by 1. When there is a change in the existing neighbour information, a new incremented version number is used. The deleted neighbours are not sent. |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofNeighbourCell | Maximum no. of Neighbour Cell information per Serving cell. The value is <65535>. |

### 9.3.39 Serving Cell PCI

This IE is defined in [4] clause 6.2.2.14.

### 9.3.40 Serving Cell ARFCN

This IE is defined in [4] clause 6.2.2.15.

### 9.3.41 NR CGI

This IE is defined in [4] clause 6.2.3.7.

### 9.3.42 NR PCI

This IE is defined in [4] clause 6.2.3.29.

### 9.3.43 NR TAC

This IE is defined in [4] clause 6.2.3.31.

### 9.3.44 NR Frequency Info

This IE is defined in [4] clause 6.2.3.36.

### 9.3.45 E-UTRA CGI

This IE is defined in [4] clause 6.2.3.11.

### 9.3.46 E-UTRA PCI

This IE is defined in [4] clause 6.2.3.32.

### 9.3.47 E-UTRA TAC

This IE is defined in [4] clause 6.2.3.34.

### 9.3.48 E-UTRA ARFCN

This IE is defined in [4] clause 6.2.3.33.

### 9.3.49 Call Process Breakpoint ID

This IE uniquely identifies a call Process breakpoint for a given call process type.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Call Process Breakpoint ID | M |  | INTEGER (1.. 65535, …) |  |

### 9.3.50 Call Process Breakpoint Name

This IE defines the name of a given call Process breakpoint.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Call Process Breakpoint Name | M |  | PrintableString (SIZE(1..150, …)) |  |

### 9.3.51 RAN Parameter Definition

This IE specifies the definition of a RAN parameter that can be controlled by the RIC when the RAN parameter is of a STRUCTURE type or a LIST type. The parameters and their types are given in Section 8.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **CHOICE** *RAN Parameter Type* | M |  |  | A RAN Parameter can either be a LIST or a STRUCTURE. |
| ***>LIST*** |  |  |  |  |
| >>List of RAN Parameter |  | *1..<maxnoofItemsinList>* |  |  |
| >>>RAN Parameter ID | M |  | 9.3.8 |  |
| >>>RAN Parameter Name | M |  | 9.3.9 | This IE shall be ignored when included in RIC SUBSCRIPTION REQUEST message. |
| >>>RAN Parameter Definition | O |  | 9.3.51 | If not included for the RAN Parameter ID of a STRUCTURE type or a LIST type, then all the itemized RAN parameters under this RAN Parameter ID are assumed to be supported.  Shall not be included If the RAN Parameter ID is of an ELEMENT type. |
| ***>STRUCTURE*** |  |  |  |  |
| >>Sequence of RAN Parameters |  | *1..<maxnoofParametersinStructure>* |  |  |
| >>>RAN Parameter ID | M |  | 9.3.8 |  |
| >>>RAN Parameter Name | M |  | 9.3.9 | This IE shall be ignored when included in RIC SUBSCRIPTION REQUEST message. |
| >>>RAN Parameter Definition | O |  | 9.3.51 | If not included for the RAN Parameter ID of a STRUCTURE type or a LIST type, then all the itemized RAN parameters under this RAN Parameter ID are assumed to be supported.  Shall not be included If the RAN Parameter ID is of an ELEMENT type. |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofItemsinList | Maximum no. of RAN parameters supported in a list. The value is <*65535*>. |
| maxnoofParametersinStructure | Maximum no. of RAN parameters supported in a structure. The value is <*65535*>. |

## 9.4 Information Element Abstract Syntax (with ASN.1)

### 9.4.1 General

E2SM-RC ASN.1 definition conforms to ITU-T Rec. X.680 [5] and ITU-T Rec. X.681 [6].

Sub clause 9.4.2 presents the Abstract Syntax of the E2SM information elements to be carried within the E2AP [3] protocol messages with ASN.1. In case there is contradiction between the ASN.1 definition in this sub clause and the tabular format in sub clause 9.2 and 9.3, the ASN.1 shall take precedence, except for the definition of conditions for the presence of conditional elements, in which the tabular format shall take precedence.

If an E2SM information element carried as an OCTET STRING in an E2AP [3] message that is not constructed as defined above is received, this shall be considered as Abstract Syntax Error, and the message shall be handled as defined for Abstract Syntax Error in clause 9.

### 9.4.2 Information Element Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- E2SM-RC Information Element Definitions

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E2SM-RC-IEs {

iso(1) identified-organization(3) dod(6) internet(1) private(4) enterprise(1) oran(53148) e2(1) version1(1) e2sm(2) e2sm-RC-IEs (3)}

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

#### -- E2SM Common IEs

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

CGI,

E-UTRA-ARFCN,

EUTRA-CGI,

E-UTRA-PCI,

E-UTRA-TAC,

FiveGS-TAC,

InterfaceIdentifier,

InterfaceType,

Interface-MessageID,

NRFrequencyInfo,

NR-CGI,

NR-PCI,

RANfunction-Name,

RIC-Format-Type,

RIC-Style-Name,

RIC-Style-Type,

RRC-MessageID,

ServingCell-ARFCN,

ServingCell-PCI,

UEID

FROM E2SM-COMMON-IEs;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

#### -- CONSTANTS

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxnoofMessages INTEGER ::= 65535

maxnoofE2InfoChanges INTEGER ::= 65535

maxnoofUEInfoChanges INTEGER ::= 65535

maxnoofRRCstate INTEGER ::= 8

maxnoofParametersToReport INTEGER ::= 65535

maxnoofPolicyConditions INTEGER ::= 65535

maxnoofAssociatedRANParameters INTEGER ::= 65535

maxnoofUEID INTEGER ::= 65535

maxnoofCellID INTEGER ::= 65535

maxnoofRANOutcomeParameters INTEGER ::= 255

maxnoofParametersinStructure INTEGER ::= 65535

maxnoofItemsinList INTEGER ::= 65535

maxnoofUEInfo INTEGER ::= 65535

maxnoofCellInfo INTEGER ::= 65535

maxnoofUEeventInfo INTEGER ::= 65535

maxnoofRANparamTest INTEGER ::= 255

maxnoofNeighbourCell INTEGER ::= 65535

maxnoofRICStyles INTEGER ::= 63

maxnoofCallProcessTypes INTEGER ::= 65535

maxnoofCallProcessBreakpoints INTEGER ::= 65535

maxnoofInsertIndication INTEGER ::= 65535

maxnoofControlAction INTEGER ::= 65535

maxnoofPolicyAction INTEGER ::= 65535

maxnoofInsertIndicationActions INTEGER ::= 63

maxnoofMulCtrlActions INTEGER ::= 63

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

#### -- IEs

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

LogicalOR ::= ENUMERATED {true, false, ...}

NeighborCell-List ::= SEQUENCE (SIZE(1..maxnoofNeighbourCell)) OF NeighborCell-Item

NeighborCell-Item ::= CHOICE {

ranType-Choice-NR NeighborCell-Item-Choice-NR,

ranType-Choice-EUTRA NeighborCell-Item-Choice-E-UTRA,

...

}

NeighborCell-Item-Choice-NR ::= SEQUENCE {

nR-CGI NR-CGI,

nR-PCI NR-PCI,

fiveGS-TAC FiveGS-TAC,

nR-mode-info ENUMERATED {fdd, tdd, ...},

nR-FreqInfo NRFrequencyInfo,

x2-Xn-established ENUMERATED {true, false, ...},

hO-validated ENUMERATED {true, false, ...},

version INTEGER (1..65535, ...),

...

}

NeighborCell-Item-Choice-E-UTRA ::= SEQUENCE {

eUTRA-CGI EUTRA-CGI,

eUTRA-PCI E-UTRA-PCI,

eUTRA-ARFCN E-UTRA-ARFCN,

eUTRA-TAC E-UTRA-TAC,

x2-Xn-established ENUMERATED {true, false, ...},

hO-validated ENUMERATED {true, false, ...},

version INTEGER (1..65535, ...),

...

}

NeighborRelation-Info ::= SEQUENCE {

servingCellPCI ServingCell-PCI,

servingCellARFCN ServingCell-ARFCN,

neighborCell-List NeighborCell-List,

...

}

RRC-State ::= ENUMERATED {rrc-connected, rrc-inactive, rrc-idle, any, ...}

-------------------------------

#### -- Event Trigger related IEs

-------------------------------

EventTrigger-Cell-Info ::= SEQUENCE {

cellInfo-List SEQUENCE (SIZE(1..maxnoofCellInfo)) OF EventTrigger-Cell-Info-Item,

...

}

EventTrigger-Cell-Info-Item ::= SEQUENCE {

eventTriggerCellID RIC-EventTrigger-Cell-ID,

cellType CHOICE {

cellType-Choice-Individual EventTrigger-Cell-Info-Item-Choice-Individual,

cellType-Choice-Group EventTrigger-Cell-Info-Item-Choice-Group,

...

},

logicalOR LogicalOR OPTIONAL,

...

}

EventTrigger-Cell-Info-Item-Choice-Individual ::= SEQUENCE {

cellGlobalID CGI,

...

}

EventTrigger-Cell-Info-Item-Choice-Group ::= SEQUENCE {

ranParameterTesting RANParameter-Testing,

...

}

EventTrigger-UE-Info ::= SEQUENCE {

ueInfo-List SEQUENCE (SIZE(1..maxnoofUEInfo)) OF EventTrigger-UE-Info-Item,

...

}

EventTrigger-UE-Info-Item ::= SEQUENCE {

eventTriggerUEID RIC-EventTrigger-UE-ID,

ueType CHOICE {

ueType-Choice-Individual EventTrigger-UE-Info-Item-Choice-Individual,

ueType-Choice-Group EventTrigger-UE-Info-Item-Choice-Group,

...

},

logicalOR LogicalOR OPTIONAL,

...

}

EventTrigger-UE-Info-Item-Choice-Individual ::= SEQUENCE {

ueID UEID,

ranParameterTesting RANParameter-Testing OPTIONAL,

...

}

EventTrigger-UE-Info-Item-Choice-Group ::= SEQUENCE {

ranParameterTesting RANParameter-Testing,

...

}

EventTrigger-UEevent-Info ::= SEQUENCE {

ueEvent-List SEQUENCE (SIZE(1..maxnoofUEeventInfo)) OF EventTrigger-UEevent-Info-Item,

...

}

EventTrigger-UEevent-Info-Item ::= SEQUENCE {

ueEventID RIC-EventTrigger-UEevent-ID,

logicalOR LogicalOR OPTIONAL,

...

}

-------------------------------

#### -- RAN Parameter related IEs

-------------------------------

RANParameter-ID ::= INTEGER (1..4294967295, ...)

RANParameter-Name ::= PrintableString (SIZE(1..150, ...))

RANParameter-Definition ::= SEQUENCE {

ranParameter-Definition-Choice RANParameter-Definition-Choice,

...

}

RANParameter-Definition-Choice ::= CHOICE {

choiceLIST RANParameter-Definition-Choice-LIST,

choiceSTRUCTURE RANParameter-Definition-Choice-STRUCTURE,

...

}

RANParameter-Definition-Choice-LIST ::= SEQUENCE {

ranParameter-List SEQUENCE (SIZE(1..maxnoofItemsinList)) OF RANParameter-Definition-Choice-LIST-Item,

...

}

RANParameter-Definition-Choice-LIST-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-name RANParameter-Name,

ranParameter-Definition RANParameter-Definition OPTIONAL,

...

}

RANParameter-Definition-Choice-STRUCTURE ::= SEQUENCE {

ranParameter-STRUCTURE SEQUENCE (SIZE(1..maxnoofParametersinStructure)) OF RANParameter-Definition-Choice-STRUCTURE-Item,

...

}

RANParameter-Definition-Choice-STRUCTURE-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-name RANParameter-Name,

ranParameter-Definition RANParameter-Definition OPTIONAL,

...

}

RANParameter-Value ::= CHOICE {

valueBoolean BOOLEAN,

valueInt INTEGER,

valueReal REAL,

valueBitS BIT STRING,

valueOctS OCTET STRING,

valuePrintableString PrintableString,

...

}

RANParameter-ValueType ::= CHOICE {

ranP-Choice-ElementTrue RANParameter-ValueType-Choice-ElementTrue,

ranP-Choice-ElementFalse RANParameter-ValueType-Choice-ElementFalse,

ranP-Choice-Structure RANParameter-ValueType-Choice-Structure,

ranP-Choice-List RANParameter-ValueType-Choice-List,

...

}

RANParameter-ValueType-Choice-ElementTrue ::= SEQUENCE {

ranParameter-value RANParameter-Value,

...

}

RANParameter-ValueType-Choice-ElementFalse ::= SEQUENCE {

ranParameter-value RANParameter-Value OPTIONAL,

-- C-ifControl: This IE shall be present if it is part of a RIC Control Request message. Otherwise it is optional.

...

}

RANParameter-ValueType-Choice-Structure ::= SEQUENCE {

ranParameter-Structure RANParameter-STRUCTURE,

...

}

RANParameter-ValueType-Choice-List ::= SEQUENCE {

ranParameter-List RANParameter-LIST,

...

}

RANParameter-STRUCTURE ::= SEQUENCE {

sequence-of-ranParameters SEQUENCE (SIZE(1..maxnoofParametersinStructure)) OF RANParameter-STRUCTURE-Item OPTIONAL,

...

}

RANParameter-STRUCTURE-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-valueType RANParameter-ValueType,

...

}

RANParameter-LIST ::= SEQUENCE {

list-of-ranParameter SEQUENCE (SIZE(1..maxnoofItemsinList)) OF RANParameter-STRUCTURE,

...

}

RANParameter-Testing ::= SEQUENCE (SIZE(1..maxnoofRANparamTest)) OF RANParameter-Testing-Item

RANParameter-TestingCondition ::= CHOICE {

ranP-Choice-comparison ENUMERATED {equal, difference, greaterthan, lessthan, contains, starts-with, ...},

ranP-Choice-presence ENUMERATED {present, configured, rollover, non-zero, ...},

...

}

RANParameter-Testing-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-Type CHOICE {

ranP-Choice-List RANParameter-Testing-Item-Choice-List,

ranP-Choice-Structure RANParameter-Testing-Item-Choice-Structure,

ranP-Choice-ElementTrue RANParameter-Testing-Item-Choice-ElementTrue,

ranP-Choice-ElementFalse RANParameter-Testing-Item-Choice-ElementFalse,

...

},

...

}

RANParameter-Testing-Item-Choice-List ::= SEQUENCE {

ranParameter-List RANParameter-Testing-LIST,

...

}

RANParameter-Testing-Item-Choice-Structure ::= SEQUENCE {

ranParameter-Structure RANParameter-Testing-STRUCTURE,

...

}

RANParameter-Testing-Item-Choice-ElementTrue ::= SEQUENCE {

ranParameter-value RANParameter-Value,

...

}

RANParameter-Testing-Item-Choice-ElementFalse ::= SEQUENCE {

ranParameter-TestCondition RANParameter-TestingCondition,

ranParameter-Value RANParameter-Value OPTIONAL,

logicalOR LogicalOR OPTIONAL,

...

}

RANParameter-Testing-LIST ::= SEQUENCE (SIZE(1..maxnoofItemsinList)) OF RANParameter-Testing-Item

RANParameter-Testing-STRUCTURE ::= SEQUENCE (SIZE(1..maxnoofParametersinStructure)) OF RANParameter-Testing-Item

----------------------------

#### -- RIC Service related IEs

----------------------------

RAN-CallProcess-ID ::= INTEGER (1..4294967295, ...)

RIC-CallProcessType-ID ::= INTEGER (1..65535, ...)

RIC-CallProcessType-Name ::= PrintableString (SIZE(1..150, ...))

RIC-CallProcessBreakpoint-ID ::= INTEGER (1..65535, ...)

RIC-CallProcessBreakpoint-Name ::= PrintableString (SIZE(1..150, ...))

RIC-ControlAction-ID ::= INTEGER (1..65535, ...)

RIC-ControlAction-Name ::= PrintableString (SIZE(1..150, ...))

RIC-EventTriggerCondition-ID ::= INTEGER (1..65535, ...)

RIC-EventTrigger-UE-ID ::= INTEGER (1..65535, ...)

RIC-EventTrigger-UEevent-ID ::= INTEGER (1..65535, ...)

RIC-EventTrigger-Cell-ID ::= INTEGER (1..65535, ...)

RIC-InsertIndication-ID ::= INTEGER (1..65535, ...)

RIC-InsertIndication-Name ::= PrintableString (SIZE(1..150, ...))

RIC-PolicyAction ::= SEQUENCE {

ric-PolicyAction-ID RIC-ControlAction-ID,

ranParameters-List SEQUENCE (SIZE(1..maxnoofAssociatedRANParameters)) OF RIC-PolicyAction-RANParameter-Item OPTIONAL,

...,

ric-PolicyDecision ENUMERATED {accept, reject, ...} OPTIONAL

}

RIC-PolicyAction-RANParameter-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-valueType RANParameter-ValueType,

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

#### -- E2SM-RC Service Model IEs

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- Event Trigger OCTET STRING contents

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E2SM-RC-EventTrigger ::= SEQUENCE {

ric-eventTrigger-formats CHOICE {

eventTrigger-Format1 E2SM-RC-EventTrigger-Format1,

eventTrigger-Format2 E2SM-RC-EventTrigger-Format2,

eventTrigger-Format3 E2SM-RC-EventTrigger-Format3,

eventTrigger-Format4 E2SM-RC-EventTrigger-Format4,

eventTrigger-Format5 E2SM-RC-EventTrigger-Format5,

...

},

...

}

E2SM-RC-EventTrigger-Format1 ::= SEQUENCE {

message-List SEQUENCE (SIZE(1..maxnoofMessages)) OF E2SM-RC-EventTrigger-Format1-Item,

globalAssociatedUEInfo EventTrigger-UE-Info OPTIONAL,

...

}

E2SM-RC-EventTrigger-Format1-Item ::= SEQUENCE {

ric-eventTriggerCondition-ID RIC-EventTriggerCondition-ID,

messageType MessageType-Choice,

messageDirection ENUMERATED {incoming, outgoing, ...} OPTIONAL,

associatedUEInfo EventTrigger-UE-Info OPTIONAL,

associatedUEEvent EventTrigger-UEevent-Info OPTIONAL,

logicalOR LogicalOR OPTIONAL,

...

}

MessageType-Choice ::= CHOICE {

messageType-Choice-NI MessageType-Choice-NI,

messageType-Choice-RRC MessageType-Choice-RRC,

...

}

MessageType-Choice-NI ::= SEQUENCE {

nI-Type InterfaceType,

nI-Identifier InterfaceIdentifier OPTIONAL,

nI-Message Interface-MessageID OPTIONAL,

...

}

MessageType-Choice-RRC ::= SEQUENCE {

rRC-Message RRC-MessageID,

...

}

E2SM-RC-EventTrigger-Format2 ::= SEQUENCE {

ric-callProcessType-ID RIC-CallProcessType-ID,

ric-callProcessBreakpoint-ID RIC-CallProcessBreakpoint-ID,

associatedE2NodeInfo RANParameter-Testing OPTIONAL,

associatedUEInfo EventTrigger-UE-Info OPTIONAL,

...

}

E2SM-RC-EventTrigger-Format3 ::= SEQUENCE {

e2NodeInfoChange-List SEQUENCE (SIZE(1..maxnoofE2InfoChanges)) OF E2SM-RC-EventTrigger-Format3-Item,

...

}

E2SM-RC-EventTrigger-Format3-Item ::= SEQUENCE {

ric-eventTriggerCondition-ID RIC-EventTriggerCondition-ID,

e2NodeInfoChange-ID INTEGER (1..512, ...),

associatedCellInfo EventTrigger-Cell-Info OPTIONAL,

logicalOR LogicalOR OPTIONAL,

...

}

E2SM-RC-EventTrigger-Format4 ::= SEQUENCE {

uEInfoChange-List SEQUENCE (SIZE(1..maxnoofUEInfoChanges)) OF E2SM-RC-EventTrigger-Format4-Item,

...

}

E2SM-RC-EventTrigger-Format4-Item ::= SEQUENCE {

ric-eventTriggerCondition-ID RIC-EventTriggerCondition-ID,

triggerType TriggerType-Choice,

associatedUEInfo EventTrigger-UE-Info OPTIONAL,

logicalOR LogicalOR OPTIONAL,

...

}

TriggerType-Choice ::= CHOICE {

triggerType-Choice-RRCstate TriggerType-Choice-RRCstate,

triggerType-Choice-UEID TriggerType-Choice-UEID,

triggerType-Choice-L2state TriggerType-Choice-L2state,

...

}

TriggerType-Choice-RRCstate ::= SEQUENCE {

rrcState-List SEQUENCE (SIZE(1..maxnoofRRCstate)) OF TriggerType-Choice-RRCstate-Item,

...

}

TriggerType-Choice-RRCstate-Item ::= SEQUENCE {

stateChangedTo RRC-State,

logicalOR LogicalOR OPTIONAL,

...

}

TriggerType-Choice-UEID ::= SEQUENCE {

ueIDchange-ID INTEGER (1..512, ...),

...

}

TriggerType-Choice-L2state ::= SEQUENCE {

associatedL2variables RANParameter-Testing,

...

}

E2SM-RC-EventTrigger-Format5 ::= SEQUENCE {

onDemand ENUMERATED {true, ...},

associatedUEInfo EventTrigger-UE-Info OPTIONAL,

associatedCellInfo EventTrigger-Cell-Info OPTIONAL,

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- Action Definition OCTET STRING contents

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E2SM-RC-ActionDefinition ::= SEQUENCE {

ric-Style-Type RIC-Style-Type,

ric-actionDefinition-formats CHOICE {

actionDefinition-Format1 E2SM-RC-ActionDefinition-Format1,

actionDefinition-Format2 E2SM-RC-ActionDefinition-Format2,

actionDefinition-Format3 E2SM-RC-ActionDefinition-Format3,

...,

actionDefinition-Format4 E2SM-RC-ActionDefinition-Format4

},

...

}

E2SM-RC-ActionDefinition-Format1 ::= SEQUENCE {

ranP-ToBeReported-List SEQUENCE (SIZE(1..maxnoofParametersToReport)) OF E2SM-RC-ActionDefinition-Format1-Item,

...

}

E2SM-RC-ActionDefinition-Format1-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

...,

ranParameter-Definition RANParameter-Definition OPTIONAL

}

E2SM-RC-ActionDefinition-Format2 ::= SEQUENCE {

ric-PolicyConditions-List SEQUENCE (SIZE(1..maxnoofPolicyConditions)) OF E2SM-RC-ActionDefinition-Format2-Item,

...

}

E2SM-RC-ActionDefinition-Format2-Item ::= SEQUENCE {

ric-PolicyAction RIC-PolicyAction,

ric-PolicyConditionDefinition RANParameter-Testing OPTIONAL,

...

}

E2SM-RC-ActionDefinition-Format3 ::= SEQUENCE {

ric-InsertIndication-ID RIC-InsertIndication-ID,

ranP-InsertIndication-List SEQUENCE (SIZE(1..maxnoofAssociatedRANParameters)) OF E2SM-RC-ActionDefinition-Format3-Item,

ueID UEID OPTIONAL,

...

}

E2SM-RC-ActionDefinition-Format3-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

...,

ranParameter-Definition RANParameter-Definition OPTIONAL

}

E2SM-RC-ActionDefinition-Format4 ::= SEQUENCE {

ric-InsertStyle-List SEQUENCE (SIZE(1.. maxnoofRICStyles)) OF E2SM-RC-ActionDefinition-Format4-Style-Item,

ueID UEID OPTIONAL,

...

}

E2SM-RC-ActionDefinition-Format4-Style-Item ::= SEQUENCE {

requested-Insert-Style-Type RIC-Style-Type,

ric-InsertIndication-List SEQUENCE (SIZE(1..maxnoofInsertIndicationActions)) OF E2SM-RC-ActionDefinition-Format4-Indication-Item,

...

}

E2SM-RC-ActionDefinition-Format4-Indication-Item ::= SEQUENCE {

ric-InsertIndication-ID RIC-InsertIndication-ID,

ranP-InsertIndication-List SEQUENCE (SIZE(1..maxnoofAssociatedRANParameters)) OF E2SM-RC-ActionDefinition-Format4-RANP-Item,

...

}

E2SM-RC-ActionDefinition-Format4-RANP-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

...,

ranParameter-Definition RANParameter-Definition OPTIONAL

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- Indication Header OCTET STRING contents

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E2SM-RC-IndicationHeader ::= SEQUENCE {

ric-indicationHeader-formats CHOICE {

indicationHeader-Format1 E2SM-RC-IndicationHeader-Format1,

indicationHeader-Format2 E2SM-RC-IndicationHeader-Format2,

...,

indicationHeader-Format3 E2SM-RC-IndicationHeader-Format3

},

...

}

E2SM-RC-IndicationHeader-Format1 ::= SEQUENCE {

ric-eventTriggerCondition-ID RIC-EventTriggerCondition-ID OPTIONAL,

...

}

E2SM-RC-IndicationHeader-Format2 ::= SEQUENCE {

ueID UEID,

ric-InsertStyle-Type RIC-Style-Type,

ric-InsertIndication-ID RIC-InsertIndication-ID,

...

}

E2SM-RC-IndicationHeader-Format3 ::= SEQUENCE {

ric-eventTriggerCondition-ID RIC-EventTriggerCondition-ID OPTIONAL,

ueID UEID OPTIONAL,

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- Indication Message OCTET STRING contents

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E2SM-RC-IndicationMessage ::= SEQUENCE {

ric-indicationMessage-formats CHOICE {

indicationMessage-Format1 E2SM-RC-IndicationMessage-Format1,

indicationMessage-Format2 E2SM-RC-IndicationMessage-Format2,

indicationMessage-Format3 E2SM-RC-IndicationMessage-Format3,

indicationMessage-Format4 E2SM-RC-IndicationMessage-Format4,

indicationMessage-Format5 E2SM-RC-IndicationMessage-Format5,

...,

indicationMessage-Format6 E2SM-RC-IndicationMessage-Format6

},

...

}

E2SM-RC-IndicationMessage-Format1 ::= SEQUENCE {

ranP-Reported-List SEQUENCE (SIZE(1..maxnoofAssociatedRANParameters)) OF E2SM-RC-IndicationMessage-Format1-Item,

...

}

E2SM-RC-IndicationMessage-Format1-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-valueType RANParameter-ValueType,

...

}

E2SM-RC-IndicationMessage-Format2 ::= SEQUENCE {

ueParameter-List SEQUENCE (SIZE(1..maxnoofUEID)) OF E2SM-RC-IndicationMessage-Format2-Item,

...

}

E2SM-RC-IndicationMessage-Format2-Item ::= SEQUENCE {

ueID UEID,

ranP-List SEQUENCE (SIZE(1..maxnoofAssociatedRANParameters)) OF E2SM-RC-IndicationMessage-Format2-RANParameter-Item,

...

}

E2SM-RC-IndicationMessage-Format2-RANParameter-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-valueType RANParameter-ValueType,

...

}

E2SM-RC-IndicationMessage-Format3 ::= SEQUENCE {

cellInfo-List SEQUENCE (SIZE(1..maxnoofCellID)) OF E2SM-RC-IndicationMessage-Format3-Item,

...

}

E2SM-RC-IndicationMessage-Format3-Item ::= SEQUENCE {

cellGlobal-ID CGI,

cellContextInfo OCTET STRING OPTIONAL,

cellDeleted BOOLEAN OPTIONAL,

neighborRelation-Table NeighborRelation-Info OPTIONAL,

...

}

E2SM-RC-IndicationMessage-Format4 ::= SEQUENCE {

ueInfo-List SEQUENCE (SIZE(0..maxnoofUEID)) OF E2SM-RC-IndicationMessage-Format4-ItemUE,

cellInfo-List SEQUENCE (SIZE(0..maxnoofCellID)) OF E2SM-RC-IndicationMessage-Format4-ItemCell,

...

}

E2SM-RC-IndicationMessage-Format4-ItemUE ::= SEQUENCE {

ueID UEID,

ueContextInfo OCTET STRING OPTIONAL,

cellGlobal-ID CGI,

...

}

E2SM-RC-IndicationMessage-Format4-ItemCell ::= SEQUENCE {

cellGlobal-ID CGI,

cellContextInfo OCTET STRING OPTIONAL,

neighborRelation-Table NeighborRelation-Info OPTIONAL,

...

}

E2SM-RC-IndicationMessage-Format5 ::= SEQUENCE{

ranP-Requested-List SEQUENCE (SIZE(0..maxnoofAssociatedRANParameters)) OF E2SM-RC-IndicationMessage-Format5-Item,

...

}

E2SM-RC-IndicationMessage-Format5-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-valueType RANParameter-ValueType,

...

}

E2SM-RC-IndicationMessage-Format6 ::= SEQUENCE {

ric-InsertStyle-List SEQUENCE (SIZE(1.. maxnoofRICStyles)) OF E2SM-RC-IndicationMessage-Format6-Style-Item,

...

}

E2SM-RC-IndicationMessage-Format6-Style-Item ::= SEQUENCE {

indicated-Insert-Style-Type RIC-Style-Type,

ric-InsertIndication-List SEQUENCE (SIZE(1..maxnoofInsertIndicationActions)) OF E2SM-RC-IndicationMessage-Format6-Indication-Item,

...

}

E2SM-RC-IndicationMessage-Format6-Indication-Item ::= SEQUENCE {

ric-InsertIndication-ID RIC-InsertIndication-ID,

ranP-InsertIndication-List SEQUENCE (SIZE(0..maxnoofAssociatedRANParameters)) OF E2SM-RC-IndicationMessage-Format6-RANP-Item ,

...

}

E2SM-RC-IndicationMessage-Format6-RANP-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-valueType RANParameter-ValueType,

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- Call Process ID OCTET STRING contents

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E2SM-RC-CallProcessID ::= SEQUENCE {

ric-callProcessID-formats CHOICE {

callProcessID-Format1 E2SM-RC-CallProcessID-Format1,

...

},

...

}

E2SM-RC-CallProcessID-Format1 ::= SEQUENCE {

ric-callProcess-ID RAN-CallProcess-ID,

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- Control Header OCTET STRING contents

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E2SM-RC-ControlHeader ::= SEQUENCE {

ric-controlHeader-formats CHOICE {

controlHeader-Format1 E2SM-RC-ControlHeader-Format1,

...,

controlHeader-Format2 E2SM-RC-ControlHeader-Format2

},

...

}

E2SM-RC-ControlHeader-Format1 ::= SEQUENCE {

ueID UEID,

ric-Style-Type RIC-Style-Type,

ric-ControlAction-ID RIC-ControlAction-ID,

ric-ControlDecision ENUMERATED {accept, reject, ...} OPTIONAL,

...

}

E2SM-RC-ControlHeader-Format2 ::= SEQUENCE {

ueID UEID OPTIONAL,

ric-ControlDecision ENUMERATED {accept, reject, ...} OPTIONAL,

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- Control Message OCTET STRING contents

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E2SM-RC-ControlMessage ::= SEQUENCE {

ric-controlMessage-formats CHOICE {

controlMessage-Format1 E2SM-RC-ControlMessage-Format1,

...,

controlMessage-Format2 E2SM-RC-ControlMessage-Format2

},

...

}

E2SM-RC-ControlMessage-Format1 ::= SEQUENCE {

ranP-List SEQUENCE (SIZE(0..maxnoofAssociatedRANParameters)) OF E2SM-RC-ControlMessage-Format1-Item,

...

}

E2SM-RC-ControlMessage-Format1-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-valueType RANParameter-ValueType,

...

}

E2SM-RC-ControlMessage-Format2 ::= SEQUENCE {

ric-ControlStyle-List SEQUENCE (SIZE(1.. maxnoofRICStyles)) OF E2SM-RC-ControlMessage-Format2-Style-Item,

...

}

E2SM-RC-ControlMessage-Format2-Style-Item ::= SEQUENCE {

indicated-Control-Style-Type RIC-Style-Type,

ric-ControlAction-List SEQUENCE (SIZE(1..maxnoofMulCtrlActions)) OF E2SM-RC-ControlMessage-Format2-ControlAction-Item,

...

}

E2SM-RC-ControlMessage-Format2-ControlAction-Item ::= SEQUENCE {

ric-ControlAction-ID RIC-ControlAction-ID,

ranP-List E2SM-RC-ControlMessage-Format1,

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- Control Outcome OCTET STRING contents

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E2SM-RC-ControlOutcome ::= SEQUENCE {

ric-controlOutcome-formats CHOICE {

controlOutcome-Format1 E2SM-RC-ControlOutcome-Format1,

...,

controlOutcome-Format2 E2SM-RC-ControlOutcome-Format2,

controlOutcome-Format3 E2SM-RC-ControlOutcome-Format3 },

...

}

E2SM-RC-ControlOutcome-Format1 ::= SEQUENCE {

ranP-List SEQUENCE (SIZE(0..maxnoofRANOutcomeParameters)) OF E2SM-RC-ControlOutcome-Format1-Item,

...

}

E2SM-RC-ControlOutcome-Format1-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-value RANParameter-Value,

...

}

E2SM-RC-ControlOutcome-Format2 ::= SEQUENCE {

ric-ControlStyle-List SEQUENCE (SIZE(1.. maxnoofRICStyles)) OF E2SM-RC-ControlOutcome-Format2-Style-Item,

...

}

E2SM-RC-ControlOutcome-Format2-Style-Item ::= SEQUENCE {

indicated-Control-Style-Type RIC-Style-Type,

ric-ControlOutcome-List SEQUENCE (SIZE(1..maxnoofMulCtrlActions)) OF E2SM-RC-ControlOutcome-Format2-ControlOutcome-Item,

...

}

E2SM-RC-ControlOutcome-Format2-ControlOutcome-Item ::= SEQUENCE {

ric-ControlAction-ID RIC-ControlAction-ID,

ranP-List SEQUENCE (SIZE(1..maxnoofAssociatedRANParameters)) OF E2SM-RC-ControlOutcome-Format2-RANP-Item,

...

}

E2SM-RC-ControlOutcome-Format2-RANP-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-value RANParameter-Value,

...

}

E2SM-RC-ControlOutcome-Format3 ::= SEQUENCE {

ranP-List SEQUENCE (SIZE(0..maxnoofRANOutcomeParameters)) OF E2SM-RC-ControlOutcome-Format3-Item,

...

}

E2SM-RC-ControlOutcome-Format3-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-valueType RANParameter-ValueType,

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- RAN Function Definition IEs

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E2SM-RC-RANFunctionDefinition ::= SEQUENCE{

ranFunction-Name RANfunction-Name,

ranFunctionDefinition-EventTrigger RANFunctionDefinition-EventTrigger OPTIONAL,

ranFunctionDefinition-Report RANFunctionDefinition-Report OPTIONAL,

ranFunctionDefinition-Insert RANFunctionDefinition-Insert OPTIONAL,

ranFunctionDefinition-Control RANFunctionDefinition-Control OPTIONAL,

ranFunctionDefinition-Policy RANFunctionDefinition-Policy OPTIONAL,

...

}

-------------------------------

-- Event Trigger

-------------------------------

RANFunctionDefinition-EventTrigger ::= SEQUENCE {

ric-EventTriggerStyle-List SEQUENCE (SIZE(1..maxnoofRICStyles)) OF RANFunctionDefinition-EventTrigger-Style-Item,

ran-L2Parameters-List SEQUENCE (SIZE(1..maxnoofAssociatedRANParameters)) OF L2Parameters-RANParameter-Item OPTIONAL,

ran-CallProcessTypes-List SEQUENCE (SIZE(1..maxnoofCallProcessTypes)) OF RANFunctionDefinition-EventTrigger-CallProcess-Item OPTIONAL,

ran-UEIdentificationParameters-List SEQUENCE (SIZE(1..maxnoofAssociatedRANParameters)) OF UEIdentification-RANParameter-Item OPTIONAL,

ran-CellIdentificationParameters-List SEQUENCE (SIZE(1..maxnoofAssociatedRANParameters)) OF CellIdentification-RANParameter-Item OPTIONAL,

...

}

RANFunctionDefinition-EventTrigger-Style-Item ::= SEQUENCE {

ric-EventTriggerStyle-Type RIC-Style-Type,

ric-EventTriggerStyle-Name RIC-Style-Name,

ric-EventTriggerFormat-Type RIC-Format-Type,

...

}

L2Parameters-RANParameter-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-name RANParameter-Name,

...,

ranParameter-Definition RANParameter-Definition OPTIONAL

}

UEIdentification-RANParameter-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-name RANParameter-Name,

...,

ranParameter-Definition RANParameter-Definition OPTIONAL

}

CellIdentification-RANParameter-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-name RANParameter-Name,

...,

ranParameter-Definition RANParameter-Definition OPTIONAL

}

RANFunctionDefinition-EventTrigger-CallProcess-Item ::= SEQUENCE {

callProcessType-ID RIC-CallProcessType-ID,

callProcessType-Name RIC-CallProcessType-Name,

callProcessBreakpoints-List SEQUENCE (SIZE (1..maxnoofCallProcessBreakpoints)) OF RANFunctionDefinition-EventTrigger-Breakpoint-Item,

...

}

RANFunctionDefinition-EventTrigger-Breakpoint-Item ::= SEQUENCE {

callProcessBreakpoint-ID RIC-CallProcessBreakpoint-ID,

callProcessBreakpoint-Name RIC-CallProcessBreakpoint-Name,

ran-CallProcessBreakpointParameters-List SEQUENCE (SIZE (1..maxnoofAssociatedRANParameters)) OF CallProcessBreakpoint-RANParameter-Item OPTIONAL,

...

}

CallProcessBreakpoint-RANParameter-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-name RANParameter-Name,

...,

ranParameter-Definition RANParameter-Definition OPTIONAL

}

-------------------------------

-- Report

-------------------------------

RANFunctionDefinition-Report ::= SEQUENCE {

ric-ReportStyle-List SEQUENCE (SIZE(1..maxnoofRICStyles)) OF RANFunctionDefinition-Report-Item,

...

}

RANFunctionDefinition-Report-Item ::= SEQUENCE {

ric-ReportStyle-Type RIC-Style-Type,

ric-ReportStyle-Name RIC-Style-Name,

ric-SupportedEventTriggerStyle-Type RIC-Style-Type,

ric-ReportActionFormat-Type RIC-Format-Type,

ric-IndicationHeaderFormat-Type RIC-Format-Type,

ric-IndicationMessageFormat-Type RIC-Format-Type,

ran-ReportParameters-List SEQUENCE (SIZE (1..maxnoofAssociatedRANParameters)) OF Report-RANParameter-Item OPTIONAL,

...

}

Report-RANParameter-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-name RANParameter-Name,

...,

ranParameter-Definition RANParameter-Definition OPTIONAL

}

-------------------------------

-- Insert

-------------------------------

RANFunctionDefinition-Insert ::= SEQUENCE {

ric-InsertStyle-List SEQUENCE (SIZE(1..maxnoofRICStyles)) OF RANFunctionDefinition-Insert-Item,

...

}

RANFunctionDefinition-Insert-Item ::= SEQUENCE {

ric-InsertStyle-Type RIC-Style-Type,

ric-InsertStyle-Name RIC-Style-Name,

ric-SupportedEventTriggerStyle-Type RIC-Style-Type,

ric-ActionDefinitionFormat-Type RIC-Format-Type,

ric-InsertIndication-List SEQUENCE (SIZE(1..maxnoofInsertIndication)) OF RANFunctionDefinition-Insert-Indication-Item OPTIONAL,

ric-IndicationHeaderFormat-Type RIC-Format-Type,

ric-IndicationMessageFormat-Type RIC-Format-Type,

ric-CallProcessIDFormat-Type RIC-Format-Type,

...

}

RANFunctionDefinition-Insert-Indication-Item ::= SEQUENCE {

ric-InsertIndication-ID RIC-InsertIndication-ID,

ric-InsertIndication-Name RIC-InsertIndication-Name,

ran-InsertIndicationParameters-List SEQUENCE (SIZE (1..maxnoofAssociatedRANParameters)) OF InsertIndication-RANParameter-Item OPTIONAL,

...

}

InsertIndication-RANParameter-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-name RANParameter-Name,

...,

ranParameter-Definition RANParameter-Definition OPTIONAL

}

-------------------------------

-- Control

-------------------------------

RANFunctionDefinition-Control ::= SEQUENCE {

ric-ControlStyle-List SEQUENCE (SIZE(1..maxnoofRICStyles)) OF RANFunctionDefinition-Control-Item,

...

}

RANFunctionDefinition-Control-Item ::= SEQUENCE {

ric-ControlStyle-Type RIC-Style-Type,

ric-ControlStyle-Name RIC-Style-Name,

ric-ControlAction-List SEQUENCE (SIZE(1..maxnoofControlAction)) OF RANFunctionDefinition-Control-Action-Item OPTIONAL,

ric-ControlHeaderFormat-Type RIC-Format-Type,

ric-ControlMessageFormat-Type RIC-Format-Type,

ric-CallProcessIDFormat-Type RIC-Format-Type OPTIONAL,

ric-ControlOutcomeFormat-Type RIC-Format-Type,

ran-ControlOutcomeParameters-List SEQUENCE (SIZE(1..maxnoofRANOutcomeParameters)) OF ControlOutcome-RANParameter-Item OPTIONAL,

...

}

ControlOutcome-RANParameter-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-name RANParameter-Name,

...,

ranParameter-Definition RANParameter-Definition OPTIONAL

}

RANFunctionDefinition-Control-Action-Item ::= SEQUENCE {

ric-ControlAction-ID RIC-ControlAction-ID,

ric-ControlAction-Name RIC-ControlAction-Name,

ran-ControlActionParameters-List SEQUENCE (SIZE (1..maxnoofAssociatedRANParameters)) OF ControlAction-RANParameter-Item OPTIONAL,

...

}

ControlAction-RANParameter-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-name RANParameter-Name,

...,

ranParameter-Definition RANParameter-Definition OPTIONAL

}

-------------------------------

-- Policy

-------------------------------

RANFunctionDefinition-Policy ::= SEQUENCE {

ric-PolicyStyle-List SEQUENCE (SIZE(1..maxnoofRICStyles)) OF RANFunctionDefinition-Policy-Item,

...

}

RANFunctionDefinition-Policy-Item ::= SEQUENCE {

ric-PolicyStyle-Type RIC-Style-Type,

ric-PolicyStyle-Name RIC-Style-Name,

ric-SupportedEventTriggerStyle-Type RIC-Style-Type,

ric-PolicyAction-List SEQUENCE (SIZE(1..maxnoofPolicyAction)) OF RANFunctionDefinition-Policy-Action-Item OPTIONAL,

...

}

RANFunctionDefinition-Policy-Action-Item ::= SEQUENCE {

ric-PolicyAction-ID RIC-ControlAction-ID,

ric-PolicyAction-Name RIC-ControlAction-Name,

ric-ActionDefinitionFormat-Type RIC-Format-Type,

ran-PolicyActionParameters-List SEQUENCE (SIZE (1..maxnoofAssociatedRANParameters)) OF PolicyAction-RANParameter-Item OPTIONAL,

ran-PolicyConditionParameters-List SEQUENCE (SIZE (1..maxnoofAssociatedRANParameters)) OF PolicyCondition-RANParameter-Item OPTIONAL,

...

}

PolicyAction-RANParameter-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-name RANParameter-Name,

...,

ranParameter-Definition RANParameter-Definition OPTIONAL

}

PolicyCondition-RANParameter-Item ::= SEQUENCE {

ranParameter-ID RANParameter-ID,

ranParameter-name RANParameter-Name,

...,

ranParameter-Definition RANParameter-Definition OPTIONAL

}

END

-- ASN1STOP

## 9.5 Message transfer syntax

E2SM-RC shall use the ASN.1 Basic Packed Encoding Rules (BASIC-PER) Aligned Variant as transfer syntax, as specified in ITU-T Rec. X.691 [9].

# 10 Handling of Unknown, Unforeseen and Erroneous Protocol Data

Section 10 of TS 36.413 [13] is applicable for the purposes of the present document.

# Annex A: Examples on IE Contents

## A.1 Introduction

This annex presents example applications of selected use cases showing alternative solutions using different combinations of RIC Services Report, Insert, Control and/or Policy.

## A.2 Connected mode mobility based on UE measurement report

### A.2.1 Assumptions

This example is based on the following assumptions:

1 O-CU-CP, or gNB for aggregated deployments, has E2 interface to Near-RT RIC and supports one or more RIC services using E2SM-RC.

2 UE is in RRC CONNECTED state using NR access and has successfully attached to a 5G Core Network (5GC)

3 UE has been previously configured to send RRC Measurement Reports.

4 UE sends a RRC Measurement Report containing one or more neighbour cell measurements applicable for an inter-cell connected mode mobility event (i.e. a Handover)

5 O-CU-CP, or gNB for aggregated deployments, uses one or more RIC Services to complete the handover decision and either execute handover (i.e. using procedure described in 3GPP 38.300 section 9.2.3) or ignores measurement report.

Step 5 may be realized using one or more of the following solutions:

i) According to a previously established RIC Subscription procedure, the arrival of the RRC Measurement Report triggers an Event Trigger which results in the E2 Node suspending the ongoing call process and sending a RIC Service INSERT message to the Near-RT RIC. The Near-RT RIC takes the Handover Decision and sends a RIC Service CONTROL message carrying the response which is used by the E2 node to resume the call process.

ii) According to a previously established RIC Subscription procedure the arrival of the RRC Measurement Report triggers an Event Trigger which results in the E2 Node executing a RIC Service POLICY which is used to modify the default Handover Decision and so modifies the remaining steps in the ongoing call process.

### A.2.2 Solution using RIC Services Insert and Control

Editor’s Note: FFS

### A.2.3 Solution using RIC Service Policy ("Offset" based approach)

This section provides a solution for the Connected Mode Mobility event call flow using the RIC Service Policy using the “Offset” approach. Corresponding example message content are provided for the *RIC Event Trigger Definition* IE and *RIC Action Definition* IE contents for the Connected Mode Mobility service (Policy Style 3) sent from the RIC to the E2 node to establish a policy used to provide guidance for the handling of incoming RRC Measurement reports from a UE connected to a 5GC network using Standalone (SA) access.

#### A2.3.1 Assumptions

This example is based on the following design assumptions:

1 Event trigger defined using Style 2 (Call Process Breakpoint), Type 3 (Mobility Management) and Id 1 (handover Preparation) with the assumption that this breakpoint corresponds to the point of the UE call process code in a gNB where a handover decision is to be taken based on a received RRC Measurement report.

a. *Event Trigger Definition* IE RAN parameters for *Associated E2 Node Info* IE are not used

b. *Event Trigger Definition* IE RAN parameters for *Associated UE Info* IE are used to offer filtering of UE between those subject to Policy handling and those to be handled using default parameters. In this example RAN parameters for discrimination based on Slice and Group (aka SPID) are described.

2 Policy defined using Style 3 (Connected Mobile Mobility), Policy Action ID 1 (Policy for Handover control)

a. *Policy Condition Definition* IE RAN parameters used to map UE to an appropriate Policy Action. In this example RAN parameters based on Serving Cell and Explicit UE List membership are described.

b. *Policy Action Definition* IE parameters used to define a set of offsets (+positive, zero or -negative values) to be applied to default measurement thresholds to calculate policy modified threshold used during Handover decision prior to Handover execution.

3 Depending upon the outcome of the decision the gNB either:

a. Proceeds with handover execution using information obtained from the measurement report, stored UE context information and result of subsequent network transactions

b. Ignores measurement report and continues any other required call processing

A picture containing text

Description automatically generated

Figure A4.1.2-1: Example call flow for Handover preparation with extensions added to implement E2 Policy service in GREEN

#### A.2.3.2 RIC Event Trigger Definition IE contents

*RIC Event Trigger Definition* IE contains RAN Parameter lists for *Associated E2 Node Info* IE and *Associated UE info* IE. In this example, only the *Associated UE info* IE is used where the set of target UEs for the event is defined by a given slice (SST=sst1, SD=sd1) and group (IRFSP=irfsp1)

Additional sets of target UEs may be supported using the same RAN Parameter list with different target values for SST, SD and IRFSP. These would be combined within the *Associated E2 Node Info* IE using the optional "Logical OR" flag (see section 9.3.26).

The contents of the *RAN Parameter Testing for UE Group* IE (defined in 8.1.3) for the above scenario are as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **Value type** | **Key flag** | **Value** | **Test condition** | **Semantics Description** |
| 10 | STRUCTURE |  |  |  | S-NSSAI |
| 11 | ELEMENT | FALSE | sst1 | equal | >SST |
| 12 | ELEMENT | FALSE | sd1 | equal | >SD |
| 20 | STRUCTURE |  |  |  | Group ID |
| 21 | ELEMENT | FALSE | Irfsp1 | equal | >IRFSP |

#### A.2.3.3 RIC Action Definition IE contents

*RIC Action Definition* IE contains RAN Parameter lists for *Policy Condition Definition* IE and *Policy Action Definition* IE.

In this example the *Policy Condition Definition* IE is used to define the set of target UEs that are to be assigned a given *Policy Action Definition* IE based on a given Serving Cell (nr-cgi1) and membership of a given Explicit UE List (HOList1). The corresponding *Policy Action Definition* IE is used to set the measurement threshold offset for A3 RSRP measurement threshold (A3-rsrp-off1)

Different values of NR-CGI and/or Explicit UE List ID may be used in each Policy condition in the *Action Definition* IE, each with a corresponding different Policy Action definition.

The contents of the *Policy Condition Definition* IE (defined using RAN parameters in sections 8.5.4 and 8.1.3) for the above scenario are as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **Value type** | **Key flag** | **Value** | **Test condition** | **Semantics Description** |
| 501 | LIST |  |  |  | List of Serving cells |
| 502 | STRUCTURE |  |  |  | >Serving cell item |
| 503 | STRUCTURE |  |  |  | >>CHOICE Serving Cell Type |
| 504 | STRUCTURE |  |  |  | >>>Serving NR Cell |
| 505 | ELEMENT | FALSE | nr-cgi1 | equal | >>>>Serving NR CGI |
| 30 | ELEMENT | FALSE | HOList1 | Equal | Explicit UE List ID |

Editor's Note:  
Section 8.1, 8.5.4 and/or 8.5.1 to be modified to support Policy condition using RAN Parameters from 8.1.3

The contents of the *Policy Action Definition* IE (defined using RAN parameters in sections 8.5.4.1.2) for the above scenario are as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **RAN Parameter ID** | **Value type** | **Key flag** | **Value** | **Semantics Description** |
| 121 | STRUCTURE |  |  | A3 Event Threshold offset |
| 122 | ELEMENT | FALSE | A3-rsrp-off1 | >A3 RSRP offset (+/- x dB) |

# Revision History

|  |  |  |
| --- | --- | --- |
| **Date** | **Revision** | **Description** |
| 2020.09.25 | 00.00.01 | Initial instantiation of E2SM-UE |
| 2020.10.30 | 00.00.01 | Change of title to E2SM-RC |
| 2020.11.04 | 00.00.00 | Agreed baseline skeleton document with title E2SM-RC (RAN Control) |
| 2021.01.20 | 01.00.01 | Running version created with inclusion of approved sections 1-5 |
| 2021.04.28 | 01.00.02 | Addition of: <NOK-2021.03.25-WG3-CR-0003-Section6.1-v04> agreed WG3#92 <NOK-2021.03.25-WG3-CR-0004-E2SM-RC-Section6.2-v04> agreed WG3#96 <NOK-2021.04.06-WG3-CR-0005-Section7-v04> agreed WG3#95 |
| 2021.05.06 | 01.00.03 | Addition of:  <RSYS-2021.04.13-WG3-D-E2SM-RC-REPORT-UEState\_CR\_v0.6> agreed WG3#96 |
| 2021.06.10 | 01.00.04 | Addition of:  <MAV.AO-2021-05-19-WG3-CR-0001-E2SM-RC+Control+Services\_v18> agreed at WG3#98  < NOK-2021.06.04-WG3-CR-0008-E2SM-RC rearrangement-v01> agreed at WG3#102  Also general editorial clean-up removing BOLD in headings, renumbering former section 8 references, adding editorial notes. |
| 2021.07.12 | 01.00.05 | Integration of Consensus CRs from Drafting Team  WG3-2021.07.09-WG3-E2SM-RC-EventTrigger-v14.docx  WG3-2021.06.17-WG3- E2SM-RC-REPORTService-v07.docx  WG3-2021.07.04.WG3-CR.E2SM-RC-Insert Control Policy Services-v17.docx |
| 2021.07.14 | 01.00.06 | Inclusion of ASN.1 and clean up |
| 2021.08.10 | 01.00 | TSC Approved |
| 2021.08.18 | 01.01.00 | V01.01 baseline including editorial corrections |
| 2021.10.13 | 01.01.01 | Incorporated WG3 Agreed CRs –   * RSYS.AO-2021.07.26-WG3-CR-0006-E2SM-RC-REPORT-CellIDInfo\_v0.6.docx – Agreed in WG3#111 * NOK.AO-2021.09.20-WG3-CR-0013-E2SM-RC-ASN1cleaning-v02.docx – Agreed in WG3#114 * CICT-2021.09.28-WG3-CR-0006-E2SM-RC-Editorial modification-v1.docx – Agreed in WG3#116 * NOK-2021.07.31-WG3-CR-0010-E2SM-RC-AnnexA-policy-v04.docx – Agreed in WG3#116 |
| 2021.11.09 | 01.01.02 | Incorporated WG3 Agreed CRs –   * MAV.AO.2021-10-19.O-RAN.WG3.E2SM-RC-v01.01.01-CR-0002 on Supported Service Style and RAN Parameter Corrections-v01.docx - Agreed in WG3#118 * RSYS.AO-2021.10.18-WG3-CR-0008-E2SM-RC-Corrections-II\_v4.docx - Agreed in WG3#119 * NOK-2021.07.31-WG3-CR-0012-E2SM-RC-Section8.5reference8.1-v04.docx - Agreed in WG3#120 |
| 2021.11.16 | 01.01.03 | Incorporated WG3 Agreed CRs –   * MAV.AO-2021.11.04.WG3-CR-0005.E2SM-RC v01.01 CR on RAN Function Definition-v06.docx |
| 2021.11.17 | 01.01.04 | Incorporated WG3 Agreed CRs –   * RSYS-2021.10.05-WG3-CR-0007-E2SM-RC-Corrections-I\_v0.2.docx - Agreed in WG3#117 * Editorial Cleanup |
| 2021.11.22 | 01.01.05 | Copyright year modified based on WG3 voting review |
| 2022.01.19 | 01.01.06 | Fixed Footer on Cover Sheet |
| 2022.02.07 | 01.01 | Final version for November 2021 publication |
| 2022.03.11 | 01.02.01 | Incorporated WG3 Agreed CRs –   * CICT.AO-2021.10.29-WG3-CR-0008-E2SM-RC-Multiple-Actions-v05.docx – Agreed in WG3#128 * RSYS.AO-2022.02.06-WG3-CR-0009-E2SM-RC-Minor Fixes\_v2.docx – Agreed in WG3#131 |
| 2022.03.24 | 01.02.02 | Incorporated WG3 Agreed CRs –   * NEC-2022.03.08-WG3-CR-0003-E2SM-RC- Wrong parameters and reference in DRB QoS Configuration -v02.docx– Agreed in WG3#136 * NOK.AO-2022.02.21-WG3-CR-0015-E2SM-RC-RAN function Definition correction-v04.docx – Agreed in WG3#136 * NOK-2022.03.14-WG3-CR-0016-E2SM-RC-RAN Parameter table corrections-v03.docx – Agreed in WG3#136 * MAV.RSYS-2022.03.09-WG3-CR-0002-E2SM-RC-Rapporteur Correction-I-v03.docx – Agreed in WG3#137 * RSYS.AO-2022.03.09-WG3-CR-0011-E2SM-RC-PolicyDecisionNewIE-v01.docx – Agreed in WG3#137 * MAV.AO-2022.03.15-WG3-CR-0009-E2SM-RC-Measurement Report Configuration-v09.docx – Agreed in WG3#137 |
| 2022.04.01 | 01.02.03 | Editorial corrections based on the comments during voting.   * Modified upper case to lower case of “Name” in ranParameter-Name in ASN.1 in L2Parameters-RANParameter-Item * Typo of Table name in 7.8 corrected * Cross Reference provided for Table names in 7.8 |
| 2022.06.29 | 01.02 | Final version for March 2022 Publication |
| 2022.07.20 | 01.02.04 | Incorporated WG3 Agreed CRs –   * NOK-2022.06.08-WG3-CR-0017-E2SM-RC-RAN Parameter ID correction-v03.docx– Agreed in WG3#154 |
| 2022.07.20 | 01.02.05 | Aligned to new Template |

# History

|  |  |  |
| --- | --- | --- |
| **Date** | **Revision** | **Description** |
| 2021.08.10 | 01.00 | TSC Approved |
| 2022.02.07 | 01.01 | Final version for November 2021 publication |
| 2022.06.29 | 01.02 | Final version for March 2022 Publication |
|  |  |  |